## NGCCOPY

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGCCOPY COPYRIGHT (C) (&00) (&01). ALL RIGHTS RESERVED

## NGCLOAD

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGCLOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## NGCSTRT

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGCSTRT Procedure '(&00)', Version '(&01)' of '(&02)' started from file '(&03)'

## NGC0A00

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A00 (&01) VERSION (&00) READY

### Meaning

End of program initialization phase.

## NGC0A01

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NGC0A01 ENTER '(&00)' STATEMENT

### Meaning

IOGEN expects a control statement.

### Response

Enter an IOGEN statement.

## NGC0A02

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A02 (&01) TERMINATED (&00)

### Meaning

The program has terminated (normally or abnormally).
(&00): NORMALLY: without errors
(PLEASE CHECK MESSAGES!): with errors

### Response

See error messages in the case of an abnormal termination.

## NGC0A03

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A03 '(&00)' GENERATED

### Meaning

The IOCGEN run has been completed; the PAM file is generated.

## NGC0A04

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A04 NUMBER OF GENERATED (&00)-UNITS : (&01)

## NGC0A11

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A11 IOGEN INTERNAL ERROR IN '(&00)'. ERROR CODE: (&01)

### Meaning

Internal function (&00) issued an error Code (&01).

### Response

Send an error notice to the diagnosis department.

## NGC0A20

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A20 '(&00)' TABLE OVERFLOW

### Meaning

Too many statements of the specified type.

### Response

Reduce the number of statements of the specified type.

## NGC0A21

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A21 MORE THAN (&00) SYSFILE STATEMENTS READ. ALL SUBSEQUENT SYSFILE STATEMENTS IGNORED

### Meaning

Too many SYSFILE statements have been issued.

## NGC0A22

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A22 (&00) STATEMENT ON WRONG PLACE. STATEMENT IS IGNORED

### Meaning

The statement cannot be accepted on this place. It is ignored.

## NGC0A29

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A29 OBSOLETE VALUE '(&03)' OF '(&02)' OPERAND IN '(&01)' STMT REPLACED BY '(&00)'

### Meaning

(&00): new value
(&01): statement
(&02): operand
(&03): specified (obsolete) value.

## NGC0A3A

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A3A NO REPLACEMENT OF FILE '(&00)' REQUESTED

### Meaning

IOGEN detected that the file (&00) exists. In the CPGOPT statement
REPLACE=N
has been specified, so the file (&00) may not be replaced.

### Response

Erase or rename the file (&00), or specify REPLACE=Y in the CPGOPT
statement.

## NGC0A30

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A30 VALUE '(&02)' OF '(&01)' OPERAND IN '(&00)' STATEMENT INVALID. (&03)

### Meaning

(&00): statement
(&01): operand
(&02): specified value
(&03): further information

### Response

Correct input.

## NGC0A31

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A31 MISSING '(&01)' OPERAND IN '(&00)' STATEMENT

### Meaning

(&00): statement
(&01): operand.

## NGC0A32

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A32 STATEMENT '(&00)' IS INVALID (&01)

### Meaning

The statement (&00) specified by the user was not a valid
IOGEN statement.

### Response

Enter a correct statement.

## NGC0A33

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A33 STATEMENT '(&00)' IS PRIVILEGED

## NGC0A34

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A34 SYNTAX ERROR IN PRECEDING STATEMENT

## NGC0A35

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A35 DUPLICATE '(&00)' STATEMENT. ONLY THE FIRST ONE WILL BE PROCESSED

## NGC0A36

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A36 MANDATORY '(&00)' STATEMENT IS MISSING

### Response

Wait for further messages.

## NGC0A37

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A37 DUPLICATE VALUE '(&02)' OF '(&01)' OPERAND IN '(&00)' STATEMENT

### Meaning

The operand (&01) has already been specified in the same or another
statement (&00).

### Response

Wait for further message.

## NGC0A38

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A38 TOO MANY '(&01)' OPERANDS IN '(&00)' STATEMENT

### Meaning

The maximum permissible number of the specified operands is restricted
and has been exceeded.
(&00): name of the erroneous IOGEN statement.
(&01): name of an operand in this statement.

### Response

Correct operand(s).

## NGC0A39

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A39 '(&02)' OPERAND INVALID IN '(&01)' STATEMENT DUE TO '(&00)'

### Response

Correct the operand, if necessary.

## NGC0A40

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A40 PRECEDING STATEMENT IS IGNORED

## NGC0A41

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A41 DEFAULT VALUE '(&00)' ASSUMED

## NGC0A42

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A42 END OF INPUT IS ASSUMED BY IOGEN

## NGC0A43

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A43 SUBSEQUENT STATEMENTS OF TYPE '(&00)' ARE IGNORED

## NGC0A44

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A44 *** IOGEN PROCESS ABORTED WITH UNDEFINED RESULT ***

### Response

Correct errors and restart IOGEN.

## NGC0A45

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A45 '(&00)' OPERAND IS IGNORED (&01)

### Response

Correct the operand, if necessary.

## NGC0A46

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A46 LOGICAL CONTROL UNIT SPEC. ERROR FOUND WHILE PROCESSING C.U.

### Meaning

IOCGEN found a specification error while building a logical control unit.
A logical control unit can have a maximum of 4 channel paths, max. 4
physical control units and max. 32 devices. Max. 256 logical control units
are allowed.

### Response

Correct unit attachments and rerun IOGEN.

## NGC0A47

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A47 MORE THAN 16 LOGICAL CONTROL UNITS ASSIGNED TO CHANNEL '(&00)'

### Meaning

IOCGEN has found more than 16 logical control units assigned to channel
mnemonic (&00). A maximum of 16 logical control units can be assigned to
one channel.

### Response

Ensure that no more than 16 logical control units are assigned to one
channel and rerun IOGEN.

## NGC0A48

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A48 ADDRESS OF DEVICE '(&00)' EXCEEDS ADDRESS RANGE OF THE CONTROL UNIT '(&01)'

### Meaning

The address of the device (&00) is outside of the valid
address range of the control unit (&01).
IOGEN stops processing.

### Response

Correct unit attachments and rerun IOGEN.

## NGC0A49

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A49 INCORRECT PAV-DEFINITION FOR DEVICE '(&00)'. REASON: '(&01)'

### Meaning

The device (&00) was defined as PAV-device without
a valid BASE-device.

### Response

Check hardware configuration.

## NGC0A50

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A50 ATTACHMENT MNEMONIC '(&00)' OF '(&01)' UNIT '(&02)' NOT DEFINED IN '(&03)' TABLE

### Meaning

(&00): attachment mnemonic
(&01): type of unit to be attached (DEVICE or CONTROLLER)
(&02): mnemonic of unit to be attached.
(&03): type of attachment unit expected (CTL or CHN).

### Response

Correct input and rerun IOGEN.

## NGC0A51

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A51 NO '(&00)' IS ATTACHED TO '(&01)' UNIT '(&02)'

### Meaning

A unit ( CHN or CTL) is defined without any unit attached to it.
(&00): type of units to be attached (CONTROLLER or DEVICE)
(&01): type of incorrectly defined unit (CHN or CTL)
(&02): mnemonic of incorrectly defined unit.

### Response

Wait for further messages.

## NGC0A52

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A52 '(&00)' UNIT '(&01)' IS IGNORED

### Meaning

The specified hardware unit is not generated into the system.
(&00): unit type (DVC, CTL or CHN)
(&01): unit mnemonic.

### Response

Correct the error, if necessary, and rerun IOGEN.

## NGC0A53

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A53 '(&00)' UNIT '(&01)' IS ATTACHED TO '(&02)' OF DIFFERENT TYPES

### Meaning

A hardware unit is attached to channels or controllers of
different types.
(&00): unit type (DEVICE or CONTROLLER)
(&01): unit mnemonic
(&02): type of attachment units (CONTROLLERS or CHANNELS).

### Response

Correct the error and rerun IOGEN.

## NGC0A54

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A54 DEVICES '(&00)' AND '(&01)' HAVE THE SAME DEVICE ADDRESS

### Meaning

(&00),(&01): device mnemonics.

### Response

Correct input and rerun IOGEN.

## NGC0A56

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A56 INCONSISTENT (&00) CONFIGURATION

### Meaning

The hardware or console configuration is inconsistent. Specific messages
have already been displayed.
(&00): HARDWARE or CONSOLE.

### Response

Correct input and rerun IOGEN.

## NGC0A57

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A57 '(&00)' UNIT '(&01)' IS ATTACHED TO '(&02)' UNIT '(&03)' OF WRONG TYPE

### Response

Correct input and rerun IOGEN.

## NGC0A58

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A58 '(&00)' UNIT '(&01)' AND '(&02)' UNIT '(&03)' ARE ATTACHED TO DIFFERENT '(&04)' UNITS

### Meaning

The (&00) unit (&01) and the (&02) unit (&03) have to be attached to
the same (&04) unit.
(&01)(&03) : mnemonics of device units
(&04) : CONTROLLER or CHANNEL or CTL/CHN.

### Response

Correct input and rerun IOGEN.

## NGC0A59

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A59 ADDRESS RANGE OVERLAP OF THE CONTROL UNITS '(&00)' AND '(&01)'

### Meaning

Conflicting address ranges were found for these control units.
Configuration may cause a hardware error.
IOGEN stops processing.

### Response

Check hardware configuration.

## NGC0A60

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A60 CONTROL UNITS '(&00)' AND '(&01)' HAVE THE SAME WWPN AT CHANNEL '(&02)'

### Meaning

(&00),(&01): controller mnemonics.
Conflicting WWPN (target-id) definitions were found for
these control units at the given channel.

### Response

Change hardware definitions and rerun IOGEN.

## NGC0A61

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A61 DEVICE ATTACHMENTS OF CONTROL UNIT '(&00)' HAVE DIFFERENT VALUES IN THE HIGHER BYTE OF THE LUN

### Meaning

(&00): controller mnemonic.
At the given control unit there exist device attachments,
for which the higher bytes of the 2-byte-LUN (logical unit
number) are not identical. This is not allowed.

### Response

Change hardware definitions and rerun IOGEN.

## NGC0A62

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A62 CONTROL UNITS '(&00)' AND '(&01)' HAVE THE SAME WWPN AND IDENTICAL VALUES IN THE HIGHER BYTE OF THE LUN OF THE ATTACHED DEVICES

### Meaning

(&00),(&01): controller mnemonics.
In case of identical WWPN definitions for two or more control
units the higher byte of the LUN of the attached devices
must be different for every control unit.

### Response

Change hardware definitions and rerun IOGEN.

## NGC0A63

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A63 DIRECT CONNECTED CONTROL UNIT '(&00)' NOT SINGLE AT CHANNEL '(&01)'

### Meaning

(&00): controller mnemonic.
(&01): channel path identifier of the channel.
The specified control unit was defined as direct connected
to a type FC channel. Additional connections to this
channel are not possible.

### Response

Change hardware definitions and rerun IOGEN.

## NGC0A64

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A64 DEVICES WITH DIFFERENT TIMEOUT REQUIREMENTS AT CONTROL UNIT '(&00)'

### Meaning

(&00): controller mnemonic.
Devices with different timeout requirements are
attached to this controller.
The parameter for the timeout handling in the
channel system is only possible on the controller
level. IOGEN sets the parameter to inhibit timeout
actions for this controller.

### Response

If possible, use separate controllers for devices
with different requirements.

## NGC0A65

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A65 TAPES COMBINED WITH DISKS AT CHANNEL '(&00)'

### Meaning

(&00): channel path identifier of the channel.
Combining tapes with disks at
a type FC channel may lead to timeout
problems in the FC protocol of the channel.

### Response

Use a separate FC channel for tape connections.

## NGC0A66

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A66 IDENTICAL LUN(S) AT CONTROLLERS '(&00)' AND '(&01)' TO CHANNEL '(&02)'

### Meaning

The named controllers are connected with the same port
(WWPN) to the same channel(s) and they have at least one
common LUN. This configuration is not possible.
IOGEN stops processing.
(&00),(&01): Mnemonics and WWPN of the controllers
(&02): CHANNEL-PATH-ID of one of the channels

### Response

Correct input and rerun IOGEN.

## NGC0A67

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A67 NOT ALLOWED COMBINATION OF DEVICES AT CONTROLLER '(&00)'

### Meaning

The mix of FAST-DPAV alias devices and other devices at the same
logical controller is not supported.

### Response

Correct hardware configuration.

## NGC0A68

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A68 NO BASE DEVICES FOR ALIAS DEVICE(S) '(&00)' AT CONTROLLER '(&01)'

### Meaning

The named alias devices shall be used for FAST-DPAV, but
there are no matching base devices. The base devices
must have identical channel connections as the alias devices
and their device numbers must be lower than those of
the alias devices.

### Response

Correct hardware configuration.

## NGC0A69

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0A69 NOT ALLOWED COMBINATION OF CONTROLLER ATTACHMENTS AT CHANNEL '(&00)'

### Meaning

The mix of direct attached controller and controller that
are attached via switch to a type FC channel is not possible.

### Response

Correct hardware configuration.

## NGC0I30

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0I30 INPUT RECORD EXCEEDS 1024 BYTES. RECORD TRUNCATED

### Response

Correct input.

## NGC0I33

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0I33 INPUT NESTING DEPTH IS '(&00)'. NO HIGHER VALUES PERMITTED

### Meaning

The nesting depth of the input files has been exceeded.

## NGC0I34

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0I34 FILE '(&00)' IS NOT CATALOGED OR EMPTY

### Meaning

An empty or non-existing file was specified in a SYSFILE statement.
(&00): name of the incorrect file.

### Response

Correct input.

## NGC0I35

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0I35 FILE '(&00)' IS IN USE

### Meaning

(&00): name of the locked file.

### Response

Rerun IOGEN later.

## NGC0I36

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0I36 FILE '(&00)' IS NOT OF TYPE ISAM/SAM

### Meaning

A file of wrong type was specified in a SYSFILE statement.
(&00): name of the incorrect file.

### Response

Correct input.

## NGC0001

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0001 ALLOCATION OF MORE MEMORY FAILED

### Meaning

Alloction of more memory by calling alloc/realloc failed

## NGC0010

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0010 INTERNAL ERROR IN CALLING MSG7X

### Meaning

MSG7X-hiding routine of IOGEN or IOCGEN reports an error
Possible are
erroneous parameterlist of hiding routine
erroneous parameterlist of MSG7X-call

## NGC0011

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NGC0011 ERROR ON SYSLST

### Meaning

Error during writing on SYSLST.

## NGC0024

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0024 IOCF GENERATOR VERSION (&00) READY

## NGC0025

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0025 (&00) GENERATED

## NGC0026

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0026 (&00) NORMALLY TERMINATED

### Meaning

The program has normally terminated.

## NGC0027

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NGC0027 IOCGEN terminated abnormally

## NGC0050

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0050 DMS ERROR ON FILE '(&00)' DURING '(&01)'. DMS ERROR CODE = (&02). ERROR INF IN SYSTEM MODE: /HELP-MESS OR /HELP (&02)

### Meaning

For more detailed information on the DMS error enter the /HELP-MESS or
/HELP command in system mode or see the manual 'System Messages',
'DMS Disk Processing', or 'DMS Tape Processing'.

## NGC0051

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0051 SYSTEM-SYNTAXFILE MODIFIED (NOT ACTIVATED)

### Meaning

SINPRC.IOGEN was called for modification (not activation) of IOGEN system
syntax file

## NGC0052

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0052 IOGEN SYSSPR FILE MODIFIED

### Meaning

SINPRC.IOGEN was called for modification of IOGEN SYSSPR file

## NGC0053

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC0053 IOGEN USER-SYNTAXFILE MODIFIED

### Meaning

SINPRC.IOGEN was called for modification of IOGEN user syntax
file

## NGC1001

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1001 ALLOCATION OF MORE MEMORY FAILED

### Meaning

Alloction of more memory by calling alloc/realloc failed

## NGC1002

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1002 STATEMENT CAN NOT BE IDENTIFIED

## NGC1003

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1003 INTERNAL IOCGEN ERROR: WRONG SIZE-SPECIFICATION IN FREE_UPD OR IN FR_INT_U

## NGC1004

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1004 END STATEMENT IS MISSING

## NGC1005

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1005 WRONG CHANNEL TYPE IS SPECIFIED

## NGC1006

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1006 CHPID IS MULTIPLE DEFINED

## NGC1007

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1007 CHANNEL CONNECTION NOT FOUND

## NGC1008

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1008 RDATA REPORTS ERROR

## NGC1009

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1009 CMPG SIZE OVERFLOW

## NGC1010

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1010 CONTROLLER MNEMONIC IS MULTIPLE DEFINED

## NGC1011

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1011 CONTROLLER CONNECTION NOT FOUND

## NGC1012

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1012 ERROR IN OPENING OF IOCF FILE

## NGC1013

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1013 ERROR IN WRITING THE IOCF FILE

## NGC1014

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1014 FIRST STATEMENT MUST BE FOR-STATEMENT

## NGC1015

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1015 CREATION OF IOCF FILE FAILED

## NGC1016

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1016 INTERNAL ERROR IN CALCULATION OF DEVICE PATHS

## NGC1017

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1017 CLOSING OF IOCF FILE FAILED

## NGC1018

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1018 OPENING OF SYSLST FAILED

## NGC1019

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1019 FOR-STATEMENT CONTAINS WRONG IOCF IDENTIFIER

## NGC1020

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1020 INT_EBC INPUT ERROR

## NGC1021

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1021 CTL LIST IS CREATED WITH ERRORS

## NGC1022

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1022 SYSTEM CALL REPORTS ERROR BY SET-FILE-LINK OF IOCF PAM-FILE

## NGC1025

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC1025 (&00) GENERATED

## NGC1026

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NGC1026 Overrun allowable IORSF length

### Meaning

The configuration is too large. Thereby the allowable length of IORSF
is overrun.

## NGC2010

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC2010 INCORRECT ORDER OF STATEMENTS

### Meaning

The order of the statements for the program is incorrect.

## NGC2011

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC2011 LOGICAL CONTROL UNIT SPEC. ERROR FOUND WHILE PROCESSING C.U.

### Meaning

IOCGEN found a specification error while building a logical control unit.
Look up the maximal values in the manual.

### Response

Correct unit attachments and rerun IOGEN.

## NGC2012

Destination: USER-TASK, CONSOLE Routing code: A Weight: 50

Warranty : NO

NGC2012 MORE THAN 16 LOGICAL CONTROL UNITS ASSIGNED TO CHANNEL '(&00)'

### Meaning

IOCGEN has found more than 16 logical control units assigned to channel
mnemonic (&00). A maximum of 16 logical control units can be assigned to
one channel.

### Response

Ensure that no more than 16 logical control units are assigned to one
channel and rerun IOGEN.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages