## HSV0001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0001 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL OBTAIN SYSTEM INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0002 ERROR DURING THE SVP FUNCTION DIAGNOSE MSSFCALL OBTAIN SIDE INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
0110 OK, Information delivered. The SIDE belongs to another
configuration.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0003 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY SIDE ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The SIDE was switched to "online".
0120 The SIDE was already "online".
0040 Hardware error.
03F0 Wrong SIDE Identifier specified.
04F0 The SIDE belongs to another configuration.
05F0 The SIDE belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0004

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0004 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY SIDE OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The SIDE was switched to "offline".
0120 The SIDE was already "offline".
0040 Hardware error.
0240 Error in the SVP.
03F0 Wrong SIDE Identifier specified.
04F0 The SIDE belongs to another configuration.
05F0 The SIDE belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
07F0 Not all elements are "offline".
08F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0005

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0005 ERROR DURING SVP FUNCTION OBTAIN CHANNEL PATH INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0006

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0006 ERROR DURING SVP FUNCTION VARY CHANNEL PATH ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The CHANNEL PATH was switched to "online".
0120 The CHANNEL PATH was already "online".
0040 Hardware error.
0140 The IOSIDE was "busy" and could not execute the function.
0240 Error in the SVP.
03F0 Wrong CHANNEL PATH Identifier specified.
04F0 The CHANNEL PATH belongs to another configuration.
05F0 The CHANNEL PATH belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
08F0 Not executable on the configuration.
0DF0 The IOSIDE is not assigned.
0400 Hardware error.
0401 The CHANNEL PATH is not installed or already "online"
or switching online is disabled.
0402 The CHANNEL CONTROLLER is not "online".
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0007 ERROR DURING SVP FUNCTION CHANNEL PATH OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The CHANNEL PATH was switched to "offline".
0120 The CHANNEL PATH was already "offline".
0040 Hardware error.
0140 The IOSIDE was "busy" and could not execute the function.
0240 Error in the SVP.
03F0 Wrong CHANNEL PATH Identifier specified.
04F0 The CHANNEL PATH belongs to another configuration.
05F0 The CHANNEL PATH belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
08F0 Not executable on the configuration.
0DF0 The IOSIDE is not assigned.
0400 Hardware error.
0401 The CHANNEL PATH is not installed or switching offline is
disabled.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0008

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0008 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL OBTAIN IOSIDE INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered. The IOSIDE is "online".
0110 OK, information delivered. The IOSIDE is "offline".
0410 OK, information delivered. The IOSIDE is the only IOSIDE.
0040 Hardware error.
0140 The IOSIDE was "busy" and could not execute the function.
03F0 Wrong IOSIDE Identifier specified.
04F0 The IOSIDE belongs to another configuration.
05F0 The IOSIDE belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0009

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0009 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY IOSIDE ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The IOSIDE was switched to "online".
0120 The IOSIDE was already "online".
0040 Hardware error.
0140 The IOSIDE was "busy" and could not execute the function.
03F0 Wrong IOSIDE Identifier specified.
04F0 The IOSIDE belongs to another configuration.
05F0 The IOSIDE belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
0DF0 The IOSIDE is not assigned.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0010 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY IOSIDE OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The IOSIDE was switched to "offline".
0120 The IOSIDE was already "offline".
0040 Hardware error.
0140 The IOSIDE was "busy" and could not execute the function.
03F0 Wrong IOSIDE Identifier specified.
04F0 The IOSIDE belongs to another configuration.
05F0 The IOSIDE belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
07F0 Not all CHANNEL PATHS are "offline".
08F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0011

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0011 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL OBTAIN STORAGE ELEMENT INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
0110 OK, information delivered. The STORAGE ELEMENT is "offline".
0040 Hardware error.
03F0 Wrong STORAGE ELEMENT Identifier specified.
04F0 The STORAGE ELEMENT belongs to another configuration.
05F0 The STORAGE ELEMENT belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0012

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0012 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL OBTAIN HIGHEST STORAGE ELEMENT ID

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
0040 Hardware error.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0013

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0013 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY STORAGE ELEMENT ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The STORAGE ELEMENT was switched to "online".
0120 The STORAGE ELEMENT was already "online".
0040 Hardware error.
03F0 Wrong STORAGE ELEMENT Identifier specified.
04F0 The STORAGE ELEMENT belongs to another configuration.
05F0 The STORAGE ELEMENT belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0014

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0014 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY STORAGE ELEMENT OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The STORAGE ELEMENT was switched to "offline".
0120 The STORAGE ELEMENT was already "offline".
0040 Hardware error.
03F0 Wrong STORAGE ELEMENT Identifier specified.
04F0 The STORAGE ELEMENT belongs to another configuration.
05F0 The STORAGE ELEMENT belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
09F0 Invalid address or address range specified.
0AF0 Inaccessible storage specified or address relocation needed
but not specified.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0015

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0015 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY STORAGE PHYSICALLY ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The storage was switched to "online".
0120 The storage was already "online".
0040 Hardware error.
04F0 The storage belongs to another configuration.
05F0 The storage belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
09F0 Invalid address or address range specified.
0CF0 All storage is currently assigned.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0016

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0016 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL VARY STORAGE PHYSICALLY OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The storage was switched to "offline".
0120 The storage was already "offline".
0040 Hardware error.
04F0 The storage belongs to another configuration.
05F0 The storage belongs to another configuration.
06F0 The SVP function is not executable on this configuration.
09F0 Invalid address or address range specified.
0AF0 Inaccessible storage specified.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0017

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0017 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL READ IOCDS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
xx20 The requested function was completed.
xx returns further information (logical OR):
80 The IOCDS was open for write. The returned data may be
invalid.
40 The IOCDS is the active IOCDS.
20 The IOCDS was updated since the last IMPL.
0040 Hardware error.
4040 Error during open or read of the IOCDS.
40F0 The IOCDS block number is invalid.
41F0 The IOCDS is not open.
42F0 Invalid IOCDS specified.
50F0 The IOCDS end was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0018

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0018 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL WRITE IOCDS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
xx20 The requested function was completed.
xx returns further information (logical OR):
80 The IOCDS was already open for write.
40 The IOCDS is the active IOCDS.
20 The IOCDS was updated since the last IMPL.
0040 Hardware error.
4040 Error during open or write of the IOCDS.
40F0 The IOCDS block number is invalid.
41F0 The IOCDS is not open.
42F0 Invalid IOCDS specified.
50F0 The IOCDS end was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0019

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0019 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL READ ACTIVE IOCDS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
xx20 The requested function was completed.
xx returns further information (logical OR):
80 The IOCDS was open for write. The returned data may be
invalid.
40 The IOCDS is the active IOCDS.
20 The IOCDS was updated since the last IMPL.
0040 Hardware error.
4040 Error during open or read of the IOCDS.
40F0 The IOCDS block number is invalid.
41F0 The IOCDS is not open.
42F0 Invalid IOCDS specified.
50F0 The IOCDS end was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0020

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0020 ERROR DURING THE SVP FUNCTION DIAGNOSE WRITE CONSOLE.

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.

## HSV0021

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0021 ERROR DURING THE SVP FUNCTION DIAGNOSE HARDWARE SUPPORT FUNCTION READ CORER INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.

## HSV0022

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0022 ERROR DURING THE SVP FUNCTION DIAGNOSE HARDWARE SUPPORT FUNCTION CLEAR CORER IN MEMORY UNIT

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.

## HSV0023

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0023 ERROR DURING SVP FUNCTION READ IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0001 The IORSF end was exceeded.
0300 Command not supported.
1101 The indicated SVP cannot operate.
1102 The IORSF number is too large.
1103 The start sector number exceeded the maximum sector of the
IORSF file.
3000 IORSF file access error.
3500 The buffer busy condition was detected.
3600 The IO-configuration is not supported or a logical error
was detected.
xx20 The requested function was completed.
xx returns further information (logical OR):
80 The IORSF was open for write. The returned data may be
invalid.
40 The IORSF is the active IORSF.
20 The IORSF was updated since the last IMPL.
0040 Hardware error.
4040 Error during open or read of the IORSF.
40F0 The IORSF block number is invalid.
41F0 The IORSF is not open.
42F0 Invalid IORSF specified.
50F0 The IORSF end was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0024

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0024 ERROR DURING SVP FUNCTION WRITE IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0001 The IORSF end was exceeded.
0300 Command not supported.
1101 The indicated SVP cannot operate.
1102 The IORSF number is too large.
1103 The start sector number exceeded the maximum sector of the
IORSF file.
3000 IORSF file access error.
3100 Write-open operation for IORSF failed.
3101 Write-close operation for IORSF failed.
3200 The IORSF is already in write-open status.
3300 The IORSF is not in write-open status.
3400 The IORSF is write-protected.
3500 The buffer busy condition was detected.
3600 The IO-configuration is not supported or a logical error
was detected.
xx20 The requested function was completed.
xx returns further information (logical OR):
80 The IORSF was already open for write.
40 The IORSF is the active IORSF.
20 The IORSF was updated since the last IMPL.
0040 Hardware error.
4040 Error during open or write of the IORSF.
40F0 The IORSF block number is invalid.
41F0 The IORSF is not open.
42F0 Invalid IORSF specified.
50F0 The IORSF end was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0025

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0025 ERROR DURING SVP FUNCTION READ ACTIVE IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0001 The IORSF end was exceeded.
1103 The start sector number exceeded the maximum sector of the
IORSF file.
3000 IORSF file access error.
xx20 The requested function was completed.
xx returns further information (logical OR):
80 The IORSF was open for write. The returned data may be
invalid.
40 The IORSF is the active IORSF.
20 The IORSF was updated since the last IMPL.
0040 Hardware error.
4040 Error during open or read of the IORSF.
40F0 The IORSF block number is invalid.
41F0 The IORSF is not open.
42F0 Invalid IORSF specified.
50F0 The IORSF end was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0026

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0026 ERROR DURING THE SVP FUNCTION GET GLOBAL CONFIGURATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
0110 Information may not be up to date.
E1F0 The GSU is in power off state.
E2F0 The GSU is offline.
E3F0 The GSU is assigned to another GCMP.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0027

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0027 ERROR DURING THE SVP FUNCTION GET GSU INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
0110 Information may not be up to date.
E1F0 The GSU is in power off state.
E2F0 The GSU is offline.
E3F0 The GSU is assigned to another GCMP.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0028

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0028 ERROR DURING THE SVP FUNCTION GET GSU FAILURE INDICATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
0110 Information may not be up to date.
E1F0 The GSU is in power off state.
E2F0 The GSU is offline.
E3F0 The GSU is assigned to another GCMP.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0029

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0029 ERROR DURING THE SVP FUNCTION RESET GSU FAILURE INDICATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 The call was executed.
E0F0 The caller has no authorization for this function.
E1F0 The GSU is in power off state.
E2F0 The GSU is offline.
E3F0 The GSU is assigned to another GCMP.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0030

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0030 ERROR DURING THE SVP FUNCTION READ HARDWARE STORAGE AREA

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 OK, information delivered.
0040 Hardware error.
4040 Error during open or read of the HSA.
41F0 The HSA-file is not open.
50F0 The end of HSA-file was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0031

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0031 ERROR DURING THE SVP FUNCTION MODIFY ACCESS BITS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 The call was executed.
0301 The caller has no authorization for this function.
1101 Number of protection blocks too large.
E0F0 The caller has no authorization for this function.
E1F0 The GSU is in power off state.
E2F0 The GSU is offline.
E3F0 The GSU is assigned to another GCMP.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0032

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0032 ERROR DURING THE SVP FUNCTION GET GLOBAL CONNECTION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0033

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0033 ERROR DURING THE SVP FUNCTION MODIFY GLOBAL CONNECTION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
11F0 The SSU could not connected in guestsystem because
SSU is not assigned to guestsystem.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0041

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0041 ERROR DURING THE SVP FUNCTION GET IPL DEVICE LIST

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0042

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0042 ERROR DURING THE SVP FUNCTION MODIFY IPL DEVICE LIST

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0043

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0043 ERROR DURING THE SVP FUNCTION CONNECT SSU

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
11F0 The SSU could not be connected in guestsystem because
SSU is not assigned to guestsystem.
1111 The SSU could not be connected because SSU is not in correct
state (neither offline nor operational).
0401 The SSU could not be connected because SSU is not available
(maybe Power Off).
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0044

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0044 ERROR DURING THE SVP FUNCTION DISCONNECT SSU

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
PARE The given SSU-number is wrong.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0045

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0045 ERROR DURING THE SVP FUNCTION CONNECT SCMP CORE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
11F0 A SSU could not connected in guestsystem because
SSU is not assigned to guestsystem.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0046

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0046 ERROR DURING THE SVP FUNCTION CONNECT LOCAL CLUSTER

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0047

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0047 ERROR DURING THE SVP FUNCTION DISCONNECT CLUSTER

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0050

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0050 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP READ IO-UNIT FROM IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0301 The caller has no authorization for this function.
1104 The specified unit type is unknown.
1105 The specified I/O unit does not exist in IORSF.
BUSY The DIAGNOSE instruction was completed with condition code 1
or 2.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0051

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0051 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP ADD IO-UNIT TO IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0301 The caller has no authorization for this function.
0421 Insufficient hardware space to store control information.
1103 No empty area to store specified I/O unit.
1104 The specified unit type is unknown.
1105 The specified I/O unit does not exist or already exist.
1106 Effective byte length is wrong.
1107 No unit to which specified i/0 unit can be connected.
1108 Condition for replacing or adding an I/O unit is not met.
1109 Replacement code or unit type not supported by hardware.
BUSY The DIAGNOSE instruction was completed with condition code 1
or 2.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0052

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0052 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP DELETE IO-UNIT FROM IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0301 The caller has no authorization for this function.
0421 Insufficient hardware space to store control information.
1103 No empty area to store specified I/O unit.
1104 The specified unit type is unknown.
1105 The specified I/O unit does not exist.
1106 Effective byte length is wrong.
1107 A lower-level unit is connected to specified I/O unit.
1108 Condition for replacing or deleting an I/O unit is not met.
1109 Replacement code or unit type not supported by hardware.
BUSY The DIAGNOSE instruction was completed with condition code 1
or 2.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0056

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0056 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP VARY SSU ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0057

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0057 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP VARY SSU OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0058

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0058 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP LOCAL CLUSTER ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0059

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0059 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP VARY CLUSTER ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0060

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0060 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP VARY CLUSTER OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0061

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0061 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP CREATE SCMP

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0062

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0062 ERROR DURING THE SVP FUNCTION DIAGNOSE RSC DR-CONTROL

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0063

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0063 ERROR DURING THE SVP FUNCTION DIAGNOSE RSC DR-RESPONSE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0064

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0064 ERROR DURING THE SVP FUNCTION DIAGNOSE READ FIRMWARE-INFO

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0069

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0069 ERROR DURING THE SVP FUNCTION DIAGNOSE DEFINE MEMORY DOMAINS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0070

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0070 ERROR DURING THE SVP FUNCTION DIAGNOSE WRITE VM DATA

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages