## TIA0101

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0101 UNRECOVERABLE ERROR WHEN REQUESTING MEMORY SPACE USING '$GETMEM'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

An error has occurred when requesting memory space using the $GETMEM
macro.

### Response

Send the system dump to the diagnostics staff.

## TIA0102

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0102 UNRECOVERABLE ERROR WHEN RELEASING MEMORY SPACE USING '$RETMEM'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

An error has occurred when releasing memory space using the $RETMEM macro.

### Response

Send the system dump to the diagnostics staff.

## TIA0103

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0103 UNRECOVERABLE BOURSE ERROR DURING '$CRLOCK' OR '$NBCREA' MACRO. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0104

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0104 UNRECOVERABLE BOURSE ERROR DURING '$GTLOCK' OR '$NBRSIG' MACRO. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0105

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0105 UNRECOVERABLE BOURSE ERROR DURING '$RLLOCK' MACRO. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0106

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0106 UNRECOVERABLE ERROR WHEN ACCESSING TCB VIA '$TANC' OR '$EZFCAN' MACRO. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0107

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0107 UNRECOVERABLE TIMER ERROR DURING '$BTIMEL' MACRO. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0108

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0108 UNRECOVERABLE SLOT ERROR DURING '$OPNSL' MACRO. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

Send the system dump to the diagnostics staff.

## TIA0111

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0111 UNRECOVERABLE ERROR DURING BCAM MACRO 'ENABAP'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0112

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0112 UNRECOVERABLE ERROR DURING BCAM MACRO 'CREDIST'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0113

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0113 UNRECOVERABLE ERROR DURING BCAM MACRO 'ACCON'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0114

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0114 UNRECOVERABLE ERROR DURING BCAM MACRO 'SENDLET'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0115

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0115 UNRECOVERABLE ERROR DURING BCAM MACRO 'RECLET'. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Response

Send the system dump to the diagnostics staff.

## TIA0121

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0121 UNRECOVERABLE ERROR DURING VTSU INITIALIZATION. TASK TERMINATED

### Meaning

An error has occurred during the VTSU call GET BLOCKLENGTH, INITIATE,
CHANGE or STATUS.
The task is terminated abnormally except if VTSU sub-system is not
created or is in delete phase.

### Response

Send the system dump to the diagnostics staff.

## TIA0122

Destination: CONSOLE Routing code: C Weight: 70

Warranty : YES

TIA0122 UNRECOVERABLE VTSU ERROR WHEN UPDATING DISPLAY TERMINAL ATTRIBUTES. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

An error has occurred during the VTSU call CHANGE.

### Response

Send the system dump to the diagnostics staff.

## TIA0123

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0123 ERROR DURING TIAM PROGRAM TERMINATION PROCESSING. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

An error has occurred during the VTSU call CHANGE while the standard
procedures for program termination were being executed.

### Response

Send the system dump to the diagnostics staff.

## TIA0124

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0124 INVALID 'APREF' OR 'CREF' IN BCAM ANNOUNCEMENT. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

The BCAM announcement contains an invalid application or connection
reference.

### Response

Send the system dump to the diagnostics staff.

## TIA0125

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0125 ILLEGAL ANNOUNCEMENT. TASK TERMINATED ABNORMALLY. TAKE SYSTEM DUMP

### Meaning

TIAM has received an illegal announcement.

### Response

Send the system dump to the diagnostics staff.

## TIA0131

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0131 ILLEGAL MESSAGETYPE IN 'NEABT' PROTOCOL. TASK TERMINATED ABNORMALLY

### Meaning

TIAM gets a message with illegal messagetype in NEABT protocol.

### Response

None.

## TIA0132

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0132 MESSAGE LENGTH < 8 BYTES. TASK TERMINATED ABNORMALLY

### Meaning

TIAM has received a message of less than 8 bytes.

## TIA0133

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0133 RECORD LENGTH < 4 BYTES. TASK TERMINATED ABNORMALLY

### Meaning

TIAM has received a record of less than 4 bytes.

## TIA0134

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0134 TIAM ERROR DURING DYNAMIC STATUS REQUEST. TASK TERMINATED.

### Meaning

Unrecoverable error during dynamic status request of the terminal.
Possible error reasons are :
- internal error
- BCAM letter lost
- negative acknowledgement
- terminal disconnected
- BCAM shortage
- error with VTSUCB
- invalid coded character set name

### Response

Check terminal/partner characteristics and build up a new connection to
the station.

## TIA0135

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0135 ERROR DETECTED BY VTSU IN CONNECTION LETTER. TASK TERMINATED ABNORMALLY

### Meaning

Error in connection letter during the VTSU call INIT BY CONNECTION LETTER
or GET BLOCK LEN WITH CONL.

## TIA0200

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0200 TERMINAL ATTRIBUTES INFORMATION NOT AVAILABLE

### Meaning

Possible errors :
- command used in batch mode
- system error detected during access of terminal attributes

### Response

Check environment and retry.

## TIA0300

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0300 $DIALOG APPLICATION CORRECTLY STARTED ON HOST (&00)

## TIA0301

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0301 $DIALOG APPLICATION TERMINATED ON HOST (&00)

## TIA0302

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0302 $DIALOG ($RBATCH) APPLICATION CANNOT BE STARTED ON HOST (&00)

### Meaning

Possible reasons :
- BCAM is not active or is in shutdown,
- Invalid/Unknown HOST-NAME specified.

## TIA0303

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0303 $DIALOG APPLICATION NOT STARTED ON HOST (&00)

## TIA0304

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0304 $DIALOG APPLICATION STILL ACTIVE ON HOST (&00)

## TIA0305

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0305 STOP OF $DIALOG APPLICATION ALREADY INITIATED ON HOST (&00)

## TIA0306

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0306 $DIALOG APPLICATION ALREADY STARTED ON HOST (&00)

## TIA0307

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0307 HOST (&00) NOT ACTIVE. START OF $DIALOG APPLICATION POSTPONED

### Meaning

Specified host has been correctly defined but is not active.
The command is postponed and will be completed if the host
is activated within 15 minutes. Otherwise, the command will
not be completed.

### Response

Activate the host with a /BCACT command

## TIA0308

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0308 $DIALOG APPLICATION ON HOST (&00) IS TERMINATING

## TIA0309

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0309 $DIALOG APPLICATION STILL STARTING ON HOST (&00)

## TIA0310

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA0310 END OF INTERACTIVE ($DIALOG) SESSION ON HOST (&00) WITHIN (&01) MINUTES

## TIA05F1

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA05F1 ERROR DURING CREATION OF TIAM AND RBAM CONTROL TASKS. NO INTERACTIVE OR REMOTE BATCH PROCESSING POSSIBLE. BCAM INITIALIZATION CONTINUES

### Meaning

The control task for the TIAM and RBAM access methods could not be
created.
No interactive or remote batch processing is possible.

### Response

Once BCAM initialization has been terminated, enter the /BCEND command.
After the BCAM termination message has been issued, restart BCAM by
entering the /DCSTART command.
If the error recurs, initiate SLED.

## TIA05F3

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA05F3 DUE TO INSUFFICIENT MEMORY SPACE NO INTERACTIVE OR REMOTE BATCH PROCESSING POSSIBLE. BCAM INITIALIZATION CONTINUES

### Meaning

A shortage of memory space has occurred during initialization of the TIAM
and RBAM data structures.

### Response

Once BCAM initialization has been terminated, enter the /BCEND command.
After the BCAM termination message has been issued, restart BCAM by
entering the /DCSTART command.
If the error recurs, initiate SLED.

## TIA05F4

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA05F4 WARNING: TIAM DATA STRUCTURE LOCKED. MEMORY SPACE HAS NOT BEEN RELEASED

### Meaning

The TIAM data structure is locked by an interactive task or the TIAM
control task and cannot be released.

### Response

If the error recurs, notify the system administrator.

## TIA050A

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA050A WARNING: 'ACKNOWLEDGE-OUTPUT' OPERAND NOT SUPPORTED BY THIS DEVICE

### Meaning

This device does not support modifications to the transport
acknowledgment.

## TIA050C

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA050C WARNING: ONLY FIRST CHARACTER OF 'SUBSTITUTE-CHARACTER' OPERAND USED

### Meaning

This message is issued in response to the terminal command
/MODIFY-TERMINAL-OPTION with the operand SUBSTITUTE-CHARACTER,
whenever more than one character has been specified for this operand.

## TIA050D

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA050D WARNING: INVALID VALUE FOR 'SUBSTITUTE-CHARACTER' OPERAND

### Meaning

This message is issued in response to the terminal command
/MODIFY-TERMINAL-OPTION with the operand SUBSTITUTE-CHARACTER,
whenever the specified replacement character is not permitted.

## TIA050E

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA050E WARNING: 'BACKSPACE' FUNCTION NOT SUPPORTED BY DEVICE

### Meaning

The 'BACKSPACE' function is only supported by printer terminals.

## TIA050F

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA050F WARNING: INVALID VALUE FOR 'BACKSPACE' FUNCTION

### Meaning

The specified character is not allowed for the BACKSPACE function.

## TIA0500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TIA0500 WARNING : COMMAND ACCEPTED BUT AT LEAST ONE PARAMETER IS IGNORED DUE TO A SYNTACTICAL OR SEMANTICAL ERROR

## TIA0501

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0501 WARNING: COMMAND ACCEPTED BUT NOT EFFECTIVE UNTIL PROGRAM RETURNS OVERFLOW CONTROL TO SYSTEM

### Meaning

The type of the overflow control has been changed.
For the moment the change has no effect because overflow is controlled
by the user program itself. The change will only be effective once
overflow control is returned to the system.

## TIA0502

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TIA0502 MISSING OR INVALID OPERAND. COMMAND NOT EXECUTED

## TIA0503

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0503 WARNING: SPECIFIED LINE LENGTH NOT WITHIN PERMITTED RANGE

### Meaning

The values 10....255 are permitted.

## TIA0504

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0504 WARNING: TIME SPECIFICATION FOR OVERFLOW CONTROL ONLY ALLOWED WITH SUBOPERAND 'TIME'. 'OVERFLOW-CONTROL' OPERAND IGNORED

## TIA0505

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0505 WARNING: OVERFLOW CONTROL NOT SUPPORTED BY DEVICE

## TIA0506

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0506 WARNING: OVERFLOW CONTROL WITH MAXIMUM NUMBER OF LINES NOT SUPPORTED BY DEVICE

### Meaning

Overflow control is not possible on this display terminal.

## TIA0507

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0507 WARNING: VALUE SPECIFIED FOR MAXIMUM LINE LENGTH NOT WITHIN PERMITTED RANGE

### Meaning

The values 3....255 are permitted.

## TIA0508

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0508 WARNING: LOGICAL END-OF-LINE CHARACTER NOT SUPPORTED BY DEVICE

## TIA0509

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0509 WARNING: WRITE/READ MODE NOT SUPPORTED BY DEVICE

### Meaning

The operating modes READ MODIFIED and READ UNPROTECTED are not supported
by this device.

## TIA0510

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0510 WARNING: INVALID CHARACTER SPECIFIED FOR LOGICAL END OF LINE

### Meaning

The logical end-of-line character specified is not printable.

## TIA0511

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0511 WARNING: ONLY FIRST CHARACTER OF OPERAND FOR END OF LINE USED

### Meaning

More than one character has been specified for the logical end of line.

## TIA0512

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0512 WARNING: ONLY ONE VALUE ALLOWED FOR OVERFLOW CONTROL

## TIA0513

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

TIA0513 WARNING: NO LOCAL HARDCOPY UNIT ASSIGNED

### Meaning

No local hardcopy unit was assigned during connection setup.

### Response

Check the PDN generation to see whether a local hardcopy unit has been
assigned and, if necessary, specify OPCH in the OPNCON command at
connection setup.

## TIA0514

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TIA0514 WARNING: INVALID CODED-CHARACTER-SET VALUE

### Meaning

Possible error situations are :
- use of 8-BIT user default on 7-BIT terminal,
- no user default coded-character-set defined,
- invalid user default coded-character-set, ...
- invalid coded-character-set,
- XHCS not available,
- coded-character-set not supported by the device,
- no 8-bit terminal

### Response

Check terminal type, used coded-character-set or user default
coded-character-set.

## TIA0515

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TIA0515 WARNING: MODIFICATION OF CODED-CHARACTER-SET NOT ALLOWED WHEN PROGRAM LOADED

## TIA0516

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TIA0516 WARNING: PROMPT CAN NOT BE MODIFIED DUE TO A TOO LOW OMNIS VERSION

### Meaning

The OMNIS version you are connected with doesn't allow to modify
prompting. The minimal required version is V8.2.

## TIA0517

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TIA0517 WARNING: INVALID SYNTAX FOR PROMPT OPERAND

### Meaning

Non printable characters are not allowed in prompts

### Response

Correct parameter(s) and reenter command

## TIA0518

Destination: USER-TASK Routing code: Weight:

Warranty : NO

TIA0518 WARNING: PROMPT OPERAND TOO LONG

### Meaning

After substitution of #P, #S, #H, #J and #U , the resulting string is too
long.

## TIA0519

Destination: USER-TASK Routing code: Weight:

Warranty : NO

TIA0519 WARNING: INVALID VTSU-B VERSION

### Meaning

The VTSU-B version on the system doesn't support some operands of the
/MODIFY-TERMINAL-OPTIONS.

## TIA0520

Destination: USER-TASK Routing code: Weight:

Warranty : NO

TIA0520 ROLL-UP NOT SUPPORTED BY DEVICE

## TIA0590

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0590 NO TIAM TASK TERMINATION PROCESSING POSSIBLE. TASK TERMINATION CONTINUES

### Meaning

The TIAM task termination cannot be processed because the TCB or terminal
entry table (TET) cannot be accessed.

## TIA0591

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

TIA0591 TIAM DATA STRUCTURE LOCKED. THIS TASK MAY BE IN A LOOP

### Meaning

It was not possible to access the TIAM data structure within 5 minutes.
Another access attempt is made.

### Response

If this message recurs for several tasks, there may be an error in the
TIAM control task. In this case the lock only can be removed by entering
the /BCEND command.

## TIA1000

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TIA1000 INTERNAL ERROR IN MODULE (&00), INTERNAL ERROR NUMBER (&01).CONTACT SYSTEM ADMINISTRATOR

### Meaning

The inserts are meant to help the systemdiagnosis.
Other diagnose information (dump and or serslog) also taken.

### Response

If present, please send the following data to the systemdiagnosis :
- error message with inserts,
- serslog files,
- systemdump,
- procedure to reproduce the problem.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages