## RBP0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0000 BS2000 REMOTE BATCH MONITORING

### Meaning

The system is ready to accept input from the remote batch terminal.
It is output after a dial-in connection is established
or after a message of job output termination.

### Response

The user may submit input to the RBP system any time
after receipt of this message.

## RBP0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0001 COMMAND ACCEPTED (&00)

### Meaning

The actual message contents is described as follows:
"R001 COMMAND ACCEPTED (command).".
This message acknowledges the acceptance and processing
of a valid batch processing
command.

## RBP0002

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

RBP0002 JOB ACCEPTED (&00)

### Meaning

The actual message contents is described as follows:
"R002 JOB ACCEPTED (jobname) (user identification) (alternate) (TSN)".
This message acknowledges the receipt of a job. The job (jobname)
submitted by the user (user identification) with optional alternate
output recipient (alternate) has
been submitted for execution.

## RBP0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0003 JOB COMPLETED (&00)

### Meaning

The actual message contents is described as follows:
"R003 JOB COMPLETED (jobname) (user identification) (alternate) (TSN)".
This message acknowledges that the batch job (jobname) submitted by the
user (user identification) with optional alternate output
recipient (alternate) has completed execution.

### Response

If "immediate" job output was requested, it will be queued to the
submitting batch terminal or central printer automatically by the
system. If "deferred" job output was requested,
the submitting or the alternate user must retrieve
the output with an ROUT command.

## RBP0004

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0004 (&00): OUTPUT AVAILABLE FOR (&01) FROM (&02)

### Meaning

The output from a job which was submitted
to a remote batch terminal (&02) "terminal identification"
is available for an inactive user (&01) "user identification".

### Response

The central operator should contact the
user and advise of pending job output.

## RBP0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0005 RLOGOFF EFFECTED BY THE SYSTEM

### Meaning

This message is issued when a batch
processing session is not terminated by an
RLOGOFF command.

## RBP0006

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0006 (&00)

### Meaning

The actual message contents is described as follows:
"R006 JOB:(jobname) (user identification) (terminal identification)
(alternate) STATUS:(status).".
This message is output in response to
the RSTATUS command. It advises the status
of a job (jobname) submitted by the user
(user identification) from the batch terminal (terminal
identification) with optional alternate output recipient
(alternate).

## RBP0007

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0007 JOB DELETED (&00)

### Meaning

The actual message contents is described as follows:
"R007 JOB DELETED (jobname) (user identification) (alternate) (TSN)".
This message is issued in response to an
ROUT command with DELETE-parameter. It advises that
a job (jobname) submitted by the (user identification)
with alternate output recipient (alternate) has been
deleted from the system.

## RBP0008

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0008 (&00)

### Meaning

The actual message contents is described as follows:
"R008 HHMM FROM:(user identification) (terminal identification)
TO:(user identification) (terminal identification) Message:(message).".
This message is generated by the RMSG
command processor. HHMM is the time
(hours-minutes) at which the /RMSG command
was accepted by the RBP system.

## RBP0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0009 FORM '(&00)' DOES NOT EXIST IN SPOOL PARAMETER FILE FOR REMOTE STATION 8415/8418

### Meaning

The FORM specified in the /PRINT-FILE or /PRINT command or in the
PRNT macro does not exist in the SPOOL parameter file for the
remote station 8415/8418.
If the form exists for a central printer the print is redirected to it.

### Response

Include the form (&00) in the SPOOL parameter file for
remote station 8415/8418.

## RBP0010

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

RBP0010 JOB REJECTED UNDEFINED ENTRY (&00)

### Meaning

The actual message contents is described as follows:
1.) "R010 JOB REJECTED UNDEFINED ENTRY (jobname)
(user identification) (alternate).".
2.) "R010 JOB REJECTED UNDEFINED ENTRY (R-command)"
The first form of the message is output
if a RJOB command is not immediately
followed by a job (LOGON).
The second form of the message is output
if the system is expecting a job or
batch processing command and, instead,
receives an undefined entry.
In both cases, the system ignores all
input until it receives a valid job or
batch processing command.

### Response

Correct input deck and resubmit.

## RBP0011

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0011 JOB REJECTED. SYSTEM RESOURCE UNAVAILABLE

### Meaning

The actual message contents is described as follows:
"R011 JOB REJECTED. SYSTEM RESOURCE UNAVAILABLE (/LOGON command).".
The job, identified by the /SET-LOGON-PARAMETERS or /LOGON command,
was rejected because the system could not catalog or allocate the
disc file memory required to SPOOLIN the job.
This message is also output under some system component failure
conditions.
In both cases, the RBP facility continues to look for job and batch
processing command input.

### Response

Resubmit the job.

## RBP0012

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0012 JOB REJECTED. LOGON INVALID.

### Meaning

The actual message contents is described as follows:
"R012 JOB REJECTED. LOGON INVALID (/LOGON command).".
The job, identified by the /LOGON command
was rejected because one or more of the
command operands is invalid.

### Response

Correct the /LOGON command and resubmit the job.

## RBP0013

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0013 JOB REJECTED. PASSWORD INVALID (&00)

### Meaning

The specified password in the command
is invalid
(&00): Command image.

### Response

Correct the password and retry.

## RBP0014

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0014 JOB REJECTED INSUFFICIENT CPU TIME (&00)

### Meaning

There is no more CPU time available
for the user under the specified account number.
(&00): Command image.

### Response

Please call the central administrator
to add some CPU Time under that account
number.

## RBP0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0015 SYSTEM SHUTDOWN - REMOTE BATCH TERMINATING

### Meaning

The system operator has issued a /SHUTDOWN command,
and the system is about to shut down.

## RBP0016

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

RBP0016 JOB REJECTED. INCOMPLETE JOB '(&00)'

### Meaning

An EOT has been received during SPOOLIN Data (Device Type= 740 RCA).

### Response

Retry job.

## RBP0017

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0017 CLOSE ERROR ON FILE (&00) ON REMOTE STATION (&01)

### Meaning

SPOOLOUT task received CLOSE error
while trying to close
the file (&00) destinated to remote
station (&01).
(&00): filename
(&01): logical station name.

## RBP0018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0018 MONITORING JOB VARIABLE (&00) NOT ACCESSIBLE. REASON IS: (&01). PROCESSING CONTINUES

### Meaning

The JOB VARIABLE with which the task is associated is not
accessible. The state of the task is/was not indicated. As
MONITORING JOB VARIABLE (&00) the JOB VARIABLE name given in the
"MONJV" parameter is inserted. As REASON a return code of the
JVS is inserted. Replacing the leftmost "0" with "J" delivers the
corresponding message ID. At the 2nd occurrence of the message due
to an analogous command (i.e. at /LOGOFF due to the /LOGON with
"MONJV=" parameter) an "FFFF" as REASON indicates that the REASON
from the first time just has been inherited.

## RBP0019

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0019 (&00) ERROR: (&01) ON REMOTE STATION (&02)

### Meaning

An error occurred during the process.
(&00): type of error
: DMS: DMS error;
: INH: after SSVINH call;
(&01): DMS --> all DMS error code.
: INH --> X'01' UNKNOWN Operation code
X'02' UNKNOWN FCB Type
X'04' Inadequate Operation code
X'08' A(file-Name) = 0
X'10' L(file-Name) = 0
X'20' Incorrect FCB type
X'40' REQM or RELM error
X'80' SETL ERROR
(&02): logical station name.

## RBP0020

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0020 COMMAND REJECTED OPERAND ERROR (&00)

### Meaning

The actual message contents is described as follows:
"R020 COMMAND REJECTED OPERAND ERROR (&00).".
This message advises that the operand
field of a batch command (&00) is incorrect.
The system does not process this command (&00),
but continues with the next entry in the
input stream.

### Response

Determine the operand in error, correct,
and resubmit the command (&00).

## RBP0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0021 COMMAND REJECTED RSTART REQUIRED (&00)

### Meaning

An RSTART command must be the first command submitted
at an inactive batch terminal. The system continues to
ignore all entries in the input stream until
a valid RSTART command is detected.
(&00): Rejected command.

### Response

The user must submit a valid RSTART command.

## RBP0022

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0022 COMMAND REJECTED RLOGON REQUIRED (&00)

### Meaning

A user must be identified to the system through an
RLOGON command before any job input or utility commands
(ROUT, RMSG, RSTATUS) are accepted by the system.
The system continues to ignore all entries in the input
stream until a valid RLOGON or RSTOP command is detected.
(&00): Rejected command.

### Response

The user must submit a valid RLOGON command.

## RBP0023

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

RBP0023 COMMAND REJECTED ILLOGICAL SEQUENCE (&00)

### Meaning

The actual message contents is described as follows:
"R023 COMMAND REJECTED ILLOGICAL SEQUENCE (&00).".
This message identifies a command (&00) in the
input stream which has no meaning to the
system because of its position in the
stream or because it has been input through
a central card reader and is valid only if
entered through a remote batch terminal.

### Response

Correct the command sequence and reenter.

## RBP0024

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0024 COMMAND REJECTED RESOURCE UNAVAILABLE (&00)

### Meaning

The actual message contents is described as follows:
"R024 COMMAND REJECTED RESOURCE UNAVAILABLE (&00).".
This message is output if a system
component fails during the processing
of a command.

### Response

If the system is operational, an attempt
may be made to reenter the command.

## RBP0025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0025 BS2000 REMOTE STATION ALREADY CONNECTED

### Meaning

The station which is specified in the command /RSTART station-name, is
already connected to another remote station.

### Response

- Retry the command with another allowed station name, other
- wait for disconnection of the wanted station.

## RBP0026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0026 FORM PARAMETER DOES NOT EXIST FOR RBP IN SPOOL PARAMETER FILE. COMMAND REJECTED

### Meaning

The form specified in the /RSTART command or the default value 'STD...' is
not defined for RBP station in the SPOOL parameter file.

### Response

- Use /RSTART command with a form name existing in the SPOOL parameter
file
or
- ask the SPOOL administrator to add the form desired
into the SPOOL.PARAMETERS file for RBP station (8415/8418).

## RBP0027

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0027 INTERNAL ERROR DURING PROCESSING IN MODULE (&00). RBP TERMINATED FOR THIS TASK

### Meaning

An internal error occurred during RBP processing of a spoolout.
The operator receives a message to indicate the reason of the error.

## RBP0030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0030 COMMAND REJECTED JOB OUTPUT RESERVED BY SUBMITTER (&00)

### Meaning

This message is sent to an alternate output
recipient who is attempting to claim
job output through ROUT command. The deferred
output has already been claimed
by the submitting user.

## RBP0031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0031 COMMAND REJECTED JOB OUTPUT RESERVED BY ALTERNATE (&00)

### Meaning

This message is sent to a user who
submitted a job and is attempting to
claim job output through an ROUT command.
The deferred output has already been
claimed by the alternate output recipient.

## RBP0032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0032 COMMAND REJECTED JOB EXECUTING (&00)

### Meaning

This message is sent to a user who is
attempting to claim output from a job
that is still executing. Deferred job
can not be claimed until a job has finished
execution.

### Response

The user must wait for job completion
before claiming output.

## RBP0033

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0033 CMD REJECTED: OUTPUT FOR CENTRAL SITE (&00)

### Meaning

This message is sent to a remote user who is attempting to claim output
that has been already directed to a central printer via the command (&00).

## RBP0034

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0034 COMMAND REJECTED JOB NOT IN SYSTEM (&00)

### Meaning

The actual message contents is described as follows:
"R034 COMMAND REJECTED JOB NOT IN SYSTEM (&00).".
This message is sent to a user who is
requesting service for a job that is
not in the system. If the job was in the
system prior to the processing of this
command, the message implies that job
output has completed and all references to
the job have been deleted.

## RBP0035

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0035 COMMAND REJECTED INVALID RECIPIENT (&00)

### Meaning

The actual message contents is described as follows:
"R035 COMMAND REJECTED INVALID RECIPIENT (&00).".
This message is sent to a user who is
requesting service for a job that was not
submitted by him or did not specify him
as a valid output recipient.

## RBP0036

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0036 COMMAND REJECTED INACTIVE ADDRESS (&00)

### Meaning

The actual message contents is described as follows:
"R036 COMMAND REJECTED INACTIVE ADDRESS (&00).".
This message is sent to a user who has
attempted to contact an inactive user
or batch terminal through the RMSG command.

## RBP0037

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0037 COMMAND REJECTED NO JOB OUTSTANDING (&00)

### Meaning

No jobs outstanding for user identification requesting RSTATUS.

## RBP0040

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

RBP0040 SPOOLIN TERMINATED RESOURCE UNAVAILABLE

### Meaning

The actual message contents is described as follows:
"R040 SPOOLIN TERMINATED RESOURCE UNAVAILABLE.".
This message is output if a system component
fails during the initialization of
the Remote Batch SPOOLIN task.

### Response

If the system is operational, an attempt
may be made to retry the /START-CARD-INPUT resp. /RCARD command.

## RBP0041

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0041 SPOOLIN TERMINATED. COULD NOT ACQUIRE CARD READER

### Meaning

This message is output if all of the central card readers are logically
allocated to one or more system tasks.

### Response

Wait until a card reader is available.

## RBP0050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0050 REMOTE STATION NOT IDENTIFIED

### Meaning

The batch terminal has not been identified with a
valid id or with a valid id which is already in use.

### Response

Enter a valid terminal identification.

## RBP0051

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0051 BSET FILE ERROR

### Meaning

I/O error encountered in updating BSET file.

### Response

May be ignored or system may be shutdown.

## RBP0052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0052 BJET FILE ERROR

### Meaning

I/O error encountered in updating BJET file.

### Response

May be ignored or system may be shutdown.

## RBP0061

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0061 (&00): LINE NOT IN SID TABLE

### Meaning

The line of the remote terminal cannot be found.

### Response

Verify the generation of the system.

## RBP0062

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0062 (&00): NO BSET IN MEMORY

### Meaning

There is no batch station entry table in the system.

### Response

Verify the generation of the system.

## RBP0063

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0063 (&00): NO RBP MODULES IN SYSTEM

### Meaning

There are no RBP modules in the system.

### Response

Verify the generation of the system.

## RBP0064

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0064 (&00): REQM ERROR

### Meaning

REQM error during initialization of remote SPOOLIN processing.
(&00)= SPIN: Message from module ECRBSPIN

## RBP0065

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0065 (&00): RBP BUFFER REQM ERROR

### Meaning

REQM error during allocation of RBP work area.
(&00): SPIN: Message from module ECRBSPIN.

## RBP0066

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0066 (&00): BUFFER ERROR

### Meaning

Error during access to the RBP buffer.

## RBP0067

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0067 (&00): EAM OPEN ERROR

### Meaning

The reopen of the EAM file can not be done.

### Response

This message can be ignored but no printing of this file will be done.

## RBP0068

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0068 (&00): EAM READ ERROR

### Meaning

Error during GET operation of an EAM block.

### Response

This message can be ignored.

## RBP0069

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0069 (&00): EAM CLOSE ERROR

### Meaning

Error during CLOSE Operation of an EAM file.

### Response

This message can be ignored.

## RBP0070

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0070 (&00): BATCH STATION ENTRY ERROR

### Meaning

The PUT into the batch station entry table cannot be correctly processed.
The task is terminated through $TRMT 0050.
(&00)= SMSG: message from routine ECLRSMSG
in module ECLRSPPS.

### Response

It is advised to halt the system and take a dump.

## RBP0071

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0071 (&00): QUEUE ERROR

### Meaning

The PUT into the batch station entry table or
the closing of a queue can not be processed.
(&00)= SPPS: Message from module ECLRSPPS.

### Response

It is advised to stop the system and take a dump.

## RBP0072

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0072 (&00): BATCH JOB ENTRY ERROR

### Meaning

The access to the BJE (batch job entry table) can not be correctly
processed. The task is terminated through $TRMT 0050.

### Response

It is advised to halt the system and take a dump.

## RBP0073

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0073 (&00): RELM MSG. BUFFER ERROR

### Meaning

The message buffer can not be correctly released.

### Response

This message can be ignored.

## RBP0074

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

RBP0074 (&00): RELM WORK AREA ERROR

### Meaning

The work area can not be correctly released.

### Response

This message can be ignored.

## RBP0075

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0075 (&00): START RBP TERMINATION

### Meaning

The termination processing is started.

## RBP0076

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0076 (&00) *** WARNING: BJET IS FILLED UP

### Meaning

The 199 entries of the BJET are in use.

### Response

The operator has to stop immediately central spoolin,
to set RBPLMT to 0 with a BIAS command, to warn the
interactive users not to use print's with remote
destination and to wait that the output processing
has freed some entries.

## RBP0081

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0081 SYNTACTICAL ERROR. /RDIR CMD REJECTED

### Meaning

As there is only one parameter in the /RDIR command, the only
possible reason is that the terminal identification has a wrong
syntax.

### Response

Reenter the command /RDIR with a correct terminal identification.

## RBP0082

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0082 USER IS NOT ALLOWED TO USE /RDIR CMD. CMD REJECTED

### Meaning

The current user must be the SPOOL administrator to be
allowed to work with the /RDIR command.

## RBP0083

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0083 NO OUTSTANDING OUTPUT FOR STATION '(&00)'. COMMAND IGNORED

### Meaning

/REDIRECT-PRINT-JOB command is not processed.

## RBP0084

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0084 COMMAND ACCEPTED. (&00) PRINTS LINKED TO REMOTE STATION '(&01)' REDIRECTED TO CENTRAL PRINTER

### Meaning

The /REDIRECT-PRINT-JOB command is processed.
All non deferred printouts destinated to the remote station (&01) are
redirected to a central printer.
(&00): number of prints
(&01): logical name of the remote station.

## RBP0085

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0085 BEGIN OF WORK SESSION FOR USER (&00) ON REMOTE STATION (&01) (&02) (&03)

### Meaning

Warns the operator who is working at the remote station defined by
its logical name, processor name and station name.

## RBP0086

Destination: USER-TASK, CONSOLE Routing code: P Weight: 99

Warranty : NO

RBP0086 SPECIFIED TSN ALREADY BEING SPOOLED OUT. /PRIORITY COMMAND IGNORED

### Meaning

The attempt to change the priority level is rejected as spoolout has
already commenced.

## RBP0087

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

RBP0087 DEVICE ID UNKNOWN. COMMAND REJECTED

### Meaning

The device ID specified in the /REDIRECT-PRINT-JOB command
is not contained in the BSET (Batch Station Entry Table).

## RBP0088

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

RBP0088 "EQUISAM" CORRUPTION

### Meaning

The EQUISAM queue is corrupted and the print requests cannot be
redirected to the central printer.

## RBP0089

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0089 USER ALREADY CONNECTED. CMD REJECTED (&00)

### Meaning

The user specified in the /RLOGON command (&00) is
already connected on another remote station.
The system continues with the next entry in the input
stream.

### Response

Wait for disconnection of the user on the other
remote station before resubmitting the command.

## RBP0090

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0090 THE SPOOL ADMINISTRATOR TASK DID NOT REPLY WITHIN TIME LIMIT. RETRY COMMAND LATER

### Meaning

The SPOOL administrator task is locked. The command /REDIRECT-PRINT-JOB
cannot be processed.
This can occur if the administrator task is in crash and the operator does
not react to the message.

## RBP0091

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0091 CARD READER (&00) HAS BEEN RELEASED

### Meaning

The card reader has been released by the operator using the command
/RC UNIT=MN,CYCLE=NO.
(&00): mnemonic device name of the card reader.

## RBP0092

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

RBP0092 DEVICE (&00) NOT ASSIGNED TO SYSTEM

### Response

Spoolout cannot continue until the operator has assigned the device to
the system using the appropriate ATTACH command.

## RBP0501

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RBP0501 SPOOL QUEUE MANAGER INTERNAL ERROR (&00). ABNORMAL TASK TERMINATION CALLED

### Meaning

(&00): 0001 EQS failure (SEQMGET)
0002 EQS failure (SEQMMOC)
0003 EQS failure (SEQMDEL)
0004 EQS failure (SEQMADD)
0010 Memory pools failure (ENAMP)
0011 Memory pools failure (SSVMPFF)
0012 Memory pools failure (DISMP)
0020 Bourse mechanism failure ($NENQBO)

### Response

See System-dump.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages