## SDDCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDDCOPY Copyright (C) '(&00)' '(&01)' All Rights Reserved

## SDDLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDDLOAD Program '(&00)',Version '(&01)' of '(&02)' loaded

## SDD0001

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0001 ERROR '(&00)' FROM INTERFACE '(&01)'

### Meaning

(&00) : return code from interface standard header
(&01) : system/internal interface name

## SDD0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0002 System interface error. Command rejected. Contact System Support Staff

### Meaning

A problem occurred with a system interface during the command processing.

### Response

Refer to the previous error messages sent to SYSOUT and contact the
System Support Staff.

## SDD0003

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0003 ERROR '(&00)' FROM INTERFACE '(&01)'. ERROR LOGGING SEQUENCE NUMBER IS '(&02)'

### Meaning

(&00) : return code from interface standard header
(&01) : system interface name
(&02) : error logging sequence number

## SDD0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0101 CLASS '(&00)' MEMORY REQUEST ERROR

### Meaning

(&00) : memory class

## SDD0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0102 CLASS '(&00)' MEMORY RELEASE ERROR

### Meaning

(&00) : memory class

## SDD0200

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0200 DPRINTCM SUBSYSTEM CAN NOT BE CREATED. '(&00)' SUBSYSTEM NOT PRESENT

### Meaning

(&00) : subsystem name

### Response

Create the corresponding subsystem to allow full DPRINT functionality.

## SDD0201

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0201 DPRINTCM SUBSYSTEM CAN NOT BE CREATED.SYSDPRNT USER IDENTIFICATION NOT CATALOGUED

### Response

Create SYSDPRNT user identification and retry command.

## SDD0202

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0202 DPRINTCM SUBSYSTEM CAN NOT BE CREATED OR RESUMED. '(&00)' TASK CAN NOT BE CREATED

### Meaning

(&00) : TSN OF THE TASK :
DPMG or DFTM or DPRP or DNET or DWDG or DWTC

## SDD0203

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0203 DPRINTCM SUBSYSTEM CAN NOT BE CREATED. SPOOL PARAMETERS INTERNAL VERSION '(&00)' NOT SUPPORTED

### Meaning

(&00) : spool parameters internal version

### Response

Use SPSERVE to migrate the spool parameters to the supported version.

## SDD0204

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0204 DPRINTCM CAN NOT BE CREATED OR RESUMED. DPRINT OBJECTS INITIALIZATION FAILED

### Meaning

An internal error has been reported by the structure manager.

## SDD0205

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0205 DPRINTCM CAN NOT BE CREATED OR RESUMED. BCAM INFORMATION NOT COMPLETE

### Meaning

DPRINTCM subsystem is not able to work without BCAM.

### Response

Start BCAM and retry.

## SDD0206

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0206 DPRINTCM SUBSYSTEM CAN NOT BE CREATED. FT-BS2000 NOT ACTIVE

### Meaning

FT-BS2000 must be active to allow full DPRINT functionality.

### Response

Use the /START-FT command to activate FT-BS2000

## SDD0207

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0207 DPRINTCM SUBSYSTEM CAN NOT BE CREATED. DMS ERROR '(&00)' DURING 'GET', 'FILE' OR 'OPEN' PROCESSING. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG
in system mode or see the BS2000 manual 'System Messages'.

### Response

Try to correct the DMS error and retry startup.

## SDD0208

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0208 DPRINTCM SUBSYSTEM CAN NOT BE CREATED. INVALID SPECIFICATION IN '(&00)' PARAMETER FILE

### Meaning

The (&00) file does not exist
or a bad information has been introduced in the file.

### Response

Correct or restore the (&00) file and retry startup

## SDD0210

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0210 DPRINTCM SUBSYSTEM CAN NOT BE STOPPED OR HELD. '(&00)' TASK NOT ACCESSIBLE

### Meaning

(&00) : tsn of the task
DPMG or DFTM or DPRP or DNET or DWDG or DWTC

## SDD0211

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0211 DPRINT '(&00)' TASK CAN NOT BE USED ANYMORE

### Meaning

(&00) : tsn of the task
The task is no more accessible. No more action can be performed.

### Response

Unload DPRINTCM, load it again and retry.

## SDD0212

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0212 '(&00)' TASK IS READY

### Meaning

(&00) : tsn of the task

## SDD0213

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0213 '(&00)' TASK NORMAL TERMINATION

### Meaning

(&00) : tsn of the task

## SDD0214

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0214 '(&00)' TASK ABNORMAL TERMINATION

### Meaning

(&00) : tsn of the task

## SDD0215

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0215 '(&00)' TASK DE-INIT BEGIN

### Meaning

(&00) : tsn of the task

## SDD0300

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0300 DMS ERROR '(&00)' FROM INTERFACE '(&01)' FOR FILE '(&02)'. FURTHER INFORMATION : /HELP-MSG DMS(&00)

### Meaning

(&00) : DMS error code
(&01) : DMS interface name
(&02) : filename

## SDD0400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0400 ERROR OCCURRED DURING INSERTION/UPDATE OF SCB IN EQUISAMQ FILE OR SLOT CREATION FOR TSN '(&00)'. PROCESSING CONTINUES ON SERVER SIDE

### Meaning

An internal error occurred during the EQUISAMQ file update
or during slot creation for job tsn (&00).
The job processing can continue on the server, without notifying the
client.

## SDD0500

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDD0500 DMS/format error '(&01)' when processing file '(&00)'. Processing continues

### Meaning

(&00): filename
(&01): DMS error code or 'FRMT' in case of format error
In case of DMS error, more information can be found with
/HELP-MSG DMS(&01)
Default values for accounting information are taken from
DPRINTCM parameter file (SYSSSI).

## SDD0700

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0700 SPOOL '(&00)' TASK NOT ACCESSIBLE

### Meaning

Due to a communication problem with a SPOOL task, the SPOOL request is
unsuccessfully terminated.
(&00) : tsn of the task

## SDD0701

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD0701 STRUCTURE MANAGER ERROR

## SDD0800

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0800 ILLEGAL COMBINATION OF OPERANDS. COMMAND REJECTED

### Meaning

The operand syntax is correct but their combination is not allowed.

### Response

Correct command and retry.

## SDD0801

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0801 LOGICAL VALIDATION PROBLEM DURING COMMAND PROCESSING. COMMAND REJECTED

## SDD0900

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD0900 PRM ERROR '(&00)' FOR FILE '(&01)'. FURTHER INFORMATION : /HELP-MSG (&02)

### Meaning

(&00) : PRM error code
(&01) : filename
(&02) : corresponding message

## SDD1100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD1100 /START-DPRINT-LOGGING OR /STOP-DPRINT-LOGGING COMMAND CURRENTLY PROCESSED. COMMAND REJECTED

### Meaning

The commands are processed sequentially. No command may be
issued as long as another one is still being processed

### Response

Retry command later.

## SDD1101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD1101 '(&00)' COMMAND ALREADY PROCESSED. COMMAND REJECTED

### Meaning

(&00) : command name :
/START-DPRINT-LOGGING or /STOP-DPRINT-LOGGING

## SDD1102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD1102 DPRINT LOGGING FILE '(&00)' OPENED

### Meaning

(&00) : filename

## SDD1103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD1103 DPRINT LOGGING FILE '(&00)' CLOSED

### Meaning

(&00) : filename

## SDD1104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD1104 COMMAND RESTRICTED TO SPOOL ADMINISTRATOR OR OPERATOR. COMMAND REJECTED

## SDD1105

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1105 ERROR FROM MACRO '(&00)'; RETURN CODE : '(&01)'; SUBID : '(&02)'

## SDD1106

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1106 SERVER TASK '(&00)'; CODE : '(&01)'; MODULE : '(&02)'; DISPLACEMENT : '(&03)'

### Meaning

&00 : tsn of server task
&01 : return code of interface (whose name is given in SDD0001)
&02 : name of the module where the interface is called
&03 : displacement in the module where the interface is called.
This message has to be interpreted as a warning or error message
In case of problem, retrieve it from the conslog file for diagnose.

## SDD1107

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1107 CLUSTER OR HOST '(&00)' AVAILABLE

### Meaning

(&00) : cluster name or host name
The cluster or the host (&00) is now available again.

## SDD1108

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1108 CLUSTER OR HOST '(&00)' NOT AVAILABLE

### Meaning

(&00) : cluster name or host name
The cluster or the host (&00) is no more available.

## SDD1109

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1109 $CREAT ERROR DURING DNET TASK RECOVERY. DNET TASK RECOVERY ABORTED

## SDD1110

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1110 TCP APPLICATION '(&00)' WITH INTERNET ADDRESS '(&01)' AND PORT NUMBER '(&02)' IS '(&03)'

### Meaning

(&00) : application name
(&01) : internet address of the host with which the application
is connected/disconnected
(&02) : port number of the host with which the application is
is connected/disconnected
(&03) : ATTACHED : the TCP application is attached to the host
DETACHED : the TCP application is removed from the host.

## SDD1111

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1111 SERVER TASK ABNORMAL TERMINATION

## SDD1112

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1112 TRACE SHUTDOWN PROBLEM; DPRT TASK STILL LIVING AFTER +/- 2 MINUTES

## SDD1113

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1113 ERROR OCCURED IN DPRINT CENTRAL SERVER TASK DNET. CENTRAL SERVER TASK TO BE CONTINUED ? REPLY (Y=YES(BE SURE COMMUNICATIONS ARE AVAILABLE); N=NO (DNET TASK WILL NOT EXIST ANY MORE))

### Meaning

Y : DNET task will be restarted.
Care must be taken that communications are available
N : DNET task will be destroyed

## SDD1114

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD1114 /START-DPRINT-LOGGING COMMAND ACCEPTED. SYSTEM TRACE MANAGER HAS DISABLED DPRINT LOGGING. PROCESSING CONTINUES

## SDD2000

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2000 HOME HOST CONFIGURATION MANAGER IS WAITING FOR RESPONSE FROM HOST '(&00)'. WAIT PROCESSING TO BE CONTINUED ? REPLY (Y=YES (STILL WAIT RESPONSE);N=NO (ABORT THE WAIT PROCESSING))

### Meaning

(&00) : remote host name

### Response

The following responses may be given :
During startup/restart :
- the completion of transfer of configuration file from master
- the completion of attachment of a remote slave host
During shutdown :
- the completion of transfer of cluster administration right to a slave
HOST

## SDD2001

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2001 HOME HOST NOT DEFINED IN DPRINT CONFIGURATION FILE OF CLUSTER MASTER HOST

## SDD2002

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2002 HOME HOST ATTACHMENT TO LOCAL CLUSTER CONFIGURATION FAILED. '(&00)' STARTUP/RESTART PROCESSING TO BE CONTINUED ? REPLY (Y=YES (CREATE A PRIVATE CLUSTER); N=NO (ABORT (&00) STARTUP/RESTART)

### Meaning

An error occurred during home host attachment to the constituted local
cluster. Possible errors are :
-The cluster master host is not started.
- The home host is no more defined in the configuration file of the
contacted cluster master.
- Internal error on cluster master host during home host attachment
processing.
- Transfer of master configuration file not possible (FT error).
- Attachment aborted (response = N to message SDD2000).
- Remote host(s) communication error.
- Inconsistency detected in the configuration file.
(&00) : subsystem name : DPRINTCL,DPRINTSV,DPRINTCM

### Response

N : The startup of &00 is aborted or the restart of DPRINTCM is aborted
(in this case the only accepted orders on configuration are
/STOP-SUBSYSTEM ..)
Y : The host is removed from the local cluster and put
in a private cluster (one host cluster).
-Automatic attachment when the master host is started.
After error correction the host may be:
- either reincluded in the local cluster in which it was previously
connected by a command /VERIFY-DPRINT-CONSISTENCY issued
on the local cluster master host (not on the private cluster)
- or included in another cluster by the command /MODIFY-DPRINT-CLUSTER
- or work alone in the private cluster.

## SDD2003

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2003 DPRINT CONFIGURATION FILE MAY BE OUT OF DATE. HOME DPRINT CONFIGURATION TO BE USED FOR THE CLUSTER ? REPLY (Y=YES (SOME MODIFICATIONS MAY BE LOST; N=NO (ABORT HOME HOST ATTACHMENT TO CLUSTER))

### Meaning

The home host is the first host of the cluster to be loaded
but has abnormally terminated the previous DPRINT session
or was not the last to be downloaded during the previous session.
The home configuration file is therefore perhaps out of date.

### Response

Y : the home configuration is used as reference for the whole cluster.
N : the startup may be stopped or a private cluster may be constituted.

## SDD2004

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2004 DPRINT CONFIGURATION FILE CANNOT BE TRANSFERRED TO HOST '(&00)' DUE TO FILE TRANSFER ERROR

### Meaning

A File Transfer error has been detected during transfer of configuration
file from master host to local host.

## SDD2005

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2005 INCONSISTENCY DETECTED IN DPRINT CONFIGURATION FILE

## SDD2006

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2006 HOST '(&00)' ATTACHED TO THE LOCAL CLUSTER

## SDD2007

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2007 DMS ERROR '(&00)' FROM INTERFACE '(&01)' FOR FILE '(&02)'. RETRY ? REPLY (Y=YES ; N=NO (A PRESET FILE IS CREATED FOR THIS SESSION))

### Meaning

A DMS error occurred during processing of the file (&02). For more details
about DMS error code, enter /HELP-MSG DMS(&00)
(&00) : DMS error code
(&01) : DMS interface name
(&02) : filename

### Response

Y : the file (&02) can be repaired or another DPRINT configuration file
can be imported under the same filename; the retry operation can thus be
performed.
N : no retry operation is performed. A default DPRINT configuration file
will be created.

## SDD2008

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2008 DPRINT CONFIGURATION FILE IS RESET TO ITS PREVIOUS STATE. MODIFICATIONS OF LAST DPRINTCM SESSION ARE LOST. PROCESSING CONTINUES

### Meaning

The DPRINT configuration file could not be opened.
The copy made at the beginning of the last DPRINTCM session is used.
All modifications done during the previous DPRINTCM session have thus to
be entered again.

## SDD2009

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2009 A PRESET DPRINT CONFIGURATION FILE '(&00)' IS CREATED FOR THIS SESSION

### Meaning

An error occurred while processing the DPRINT configuration file.
A preset one (&00) is assigned and contains default values.

## SDD2010

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2010 A NEW DPRINT CONFIGURATION FILE '(&00)' IS CREATED WITH DEFAULT VALUES

## SDD2013

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2013 FILE '(&00)' IS BEING PROCESSED

### Meaning

The DPRINT configuration startup is processing the (&00) file
(&00) : DPRINT configuration filename

## SDD2014

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2014 FILE '(&00)' PROCESSING COMPLETED

### Meaning

The DPRINT configuration startup has finished to process (&00) file.
(&00) : DPRINT configuration filename

## SDD2015

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2015 ANY FURTHER DPRINT CONFIGURATION UPDATE WILL OCCUR ONLY INTO MEMORY

### Meaning

A DMS error occurred on the DPRINT configuration file which prevents the
file from being updated.
(An SDD0300 message has been previously sent to console)
From now, the updates will not appear any more in the DPRINT
configuration file.
If this happens on the master host, take care that the DPRINT
configuration file can not be transferred to the slave hosts
for configuration modifications.

### Response

Try to correct the DMS problem, unload DPRINTCM and load it again
to keep coherence or change master.

## SDD2016

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2016 TIME OUT FOR LOCAL HOST ATTACHMENT REACHED

### Meaning

The local host is waiting for the confirmation from cluster master of
attachment to the local cluster.

## SDD2017

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2017 TIME OUT FOR NEW CLUSTER MASTER DESIGNATION REACHED

### Meaning

The master of the cluster tries to designate a successor before
terminating its shutdown
but does not receive response from remote host.

## SDD2018

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2018 TIME OUT FOR REMOTE HOST ATTACHMENT REACHED

### Meaning

The master host is waiting for the confirmation of attachment of a remote
host.
The remote host is in attachment phase but has not already sent the result
of attachment processing.

## SDD2019

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2019 TIMEOUT FOR CONFIGURATION FILE TRANSFER TO HOST '(&00)' REACHED. WAIT PROCESSING TO BE CONTINUED ? REPLY(Y=YES(STILL WAIT FOR RESPONSE); N=NO(ABORT WAIT PROCESSING)

### Meaning

(&00) : host name
A file transfer has been initiated with the host (&00) but no information
about the transfer issue has been received.

### Response

Check that FILE TRANSFER started on local host and on master host.
Ask the FT/FTAC administrator to check the FT-OPTIONS parameters.

## SDD2020

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2020 INVALID LOCAL PRINTER NAME FOR DISTRIBUTED PRINTER '(&00)'

### Meaning

The local printer name is either not defined in the SPOOL parameters or
has an RSO printer type.
(&00) : printer name

### Response

Ask the cluster administrator to correct the distributed printer
definition in the DPRINT configuration
or the spool administrator to correct the corresponding local spool device
definition in the SPOOL parameters.
Both updates must be performed by using SPSERVE.

## SDD2021

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2021 DPRINT CONFIGURATION MANAGER STARTS ATTACHMENT TO CLUSTER MASTER HOST '(&00)'

### Meaning

Due to DPRINT configuration startup or inconsistency state
the local host is reattached to the cluster master.

## SDD2022

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2022 DPRINT CONFIGURATION MANAGER IN STARTUP PHASE. WAIT FOR COMPLETION? REPLY (Y=YES;N=NO)

### Meaning

The task is waiting for completion of DPRINT configuration manager
startup.

### Response

YES : The task waits until completion or next time out.
NO : The task is aborted.

## SDD2023

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2023 DPRINT CONFIGURATION MANAGER IN RECOVERY PHASE. WAIT FOR COMPLETION? REPLY (Y=YES;N=NO)

### Meaning

The task is waiting for completion of DPRINT configuration manager
recovery.

### Response

YES : The task waits until completion or next time out.
NO : The task is aborted.

## SDD2024

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2024 DPRINT CONFIGURATION MANAGER IN DELETE PHASE. WAIT FOR COMPLETION? REPLY (Y=YES;N=NO)

### Meaning

The task is waiting for completion of DPRINT configuration manager delete.

### Response

YES : The task waits until completion or next time out.
NO : The task is aborted.

## SDD2025

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2025 DPRINT SERVER BELONGING TO HOST '(&00)' ATTACHED TO LOCAL CLUSTER

### Meaning

(&00) : host name
The subsystem DPRINTSV is available on host (&00).
The printers attached to the corresponding server are available.

## SDD2026

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2026 DPRINT SERVER BELONGING TO HOST '(&00)' DETACHED FROM LOCAL CLUSTER

### Meaning

(&00) : host name
The subsystem DPRINTSV is no more available on host (&00).
The printers attached to the corresponding server are no more available.

## SDD2027

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2027 A PRIVATE CLUSTER HAS BEEN FORCED BY HOST '(&00)'

### Meaning

(&00) : host name
The master host has sent an order to force a private cluster on the home
host.

## SDD2028

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2028 HOME HOST REMOVED FROM LOCAL CLUSTER BY HOST '(&00)'

### Meaning

(&00) : host name
The master host has sent an order to leave the cluster.
Only the home host objects are kept in the DPRINT configuration file.

## SDD2029

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2029 HOST '(&00)' STARTS ATTACHMENT TO LOCAL CLUSTER

### Meaning

(&00) : host name

## SDD2030

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2030 HOST '(&00)' DETACHED FROM LOCAL CLUSTER

### Meaning

(&00) : host name
DPRINTCL and DPRINTSV subsystems are stopped on host (&00)

## SDD2031

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2031 DPRINT CONFIGURATION MANAGER IN ERROR

### Meaning

Due to an internal error, the configuration manager is not able to process
configuration management commands.
The DPRINT configuration manager can only support the commands :
/STOP-SUBSYSTEM DPRINTCL or /STOP-SUBSYSTEM DPRINTSV.

## SDD2032

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2032 HOME HOST INCLUDED IN THE LOCAL CLUSTER

### Meaning

The host is included in the cluster either after a startup processing
or after a /MODIFY-DPRINT-CONFIGURATION command issued on the master host.

## SDD2033

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2033 ATTACHMENT TO LOCAL CLUSTER FAILED

## SDD2034

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2034 HOME SERVER NOT DEFINED IN DPRINT CONFIGURATION FILE. DPRINTSV STARTUP ABORTED

### Meaning

The home server object must be defined in the DPRINT configuration file
before starting DPRINTSV subsystem.

### Response

The cluster administrator has first to define the home server in the
DPRINT configuration with SPSERVE.

## SDD2035

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2035 TRANSFER OF DPRINT CONFIGURATION FILE NOT POSSIBLE DUE TO PREVIOUS DMS ERROR

### Meaning

A DMS error previously occurred on the DPRINT configuration file.
(An SDD0300 message has been previously sent to console)

### Response

Change master and try again the action on the new master host.
Before restoring the previous master,
unload and load again DPRINTCM on his host.

## SDD2036

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2036 Invalid local printer name '(&00)' specified for distributed printer

### Meaning

The local printer name is either not defined in the SPOOL parameters or
has an RSO printer type.
(&00) : printer name

### Response

Ask the cluster administrator to correct the distributed printer
definition in the DPRINT configuration
or the spool administrator to correct the corresponding local spool device
definition in the SPOOL parameters.
Both updates must be performed by using SPSERVE.

## SDD2100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2100 DPRINT REMOTE CLUSTER OBJECT '(&00)' NOT DEFINED IN DPRINT CONFIGURATION FILE

### Meaning

The remote cluster name (&00) must be defined in the DPRINT configuration
to be considered as valid.
(&00) : remote cluster name

### Response

Ask the cluster administrator to define the corresponding remote cluster
object in the DPRINT configuration with SPSERVE
or use an already existing remote cluster name.

## SDD2101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2101 DPRINT HOST OBJECT '(&00)' NOT DEFINED IN DPRINT CONFIGURATION FILE

### Meaning

The host name must be defined in the DPRINT configuration and attached to
the local cluster to be considered as valid.
(&00) : host name

### Response

Ask the cluster administrator to define the corresponding host object in
the DPRINT configuration with SPSERVE
and to attach it with the /MODIFY-DPRINT-CLUSTER command or use an already
existing attached host name.

## SDD2102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2102 DPRINT SERVER OBJECT '(&00)' NOT DEFINED IN DPRINT CONFIGURATION FILE

### Meaning

The server name must be defined in the DPRINT configuration
and attached to the local cluster to be considered as valid.
(&00) : server name

### Response

Ask the cluster administrator to define the corresponding server object in
the DPRINT configuration with SPSERVE
and to attach its corresponding host with the /MODIFY-DPRINT-CLUSTER
command.

## SDD2103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2103 DPRINT PRINTER OBJECT '(&00)' NOT DEFINED IN DPRINT CONFIGURATION FILE

### Meaning

The printer name (&00) must be defined in the DPRINT configuration to be
considered as valid.
(&00) : printer name

### Response

Ask the cluster administrator to define the corresponding printer object
in the DPRINT configuration with SPSERVE
or use an already existing printer name.

## SDD2104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2104 DPRINT PRINTER POOL OBJECT '(&00)' NOT DEFINED IN DPRINT CONFIGURATION FILE

### Meaning

The printer pool (&00) must be defined in the DPRINT configuration to be
considered as valid.
(&00) : printer pool name

### Response

Ask the cluster administrator to define the corresponding printer pool
object in the DPRINT configuration with SPSERVE
or use an already existing printer pool name.

## SDD2105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2105 DPRINT ACCESS CONTROL OBJECT '(&00)' NOT DEFINED IN DPRINT CONFIGURATION FILE

### Meaning

(&00) : access control name

### Response

Ask the cluster administrator to define the corresponding access-control
object in the DPRINT configuration.

## SDD2106

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2106 INTERNAL ERROR DURING DPRINT CONFIGURATION ACCESS. COMMAND REJECTED

### Meaning

An internal error has been returned by the DPRINT configuration access
interface.

## SDD2107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2107 INVALID TYPE FOR REMOTE CLUSTER '(&00)'

### Meaning

The remote cluster is a BS2000 one and has been defined with
TYPE=*UNIX-ISO or *UNIX-TCP
or has an ISO protocol and has been defined with TYPE=*BS2000 or *UNIX-TCP
or has a TCP protocol and has been defined with TYPE=*BS2000 or *UNIX-ISO
(&00) : remote cluster name

### Response

Ask the cluster administrator to modify the type of the remote cluster,
via the //MODIFY-DPRINT-REMOTE-CLUSTER statement of SPSERVE

## SDD2108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2108 NO INFORMATION ABOUT THE SPECIFIED OBJECT(S) EXISTS. COMMAND OR STATEMENT NOT PROCESSED

### Meaning

The DPRINT configuration does not contain any information about the
specified object(s).

## SDD2109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2109 SPOOL INFORMATION NOT AVAILABLE

### Meaning

The SPOOL information hooked to the specified object are not available.
Either this information does not exist or is not accessible.
Only the distributed information is displayed.

## SDD2110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2110 ACCESS TO SPECIFIED CLUSTER DENIED. COMMAND OR STATEMENT NOT PROCESSED

### Meaning

The cluster name specified in the command/statement is not available.
Either it is not defined in the DPRINT configuration or access to this
cluster is not possible.

## SDD2111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2111 ACCESS TO REMOTE SERVER DENIED

### Meaning

The remote server on which the spool information is stored is not
accessible.

## SDD2112

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD2112 NO INFORMATION ATTACHED TO THIS OBJECT

### Meaning

The object is defined in the DPRINT configuration but does not contain any
additional information.

## SDD2113

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2113 INFORMATION TYPE NOT AVAILABLE

### Meaning

The requested type of information is not available
or meaningful for this object in this environment

## SDD2114

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD2114 Privilege too low

### Meaning

The SHOW-DPRINT-ACCESS-CONTROLS command or statement is restricted
to the Cluster Administrator;
the SHOW-DPRINT-HOSTS command or statement is restricted
to the Cluster Administrator or Print Service Administrator.

## SDD3000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3000 SCB NOT FOUND IN EQUISAMQ FILE FOR TSN '(&00)'

### Meaning

The SCB corresponding to the job with tsn '(&00)' does not exist any more.

## SDD3001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3001 FT ERROR '(&00)' FROM INTERFACE '(&01)' DURING FILE CONTAINER PROCESSING FOR TSN '(&02)'

### Meaning

An FT error '(&00)' has been detected during file transfer processing of
the print job file.
(&01) : FT interface name
(&02) : TSN of the job
For more detailed information about the FT error code see the BS2000
manual 'FT-BS2000'.

## SDD3002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3002 FT ERROR '(&00)' FROM INTERFACE '(&01)' DURING RESOURCES CONTAINER PROCESSING FOR TSN '(&02)'

### Meaning

An FT error '(&00)' has been detected during file transfer processing of
the print job resource file.
(&01) : FT interface name
(&02) : TSN of the job
For more detailed information about the FT error code see the BS2000
manual 'FT-BS2000'.

## SDD3003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3003 FT ERROR '(&00)' FROM INTERFACE '(&01)' DURING FILE CONTAINER PROCESSING FOR JOB-ID '(&02)'

### Meaning

An FT error has been detected during file transfer processing
of the print job file.
&00 : FT error
&01 : FT interface name
&02 : job identification in the remote cluster
For more detailed information about the FT error code see the BS2000
manual 'FT-BS2000'.

## SDD3004

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3004 PARTNER-NAME FOR HOST '(&00)' NOT DEFINED IN DPRINT FILE TRANSFER CONFIGURATION FILE. HOST '(&00)' IS USED AS PARTNER-NAME. PROCESSING CONTINUES

### Meaning

(&00) : host name
The FT partner-name is not defined in the file transfer configuration file
for the host (&00).

### Response

Contact the PRINT-SERVICE administrator to update
the file transfer configuration file.

## SDD3005

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3005 FT ERROR '(&00)' FROM INTERFACE NCOPY DURING DPRINT CONFIGURATION FILE PROCESSING

### Meaning

An FT error '(&00)' occurred during file transfer processing of the
configuration file.
For more information about the FT error code see the BS2000
manual 'FT-BS2000'.
In case of syntax error, the reason could be in the
definition of the SYSPAR.DPRINT.<ver> where <ver> is
the version of DPRINT.

### Response

Please, check the content of this file

## SDD3006

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3006 FILE CONTAINER CREATION ERROR FOR TSN '(&00)'

## SDD3007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3007 RESOURCES CONTAINER CREATION ERROR FOR TSN '(&00)'

## SDD3008

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3008 WARNING: SPACE SATURATION LEVEL '(&00)' FOR SYSDPRNT USER IDENTIFICATION

### Meaning

(&00) : saturation level :
1 : saturation > 74%
2 : saturation > 89%
3 : saturation > 98%

### Response

Contact System Support Staff to increase the user space available under
SYSDPRNT.
Otherwise DPRINT is locked for new print jobs processing.
Possible reasons :
- not enough user space under SYSDPRNT.
- many containers for jobs in WAIT state.
- too many print jobs in processing for the space available.

## SDD3009

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3009 SPACE SATURATION FOR SYSDPRNT USER IDENTIFICATION PREVENTS FROM CONTAINER CREATION. CONTINUE ? REPLY(Y=YES(SATURATION WILL BE CHECKED AGAIN) ; N=NO(NO MORE CHECK FOR SATURATION))

### Meaning

Contact System Support Staff to check the saturation level before replying
to the message.

### Response

Y : the saturation will be checked again before processing continuation.
N : the processing of the current job will continue without checking the
saturation any more.

## SDD3010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3010 INTERNAL ERROR DURING THE DPRINT FILE TRANSFER PROCESSING FOR TSN '(&00)'. REASON : '(&01)'

### Meaning

(&00) : TSN of the job
(&01) : internal error number :
01 : spool parameters access error on gateway.
02 : asynchronous communication error with DWTC task.
03 : structure manager internal error on gateway.
04 : asynchronous communication error with DPRP task.
05 : space saturation greater than level 2 under SYSDPRNT user
identification.
06 : CATAL interface error.
07 : error during the FT file transfer processing.
08 : system internal error (refer to the previous error messages).
09 : profile creation error on gateway host.

## SDD3011

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDD3011 WARNING: FT/FTAC SUBSYSTEM NOT LOADED OR NOT ACTIVATED

### Response

Contact the FT/FTAC administrator to reload or to reactivate FT/FTAC.
Otherwise DPRINT is locked for new print jobs processing.

## SDD3012

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3012 INCOMPLETE FILE TRANSFER REQUEST FOR SERVER TSN '(&00)'. ERROR : '(&01)'. WHOLE REQUEST WILL BE RETRIED LATER

### Meaning

The print job is put back into WFT state.
(&00) : server TSN of the print job
(&01) : error number :
1.byte: original host (where the error has been detected)
1: client host
2: gateway host
3: server host
2.byte: original system type
1: BS2000 system
2: SINIX system
3.byte: error type
1: DPRINTSV restart
2: $SYSDPRNT saturation
3: FT/FTAC not loaded or not activated
4.byte: 0

### Response

Contact the PRINT-SERVICE administrator, if requested.

## SDD3013

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3013 JOB WITH SERVER TSN '(&00)' DEFERRED BY DPRINT FILE TRANSFER PROCESSING. ERROR : '(&01)'

### Meaning

The print job is put back into the KEEP queue until it is restarted
by means of the /RESUME-PRINT-JOB command.
(&00) : server TSN of the print job
(&01) : error number (only bytes 1-4)
1.byte: original host (where the error has been detected)
1: client host
2: gateway host
3: server host
2.byte: original system type
1: BS2000 system
2: SINIX system
3.byte: error type
1: file ft-init error
2: resource container ft-init error
3: file ft-result error
4: resource container ft-result error
5: user file input error
6: file container error
7: file filtered container error
8: resource input error
9: resource container error
A: internal error
B: $SYSDPRNT saturation
C: transfer admission not found
D: SCB error
E: section error
F: spool parameters access error
G: communication error
H: structure manager error
I: FT/FTAC not loaded or not activated
J: too long waiting time for file ft-result
K: too long waiting time for resource container ft-result
L: Ft file or resource container transfer abnormally terminated
M: UFS copy error
N: file filtered ft-init error
P: DPRINTCL subsystem not loaded
4.byte: second part return code type
0: no RC
1: FT RC
2: DMS RC
3: PRM RC
The complete return code is contained in the ERCOD field of
the /SHOW-PRINT-JOB-STATUS INFORMATION=DISTRIBUTED command :
5-8.byte: DMS RC ,FT RC or PRM RC (see 4.byte value)
sub RC1-main RC1 of FT general RC when 4.byte=1
in case of PRM RC, more information in message SPR0014

### Response

Contact the PRINT-SERVICE administrator, if requested.

## SDD3014

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3014 ERROR OCCURRED DURING INSERTION OF SINIX INFORMATION IN EQUISAMQ FILE FOR JOB-ID '(&00)'

### Meaning

&00 : job identification in the remote cluster.
An error has been detected by the EQUISAMQ manager
during the insertion of the sinix information record.

### Response

Please contact the PRINT-SERVICE administrator, if requested.

## SDD3015

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3015 INTERNAL ERROR '(&00)' DURING DPRINT FILE TRANSFER PROCESSING FOR JOB-ID '(&01)'

### Meaning

An internal error has been detected during the FT procesing.
&00 : internal error number :
01: communication error
02: internal error
03: asynchronous communication error with DPRP task
04: structure manager error
05: filtered container creation error
06: $SYSDPRNT saturation
07: FT/FTAC subsystem not loaded or not activated
08: filtered container ft-init error
09: configuration file access error
&01 : job identification in the remote cluster.

### Response

Please contact the PRINT-SERVICE and/or FT administrator, if requested.

## SDD3016

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3016 SINIX INFORMATION NOT FOUND IN EQUISAMQ FILE FOR TSN '(&00)'

### Meaning

&00 : TSN of the job.
The sinix information record has not been found in the EQUISAMQ file.

### Response

Please contact the PRINT-SERVICE administrator, if requested.

## SDD3017

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3017 ERROR OCCURRED DURING UPDATE OF SINIX INFORMATION IN EQUISAMQ FILE FOR TSN '(&00)'

### Meaning

&00 : TSN of the job.
An error has been detected by the EQUISAMQ manager during the update
of the sinix information record.

### Response

Please contact the PRINT-SERVICE administrator, if requested.

## SDD3018

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3018 SPOOLOUT ABORTED. ERROR CODE '(&00)' FOR THE SINIX FILE

### Meaning

It is not possible to spoolout the SINIX JOB.
&00 : internal error number :
01 : SINIX file ft-init error
02 : SINIX file transfer abnormally terminated
03 : SINIX equisam record error on gateway
04 : CATAL interface error
05 : structure manager internal error on gateway
06 : transfer admission not found
07 : SCB error on gateway

## SDD3019

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3019 FILE TRANSFER TASK SATURATION FOR TSN '(&00)'. PROCESSING CONTINUES

### Meaning

(&00) : client TSN of the print job
The file transfer for the print job is in WAIT state for the FT product
because the number of jobs working with the FT product is too high
for the moment.

### Response

Contact the PRINT-SERVICE and/or FT administrator, if requested.

## SDD3020

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3020 FILE TRANSFER TASK SATURATION FOR SERVER TSN '(&00)'

### Meaning

(&00) : server TSN of the print job
The file transfer for the print job is in WAIT state for the FT product
on the client or gateway host
because the number of jobs working with the FT product is too high
for the moment.

### Response

Contact the PRINT-SERVICE and/or FT administrator, if requested.

## SDD3021

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDD3021 SPOOLOUT ABORTED. FT ERROR CODE '(&00)'

### Meaning

(&00) : FT return code described in FT-BS2000 user guide manual.
An FT error occurred during the DPRINT file transfer of
the user file or resources container;
the job can thus not be processed.

## SDD3022

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3022 JOB WITH SERVER TSN '(&00)' NO MORE PROCESSED BY SERVER

### Meaning

(&00) : server tsn of the print job
A /MODIFY-PRINT-JOB-ATTRIBUTES or /CANCEL-PRINT-JOB command
has been issued on the client host.
The job is no more processed on this server :
- either it has been cancelled on the client host
- or it has been redirected to another server from the client host.

## SDD3023

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD3023 SPOOLOUT ABORTED. DMS ERROR CODE '(&00)' IN INPUT FILE

### Meaning

For more detailed information about the DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the BS2000 manual
'System Messages'.
A DMS error occurred at the container file creation or at the DPRINT file
transfer of the user file; the job can thus not be processed.

## SDD3024

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDD3024 Input file greater or equal to 32 Gbytes. Spoolout aborted

### Meaning

Processing large files (greater or equal to 32 Gbytes)
is not supported. The print job cannot be processed.

## SDD4000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD4000 EQUISAMQ ACCESS PROBLEM DURING SERVER '(&00)' INITIALIZATION. PROCESSING CONTINUES

### Meaning

An error has been detected by the EQUISAMQ manager during the clean-up of
the SCB's which are currently processed by the server '(&00)'

### Response

Contact System Support Staff

## SDD4001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD4001 EQUISAMQ FILE ACCESS PROBLEM FOR TSN '(&00)'. PROCESSING CONTINUES

### Meaning

(&00) : tsn of the job.
The EQUISAMQ file access parameter list has returned an error. The
processing continues without modification of the SCB.
The job state could be incoherent on client and server sides.
The server where the job is being processed has been removed from the
DPRINT configuration.
The print job may have been modified, while its original server was down,
and redirected to another running server.

## SDD4002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD4002 SLOT MANAGER ACCESS ERROR DURING PROCESSING OF TSN '(&00)'. PROCESSING CONTINUES

### Meaning

(&00) : tsn of the job.
processing continues without modification of the slot.
processing continues without modification of the SCB.
The job state could be incoherent on client and server sides.
The server where the job is being processed has been removed from the
DPRINT configuration.
The print job may have been modified, while its original server was down,
and redirected to another running server.

## SDD4003

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD4003 PRINT JOB WITH CLIENT TSN '(&00)' AND SERVER TSN '(&01)' IS NO MORE PROCESSED BY SERVER '(&02)' OF CLUSTER '(&03)'

### Meaning

(&00) : tsn of the print job on the client/gateway host
(&01) : tsn of the print job on the server host
(&02) : server name where the print job was processed
(&03) : cluster name where the print job was processed
Either the print job has been suppressed by a /CANCEL-PRINT-JOB command
or it has been abnormally terminated during printing.

## SDD5000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD5000 DPRINT CLUSTER CREATION REQUEST FROM HOST '(&00)' ACCEPTED

## SDD5001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD5001 DPRINT CLUSTER CREATION REQUEST FROM HOST '(&00)' REJECTED

## SDD5002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD5002 DPRINT CONFIGURATION VERIFICATION REQUEST FROM HOST '(&00)' ACCEPTED. CURRENT HOST ASSIGNED AS NEW CLUSTER MASTER

## SDD6000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD6000 '(&00)' COMMAND ACCEPTED BY REMOTE CLUSTER WITH JOB-ID '(&01)'

## SDD6001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD6001 '(&00)' COMMAND REJECTED BY REMOTE CLUSTER WITH MESSAGE IDENTIFIER '(&01)'. ERROR CLASS : '(&02)'

### Meaning

(&00) : command name
(&01) : remote spooler message identifier
(&02) : error class :
1 : parameter error
2 : system error
3 : remote spooler not available
4 : privilege error
5 : file transfer protocol error
6 : protocol error
7 : object not found

## SDD6002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD6002 '(&00)' COMMAND REJECTED BY BS2000 REMOTE CLUSTER. REASON : '(&01)'

### Meaning

(&00) : command name
(&01) : error class :
1 : command executed
2 : command executed with warning
3 : syntax error
4 : semantic error
5 : system error. command rejected
6 : privilege error
7 : validation error
8 : subsystem not available

## SDD6003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD6003 COMMAND REJECTED BY REMOTE CLUSTER

### Meaning

The request is unknown by the remote cluster and can thus not be
processed.

## SDD6004

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD6004 INVALID CODED-CHARACTER-SET NAME RETURNED BY FILTER '(&00)'

### Meaning

(&00) : coded character-set name
The coded-character-set name returned by the filter
may only be EDF041 or ISO88591

### Response

Please contact Print-service Administrator.

## SDD9000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDD9000 CONFLICT BETWEEN '(&00)' AND '(&01)' OPERANDS. COMMAND REJECTED

### Meaning

The servers of a remote cluster are not known by the users of the local
cluster.
CLUSTER-NAME and SERVER-NAME may not be specified together.

### Response

Correct command and retry.

## SDD9001

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SDD9001 INVALID VALUE IN SUBSYSTEM-PARAMETER OPERAND OF (&00) DPRINTCM COMMAND

### Meaning

The subsystem-parameter operand may not be specified
oder hat einen ungueltigen Wert (/START-SUBSYSTEM).
(&00) : command name : /START-SUBSYSTEM or /STOP-SUBSYSTEM or
/RESUME-SUBSYSTEM or /HOLD-SUBSYSTEM

### Response

Correct command and retry.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages