## SFL0001

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0001 SPCONV subsystem cannot be loaded without SPOOL subsystem.

### Response

Load the SPOOL subsystem by means of the /START-SUBSYSTEM command.
Subsequent load the SPCONV subsystem.

## SFL0002

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0002 Memory allocation error for class '(&00)' memory.

### Response

Contact the system administrator.

## SFL0005

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0005 Tsn '(&00)' : Cascade of filters not supported in the frame of the interoperability.

## SFL0006

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0006 Tsn '(&01)' : Memory allocation error for class '(&00)' memory.

### Response

Contact the system administrator.

## SFL0007

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0007 Tsn '(&02)' : System error: '(&00)' interface error '(&01)'.

### Meaning

An error is occurred during the use of a system interface .
(&00) : name of the system interface.
(&01) : error code returned by the system interface.

### Response

Contact the system administrator.

## SFL0008

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0008 Tsn '(&02)' : Filter '(&00)' loading failed. $PBBND1 interface error '(&01)'.

### Meaning

An error is occurred during the loading of the filter.
(&00) : name of the filter.
(&01) : error code returned by the $PBBND1 interface.

### Response

Contact the system administrator.

## SFL0009

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0009 Tsn '(&00)' : Internal inconsistency.

### Meaning

An incoherence is appeared in a table used by the filter subsystem.

### Response

Stop and reload the filter subsystem.

## SFL0010

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0010 Tsn '(&02)' : Filter selection failed to convert the input format '(&00)' into the output format '(&01)'

### Response

Check the definition of the filter in the SPOOL PARAMETER file.

## SFL0011

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0011 Tsn '(&00)' : Read error on SPOOL PARAMETER file. Check the file.

### Response

Contact the spool administrator.

## SFL0012

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0012 Tsn '(&01)' : Filter record '(&00)' of SPOOL PARAMETER file cannot be read.

### Meaning

The filter subsystem cannot obtain the filter record (&00)
from the SPOOL PARAMETER file.

### Response

Check if the filter record always exists in the SPOOL PARAMETER file or
contact the spool administrator.

## SFL0020

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0020 Tsn '(&00)', filter '(&01)': parameter '(&02)' specified in the PRINT-DOC command is incompatible with the filter.

### Meaning

The job cannot be filtered because one parameter given in the
PRINT-DOC command is not supported by the filter (&01).
(&02) : - DOCUMENT-FORMAT
- HEADER-PAGE-TEXT
- EFO

### Response

Modify the parameter with a MOD-PR-JOB-ATT command or cancel
the job and give a new PRINT-DOC command.

## SFL0021

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0021 Tsn '(&00)', filter '(&01)': memory allocation error for class '(&02)' memory.

### Response

Contact the system administrator.

## SFL0022

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0022 Tsn '(&00)', filter '(&01)': validation error. '(&02)' not specified.

### Meaning

No value has been specified for the parameter (&02) either in
the PRINT-DOC command or in the form record of the SPOOL PARAMETER file.
(&02) : - LOOP
- ROTATION-LOOP

### Response

Modify the parameter with a MOD-PR-JOB-ATT command or cancel
the job and give a new PRINT-DOC command.

## SFL0023

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0023 Tsn '(&00)', filter '(&01)': DMS error '(&02)' during access to file '(&03)'.

### Meaning

A DMS error occurred during the access to file (&03). For more
detailed information about the DMS error code enter /HELP-MSG
in system mode or see the BS2000 manual 'SYSTEM MESSAGES'.

## SFL0024

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0024 Tsn '(&00)', filter '(&01)': '(&02)' '(&03)' cannot be read from file '(&04)'.

### Meaning

The resource specified in the user file doesn't exist or
cannot be read from the resource file (&04).
(&02) : type of the resource (FONT, SOFT-FONT, LOOP, FONT-POOL,...).
(&03) : name of the resource.

### Response

Check the resource availability in the resource file.

## SFL0025

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0025 Tsn '(&00)', filter '(&01)': user error while filtering of file '(&02)'. Invalid control byte.

### Meaning

An invalid control byte or an invalid control byte number
has been specified at the top of the page.

### Response

Check the validity of the control bytes in your file.

## SFL0026

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0026 Tsn '(&00)', filter '(&01)': user error while filtering of file '(&02)'. Record shorter than FIRST-REC value.

### Meaning

A record of the file (&02) has a length shorter than the value
given in the FIRST-REC parameter of the PRINT-DOC command.

### Response

Modify the parameter with a MOD-PR-JOB-ATT command or cancel
the job and give a new PRINT-DOC command.

## SFL0027

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0027 Tsn '(&00)', filter '(&01)': user error while filtering of file '(&02)'. Channel specified not defined.

### Meaning

The file (&02) contains a print control character (pcc) that
refers a channel not defined in the loop.

### Response

Use an other loop or modify your file.

## SFL0028

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0028 Tsn '(&00)', filter '(&01)': user error while filtering of file '(&02)'. Fob-id not found in macro '(&03)'.

### Meaning

No fob-id has been detected in the macro (&04) associated to
the fob given in the PRINT-DOC command.

### Response

Use an other fob or modify the macro.

## SFL0029

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0029 Tsn '(&00)', filter '(&01)': DMS error '(&02)' during the creation of file '(&03)'.

### Meaning

A DMS error occurred during the access to file (&03). For more
detailed information about the DMS error code enter /HELP-MSG
in system mode or see the BS2000 manual 'SYSTEM MESSAGE'.

## SFL0030

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0030 Tsn '(&00)', filter '(&01)': '(&02)' record '(&03)' cannot be read.

### Meaning

The record (&02) cannot be read from the SPOOL PARAMETER file.

### Response

Check if the record is defined in the SPOOL PARAMETER file or
contact the spool administrator.

## SFL0031

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0031 Tsn '(&00)', filter '(&01)': read error on SPOOL PARAMETER file. Check the file.

### Response

Contact the spool administrator.

## SFL0032

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0032 Tsn '(&00)', filter '(&01)': working file '(&02)' already exists.

### Meaning

A previous filtering for the same job or for a job having the
same tsn has been unsuccessfully terminated. The intermediate
file created by the filter is still present.

### Response

Erase the working file.

## SFL0033

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0033 Tsn '(&00)', filter '(&01)': SETL error on file '(&02)'.

### Response

Check the validity of the file.

## SFL0034

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0034 Tsn '(&00)', filter '(&01)': resource file '(&02)' cannot be opened.

### Response

Check if the resource file always exists or
contact the spool administrator.

## SFL0035

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0035 Tsn '(&00)', filter '(&01)': configuration file '(&02)' not correctly created.

### Meaning

The configuration file must absolutely be a SAM file with
FIXED LENGTH records.

### Response

Create a new configuration file with the correct characteristics.

## SFL0036

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0036 Tsn '(&00)', filter '(&01)': the received signature is different from the filter signature.

### Response

Either another filter has been called between the two calls to
the filter (&01) or the field containing the filter signature
in the interface parameter list has been destroyed between
the two calls.

## SFL0037

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SFL0037 Tsn '(&00)', filter '(&01)': user error while filtering of file '(&02)'. Font selection error.

### Response

Wrong TYPE1 HP control byte. The font selected with the type1
control byte has not been specified at PRINT-DOC command.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages