## EMM0001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 79

Warranty : NO

EMM0001 MEMORY LINK BOMB ERROR LOGGING ENTRY

### Response

Please send the document to your technical support.

## EMM0002

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 79

Warranty : NO

EMM0002 SLOT MANAGEMENT ERROR LOGGING ENTRY

### Response

Please send the document to your technical support.

## EMM0003

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 79

Warranty : NO

EMM0003 RELEASE PAGE ERROR LOGGING ENTRY

### Response

Please send the document to your technical support.

## EMM0005

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 79

Warranty : NO

EMM0005 PAGING DEVICE SATURATION ERROR LOGGING ENTRY

## EMM0006

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 79

Warranty : NO

EMM0006 ADDRESS SPACE SATURATION ERROR LOGGING ENTRY

## EMM0007

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 79

Warranty : NO

EMM0007 CORE SATURATION ERROR LOGGING ENTRY

## EMM0008

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM0008 SEMI-RESIDENT SATURATION LEVEL=(&00)

### Meaning

While semi-resident pages are required or pages are set semi-
resident (CSTAT-resident), a lake of frames in real memory
available for pageable pages are detected. In this case level 1
is specified. Level 0 means, there are enough pageable pages
available again.

### Response

Under VM2000 You can increase the real memory, if the guest-
system is in the corresponding attitude, otherwise the system-
load has to be reduced.

## EMM0009

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM0009 CONTIGUOUS FRAME SATURATION LEVEL=(&00)

### Meaning

Contiguous Frames means two immediately following 4K-hardware-
frames in main memory.
(&00) specifies the saturation-levels 0, 1, 2 or 3.

### Response

If the level of contiguous frames decrements to level 0 in a few
minutes, a reduction of the system-load is necessary (on /390-servers
it means a reduction of the current tasks).

## EMM2301

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2301 PAGING AREA ON VOLUME (&00). SIZE = (&01) MB

### Meaning

A paging area of size (&01) is located on volume (&00).
(&00) = VSN of the paging device
(&01) = size of the paging area in megabytes,
the format is "nnnn.nn".

## EMM2307

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2307 THE DELETION OF A PAGING-FILE ON VOLUME (&00) IS NOT POSSIBLE, BECAUSE A FILE-PROTECTION IS USED

### Meaning

The paging-file has a write-password or another protection-
attribute (GUARDS).

### Response

Please remove the write-password or the protection-attribute.

## EMM2308

Destination: CONSOLE Routing code: R Weight: 39

Warranty : NO

EMM2308 PREPARING MAIN MEMORY; (&00) OF (&01) MB PROCESSED.

## EMM2309

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : NO

EMM2309 THE SIZE OF THE BIG PAGE MEMORY IS (&00) MB.

### Meaning

The size of the Big Page Memory is specified at begin of the
system-run and every time, if the size is changed. It will
be increased, if the size of main memory is increased,
if the big page quota is increased or on lake of big pages,
after big pages are destroyed in case of CORE saturation.
It will be decreased, if the size of main memory is
decreased, if big pages are destroyed in case of
CORE saturation or if the big page quota is decreased.
(see command MODIFY-MEMORY-PARAMETERS).
The size of the big page memory does not always
corresponds to the specified BIG-PAGE-QUOTA in
MEMORY parameter service or specified by the command.
MODIFY-MEMORY-PARAMETERS. It is dependent from the
size and minimum size of main memory, and from the number
of generated LM's (if more LM's, then less big pages).

## EMM2310

Destination: CONSOLE Routing code: R Weight: 79

Warranty : NO

EMM2310 THE SIZE OF MAIN MEMORY IS (&00) MB; THE MINIMAL SIZE OF MAIN MEMORY IS (&01) MB.

## EMM2311

Destination: CONSOLE Routing code: R Weight: 79

Warranty : NO

EMM2311 MEMORY-RECONFIGURATION STARTED, CURRENT MEMORY SIZES: (&00) / (&01), DESTINATION MEMORY SIZES (&02) / (&03)

### Meaning

(&00): current memory size in megabytes,
(&01): current minimal memory size in megabytes,
(&02): destination memory size in megabytes,
(&03): destination minimal memory size in megabytes.

## EMM2312

Destination: CONSOLE Routing code: R Weight: 79

Warranty : NO

EMM2312 MEMORY-RECONFIGURATION HAS BEEN SUCCESSFULLY PROCESSED

## EMM2313

Destination: CONSOLE Routing code: R Weight: 79

Warranty : NO

EMM2313 MEMORY-RECONFIGURATION HAS BEEN PARTIALLY PROCESSED OR ERRONEOUSLY COMPLETED. CURRENT MEMORY SIZES: (&00) / (&01)

### Meaning

(&00): current memory size in megabytes,
(&01): current minimal memory size in megabytes.

## EMM2314

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2314 UNUSED PAGING-FILES CANNOT BE FOUND AT ANY TIME

### Meaning

The message indicates, that the command
SHOW-PAGING-CONFIGURATION cannot always found all
unused paging-files on the attached volume-devices.
One assumption is, that the corresponding pubset
of the volume is imported.

## EMM2316

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2316 The SIZE OF PAGING-FILE ON VOLUME (&00) EXCEEDS THE MAXIMUM ALLOWED SIZE OF 2048 GB

### Meaning

Paging-files > 2048 GB can not be accepted in the paging-
area.

### Response

Please destroy the specified paging-file and create,
if necessary, a smaller paging-file on the volume.

## EMM2317

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2317 THE SIZE OF VOLUME(S) - MARKED WITH * - IS INCREASED BY 25%, BECAUSE THE PAM-KEYS ARE USED AS PAGING-AREA

### Meaning

On some volumes (Device-type D3435) the PAM-Keys are also used as
Paging-Area. A PAM-Key has the size of 512 bytes, so the total
size of the Paging-file is greater by 25% in used case than in
unused case, as it is specified by the output of the unused volumes
calling command SHOW-PAGING-CONFIGURATION or by the output of the
file-attributes calling SHOW-FILE-ATTRIBUTES.

## EMM2350

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2350 BIG PAGE MEMORY IS NOT SUPPORTED ON /390-SERVERS

## EMM2401

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM2401 INCONSISTENCY BETWEEN MEMORY MANAGEMENT AND I/O MANAGEMENT

### Meaning

In module EMMPGFIX an inconsistency has been detected during defixing of
I/O pages in Main Memory.

### Response

Take SLED and send it to your technical support.

## EMM2501

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

EMM2501 ADDRESS TRANSLATION INCONSISTENCY. EMMASAM WAS CALLED BY: (&00)

### Meaning

Called ASAM-function can not be executed. Possible causes:
- ASAM-object (address-space, segment, page) is addressed in a wrong way.
- State of the ASAM-object does not allow the called function.
- Internal ASAM-data are inconsistent.

### Response

Please take sled and send it to your technical support.

## EMM2502

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

EMM2502 GET/RELEASE PG-LOCK EXCEPTION CAUSED BY $ASLOCK USER. $ASLOCK WAS CALLED BY: (&00) LM#=(&01) STATE=(&02) RC=(&03)

### Response

Please take sled and send it to your technical support.

## EMM2601

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2601 RMM DETECTS INCONSISTENT DATA: ADDRESS OF CALLER: (&00)

### Meaning

Central RMM error routine: inconsistent data structures are detected
whilst processing called function.

### Response

Please take sled and send it to your technical support.

## EMM2701

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2701 AR-ADDRESS TRANSLATION INCONSISTENCY. EMMALAM WAS CALLED BY: (&00)

### Meaning

Called ALAM-function can not be executed. Possible causes:
- ALAM-object (access_list, space, connection) is addressed in a wrong
way.
- Internal ALAM-data are inconsistent.

### Response

Take sled and send it to your technical support.

## EMM2800

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2800 SYSTEM ERROR OCCURED

### Response

Please contact your technical support.

## EMM2801

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2801 OPERATION (&00) IS NOT SUCCESSFULLY PROCESSED FOR ALL OPERANDS AND LIST-ELEMENTS

### Meaning

If a list of objects or a number of operands, to be executed
one after the other, is specified, this return-code means, that
an error occured during the processing of more than one object.

### Response

Please observe the additional specified messages.

## EMM2802

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2802 OPERATION (&00) IS NOT ALLOWED FOR THE SPECIFIED OPERAND

### Meaning

The object, specified by the operand, has not the necessary
properties (p.e. file-attributes), to execute the operation.

### Response

Please observe the additional specified message.

## EMM2803

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2803 MEDIUM OF THE SPECIFIED OPERAND IS NOT ALLOWED FOR OPERATION (&00)

### Meaning

A medium is a pubset, to which the paging-file belongs, a
volume, on which the paging-file is created. Is
this command-return-code returned, so the specified operation is
not allowed on the medium.

### Response

Please observe the additional specified message.

## EMM2804

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2804 STATE OF THE SPECIFIED OPERAND IS NOT ALLOWED FOR OPERATION (&00)

### Meaning

The paging-file is not in the state at the moment,
to allow the specified operation.

### Response

Please recognize the state by observing the additional specified message,
which the object must have, to allow the operation.

## EMM2805

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2805 STATE OF MEDIUM OF THE SPECIFIED OPERAND IS NOT ALLOWED FOR OPERATION (&00)

### Meaning

A medium is either a pubset, to which the paging-file belongs, a
volume, on which the paging-file is created. The
command-return-code is returned, if this medium has not the state, to
allow the specified operation.

### Response

Please recognize the state by observing the additional specified message,
which the medium must have, to allow the operation.

## EMM2806

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2806 OPERATION (&00) BREAKS PRESCRIBED LIMITS

### Meaning

The management of the virtual address space and of the paging-area
requires a number of determined limits, which may not be exceeded and
so the command is aborted.

### Response

Please recognize the concerned limit by observing the additional specified
message.

## EMM2807

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2807 OPERATION (&00) IS NOT EXECUTABLE BECAUSE OF LACK OF RESOURCES; PROCESSING IS STOPPED

### Meaning

There is a lack of resources, which is not recoverable without any
operation doing by the caller of this command. So the command is
aborted.

### Response

Please recognize the lack of resources by observing the additional
specified message.

## EMM2808

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2808 THE OPERATION (&00) WAITS FOR THE TERMINATION OF THE RUNNING IMPORT-PROCESS OF THE PUBSET (&01)

### Response

Please check, if there is a question on console according to the
import of the pubset waiting for response.

## EMM2809

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2809 SYSTEM ERROR IN PAGING-MANAGEMENT TERMINATES THE CALLER TASK

### Meaning

An error in the paging area management forces a termination of
the caller task, to be able, to diagnose the error. If the task
is a system-task, the session is abnormally terminated. A reason
for
the error possibly lies in the management of the used task locks.

### Response

Please take systemdump or sled and send it to your
technical support.

## EMM2810

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2810 PAGING-ERROR-LOGGING-ENTRY IN MODULE (&00); INCORRECT PARAMETERLIST IS: (&01)

### Meaning

By writing Error-Logging-entries internal errors are noticed, which have
no direct influence on the processing of the paging-files
or which support the diagnosis of an error.

### Response

Please send the document to your technical support.

## EMM2811

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2811 PAGING-FILE ALREADY EXISTS ON VOLUME (&00)

### Meaning

There already is a paging-file with the name SYS.PAGING.<vsn> on the
specified volume. A new creation of the paging-file is not possible.

### Response

Please delete the old paging-file with DELETE-PAGING-FILE.

## EMM2812

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2812 THE CREATION OF A PAGING-FILE ON VOLUME (&00) IS NOT ALLOWED IN A SHARED PUBSET

### Meaning

The creation of a paging-file is only possible in an exclusive SF- or
SM-Pubset.

### Response

Please organize your paging-files in exclusive SF- or SM-pubsets as
described in the manual.

## EMM2813

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2813 THE CREATION OF A PAGING-FILE ON VOLUME (&00) IS NOT ALLOWED

### Meaning

Paging-files may not lie in volumes
emulated on the Global Storage.
So the creation will be refused.

### Response

Please use volumes on disk.

## EMM2814

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2814 THE PUBSET OR THE VOLUME-SET OF THE SM-PUBSET (&00), WHERE THE PAGING-FILE SHALL BE CREATED ON VOLUME (&01), IS NOT IMPORTED

### Meaning

The creation of a paging-file requires, that the corresponding pubset
is imported and that in case of a SM-pubset the concerned volume-set
is available.

### Response

Please import the corresponding pubset (in case of a SM-pubset with
the concerned volume-set).

## EMM2815

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2815 THERE IS NOT ENOUGH SPACE ON VOLUME (&00), TO CREATE THE PAGING-FILE

### Meaning

There is not enough space for the new paging-file on the
volume in the specified size.

### Response

Please delete some other files, specify a smaller size for the paging-file
or take another volume.

## EMM2816

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2816 THE OPERATION (&00) CANNOT BE DONE FOR THE PUBSET (&01), BECAUSE IT IS A SHARED PUBSET

### Meaning

Paging file may only be taken in use, if it belongs to an
exclusive SF pubset.

### Response

Import exclusively the pubset.

## EMM2817

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2817 THE VOLUME SPECIFICATION IS WRONG, THE VOLUME (&00) IS UNKNOWN

### Meaning

There is a syntax-error in the volume-specification or the
specified volume is unknown in the current configuration.

### Response

Please repeat the command with the correct volume-specification.

## EMM2818

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2818 THE OPERATION (&00) CAN NOT BE EXECUTED FOR THE OBJECT (&01) BECAUSE OF AN INTERNAL ERROR

### Meaning

An entry is written in the error logging file, to diagnose
the error.

### Response

Please send the error logging file to your
technical support.

## EMM2819

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2819 THE COMMAND (&00) IS NOT EXECUTABLE FOR THE OBJECT (&01) BECAUSE OF LACK OF RESSOURCES

### Meaning

The execution of the command needs some ressources, which are
not available at the moment.

### Response

Please wait some minutes or reduce your system-load. After then
You can start another try.

## EMM2820

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2820 THE OPERATION (&00) CANNOT BE DONE FOR THE PUBSET (&01), BECAUSE THE PUBSET IS NOT IMPORTED

### Meaning

The operation is only possible, if the specified pubset
is exclusively imported or the concerned volume set of
a SM pubset is exclusively available.

### Response

Please import the corresponding pubset (in case of a SM pubset
with the concerned volume set).

## EMM2821

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2821 THERE IS NO PAGING-FILE ON VOLUME (&00)

### Meaning

There is no paging-file to delete.

## EMM2822

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2822 THE PAGING-FILE ON VOLUME (&00) IS STILL USED FOR PAGING

### Meaning

The paging-file can only be deleted, if it is not used anymore by
paging.

### Response

Please cancel the use by paging using the command REDUCE-PAGING-AREA
VOLUME=... or renounce the deletion.

## EMM2823

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2823 THE PUBSET OR THE VOLUME-SET OF THE SM-PUBSET (&00), WHERE THE PAGING-FILE ON VOLUME (&01) SHALL BE DELETED, IS NOT IMPORTED

### Meaning

The deletion of the paging-file is only possible, if the corresponding
pubset is imported and the concerned volume-set of a SM-pubset is
available.

### Response

Please import the corresponding pubset (in case of a SM-pubset with
the concerned volume-set).

## EMM2824

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2824 THE OPERATION (&00) CANNOT BE DONE FOR THE PUBSET (&01), BECAUSE THE MRSCAT-ENTRY IS MISSING

### Meaning

The operation is only possible, if there exists a MRSCAT entry
for the pubset

### Response

Please create a MRSCAT entry for the pubset.

## EMM2825

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2825 THE OPERATION (&00) CANNOT BE EXECUTED BECAUSE OF AN I/O-ERROR ON VOLUME (&01)

### Meaning

Probably there is an error on the specified volume.

### Response

Please check the volume and perform the corresponding corrections.

## EMM2826

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2826 THE OPERATION (&00) CANNOT BE DONE FOR THE PUBSET (&01), BECAUSE IT CONTAINS GS-VOLUMES

### Meaning

Paging-files can not be used on volumes emulated on Global
Storage.

### Response

Please delete the paging-file with DELETE-FILE or
DELETE-PAGING-FILE and create a new paging-file on a volume
without emulation on GS.

## EMM2828

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2828 THE OPERATION (&00) CAN NOT BE CONTINUED BECAUSE OF AN INTERNAL ERROR

### Meaning

An entry is written into the error logging file, to
diagnose the error.

### Response

Please send the error logging file to your
technical support.

## EMM2829

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2829 THE OPERATION (&00) IS NOT CONTINUABLE BECAUSE OF LACK OF RESSOURCES

### Meaning

The execution of the operation needs some ressources, which
are not available at the moment.

### Response

Please wait some minutes or reduce your system-load. After then
You can start another try.

## EMM2830

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2830 THE PAGING-FILE ON VOLUME (&00) IS ALREADY IN USE BY PAGING

### Meaning

The paging-file is already in use, there is nothing to do.

## EMM2832

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2832 THERE IS NO PAGING-FILE ON VOLUME (&00)

### Response

Please create a paging-file on the volume.

## EMM2834

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2834 THE PUBSET, WHERE THE PAGING-FILE ON VOLUME (&00) SHALL EXTEND THE PAGING-AREA, IS A SHARED PUBSET; THIS IS NOT ALLOWED

### Meaning

A paging-file may only be taken in use, if it belongs to an
exclusive SF- or SM-pubset.

### Response

Please import the pubset exclusive and then take the paging-
-file in use.

## EMM2835

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2835 THE VOLUME (&00), WHICH PAGING-FILE SHALL EXTEND THE PAGING-AREA, IS NOT ALLOWED

### Meaning

Paging-files can not be used on volumes emulated on Global Storage.

### Response

Please delete the paging-file with DELETE-FILE or DELETE-PAGING-FILE
and create a new paging-file on a volume without emulation on GS.

## EMM2836

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2836 THE PUBSET OR THE VOLUME-SET OF THE SM-PUBSET (&00), WHICH PAGING-FILE ON VOLUME (&01) SHALL EXTEND THE PAGING-AREA, IS NOT IMPORTED

### Meaning

The extension of the paging-area by the specified paging-file requires,
that the corresponding pubset is imported and that the concerned
volume-set of the SM-pubset is available.

### Response

Please import the corresponding pubset (in case of a SM-pubset with
the concerned volume-set).

## EMM2837

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2837 THE PAGING-FILE ON VOLUME (&00) HAS NOT THE REQUIRED FILE-ATTRIBUTES

### Meaning

The paging-file is probably not created with the command
CREATE-PAGING-FILE or SIR. It seems to be created by the command
CREATE-FILE and the further necessary attributes are not added to this
file.

### Response

Please destroy the paging-file with DELETE-FILE or DELETE-PAGING-FILE
and create a new file with CREATE-PAGING-FILE or SIR as described in
the manual.

## EMM2838

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2838 THE MASTER-CATALOG-ENTRY OF THE PUBSET (&00) IS MISSING, WHICH PAGING-FILE ON VOLUME (&01) SHALL BE PROCESSED

### Meaning

During the command-processing of the paging-commands the missing of the
Master-Catalog-entry is determined.

### Response

Please generate a new Master-Catalog-entry for the pubset and import the
pubset, before repeating the command.

## EMM2839

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2839 THE VOLUME (&00), WHICH PAGING-FILE SHALL EXTEND THE PAGING-AREA, CAN NOT BE RESERVED BY PAGING

### Meaning

A volume can only be reserved by paging, if it is reserved by the
pubset-management or by nobody else. The reservation at the moment
is not permitted together with the paging-reservation.

### Response

Please cancel the current reservation and repeat the command
EXTEND-PAGING-AREA for the paging-file.

## EMM2840

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2840 THE EXTENSION BY THE PAGING-FILE ON VOLUME (&00) EXCEEDS THE MAXIMAL SIZE OF THE PAGING AREA

### Meaning

At the moment the maximal size of the paging-area is 4 TB.

## EMM2841

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2841 THE PUBSET SPECIFICATION IS WRONG, THE PUBSET (&00) IS UNKNOWN

### Meaning

There is a syntax error in the pubset specification or the
specified pubset is unknown in the current configuration.

### Response

Please repeat the command with the correct pubset specification.

## EMM2842

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2842 THE NUMBER OF USED PAGING-FILES (VOLUMES) EXCEEDS WITH VOLUME (&00) THE MAXIMAL ALLOWED NUMBER

### Meaning

At the momemt there are maximal 4096 paging-files on volumes allowed.

## EMM2843

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2843 THE PAGING-FILE OF PUBSET (&00) ON VOLUME (&01) WILL NOT BE DESTROYED

### Meaning

By destruction of the paging-file of the home-pubset or
of a paging file, which volume is specified in the
PAGING parameter service, an automatic of the system
cannot be possible any more. So the destruction will be
refused.

### Response

It is possible, to delete the paging file with operand
FORCE=*YES. Before the deletion it is recommendable in
case of the use of the home pubset, to create a new
paging-file in sufficient size on another volume of the
home pubset, or in case of the use of the PAGING
parameter service, to update the parameter service
file with volumes, which contains paging files in
sufficient size, that the minimum size of 200 MB
will be exceeded.

## EMM2844

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2844 THE PAGING AREA OF (&00) GB, WHICH IS SPECIFIED DURING THE SYSTEM-INITIATION, EXCEEDS THE MAXIMUM SIZE OF THE PAGING-AREA

### Meaning

At the moment the maximal size of the paging-area is 4 TB.
The system-initialization will be continued.

### Response

Please specify in the Parameter-Service less or
smaller paging-files, so that your paging-area does not exceed this
border.

## EMM2845

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2845 THERE ARE NOT FOUND ANY UNUSED PAGING FILES TO ADD IN THE PAGING AREA

### Meaning

When calling the command EXTEND-PAGING-AREA with
VOLUME=*ALL, no unused paging files are found.
Possibly pubsets with existing paging files are not exclusively
imported.

### Response

Please create new paging files or import exclusively pubsets
with existing paging files.

## EMM2846

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2846 THE SYSTEM INITIATION CAN NOT BE EXECUTED BECAUSE OF AN INTERNAL ERROR DURING THE INITIALIZATION OF THE PAGING MANAGEMENT

### Response

Please contact your technical support.

## EMM2847

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2847 THE SYSTEM INITIATION IS NOT EXECUTEABLE BECAUSE OF LACK OF RESSOURCES DURING THE INITIALIZATION OF THE PAGING-MANAGEMENT

### Meaning

The necessary ressources, to execute the initialization of the
Paging-Management, are not available.

### Response

Please contact your technical support.

## EMM2848

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2848 VOLUME (&00) IS NOT USED IN PAGING-AREA, BUT IS STILL RESERVED

### Meaning

IF a paging-area greater than the maximum size of the paging-area
(4 TB) is constructed during the system initiation, the unnecessary
paging-volumes are ignored. One of these volumes are specified by
this message. Even if the volume is not used by paging, the volume
remains reserved until a command REDUCE-PAGING-AREA is specified.

### Response

Please create your paging-files in the way,
that the maximum size of the paging-area will not be exceeded.

## EMM2850

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2850 THE SIZE OF THE PAGING AREA IS: (&00) MB; THE RESERVED SIZE OF THE PAGING AREA IS: (&01) MB

### Meaning

The two important values of the virtual address space management
are specified: the maximum size of the sum of all virtual
address and data spaces of all tasks and the sum of the really
used pages in the virtual address and data spaces.

### Response

If the size of the used virtual memory gets near the size of
the available virtual memory, then we advise, to extend the
paging-area.

## EMM2851

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2851 THE PAGING-FILE ON VOLUME (&00) IS NOT USED BY PAGING

### Meaning

The paging-file is not used by paging, so a reduction of the paging-area
by this paging-file or a modification of the paging-area-attributes
makes no sense.

## EMM2853

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2853 THE REDUCTION OF THE PAGING-AREA BY THE PAGING-FILE ON VOLUME (&00) LEADS TO AN UNDERFLOW OF THE MINIMAL NECESSARY SIZE OF THE PAGING AREA

### Meaning

By executing the required reduction there is not enough paging-area
(=virtual address space) available, a saturation-state is entered,
which can lead to a system-stop. This is not allowed.

### Response

If the release of the specified volume is necessary, then extend the
paging-area with another paging-file, which has at least the same size
as the one, to be released, and after this start the reduction again.

## EMM2854

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2854 THE OPERATION (&00) IS NOT ALLOWED FOR SM PUBSET (&01) BY PUBSET SPECIFICATION

### Meaning

The creation of paging files shall not be done on all
volumes of a SM pubset.

### Response

Please use exclusiv SF pubsets or use the VSN specification,
to create a paging file in a volume of a SM pubset.

## EMM2855

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2855 A REDUCTION OF THE PAGING-AREA BY THE PAGING-FILE ON VOLUME (&00) IS NOT POSSIBLE, BECAUSE A REDUCTION OF MAIN MEMORY TAKES PLACE AT THE SAME TIME

### Response

Please wait until the main memory reduction is finished and
repeat the order.

## EMM2857

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2857 TASK WAITS, UNTIL THE DESTRUCTION OF THE PAGING-FILE ON VOLUME (&00) IS EXECUTED

### Meaning

The task of the specified Paging command (CREATE-PAGING-FILE,
EXTEND-PAGING-AREA) has caused a DELETE-PAGING-FILE command
for the specified volume, which is not finished until now.

## EMM2858

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2858 TASK WAITS, UNTIL THE REDUCTION OF THE PAGING-AREA BY VOLUME (&00) IS EXECUTED

### Meaning

The task of the specified Paging command (DELETE-PAGING-FILE,
EXTEND-PAGING-AREA) has caused a REDUCE-PAGING-AREA command
for the specified volume, which is not finished until now.

## EMM2860

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2860 WARNING! THE OPERAND-VALUE (&00) IS SPECIFIED SEVERAL TIMES

### Meaning

For an operand a list is specified, which contains a value
several times. The operation is processed only one time for
this value.

### Response

Please check the command.

## EMM2863

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2863 THERE ARE NO UNUSED PAGING-FILES

### Meaning

This message is given by calling the command SHOW-PAGING-CONFIGURATION,
when the unused paging-files shall be specified on SYSOUT, but there are
no ones.

## EMM2865

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2865 THERE IS NO PAGING-FILE ON VOLUME (&00)

### Meaning

This message is given by calling the command SHOW-PAGING-CONFIGURATION,
when for a paging-file on a specific volume is asked and this paging-file
does not exist.

## EMM2867

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM2867 THE EXISTENCE OF THE PAGING-FILE ON VOLUME (&00) IS UNKNOWN

### Meaning

This message is given by calling the command SHOW-PAGING-CONFIGURATION,
when for a paging-file on a specific volume is asked, but the existence
of the file can not be found out, because (p.e.) the corresponding pubset
is not or shared imported.

### Response

Please prepare your system in the way p.e. by importing of the
corresponding pubsets, that the required informations are available.

## EMM2868

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2868 THE EXISTENCE OF THE PAGING FILES OF THE PUBSET (&00) IS UNKNOWN

### Meaning

The existence of a paging file cannot be determined for the
pubset specified in the SHOW-PAGING-CONFIGURATION command.
Possible causes: the pubset is not imported, shared imported
or unknown.

### Response

If necessary, please import the concerned pubset.

## EMM2869

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2869 THERE IS NO PAGING FILE IN PUBSET (&00)

### Meaning

For the pubset specified in the SHOW-PAGING-CONFIGURATION command there
exist no paging files.

## EMM2870

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2870 THE PAGING-FILE ON VOLUME (&00) IS NOT PROTECTED AGAINST COMMAND DELETE-FILE (ERASE)

### Meaning

This message will be specified during the import of a pubset,
if a paging-file in this pubset is used in the paging-area and
the protection against the deletion of the paging-file can
not be installed.

### Response

Please avoid a deletion of the paging-file.

## EMM2877

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2877 THE COMMISSION TO DELETE THE PAGING-FILE ON VOLUME (&00) IS FINISHED WITH ERRORS

### Meaning

The message will be specified calling command
SHOW-PAGING-CONFIGURATION with operands VOLUME=*UNUSED/*ALL/<vsn>,
INFORMATION=*ALL, when the commission is finished with errors and
not sent to the caller or console until now. The cause of the
error will be sent to the caller of the commission and/or console.

## EMM2878

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2878 THE COMMISSION TO REDUCE THE PAGING-AREA BY VOLUME (&00) IS FINISHED WITH ERRORS

### Meaning

The message will be specified calling command
SHOW-PAGING-CONFIGURATION with operands VOLUME=*USED/*ALL/<vsn>,
INFORMATION=*ALL, when the commission is finished with errors
and not sent to the caller or console until now. The cause of the
error will be sent to the caller of the commission and/or console.

## EMM2880

Destination: USER-TASK Routing code: Weight: 79

Warranty : YES

EMM2880 THE COMMAND (&00) CANNOT BE EXECUTED ASYNCHRONOUSLY, THE SYNCHRONOUS MANAGEMENT IS STARTED

### Meaning

If an error is found during the creation of an asynchronous
commission, in the way that the commission cannot be
transmitted to the server task, the command will be
performed synchronously in the caller task.

## EMM2881

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2881 SYSTEM ERROR IN MEMORY MANAGEMENT CAUSES SNAPSHOT

### Meaning

An error in memory management provokes a snapshot.
The error does not lead to system- or task-
termination; after producing the snapshot, the
system-run continues.

### Response

Take snapshot and send it to your
technical support.

## EMM2882

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2882 ERROR IN PAGING MANAGEMENT LEADS TO SYSTEM TERMINATION! ADDRESS OF CALLER: (&00)

### Meaning

Performing the different purposes of the paging management
an inconsistent state of the paging data was found. To
analyse the problem, the system was terminated.

### Response

Take SLED and send it to your technical support.

## EMM2885

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2885 THE COMMISSION TO DELETE THE PAGING-FILE ON VOLUME (&00) IS ACCEPTED

### Meaning

The commission will be executed in a server-task. The message tells
the caller, that the commission is sent to the server-task.

## EMM2886

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2886 THE COMMISSION TO REDUCE THE PAGING-AREA BY VOLUME (&00) IS ACCEPTED

### Meaning

The commission will be executed in a server-task. The message tells
the caller, that the commission is sent to the server-task.

## EMM2888

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2888 THE COMMISSION TO DELETE THE PAGING-FILE ON VOLUME (&00) CANNOT BE EXECUTED BECAUSE OF TERMINATION OF THE SERVER-TASK

### Meaning

Ther server-task executing the commission was terminated.
The server-task was probably terminated because of an
internal error.

### Response

Please see messages of the server-task.

## EMM2889

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : YES

EMM2889 THE COMMISSION TO REDUCE THE PAGING-AREA BY VOLUME (&00) CANNOT BE EXECUTED BECAUSE OF TERMINATION OF THE SERVER-TASK

### Meaning

Ther server-task executing the commission was terminated.
The server-task was probably terminated because of an
internal error.

### Response

Please see messages of the server-task.

## EMM2891

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2891 THE COMMISSION TO DELETE THE PAGING-FILE ON VOLUME (&00) WAITS FOR EXECUTION IN THE SERVER-TASK

### Meaning

The server-task executing the commission is busy with other
commissions.

## EMM2892

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2892 THE COMMISSION TO REDUCE THE PAGING-AREA BY VOLUME (&00) WAITS FOR EXECUTION IN THE SERVER-TASK

### Meaning

The server-task executing the commission is busy with other
commissions.

## EMM2894

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2894 THE COMMISSION TO DELETE THE PAGING-FILE ON VOLUME (&00) IS JUST IN EXECUTION IN THE SERVER-TASK

### Meaning

The server-task executing the commission is still busy with
the commission.

## EMM2895

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2895 THE COMMISSION TO REDUCE THE PAGING-AREA BY VOLUME (&00) IS JUST IN EXECUTION IN THE SERVER-TASK

### Meaning

The server-task executing the commission is still busy with
the commission.

## EMM2897

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2897 THE COMMISSION TO DELETE THE PAGING-FILE ON VOLUME (&00) IS SUCCESSFULLY EXECUTED

### Meaning

This is the final message of an asynchron commission.

## EMM2898

Destination: USER-TASK, CONSOLE Routing code: R Weight: 79

Warranty : YES

EMM2898 THE COMMISSION TO REDUCE THE PAGING-AREA BY VOLUME (&00) IS SUCCESSFULLY EXECUTED

### Meaning

This is the final message of an asynchron commission.

## EMM2900

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2900 THE EMM-FUNCTION-CONTROL INITIALIZATION OF THE STARTUP IS NOT EXECUTABLE BECAUSE OF UNKNOWN HSI.

## EMM2901

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2901 SPECIFIED SHRSIZE IN MEMORY-PARAMETER-SERVICE IS TO HIGH.

## EMM2902

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2902 WRONG SHRSIZE IN MEMORY-PARAMETER-SERVICE.

## EMM2903

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2903 SPECIFIED SYSSIZE IN MEMORY-PARAMETER-SERVICE INVALID.

## EMM2904

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2904 VASSIZE NOT PROVIDED - SYSSIZE IN MEMORY-PARAMETER-SERVICE TOO HIGH.

## EMM2905

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2905 SPECIFIED SCALAR RAS-SIZE IN MEMORY-PARAMETER-SERVICE IS INVALID.

## EMM2906

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2906 WRONG MEMORY-RECONFIGURATION-PARAMETERS SPECIFIED IN MEMORY-PARAMETER-SERVICE.

## EMM2907

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2907 INVALID WORK-SPACE-CTRL SPECIFIED IN MEMORY-PARAMETER-SERVICE.

## EMM2908

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2908 INVALID ASAM-CTRL SPECIFIED IN MEMORY-PARAMETER-SERVICE.

## EMM2909

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2909 INVALID ALAM-CTRL SPECIFIED IN MEMORY-PARAMETER-SERVICE.

## EMM2910

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2910 THE FIRST ES-BLOCK IST GREATER THAN THE LAST ES-BLOCK, OR THE FIRST ES-BLOCK IS ZERO IN MEMORY-PARAMETER-SERVICE.

## EMM2911

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2911 DAB-AREA IS GREATER THAN TOTAL ES-SIZE IN MEMORY-PARAMETER-SERVICE.

## EMM2912

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2912 SEGMENT TABLE NOT ALIGNED ON 4-K-BOUNDARY AT CREATION OF THE STARTUP-ADDRESS-SPACE.

## EMM2913

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2913 DIFFERENT VERSIONS OF SYSTEM-FC AND STARTUP-FC FOUND.

## EMM2914

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2914 DIFFERENT VERSION NUMBERS OF SYSTEM-EMMDINIT AND STARTUP-FC FOUND.

## EMM2915

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2915 DIFFERENT VERSION NUMBERS OF SYSTEM-EMMINITC AND STARTUP-EMMINITC FOUND.

## EMM2916

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2916 ERROR DURING TLT-ACCESS TO GET THE TASKID OR TCB.

## EMM2917

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2917 THE CREATION OF THE GLOBAL ACCESS LIST FAILED.

## EMM2918

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2918 THE CREATION OF THE SYSTEM ACCESS LIST FAILED. ALAM RESSOURCES TEMPORARILY EXHAUSTED.

## EMM2919

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2919 THE CREATION OF THE SYSTEM ACCESS LIST FAILED. ALAM ADDRESS ERROR (BAD ERROR).

## EMM2920

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2920 THE CREATION OF THE SYSTEM ACESS LIST FAILED. COULD NOT GET ACCESS LIST DESIGNATION.

## EMM2921

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2921 THE CREATION OF THE SYSTEM ACCESS LIST FAILED. COULD NOT GET ADDRESS OF THE ACCESS LIST.

## EMM2922

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2922 THE CREATION OF THE SYSTEM ACCESS LIST FAILED. COULD NOT GET THE ADDRESS OF THE ACCESS LIST EXTENSION.

## EMM2923

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2923 THE CREATION OF SHADOW SPACE FOR SLED FAILED. LACK OF AREA IN ASAM POOL.

## EMM2924

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2924 THE CREATION OF SHADOW SPACE FOR SLED FAILED. ASAM ADDRESS ERROR AT ASAM CALL.

## EMM2925

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2925 LACK OF AREA IN ASAM-POOL AT CREATION OF FIRST ADDRESS SPACE OR AT ATTACH OF DAT TO IPL-CPU FOR STARTUP.

## EMM2926

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2926 ASAM ADDRESS ERROR AT CREATION OF FIRST ADDRESS SPACE OR AT ATTACH OF DAT TO IPL CPU.

## EMM2927

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2927 CREATION OF DAT-TABLES FOR STARTUP FAILED. LACK OF AREA IN ASAM POOL

## EMM2928

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2928 CREATION OF DAT-TABLES FOR STARTUP FAILED. ASAM ADDRESS ERROR.

## EMM2929

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2929 LACK OF AREA IN ASAM-POOL ON CREATION OF PAGE TABLES FOR THE SYSTEM PART OF FIRST ADDRESS SPACE.

## EMM2930

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2930 CREATION OF PAGE TABLES FOR THE SYSTEM PART OF FIRST ADDRESS SPACE FAILED. ASAM ADDRESS ERROR.

## EMM2931

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2931 REQUEST OF CLASS2 MEMORY FAILED BECAUSE OF SATURATION OR ERROR IN REQM-PARAMETERS.

## EMM2932

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2932 SERIOUS SVP-CALL ERROR IN GET-FUNCTION-INFORMATION.

## EMM2933

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2933 SERIOUS SVP-CALL ERROR ON TRYING TO GET HIGHEST SE-NUMBER.

## EMM2934

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2934 INITIALIZATION OF DATA FOR RECONFIGURATION OF PHYSICAL STORAGE ELEMENTS FAILED. TOO MANY STORAGE ELEMENTS..

## EMM2935

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2935 SVP-ERROR ON STORAGE-ELEMENT-INFORMATION-CALL.

## EMM2936

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2936 EXTENSION OF DAT TABLES FAILED. ASAM ADDRESS ERROR.

## EMM2937

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2937 CREATION OF DAT TABLES FOR SHARED CODE FAILED. ASAM ADDRESSFEHLER.

## EMM2938

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2938 I/O SHARING FAILED. LACK OF AREA IN ASAM-POOL.

## EMM2939

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2939 I/O SHARING FAILED. ASAM ADDRESS ERROR.

## EMM2940

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2940 CREATION OF BITMAPS FOR VMM FAILED BECAUSE OF SATURATION.

## EMM2941

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2941 CREATION OF BITMAPS BY VMM FAILED. ERROR IN REQM PARAMETERS.

## EMM2942

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2942 INITIALIZATION OF USER ADDRESS SPACE FAILED.BAD RETURN CODE FROM EMM5CREA.

## EMM2943

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2943 VAS-INITIALIZATION FAILED. TASK IS NOT PREALLOCATED.

## EMM2944

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2944 SPECIFIED SHXSIZE MEMORY-PARAMETER-SERVICE IS TOO HIGH.

## EMM2945

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2945 SPECIFIED SHXSIZE IN MEMORY-PARAMETER-SERVICE IS NOT ALIGNED.

## EMM2946

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2946 HSA ADDRESS NOT ABOVE BS2000-START-ADDRESS.SCPINFO-DATA NOT OK.

## EMM2947

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2947 NO HSA EXISTING. SCPINFO DATA NOT OK.

## EMM2948

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2948 NOT ENOUGH PREALLOCATED PAGES TO FILL THE FREE-QUEUE OF THE ASAM-POOL.

## EMM2949

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2949 CREATION OF DAT TABLES FOR EXTENDED SHARED CODE FAILED. ASAM ADDRESS ERROR.

## EMM2950

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2950 NOT ENOUGH GLOBAL SEGMENTS TO CREATE PAGES OF CLASS1-EXEC. EMMPREPA IN MODULE EMMINIT1 MUST BE INCREASED.

## EMM2951

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2951 NOT ENOUGH GLOBAL SEGMENTS TO CREATE EXPDT-PAGES. EMMPREPA IN EMMINIT1 MUST BE INCREASED.

## EMM2952

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2952 SPECIFIED SYSSIZE IN MEMORY-PARAMETER-SERVICE INCREASED TO MINIMUM SYSSIZE VALUE

## EMM2953

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

EMM2953 MAIN MEMORY IS TO SMALL. SCPINFO DATA MAY BE WRONG

## EMM2954

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

EMM2954 HW-PAGESIZE NOT SUPPORTED IN CURRENT SYSTEM, SCPINFO-DATA NOT O.K.

## EMM2955

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

EMM2955 SPECIFIED SYSSIZE IN MEMORY-PARAMETER-SERVICE INCOHERENT WITH DEFAULTED ADDRESS SPACE SIZE. ADDRESS SPACE SIZE NOW INCREASED.

## EMM2956

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2956 SPECIFIED PAGING-GSSIZE IN MEMORY-PARAMETER-SERVICE IS HIGHER THAN THE MAXIMUM SIZE OF THE TOTAL PAGING AREA

## EMM2957

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2957 SPECIFIED BIGPG-QUOTA IN MEMORY-PARAMETER-SERVICE IS HIGHER THAN 99 %

## EMM2958

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2958 SPECIFIED SHR-BIGPG-SIZE IN MEMORY-PARAMETER-SERVICE IS HIGHER THAN 256 MB

## EMM2959

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2959 SPECIFIED SHR-BIGPG-SIZE IN MEMORY-PARAMETER-SERVICE IS NOT A MULTIPLE OF 16 MB

## EMM2960

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM2960 EFFECTIVE SYSSIZE VALUE IS (&00) MB

### Meaning

(&00) specifies the value of SYSSIZE in MB.

## EMM2961

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

EMM2961 SPECIFIED PAGING-SATURATION-WARNING-LIMIT IN MEMORY-PARAMETER-SERVICE IS NOT IN ALLOWED RANGE.

## EMM2962

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

EMM2962 SPECIFIED PAGING-SATURATION-LIMITS-QUOTA IN MEMORY-PARAMETER-SERVICE IS NOT IN ALLOWED RANGE.

## EMM3001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3001 STARTUP PARAMETER MEM-RECONF IGNORED. STORAGE RECONFIGURATION NOT POSSIBLE ON THAT HARDWARE.

## EMM3002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3002 CONFIGURATION ERROR. MIN-MEMORY-SIZE defined by VM2000 COMMAND IS OUT OF RANGE.

## EMM3201

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3201 MEMORY LINK BOMBED. TASK TERMINATED WITH DUMP.

### Meaning

Memory link bombed at the end of the area to be released. The error
address matches the program counter valid when the partial page area has
been requested.

## EMM3202

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3202 $ASAM INCONSISTENCY DURING 'REQUEST/RELEASE MEMORY' PROCESSING. TASK TERMINATED WITH DUMP.

## EMM3203

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3203 INTERNAL RESOURCE SATURATION DURING 'REQUEST/RELEASE MEMORY' PROCESSING. TASK TERMINATED WITH DUMP.

## EMM3204

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3204 WHEN CALLING $GETMEM AN INCONSISTENCY IS DETECTED.

## EMM3205

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3205 WINDOW INCONSISTENCY DURING 'RELEASE-MEMORY'-PROCESSING. TASK TERMINATED WITH DUMP.

## EMM3206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM3206 INCONSISTENCY BETWEEN VMMALLOC AND VMMSERV.

### Meaning

An unrecoverable error is reported by the $NVYWIN interface.

## EMM3207

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM3207 INCONSISTENCY BETWEEN VMMALLOC AND VMMSERV.

### Meaning

An unrecoverable error is reported by the $NVYSET interface.

## EMM3208

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM3208 INVALID REQUEST MEMORY DURING RESTART/TASK TERMINATION.

### Meaning

Request memory for user space not allowed during memory reconstruction/
task-termination.

## EMM3209

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3209 WHEN CALLING $RETMEM AN INCONSISTENCY IS DETECTED.

## EMM3212

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3212 WHEN CALLING $ACCTLT AN INCONSISTENCY IS DETECTED.

## EMM3213

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3213 WITHIN THE COMPONENT VMMALLOC/INM AN INCONSISTENCY IS DETECTED.

## EMM3214

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3214 WITHIN THE COMPONENT DSSM/INM AN INCONSISTENCY IS DETECTED.

## EMM3215

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3215 WITHIN THE INM DATA TABLES AN INCONSISTENCY IS DETECTED.

## EMM3216

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3216 WITHIN THE VMMALLOC DATA TABLES AN INCONSISTENCY IS DETEXTED.

## EMM3217

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3217 WITHIN THE C5C4_FPM_QUEUE AN INCONSISTENCY IS DETECTED.

## EMM3218

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3218 WITHIN THE C5C4_PPM_QUEUE AN INCONSISTENCY IS DETECTED.

## EMM3219

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3219 WHEN CALLING $NVAINM AN INCONSISTENCY IS DETECTED.

## EMM3220

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3220 WHEN CALLING $NNMAIN AN INCONSISTENCY IS DETECTED.

## EMM3221

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3221 WHEN CALLING $INVPAG AN INCONSISTENCY IS DETECTED.

## EMM3222

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3222 WHEN CALLING $CORE AN INCONSISTENCY IS DETECTED.

## EMM3223

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3223 WHEN CALLING $NKLREQ AN INCONSISTENCY IS DETECTED.

## EMM3224

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3224 WHEN CALLING $REQFRM AN INCONSISTENCY IS DETECTED.

## EMM3225

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3225 WHEN CALLING $ECMF AN INCONSISTENCY IS DETECTED.

## EMM3226

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3226 WHEN CALLING $JITINV AN INCONSISTENCY IS DETECTED.

## EMM3301

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3301 SYSTEM ERROR DURING PROCESSING OF A 'MEMORY POOL' FUNCTION. TAKE SYSTEM DUMP!

### Meaning

A system internal inconsistency has been detected during the execution of
a MEMORY POOL function.

## EMM3303

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3303 SYSTEM ERROR DURING PROCESSING OF THE 'SHARED MEMORY' FUNCTION.

### Meaning

A system internal inconsistency has been detected during the execution of
the 'shared memory' function.

## EMM3310

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3310 NO MEMORY POOL CORRESPONDING TO SPECIFIED OPERANDS.

## EMM3311

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3311 NO CONNECTION TO THE SPECIFIED MEMORY POOL.

### Meaning

The specified memory pool is enabled in the system, but currently
there is no connection from the user-id of the caller.

## EMM3312

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3312 SYSTEM-ERROR OCCURED DURING EXECUTION OF /SHOW-MEMORY-POOL-STATUS COMMAND. COMMAND REJECTED.

### Meaning

Unexpected return code when calling an internal system funtion.
Possible reasons:
Error when determining LOGON-userid ($RDUID).

### Response

Contact the system administrator.

## EMM3313

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3313 TASK SPECIFIED IN /SHOW-MEMORY-POOL-STATUS COMMAND DOES NOT EXIST. COMMAND REJECTED.

### Meaning

The specified TSN is unknown in the system.

### Response

Correct command and retry.

## EMM3314

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3314 USER-ID / GROUP-ID SPECIFIED IN /SHOW-MEMORY-POOL-STATUS COMMAND DOES NOT EXIST. COMMAND REJECTED.

### Meaning

The specified User-Id / Group-Id is unknown in the system.

### Response

Correct command and retry.

## EMM3318

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3318 INSUFFICIENT VIRTUAL MEMORY SPACE TO EXECUTE COMMAND. COMMAND NOT EXECUTED.

### Meaning

Internal required areas could not be requested.

### Response

Try again later.
If the error occurs again contact the system administrator.

## EMM3401

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3401 INCONSISTENCY IN AN IMPLICITLY OPENED SLOT POOL. SYSTEM CRASH WITH DUMP.

### Meaning

In module EMMSLT an inconsistency has been detected in an implicitly
opened SLOT POOL during expansion or reduction.

## EMM3431

Destination: USER-TASK, CONSOLE Routing code: R Weight: 70

Warranty : NO

EMM3431 NEGATIVE RC FROM 'NAME MANAGER'. TASK TERMINATED WITH DUMP.

### Meaning

In module EMMOPN a negative returncode from the name-manager
has been received.

## EMM3501

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3501 MEMORY LINK BOMBED. TASK TERMINATED WITH DUMP.

### Meaning

Memory link bombed at the end of the area of extended memory to be
released. The error address matches the program counter valid when the
partial page area has been requested.

### Response

Please take dump and send it to your technical support.

## EMM3503

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

EMM3503 INTERNAL RESOURCE SATURATION DURING 'GET/RETURN EXTENDED MEMORY' PROCESSING. TASK TERMINATED WITH DUMP.

### Response

Take systemdump and send it to your technical support.

## EMM3504

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM3504 DURING THE INITIALIZATION OF THE PARTIAL PAGE DATA SPACE OCCURS SOME ERRORS.

### Response

Take Sled/Systemdump and sent it to your technical support.

## EMM3600

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM3600 FOR THE SPECIFIED TASK THERE IS NOT ALLOWED TO GIVE ANY INFORMATION ABOUT THE USER ADDRESS SPACE

### Meaning

The task does not run under the own user-identification.

## EMM3601

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM3601 SYSTEM ERROR OCCURED

### Response

Please contact your technical support.

## EMM3602

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM3602 THE SPECIFIED TASK DOES NOT EXIST IN THE SYSTEM

## EMM3603

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

EMM3603 THERE DOES NOT EXIST SUFFICIENT MEMORY TO PROCESS THE COMMAND

## EMM3800

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3800 AN INCONSISTENCY HAS BEEN DETECTED AT $NVMMAP CALL.

## EMM3850

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3850 A DATA INCONSISTENCY HAS BEEN DETECTED WITHIN THE FUNCTION UNIT NVMMAP. NVMISM.

## EMM3851

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3851 AN INCONSISTENCY HAS BEEN DETECTED AT $GETMEM CALL.

## EMM3852

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3852 AN INCONSISTENCY HAS BEEN DETECTED AT $OPNSL CALL.

## EMM3853

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3853 AN INCONSISTENCY HAS BEEN DETECTED AT $GETSL CALL.

## EMM3854

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3854 AN INCONSISTENCY HAS BEEN DETECTED AT $RETSL CALL.

## EMM3855

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

EMM3855 AN INCONSISTENCY HAS BEEN DETECTED AT $RETMEM CALL.

## EMM4001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM4001 DURING HOLD PROCESSING AN INCONSISTENCY IS DETECTED WHEN THE WRITTEN OUT CL6 AREA IS TO BE RELEASED.

### Meaning

A page which can't be released after having been written out into an
EAM file causes a system dump.

### Response

Take a system dump!

## EMM4002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM4002 ERROR AT REQM CALL BY UNHOLD ROUTINES.

### Response

Please take a system dump!

## EMM4003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM4003 DURING UNHOLD PROCESSING AN ERROR OCCURS WHEN ACCESSING AN EAM FILE.

## EMM5001

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

EMM5001 DURING CHANGING OF THE PAGE STATUS A SYSTEM INCONSISTENCY IS DETECTED. PROGRAMM TERMINATED ABNORMALLY.

### Meaning

PDR-Lock can not be seized / released.

## EMM6002

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

EMM6002 NEGATIVE RC FROM REQM/RELM. TASK TERMINATED WITH DUMP.

### Meaning

In the routine EMMRSTA1 a bad return code from REQM/RELM has been
received.

## EMM6003

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

EMM6003 NEGATVE RC FROM $RALS1. TASK TERMINATED WITH DUMP.

### Meaning

In the routine EMMRSTA2 a negative RC from $RALS1 has been received.

## EMM6004

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

EMM6004 A NON-ACESSABILITY IS DETECTED WHEN PERFORMING THE VALIDATION. PROGRAM TERMINATED ABNORMALLY.

### Meaning

A specified area of virtual address space can't be accessed with the
privilege of the (TPR-) routine, which has built up the area.

## EMM6005

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

EMM6005 $VALID ERROR WHEN CALLING THE $SSTX FUNCTION. PROGRAM TERMINATED ABNORMALLY.

### Meaning

An inconsistency occurs during scheduling a STXIT contingency (for
handling the event "validation error" in TU) in the validation routine.

## EMM6006

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM6006 A SYSTEM ERROR IS DETECTED WHEN INITIALIZING THE USER ACCESSKEY.

### Meaning

An Inconsistency causes task termination.

### Response

Take a system dump!!!

## EMM6051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM6051 PDR-LOCK COULD NOT BE ACQUIRED/RELEASED. PROGRAM TERMINATED WITH DUMP.

### Meaning

When processing a $NVYPAM call, the PDR-lock could not be
acquired/released.

## EMM6052

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM6052 DURING EXECUTION OF $NVYPGA ACCESS=OPEN AN INCONSISTENCY IS DETECTED.

## EMM6053

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM6053 DURING EXECUTION OF $NVYPGA ACCESS=CLOSE AN INCONSISTENCY IS DETECTED.

## EMM6054

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM6054 DURING EXECUTION OF $NVYPGA ACCESS=CLOSE AN INCONSISTENCY IS DETECTED.

## EMM6055

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM6055 DURING EXECUTION OF $NVYPGA ACCESS=CLOSE AN INCONSISTENCY IS DETECTED.

## EMM6056

Destination: USER-TASK Routing code: Weight:

Warranty : NO

EMM6056 AN INCONSISTENCY HAS BEEN DETECTED BY THE SVC 1 DISTRIBUTOR.

### Response

Plaese take a system Dump!

## EMM7001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7001 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND DAT MANAGER.

### Meaning

An inrecoverable error is reported by the $ASAM interface.

## EMM7002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7002 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND NAME MANAGER.

### Meaning

An inrecoverable error is reported by the $NNMAI Interface.

## EMM7003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7003 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND TASK LOCK MANAGER

### Meaning

An inrecoverable error is reported by the $GTLOCK ( $RLLOCK, $CRLOCK )
interface.

## EMM7004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7004 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND REAL MEMORY MANAGER.

### Meaning

An inrecoverable error is reported by the $CORE interface.

## EMM7005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7005 INCONSISTENCY WITHIN DATA SPACE MANAGER.

### Meaning

An inrecoverable error is reported by the $DSPSRV interface.

## EMM7006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7006 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND DIV MANAGEMENT.

### Meaning

An inrecoverable error is reported by the $DIVPD interface.

## EMM7007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7007 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND REAL MEMORY MANAGER.

### Meaning

An inrecoverable error is reported by the $INVPAG interface.

## EMM7008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7008 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND ACCES LIST MANAGER.

### Meaning

An inrecoverable error is reported by the $ALESRV interface.

## EMM7009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7009 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND SAT MANAGEMENT.

### Meaning

An inrecoverable error is reported by the $SATDSP interface.

## EMM7010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7010 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND VALIDATION.

### Meaning

An inrecoverable error is reported by the $VALID interface.

## EMM7011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7011 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND STXIT MANAGEMENT.

### Meaning

An inrecoverable error is reported by the $NSTGVA interface.

## EMM7012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7012 INCONSISTENCY BETWEEN DATA SPACE MANAGER AND COSMOS.

### Meaning

An inrecoverable error is reported by the $NPFCHK interface.

## EMM7013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7013 INCONSISTENCY WITHIN DATA SPACE MANAGER.

### Meaning

The internal data structure of the DSM manager is defect.

## EMM7041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7041 INCONSISTENCY BETWEEN ACCESS LIST MANAGER AND ART MANAGER.

### Meaning

An unrecoverable error is reported by the $ALAM interface.

## EMM7042

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7042 INCONSISTENCY BETWEEN ACCESS LIST MANAGER AND NAME MANAGER.

### Meaning

An unrecoverable error is reported by the $NNMAIN interface.

## EMM7043

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7043 INCONSISTENCY BETWEEN ACCESS LIST MANAGER AND TASK LOCK MANAGER.

### Meaning

An unrecoverable error is reported by the $GTLOCK or the $RLOCK interface.

## EMM7044

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7044 SYNCHRONIZATION ERROR WHILE ACCESSING A FOREIGN TASK BY THE ACCESS LIST MANAGER.

### Meaning

A release lock error is reported by the $ACCTLT interface.

## EMM7045

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

EMM7045 INCONSISTENCY BETWEEN ACCES LIST MANAGER AND VALIDATION.

### Meaning

An unrecoverable error is reported by the $VALID interface.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages