## FBDCOPY

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBDCOPY Copyright (C) (&01) (&00) All Rights Reserved

## FBDLOAD

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBDLOAD Program '(&00)' Version '(&01)' of '(&02)' loaded from file '(&03)'

## FBD1000

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1000 '(&00)' '(&01)' '(&02)' '(&03)' '(&04)'

### Meaning

Message for internal diagnosis data

## FBD1100

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1100 Subsystem '(&00)', Version '(&01)' of '(&02)' loaded

## FBD1106

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1106 VERSIONS OF BS2000 AND FDDRL NOT COMPATIBLE

### Meaning

The FDDRL version started is not released for the BS2000 version of the
current system.

## FBD1107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1107 PROGRAM NO LONGER SUPPORTED

## FBD1108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1108 WRONG START OF PROGRAM FDDRL

### Meaning

FDDRL was not started in PROGRAM-MODE=*ANY.

### Response

Start FDDRL by command /START-FDDRL

## FBD1119

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1119 INCORRECT CALL OF SUBSYSTEM FDDRL; ERROR CODE '(&00)'

### Meaning

The call of subsystem FDDRL is faulty:
- inadmissible call of SVC 143
- internal error of FDDRL (&00: error code)

## FBD1120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1120 ERROR '(&00)' DURING START OR INITIALIZATION OF SUBSYSTEM FDDRL

### Meaning

The connection to subsystem FDDRL has been processed with error.
(&00): error code
0001FFFF: The program is not (no more) supported by FDDRL.
0002FFFF: FDDRL subsystem not available, because DSSM subsystem
declarations are missing.
0003FFFF: The version of FDDRL program (phase or library) does not
suit to DSSM subsystem declarations of FDDRL
xx01xxxx: NDRCALL parameter error
0041FFFF: DSSM reports error during initiation of subsystem
00400001: User is not privileged to start FDDRL
others : See previous messages

### Response

Correct installation of subsystem FDDRL.
Start FDDRL again.

## FBD1122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1122 USER IS NOT PRIVILEGED TO START FDDRL

## FBD1123

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1123 LOADING OF SUBSYSTEM FDDRL VIA COMMAND NOT POSSIBLE

## FBD1126

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1126 (&00) MACRO PROCESSED WITH ERROR CODE '(&01)'. ABNORMAL TERMINATION

## FBD1127

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1127 (&00) MACRO PROCESSED WITH ERROR CODE '(&01)'. PROCESSING CONTINUES

## FBD1129

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1129 FDDRL REPFILE EMPTY

## FBD1130

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1130 DMS ERROR '(&01)' ON FILE '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&01). ABNORMAL TERMINATION

### Meaning

FDDRL is terminated because of an installation error.

### Response

Install FDDRL correctly

## FBD1140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1140 FDDRL PARAMETER FILE PROCESSED WITH ERRORS. ABNORMAL TERMINATION

## FBD1150

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1150 SDF MACRO '(&00)' PROCESSED WITH ERROR CODE '(&01)'. ABNORMAL TERMINATION

### Meaning

(&00): SDF macro
(&01): SDF error code
04 system error
08 parameter error
0C area too small
10 EOF (end of file)
14 wrong statement; command read
18 wrong defaults
1C wrong statement; step statement read
20 error dialog impossible
24 error dialog rejected
28 protocol area too small
2C end statement read
34 statement error; end statement read
38 SDF not loaded
3C program (FDDRL) not in syntax file
44 syntax file not found
48 SDF statement executed
4C SDF has to be loaded by system administrator
50 wrong statement; next statement read
5C invariant buffer too small
64 XHCS error
F1 wrong version of syntax file installed
F2 statement not allowed; program is terminated

## FBD1151

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1151 FDDRL FUNCTIONS HAVE NOT BEEN EXECUTED. //START-JOBS IS MISSING

### Meaning

The //END statement has been entered, without valid statements for FDDRL
functions have been executed by the //START-JOBS statement.
In batch task or procedure mode FDDRL is terminated with this warning.
In dialog mode the program termination can be prevented by reply 'N' to
message FBD1152.

## FBD1152

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

FBD1152 TERMINATE PROGRAM FDDRL? REPLY (Y=YES; N=NO)

### Meaning

Confirm the program termination.

### Response

Y: FDDRL is terminated. Entered statements for FDDRL functions are
not to be executed.
N: FDDRL is not terminated. Entered FDDRL functions may be executed
by //START-JOBS.

## FBD1153

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1153 NO VALID STATEMENTS FOR FDDRL FUNCTIONS HAVE BEEN ENTERED. //CREATE-JOBS or //START-JOBS IS IGNORED

### Meaning

The //CREATE-JOBS or //START-JOBS statement was read without valid
statements for FDDRL functions have been entered before.
The //CREATE-JOBS resp. //START-JOBS statement is ignored.

## FBD1154

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1154 NO FDDRL JOBS HAVE BEEN CREATED DURING CHECK OF DEVICES. //CREATE-JOBS IS IGNORED

### Meaning

No FDDRL job was defined because the check of the devices was terminated
with error.
The //CREATE-JOBS (rsp. //START-JOBS) statement is ignored.

## FBD1155

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1155 FDDRL STATEMENT IGNORED

### Meaning

The statement is not accepted by reason of an operand error.

## FBD1156

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1156 FDDRL JOB(S) PROCESSED WITH ERRORS. SPIN OFF ACTIVATED

### Meaning

At least one job was processed with error after //START-JOBS.

## FBD1157

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1157 OPERAND PUBSET, VALUE '(&00)' INVALID; ERROR CODE '(&01)'

### Meaning

(&00): catid of pubset
(&01): error code:
CINV: catid invalid
VSNA: function for a volumeset not allowed. A volumeset can be
saved consistently only in the frame of a SM-pubset
NOCC: the catid of control volumeset is missing in MRSCAT entry
for SM-pubset
NODT: the device type in MRSCAT entry for SM-pubset is missing
WRST: the SM-pubset has a wrong status in MRSCAT

### Response

CINV: Correct catid.
VSNA: Save complete SM-Pubset instead of one volumeset.
NOCC: Enter catid of control volumeset in MRSCAT.
NODT: Enter device type of VOLRES of control volumeset in MRSCAT.
WRST: Export pubset and wait for end of export.

## FBD1158

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1158 THE PUBSET '(&00)' IS IMPORTED. PROCESSING CONTINUES

### Meaning

Warning: The imported pubset may not be processed by FDDRL.
If a copy of the pubset is existing, this will be used,
otherwise the pubset has to be exported before the statement
//CREATE-JOBS or //START-JOBS is entered.
(&00): catid of pubset

## FBD1159

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1159 DEVICE-TYPE '(&00)' OF VOLUME/VOLUME-SET '(&01)' IS NOT SUPPORTED

### Meaning

The device type of a disk or a volumeset is not supported.
(&00): device type
(&01): VSN of a disk or catid of a volumeset

## FBD1160

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1160 OPERAND TAPE, VALUE '(&00)' INVALID; ERROR CODE '(&01)'

### Meaning

(&00): VSN of a tape volume (only one) or keyword
(&01): error code:
MARN: '*BY-VOLUME-CATALOG' can be specified only, if MAREN is
available and the tapes are administrated in the volume
catalog.
MVSF: MAREN function 'volume substitution' failed.
UNKN: The tape '(&00)' is unknown in MAREN volume catalog.
The tapes have to be either all known or all unknown in
volume catalog.
MARR: The tape '(&00)' is rejected by MAREN.
NUNI: The tapes do not have an unambiguous device type in MAREN
volume catalog
MULT: The tape '(&00)' was specified multiple.

### Response

MARN: specify tapes by VSN or make MAREN available
MVSF: correct specification or specify tapes by VSN
UNKN: correct tape specification or register tape in volume catalog
MARR: check messages of MAREN, correct tape specification
NUNI: correct specification of tapes
MULT: correct specification of tapes

## FBD1161

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1161 OPERAND TAPE-DEVICE-TYPE, VALUE '(&00)' INVALID; ERROR CODE '(&01)'

### Meaning

(&00): volume type
(&01): error code:
MARN: The specification '*BY-VOLUME-CATALOG' is not possible
because MAREN is not installed or temporarily not available.
UNKN: The specification '*BY-VOLUME-CATALOG' is not possible
because the tapes are not administrated in the volume catalog
of MAREN.
NVLD: The specification '*BY-VOLUME-CATALOG' is not possible
because the entry in MAREN volume catalog is no tape volume
type.
NEQM: The specified volume type differs from the entry in volume
catalog.

### Response

MARN: Specify volume type or make MAREN available
UNKN: Specify volume type or add volume(s) to MAREN volume catalog
NVLD: Specify volume type or correct entry in MAREN volume catalog.
NEQM: Correct volume type in operand or use suitable tape volumes.

## FBD1162

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1162 OPERAND '(&00)', VALUE '(&01)' INVALID; ERROR CODE '(&02)'

### Meaning

(&00): operand (DISK, UNIT, OVERWRITE-DISK, OVERWRITE-UNIT)
(&01): operand value
(&02): error code:
NDSK: mnemonic device name (MN) denotes no disk
WTYP: disk has wrong device type (only D3435 is allowed)
BS2V: the disk is no foreign disk (but a BS2000 disk)
WVSN: disk has wrong VSN
NUNI: both disks have not the same device type
IDNT: both disk device names are identical
MULT: the disk (VSN or MN) was specified multiple
NUMB: the number of output disks does not suit to number of
input disks

## FBD1163

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1163 ERROR DURING JOB CREATION. SPIN OFF ACTIVATED

### Meaning

The statement //CREATE-JOBS was processed with error or executed
partially.

## FBD1164

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1164 TAPE-DEVICE-TYPE '(&00)' NOT SUITABLE FOR 256 KB BLOCKS

### Meaning

Disk-sets and TAPE-FORMAT=*V16-FORMAT or V15-FORMAT require a tape device
type that supports tape blocks until the size of 256 KB.
(&00): volume type

### Response

Use a suitable tape device type or perform the save for single disks.

## FBD1165

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1165 FILE-NAME '(&00)' NOT FOUND IN VOLUME CATALOG

### Meaning

The file name (&00) does not exist in MAREN volume catalog.

## FBD1166

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1166 THE OPERAND 'NUMBER-OF-DISK-SETS' IS REDUCED TO '(&00)' (STATEMENT FOR PUBSET '(&01)')

### Meaning

The Operand NUMBER-OF-DISK-SETS is reduced to
- 1, for PROCESS-JOBS=*BY-MAINTASK
- 8, for NUMBER-OF-DISK-SETS=*BY-TASK-LIMIT and TASK-LIMIT > 8
- (n+1)/2, for a pubset with the number of n disks
(&00): new value
(&01): catid of pubset

## FBD1167

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1167 THE FDDRL PARAMETER 'SECURE-WAIT-TIME' IS REDUCED TO '7 DAYS'

### Meaning

The specified wait time is longer than 7 days.
Therefore the value is reduced to 7 days.

## FBD1168

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1168 OPERAND SAVE-ENTITY INVALID

### Meaning

The specification of several disks in one statement requires the
save entity disk-set (SAVE-ENTITY=*DISK-SET).

## FBD1169

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1169 OPERAND FILE-NAME, VALUE '(&00)' INVALID

### Meaning

DUMP-DISK, DUMP-FOREIGN-DISK:
The file name (&00) has to start with the prefix 'FDDRL'.
RELOAD-PUBSET:
The last character of the file name (&00) has to designate a valid
disk-set number.

## FBD1170

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1170 OPERAND LOCATION, VALUE '(&00)' INVALID; DEVICE-DEPOT IS UNKNOWN'

### Meaning

(&00): location

## FBD1171

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1171 OPERAND DEFAULT-PUBSET, VALUE '(&00)' INVALID; PUBSET IS UNKNOWN OR NOT IMPORTED'

### Meaning

(&00): pubset

## FBD1172

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1172 THE PUBSET '(&00)' CANNOT BE SAVED ONLINE (CAUSE '(&01)')

### Meaning

(&00): catid of pubset
(&01): cause:
DRVN: A DRV pubset cannot be saved online.
BSVN: The pubset cannot be saved online with this BS2000 version.
ICHN: The channel type S of input disk is not supported.
OCHN: The channel type S of output disk is not supported.
TCHN: The channel type S of tape device is not supported.
DABA: The DAB caching is active.

### Response

DRVN: Save pubset by splitted mirror disks
BSVN: Save pubset offline.
ICHN: Save pubset offline.
OCHN: Use output disk with channel type FC or save pubset offline.
TCHN: Use tape device with channel type FC or save pubset offline.
DABA: Switch off DAB caching during online save.
Repeat FDDRL statement.

## FBD1173

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1173 THE IMPORTED PUBSET '(&00)' IS SAVED ONLINE

### Meaning

The specified pubset is imported and will be saved online.
If the pubset should not be saved online, the pubset has to be exported
and the statement is to be repeated.
(&00): catid of pubset

## FBD1174

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1174 OPERAND STRUCTURE-OUTPUT, VALUE '(&00)' INVALID; ERROR CODE '(&01)'

### Meaning

(&00): variable name
(&01): error code
0002: syntax error in variable name
0006: variable type mismatched
nnnn: other error of macro VARINF

## FBD1202

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1202 ALLOCATION OF TAPE VOLUME '(&00)' FAILED (ERROR CODE '(&01)'). ABNORMAL JOB TERMINATION

### Meaning

- The volume is unknown
- The request was rejected by the operator
- The specified volume type is illegal for new reservation by MAREN.
(MARM117)
- The volume is not locally available (MAR4125)
(&00): VSN of tape or '*UNKNOWN'
(&01): $NKAATP return code (for diagnosis only)

## FBD1203

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1203 ALLOCATION OF DISK VOLUME '(&00)' FAILED. ABNORMAL JOB TERMINATION

### Meaning

The volume is unknown or was rejected by the operator.
(&00): VSN of disk or '*UNKNOWN'

## FBD1205

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1205 FDDRL FUNCTION '(&00)' FOR DISK/DISK-SET '(&01)' STARTED

## FBD1206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1206 FDDRL FUNCTION '(&00)' TERMINATED

## FBD1208

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1208 DISK ON DEVICE '(&00)' IS NOT A BS2000 DISK

### Meaning

The disk mounted on (&00) has not been initialized in
accordance with BS2000 norms and can therefore not be used.

## FBD1211

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1211 TAPE MOUNTED ON '(&00)' IS NOT AS SPECIFIED

### Meaning

A tape was specified by its VSN. However, the tape mounted on device
(&00) has no standard label or the wrong VSN.

## FBD1212

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1212 DISK ON DEVICE '(&00)' HAS WRONG LABEL. '(&01)' LABEL EXPECTED

### Meaning

The output disk has another label than the input disk/saved disk by the
function COPY/RELOAD.
Was the output disk assigned by the operator, the disk allocation will be
repeated. In the other cases the FDDRL job is terminated.
(&00): mnemonic name (MN) of output disk
(&01): expected label (BS2000 / NO BS2000)

### Response

Specify or assign an output disk with the same label.

## FBD1214

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1214 DISK '(&00)' ON DEVICE '(&01)' HAS WRONG FORMAT ('(&03)'). FORMAT '(&02)' EXPECTED

### Meaning

The output disk has another format than the input disk of COPY resp.
RELOAD.
It is not possible to change the format by overwriting the disk.
Was the output disk assigned by the operator, the disk allocation will be
repeated. In the other cases the FDDRL job is terminated.
(&00): VSN of output disk
(&01): mnemonic name (MN) of output disk
(&02): format of input disk (KEY/NK2/NK4)
(&03): format of output disk

### Response

Specify or assign an output disk with the correct format or
use operand OVERWRITE-DISK=*UNIT(...) to enable the internal disk
formating.

## FBD1216

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1216 ACCESS TO SVL OF DISK ON DEVICE '(&00)' NOT POSSIBLE. ABNORMAL JOB TERMINATION

### Meaning

Possible causes:
- device was detached
- command UNLOCK-DISK at a foreign system
SVL: standard volume label
(&00): mnemonic name (MN) of disk device

## FBD1217

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1217 SECURE OF TAPE DEVICE FAILED (ERROR CAUSE '(&00)'). ABNORMAL JOB TERMINATION

### Meaning

Der Versuch ein Bandgeraet zu reservieren ist fehlgeschlagen.
(&00): error cause
05: device type not available in the system
09: time out

### Response

- attach the desired tape device and repeat the run
- increase the SECURE-WAIT-TIME and repeat the run

## FBD1218

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1218 INVALID DEVICE CHARACTERISTICS OF DISK '(&00)'. USAGE OF DISK NOT POSSIBLE

### Meaning

The disk cannot be used because of wrong device characteristics.
The FDDRL job is terminated abnormally
(&00): mnemonic name (MN) of output disk

### Response

- Contact the maintenance staff to check the disk.
- In case of an emulated disk, format disk by X2000 program (bs2vol).

## FBD1220

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1220 REPLY TO PRECEDING MESSAGE INVALID. CORRECT REPLY

## FBD1230

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1230 ALL PAM PAGES OF DISK '(&00)' ON '(&01)' ARE TO BE SAVED

### Meaning

In the normal case only the allocated PAM pages, marked by F5 label, are
saved. In the present case however, all pages of the disk are to be saved.
Possible causes:
- The disk was 'online' during system crash, therefore the F5 label with
allocation information is not valid.
- The disk was separated with the SHC-OSD command /HOLD-MULTI-MIRRORING
while the belonging pubset was imported.
- The F5 label could not be completely read due to an i/o error,
and the error was skipped by 'CONTINUE'
(&00): VSN of disk
(&01): mnemonic name (MN) of disk device

## FBD1231

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1231 INPUT DISK ON '(&00)' OLDER THAN OUTPUT DISK ON '(&01)' ALTHOUGH ACTION=*SAVE. CORRECT ASSIGNMENT OF DISKS!

### Meaning

If a disk is saved, the output disk has to be older than the input disk.
A new output disk should have been initiated by means of VOLIN.

## FBD1232

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1232 OUTPUT DISK ON '(&00)' OLDER THAN INPUT DISK ON '(&01)' ALTHOUGH ACTION=*RESTORE. CORRECT ASSIGNMENT OF DISKS!

### Meaning

If a disk is restored, the output disk has to be younger than the input
disk

## FBD1233

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1233 INPUT DISK HAS TIME STAMP '(&00)'. CORRECT ASSIGNMENT OF DISKS!

### Meaning

For security reason a new initialized disk cannot be used as input disk
if operand ACTION=*RESTORE was specified.
A new initialized disk has time stamp '000000'.

## FBD1240

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1240 CAPACITY OF OUTPUT DISK '(&00)' SMALLER THAN THAT OF THE INPUT DISK/SAVED DISK ('(&02)' < '(&01)')

### Meaning

It is not possible to overwrite an output disk with a smaller capacity as
that of the input disk/saved disk by the function COPY/RELOAD.
If the output disk was assigned by the operator, another output disk is
requested. In the other cases the FDDRL job is terminated.
(&00): VSN of disk to be overwritten
(&01): Capacity of input disk/saved disk
(&02): Capacity of output disk
The capacity is given as decimal PHP value
or sedecimal in the format 'CCCCHHHH' (cylinder/tracks)

### Response

Specify or assign an output disk with the same capacity.

## FBD1241

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1241 CAPACITY OF OUTPUT DISK '(&00)' IS REDUCED TO THAT OF THE INPUT DISK/SAVED DISK ('(&02)' > '(&01)')

### Meaning

During overwriting of output disk the capacity data is taken from the
input disk.
The output disk is used afterwards with this reduced capacity.
The original capacity of output disk may be restored only by an
initialization with VOLIN.
(&00): VSN of disk to be overwritten
(&01): Capacity of input disk/saved disk
(&02): Capacity of output disk
The capacity is displayed as decimal PHP value
or sedecimal in the format 'CCCCHHHH' (cylinder/tracks)

## FBD1242

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1242 CAPACITY OF OUTPUT DISK '(&00)' DIFFERS FROM THAT OF THE INPUT DISK/SAVED DISK ('(&02)' <> '(&01)')

### Meaning

It is not possible to overwrite an output disk with another capacity
than that of the input disk/saved disk by the function COPY/RELOAD.
The FDDRL job is terminated abnormally.
(&00): VSN of disk to be overwritten
(&01): Capacity of input disk/saved disk
(&02): Capacity of output disk
The capacity is given as a PHP value.

### Response

Specify an output disk with the same capacity.

## FBD1243

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1243 THE MAXIMUM I/O LENGTH OF OUTPUT DISK '(&00)' IS SMALLER THAN THE I/O LENGTH DURING SAVE RUN ('(&01)' < '(&02)')

### Meaning

The save run was performed with TAPE-FORMAT=*V15-FORMAT.
Thereby an i/o length was used, which is greater than the maximum allowed
i/o length of output disk.
The FDDRL job is terminated abnormally.
(&00): VSN of disk to be overwritten
(&01): maximum i/o length of output disk
(&02): used i/o length during save run.

### Response

Use a suitable output disk or
repeat save run with TAPE-FORMAT=*V13-FORMAT.

## FBD1251

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1251 DISK '(&00)' MOUNTED ON DEVICE '(&01)'. OVERWRITE DISK? REPLY (Y=YES; N=NO)

### Response

Y: The disk is to be overwritten.
N: The disk is not to be overwritten.

## FBD1252

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1252 DISK '(&00)' ON DEVICE '(&01)' NOT THE SAME AS INPUT DISK MOUNTED PREVIOUSLY. REPLY (M=MOUNT; T=TERMINATE)

### Meaning

The present pubset disk is not the same as that one used at the moment of
FDDRL job generation.
Possible causes:
- The pubset was imported and exported in the meantime.
- The disk was meanwhile replaced or updated.
- Another disk with the same VSN was previously assigned as pubset disk.
(&00): VSN of disk
(&01): mnemonic name (MN) of disk device

### Response

M: Mount another disk and continue execution.
T: Terminate FDDRL job. Repeat FDDRL run for the concerned pubset.

## FBD1253

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1253 DISK '(&00)' ON DEVICE '(&01)' NOT THE SAME AS DISK MOUNTED BEFORE RESTART. REPLY (M=MOUNT; T=TERMINATE)

### Meaning

The present disk is not the same as that one used before the restart.
Possible cause: The disk was replaced or updated during the restart.
(&00): VSN of disk
(&01): mnemonic name (MN) of disk device

### Response

M: Mount another disk and continue execution.
T: Terminate FDDRL job.

## FBD1254

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1254 TIME STAMPS OF INPUT DISK '(&00)' ON '(&01)' AND OF OUTPUT DISK '(&02)' ON '(&03)' ARE IDENTICAL. REPLY (I=IGNORE; T=TERMINATE)

### Meaning

The time stamps of the input and output disks are the same. The disk
contents are presumably identical and the copy operation thus superfluous.
(&00): VSN of input disk
(&01): mnemonic name (MN) of input disk
(&02): VSN of output disk
(&03): mnemonic name (MN) of output disk

### Response

I: The disk mounted on device (&03) will be overwritten.
T: Terminate FDDRL job.

## FBD1255

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1255 DISK '(&00)' ON DEVICE/WITH DEVICE TYPE '(&01)' NOT AVAILABLE AT THE MOMENT. NEW ATTEMPT? REPLY (R=RETRY; T=TERMINATE)

### Meaning

There is no disk with the required attributes (MN, device type,
(time stamp) available. Possible causes:
1. The mount state (time stamp) of the required disk is out of date and
hat to be updated.
2. There is no disk according to device type/MN attached.
3. All suitable disks are occupied.
4. The MRSCAT entry for a SM pubset is missing
(&00): VSN of disk or '*UNKNOWN'
(&01): device type or mnemonic name (MN) of disk

### Response

case 1: Enter command /CHECK-DISK-MOUNT or
/SHOW-DISK-STATUS INFORMATION=*ALL.
case 2: Attach required disk (/ATTACH-DEVICE).
case 3: Wait for release of occupied disk.
case 4: Create MRSCAT entry for SM pubset.
R: Retry disk allocation.
T: Terminate FDDRL job.

## FBD1256

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1256 TAPE DEVICE (TYPE='(&01)', LOCATION='(&02)') OR VOLUME '(&00)' NOT AVAILABLE AT THE MOMENT. NEW ATTEMPT? REPLY (R=RETRY; T=TERMINATE)

### Meaning

The volume cannot be mounted on a tape device for the required volume
type. Possible causes:
- The operator has not attached any tape device for the required volume
type.
- All tape devices for the required volume type are occupied.
- There is no free tape device on the specified location.
- The tape volume is occupied at the moment
- The tape device type has been specified invalid.
- The tape location has been specified invalid.
(&00): VSN of tape or '*UNKNO'
(&01): tape volumetype
(&02): location or '*ANY'

### Response

R: Retry attempt for tape allocation.
T: Terminate FDDRL job.

## FBD1257

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1257 INCONSISTENCY POSSIBLE. DISK ON DEVICE '(&00)' USED BY ANOTHER SYSTEM. REPEAT FDDRL FUNCTION

### Meaning

The disk on device (&00) was used by another system. The contents may
have been changed during processing.
The FDDRL job is abnormally terminated.

### Response

The FDDRL function should be repeated.

## FBD1258

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD1258 DISK CHARACTERISTICS ON DEVICE '(&04)' WILL BE CHANGED. FORMAT(ALLOCATION UNIT): '(&00)((&02))'->'(&01)((&03))'. CONFIRM (Y=YES/N=NO)

### Meaning

If confirmation for change of disk characteristics is given,
the current characteristics will be overwritten by those of the
input disk. This also changes the utilization type of the output disk.
(&00): format old (KEY/NK)
(&01): format new (KEY/NK)
(&02): allocation unit old (6/8/64)
(&03): allocation unit new (6/8/64)
(&04): mnemonic name (MN) of output disk

### Response

Y: The disk is overwritten; the utilization type changes.
N: The disk is not overwritten. Was the output disk assigned by the
operator, another output disk is requested. In the other cases the
FDDRL job is terminated.

## FBD1259

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1259 SUBTASK CREATION DEFERRED (MACRO '(&00)', ERROR CODE '(&01)')

### Meaning

Creation of subtask not possible. Task creation will be repeated after
a waiting period. cause:
(&00): MACRO (&01): ERROR CODE
$USUBT 00800080: job class limit exceeded
$USUBT 00800081: memory shortage
$USUBT 00800082: TSN shortage
$USUBT 00800083: category overloaded
$CREA 00080004: task saturation

## FBD1260

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1260 FDDRL SUBTASK '(&00)' FOR DISK/DISK-SET '(&01)' STARTED

### Meaning

(&00): TSN of subtask
(&01): VSN of disk or name of disk-set

## FBD1261

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1261 FDDRL SUBTASK '(&00)' FOR DISK/DISK-SET '(&01)' CANCELED

### Meaning

If the maintask was canceled by /CANCEL-JOB, every active subtask is
canceled.
(&00): TSN of subtask
(&01): VSN of disk or name of disk-set

## FBD1262

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1262 FDDRL SUBTASK '(&00)' FOR DISK/DISK-SET '(&01)' TERMINATED

### Meaning

(&00): TSN of subtask
(&01): VSN of disk or name of disk-set

## FBD1263

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1263 FDDRL SUBTASKS ARE STILL ACTIVE. PROGRAM TERMINATION DEFERRED

### Meaning

The FDDRL in the maintask gets abnormal terminated.
The program termination waits for the termination of all active subtasks.
If also the subtasks should be abnormally terminated, the maintask has to
be canceled by /CANCEL-JOB command.

### Response

- Wait for normal termination of all active subtasks,
possibly the operator has to reply the question of a FDDRL subtask.
- Cancel maintask (/CANCEL-JOB) to cancel subtasks implicitly.

## FBD1269

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1269 FDDRL SUBTASK '(&00)' MAY BE BLOCKED. LAST INTERFACE CALL WAS '(&01)'

## FBD1270

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1270 NO INACTIVE JOB FOR SUBTASK FOUND

### Meaning

After the start of the subtask no inactive job for processing was found.
Possible causes:
- The start of the subtask was delayed because the job class limit was
reached
- The attachment of a free tape device was delayed
An empty tapeset is created.

## FBD1271

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1271 FDDRL JOB FOR DISK '(&00)' ON DEVICE '(&01)' STARTED

### Meaning

(&00): VSN of disk
(&01): MN of disk

## FBD1272

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1272 FDDRL JOB FOR DISK '(&00)' HAS BEEN RESET

### Meaning

If a new output tape was assigned during a tape restart, jobs have to be
processed once more, if they have been processed with the abandoned
output tape.
(&00): VSN of disk

## FBD1280

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1280 FDDRL SUBTASK IS DELAYED. ONLINE SAVE GETS ABORTED.

### Meaning

All FDDRL subtasks for online save have to reach a common synchronization
point after the tape mount.
Is the point not reached in an adequate time period
the online save gets abnormally terminated.
Possible causes:
- At least one subtask could not be started.
The job class limit might be exceeded.
- At least one subtask has not reached the synchronization point
to start the save.
Probably one subtask is waiting for a tape device.
- At least one subtask has terminated abnormally

## FBD1281

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1281 WRITE LOCK FOR PUBSET '(&00)' IS ACTIVATED

### Meaning

The write lock of the pubset was activated because of online save of the
pubset (&00)
Every task which performs write operations on the pubset is suspended to a
waiting state.

## FBD1282

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1282 THE TIME LIMIT FOR WRITE LOCK OF PUBSET '(&00)' IS EXPIRED

### Meaning

The write lock for the pubset is removed

### Response

Repeat save run and adapt the value of the operand TIME-LIMIT to the save
period.

## FBD1283

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1283 FDDRL SUBTASK '(&00)' MAY BE BLOCKED. LAST INTERFACE CALL WAS '(&01)'

## FBD1284

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1284 FDDRL SUBTASK '(&00)' IS BLOCKED BY INTERFACE CALL '(&01)'

## FBD1285

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1285 WRITE LOCK FOR DISK/PUBSET '(&00)' IS REMOVED

## FBD1286

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1286 INCONSISTENCY POSSIBLE. DISK ON DEVICE '(&00)' USED BY OTHER TASKS. REPEAT FDDRL FUNCTION

### Meaning

The write protection of the disk was reset during online save.
The contents may have been changed during save processing by other tasks.
The FDDRL job is abnormally terminated.

### Response

The FDDRL function should be repeated.

## FBD1301

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1301 TIME STAMP OF DISK '(&00)' DOES NOT MATCH WITH THAT OF DISK '(&02)'. STATEMENT FOR PUBSET '(&01)' IGNORED

### Meaning

The pubset state is inconsistent.

## FBD1302

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1302 DISK '(&00)' NOT EXCLUSIVLY AVAILABLE. STATEMENT FOR PUBSET/DISK-SET '(&01)' IGNORED

### Meaning

The SVL (standard volume label) of every disk of a pubset/disk-set has to
be accessible to be able to create the FDDRL jobs.
Possible cause:
- disk (&00) is not attached
- pubset (&01) is imported
- disk (&00) is occupied by a foreign system

### Response

- Attach the disk or export pubset or make disk available.
- Repeat statement for pubset/disk-set.

## FBD1303

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1303 MAXIMUM NUMBER OF FDDRL JOBS REACHED. STATEMENT FOR DISK/PUBSET '(&00)' IGNORED

### Meaning

The number of jobs is limited to 5000 per one //START-JOBS statement.
This limit was exceeded either while entering the statements or during
generation of jobs after //START-JOBS resp. CREATE-JOBS statement.
The statement for the given disk/pubset is ignored.
(&00): VSN if statement for disk or
catid if statement for pubset

### Response

Repeat the statement for the disk/pubset after termination of FDDRL jobs.

## FBD1308

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1308 DISK '(&00)' IS NO PUBRES OF A SINGLE FEATURE PUBSET; ERROR '(&02)'. STATEMENT FOR PUBSET '(&01)' IGNORED

### Meaning

(&00): VSN of disk
(&01): catid of PUBSET
(&02): error: disk is
2: VOLRES of a control volumeset
3: VOLRES of a standard volumeset
4: VOLRES of a standalone volumeset
5: VOLRES of a defect volumeset
9: no PUBRES, because not installed by means of installation
program

## FBD1309

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1309 DISK '(&00)' IS NO VOLRES OF A SYSTEM MANAGED PUBSET/ VOLUME SET; ERROR '(&02)'. STATEMENT FOR PUBSET '(&01)' IGNORED

### Meaning

(&00): VSN of disk
(&01): catid of PUBSET
(&02): error: disk is
1: PUBRES of a single feature pubset
4: VOLRES of a standalone volumeset
5: VOLRES of a defect volumeset
9: no VOLRES, because not installed by means of installation
program

## FBD1310

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1310 MULTIPLE STATEMENT FOR DISK '(&00)'. LAST STATEMENT IS VALID

### Meaning

The user has entered more than one statement with the same function
for the same disk. Only the last statement is processed.

## FBD1311

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1311 MULTIPLE STATEMENT FOR DISK '(&00)'. SOME OPERANDS GET UPDATED

### Meaning

The same function (COPY resp. DUMP) for one disk has been entered
first by a statement for a pubset (COPY-PUBSET resp. DUMP-PUBSET) and
afterwards by a statement for a single disk (COPY-DISK resp. DUMP-DISK).
The first statement remains valid, nevertheless it is extended by the
following additional operand values of the 2nd statement:
- for statements COPY-PUBSET/COPY-DISK the operand OVERWRITE-DISK
- for statements DUMP-PUBSET/DUMP-DISK the operands TAPE, TAPE-DEVICE-TYPE
and LOCATION

## FBD1312

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1312 MACRO '(&00)' PROCESSED WITH ERROR CODE '(&01)'. STATEMENT FOR PUBSET '(&02)' IGNORED

### Meaning

(&00): macro (&01): error
DPSIMPL 00200002 : import error: see DMS messages on console
DPSIMPL xxxxxxxx : see DMS messages on SYSOUT
$STAM xxxxxxxx : error at $STAM (MRSCAT)
DMCDMCE 00000nnn : output area too small (nnn = length)
DMCDMCE 0FBD1159 : device type not supported
DPSEXPL 00200002 : export error: see DMS messages on console
DPSEXPL xxxxxxxx : see DMS messages on SYSOUT

## FBD1313

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1313 A DISK-SET AS SAVE ENTITY REQUIRES TAPE FORMAT FROM V16.0 ONWARDS. STATEMENT FOR DISK-SET '(&00)' IGNORED

### Meaning

If a tape format for FDDRL versions < V16.0A is selected,
disk-sets may not be specified as save entity.

### Response

- //MODIFY-FDDRL-PARAMETERS TAPE-FORMAT=*V17-FORMAT or
- //MODIFY-FDDRL-PARAMETERS TAPE-FORMAT=*V16-FORMAT or
- //DUMP-PUBSET ... SAVE-ENTITY=*SINGLE-DISK

## FBD1314

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1314 DISK-SET INFORMATION BLOCK NOT FOUND ON TAPE '(&01)'. STATEMENT FOR DISK/PUBSET '(&00)' IGNORED

### Meaning

The tapes of a disk-set save run were not correctly specified or were
specified in the wrong order.
(&00): catid of pubset or
VSN of the first disk of the statement
(&01): tape VSN

## FBD1315

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1315 TAPE IS SAVE TAPE FOR PUBSET/DISK-SET '(&00)'. STATEMENT FOR PUBSET '(&01)' IGNORED

### Meaning

(&00): catid of saved pubset or name of the disk-set
(&01): catid of pubset to be restored

## FBD1316

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1316 NO TAPES ARE ASSIGNED TO THE DISK-SET '(&00)'. STATEMENT FOR PUBSET '(&01)' IGNORED

### Meaning

A pubset was saved to several disk-sets as save-entity.
During job creation of RELOAD-PUBSET no tapes can be assigned to a
disk-set.
Possible causes:
- The operand TAPE was specified with a vsn or vsn list instead of
*GROUPED-BY-DISK-SET
- For the operand TAPE=*GROUPED-BY-DISK-SET a VSN specification is
missing for one disk-set
- The operand TAPE=*BY-VOLUME-CATALOG was specified, but for one disk-set
no suitable filename was found in volume catalog of MAREN.
Hint: An own filename is created for every disk-set.
Thereby the last character of the filename is substituted by the
number of the disk-set (1..8).

## FBD1317

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1317 DISK '(&00)' WAS NOT SAVED WITHIN DISK-SET '(&01)'. STATEMENT FOR DISK-SET IGNORED

### Meaning

A disk cannot be restored, because it was not saved within the disk-set
on the tape.

## FBD1318

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1318 DISK '(&00)' WAS NOT SAVED WITHIN DISK-SET '(&01)' BUT WITHIN DISK-SET '(&02)'. STATEMENT FOR DISK-SET IGNORED

### Meaning

A disk cannot be restored, because it was not saved within the disk-set
on the tape.

## FBD1319

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1319 ERROR ('(&00)') DURING CHECK OF SAVE TAPE. STATEMENT FOR PUBSET/DISK-SET '(&01)' IGNORED

### Meaning

(&00): FDDRL message key
(&01): catid of pubset to be restored or name of the disk-set

## FBD1320

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD1320 DEVICE TYPE OF OUTPUT DISK '(&02)' IS NOT EQUAL TO DEVICE TYPE '(&01)' OF INPUT DISK/SAVED DISK '(&00)'

### Meaning

The output disk of COPY/RELOAD must have the same device type as the
input disk/saved disk.
(&00): VSN of input disk/saved disk
(&01): device type of input disk/saved disk
(&02): MN of output disk

### Response

Specify or assign an output disk with the same device type.

## FBD1321

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1321 THE NUMBER OF OUTPUT DISKS DOES NOT MATCH TO THE NUMBER OF INPUT DISKS. STATEMENT FOR DISK/PUBSET '(&00)' IGNORED

### Response

Specify the suitable number of output disks.

## FBD1322

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1322 NO OTHER JOBS ARE ALLOWED TOGETHER WITH ONLINE SAVE. STATEMENT FOR DISK/PUBSET '(&00)' IGNORED

### Response

Start job for FDDRL online save on its own.

## FBD1323

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1323 THE NUMBER OF DISK-SETS IS TOO SMALL FOR ONLINE SAVE. STATEMENT FOR PUBSET '(&00)' IGNORED

### Meaning

All disks have to be saved at the same time in case of online save.
With TAPE-FORMAT=*V17-FORMAT only 4 disks and
with TAPE-FORMAT=*V16-FORMAT only 2 disk can be saved per one disk set.

### Response

- increase NUMBER-OF-DISK-SETS resp.
- use TAPE-FORMAT=*V17-FORMAT

## FBD1324

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1324 WARNING: SUBTASK-LIMIT FOR ONLINE SAVE IS TOO SMALL

### Meaning

An ONLINE SAVE has to be processed by FDDRL Subtasks,
thereby the TASK-LIMIT may not be less than the number of subtasks.

### Response

- Process jobs by subtasks and adapt the TASK-LIMIT to the number of
subtasks:
//MODIFY-FDDRL-PARAMETERS PROCESS-JOBS=*BY-SUBTASKS(TASK-LIMIT=...)
- Use SAVE-ENTITY=*DISK-SET and adapt the NUMBER-OF-DISK-SETS to the
TASK-LIMIT.

## FBD1325

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1325 SUBTASK-LIMIT FOR ONLINE SAVE IS TOO SMALL. STATEMENT START-JOBS IGNORED

### Meaning

An ONLINE SAVE has to be processed by FDDRL Subtasks,
thereby the TASK-LIMIT may not be less than the number of subtasks.

### Response

Process jobs by subtasks and adapt the TASK-LIMIT to the number of
subtasks:
//MODIFY-FDDRL-PARAMETERS PROCESS-JOBS=*BY-SUBTASKS(TASK-LIMIT=...)

## FBD1331

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1331 OPERAND 'DATA-COMPRESSION=*YES' IS IGNORED

### Meaning

The operand DATA-COMPRESSION=*YES of the function DUMP is ignored for the
reason of a better performance, if
- the magnetic tape device performs a data compression
- a tape format greater than *V13-FORMAT is used

## FBD1400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1400 UTILITY ROUTINE '(&00)' VERSION '(&01)' READY FOR INPUT

## FBD1402

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1402 UTILITY ROUTINE '(&00)' TERMINATED

## FBD1403

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1403 (&00) HPS OF DISK '(&01)' HAVE BEEN PROCESSED

### Meaning

Termination message of FDDRL job.
(&00): number of processed HPs (half pages - 2K units of disk)

## FBD1500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1500 NO REQUESTS FOUND

### Meaning

No request complying with the specified criteria could be found.

## FBD1510

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD1510 WARNING: NO FDDRL JOBS FOUND

### Meaning

No FDDRL job complying with the specified criteria could be found.
Statement terminated with warning.

## FBD2181

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2181 INPUT DISK FOR FDDRL COPY

### Meaning

Insert for mount message NKVD013.

## FBD2182

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2182 OUTPUT DISK FOR FDDRL COPY OF DISK '(&00)'

### Meaning

Insert for mount message NKVD013.

## FBD2201

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2201 TAPE '(&03)' ON DEVICE '(&02)' AS REEL '(&01)' FOR DUMP OF DISK/DISK-SET '(&00)' USED

### Meaning

The tape with the VSN (&03) mounted on the device (&02) is used as
save tape number (&01) of the disk-set with the name (&00).
(&00): name of the disk-set or VSN of the disk
(&01): reel number of the save run
(&02): mnemonic name (MN) of tape device
(&03): VSN of the tape

## FBD2204

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2204 TAPE '(&01)' ON DEVICE '(&00)' WAS USED IN CURRENT FDDRL SAVE RUN. OVERWRITING NOT ALLOWED

### Meaning

(&00): mnemonic name (MN) of tape device
(&01): VSN of tape

## FBD2205

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2205 TAPE MOUNTED ON '(&00)' NOT OR NOT CORRECTLY LABELED. NO OVERWRITING ALLOWED

### Meaning

The tape is not or not correctly labeled or it could not be read
correctly.
Overwriting is not allowed.
(&00): mnemonic name (MN) of tape device

## FBD2206

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2206 EXPIRATION DATE ('(&02)') OF TAPE '(&01)' ON DEVICE '(&00)' NOT YET REACHED. OVERWRITING NOT ALLOWED

### Meaning

There exists an expiration date on the tape labels. This date has not
been reached until now, therefore the tape may not be overwritten.
(&00): mnemotechnic name (MN) of tape device
(&01): VSN of the tape
(&02): expiration date of the tape

### Response

Initialize the tape or use another tape.

## FBD2208

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2208 TAPE '(&03)' ON DEVICE '(&02)' AS REEL '(&01)' FOR DUMP OF DISK/DISK-SET '(&00)' COMPLETE

### Meaning

The tape with the VSN (&03) mounted on the device (&02) is as save tape
number (&01) of the disk-set (&00) complete and now a valid save tape.
(&00): name of the disk-set or VSN of the disk
(&01): reel number of save run
(&02): mnemonic name (MN) of tape device
(&03): VSN of the tape

## FBD2210

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2210 TAPE '(&01)' MOUNTED ON '(&00)' IS TOO SHORT FOR USE BY FDDRL. TAPE REJECTED

### Meaning

The tape mounted on device (&00) is too short to be used by FDDRL.
(&00): mnemonic name (MN) of tape device
(&01): VSN of tape

### Response

Mount another tape.

## FBD2211

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2211 TAPE '(&01)' MOUNTED ON '(&00)' CANNOT BE OVERWRITTEN

### Meaning

The tape is write protected.
(&00): mnemonic name (MN) of tape device
(&01): VSN of tape

## FBD2212

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD2212 (&00) HPS OF DISK '(&01)' HAVE BEEN SAVED

### Meaning

Termination message of DUMP or COPY job.
(&00): number of saved HPs (half pages - 2K units of disk)

## FBD2281

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2281 INPUT DISK FOR FDDRL DUMP

### Meaning

Insert for mount message NKVD013.

## FBD2282

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

FBD2282 FDDRL DUMP TAPE (&01) DISK (&00)

### Meaning

Insert for mount message NKVT013.
(&00): VSN of disk to be saved
(&01): reel number of the tape

## FBD2300

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD2300 ENTER VSN OF TAPE '(&01)' FOR RELOAD OF DISK/DISK-SET/PUBSET '(&00)'. REPLY (VSN; T=TERMINATE)

### Meaning

The specification of the tape with the reel number (&01) is missing.
The tape is used for restore of the disk with the VSN (&00) resp. of the
disk-set/pubset (&00).
(&00): VSN of the disk or name of disk-set or pubset
(&01): reel number of the save run or
'*LAST' for the last tape of the save run

### Response

VSN: Continue processing with this tape
T: Terminate FDDRL job

## FBD2301

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2301 TAPE OF WRONG SAVE VERSION MOUNTED ON '(&00)' FOR RELOAD OF '(&01)'

### Meaning

The tape mounted on (&00) is a continuation tape of another save run.
The tape belongs to another copy of the same save run.
(&00): MN of tape device
(&01): Name of Disk-set or VSN of the saved disk

### Response

Mount the correct tape.

## FBD2302

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2302 TAPE CANNOT BE IDENTIFIED. TAPE REJECTED

### Meaning

An i/o error occurred, so the tape cannot be identified as FDDRL save
tape. Therefore the tape cannot be used for FDDRL reload.

## FBD2303

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2303 TAPE '(&03)' ON DEVICE '(&02)' AS REEL '(&01)' FOR RELOAD OF DISK/DISK-SET '(&00)' USED

### Meaning

The tape with the VSN (&03) mounted on the device (&02) is used as
save tape number (&01) of the disk/disk-set (&00).
(&00): name of the disk-set or VSN of the disk
(&01): reel number of the save run
(&02): mnemonic name (MN) of tape device
(&03): VSN of the tape

## FBD2304

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2304 TAPE '(&03)' ON DEVICE '(&02)' AS REEL '(&00)' FOR RELOAD OF DISK/DISK-SET '(&01)' RELOADED

### Meaning

The tape with the VSN (&03) mounted on device (&02) is a save tape
number (&00) of the disk/disk-set (&01) and has been reloaded in full.
(&00): reel number of the save run
(&01): name of the disk-set or VSN of the disk
(&02): mnemonic name (MN) of tape device
(&03): VSN of the tape

## FBD2307

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2307 TAPE WITH REEL NUMBER '(&00)' FOR DISK/DISK-SET '(&03)' MOUNTED ON DEVICE '(&01)'. REEL NUMBER '(&02)' IS EXPECTED

### Meaning

The tape mounted is a save tape for disk/disk-set (&03), but it is the
wrong reel number.
(&00): mounted reel number of tapeset
(&01): mnemonic name (MN) of tape device
(&02): expected reel number
(&03): name of the disk-set or VSN of the disk

### Response

Mount the tape with the expected reel number.

## FBD2309

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2309 TAPE '(&00)' ON DEVICE '(&01)' IS SAVE TAPE FOR DISK/DISK-SET '(&02)'. SAVE TAPE FOR DISK/DISK-SET '(&03)' IS EXPECTED

### Meaning

The tape mounted is a save tape for the disk/disk-set with the VSN (&02).
However a save tape for the disk / disk-set (&03) is expected.
(&00): VSN of the tape
(&01): mnemonic name (MN) of tape device
(&02): name of disk-set or VSN of disk (saved on tape)
(&03): name of expected disk-set or VSN of expected disk

### Response

Mount the correct save tape for disk/disk-set (&03).

## FBD2311

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD2311 TAPE '(&00)' ON DEVICE '(&01)' INCONSISTENT, LABEL '(&02)' DO NOT SUIT TO BEGIN OF TAPE. ABNORMAL JOB TERMINATION

### Meaning

The end of the tape contains data from a different save run as the
data at the beginning of the tape.
Possible reasons:
- abnormal termination of the save run
(&00): VSN of tape
(&01): mnemonic name (MN) of tape device
(&02): tape trailer label (EOV1,EOF1,EOV2,EOF2,EOV3,EOF3,UTL1,UTL2)
The FDDRL job is abnormally terminated.

### Response

- Use the correct save tape after abnormal termination

## FBD2312

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2312 VOL1 LABEL OF TAPE ON DEVICE '(&00)' CANNOT BE READ

### Meaning

A reload is not possible if the tape
- was written by an FDDRL version older than V8.0A or with
- the option 'TAPE-FORMAT=SPECIAL'.
In any other case the reload will be continued.

## FBD2314

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2314 UNIMPORTANT LABEL OF TAPE ON DEVICE '(&00)' CANNOT BE READ. READ ERROR IGNORED

### Meaning

The tape is handled as if the label (HDR2/HDR3/EOF2/EOF3) was read without
error.

## FBD2315

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2315 TAPE CANNOT BE RELOADED BY THIS FDDRL VERSION

### Meaning

The tape contains data, which cannot be reloaded by this FDDRL version.

### Response

Use the correct FDDRL version for the reload.

## FBD2316

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2316 TAPE '(&00)' ON DEVICE '(&01)' INCONSISTENT. EXPECTED BLOCK NUMBER '(&02)', ACTUAL BLOCK NUMBER '(&03)'. RELOAD FUNCTION CANNOT CONTINUE

### Meaning

The tape with VSN (&00) is inconsistent. The data blocks are not in the
correct order (the actual block number does not match the expected block
number) or a distorted block was recognized.

### Response

Use the correct save tape for the reload.

## FBD2317

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2317 INVALID BLOCK HEADER ON TAPE '(&00)': '(&01)'

### Meaning

A FDDRL tape block with an invalid block header was detected.
Possible reasons:
- Abnormal termination of the save run
- Tapeblocks are missing or have not been recognized
- A tapemark is missing or has not been recognized
- Invalid repositioning by tape monitor
(&00): VSN of tape
(&01): diagnoses information (data of tapeblock begin)

### Response

At begin of tape FDDRL tries a tape restart, otherwise the FDDRL job is
terminated with DUMP

## FBD2318

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2318 DISK-SET INFORMATION BLOCK NOT FOUND ON TAPE

### Meaning

The tapes were not correctly specified or were specified in the wrong
order.

## FBD2351

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD2351 INVALID EOF/EOV LABEL OF TAPE ON DEVICE '(&00)' FOR RELOAD '(&01)'. REPLY (L=HANDLED AS LAST TAPE; N=NEXT TAPE; R=RESTART; T=TERMINATE)

### Response

L: The tape is handled as if it was the last of the current reload.
N: The tape is handled as if it is correct and a follow tape will be
requested.
R: The tape is read again from the beginning.
T: Terminate FDDRL job.

## FBD2354

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

FBD2354 TAPE '(&04)' ON DEVICE '(&03)' IS SAVE TAPE OF DISK/DISK-SET '(&00)' FROM (&01) (&02). ACCEPT TAPE? REPLY (Y=YES; N=NO)

### Meaning

The tape mounted on device (&03) is a save tape of the disk/disk-set (&00)
(&00): name of disk-set or VSN of disk
(&01): date of save (YYYY-MM-DD)
(&02): time of save (HH:MM:SS)
(&03): mnemonic name (MN) of tape device
(&04): VSN of tape

### Response

Y: the mounted tape is the correct save tape;
the disk/disk-set should be restored by this tape.
N: the mounted tape is the wrong one; it will be unloaded and released.
If the tape VSN was specified by user, the FDDRL job is terminated,
otherwise another tape is allocated.

## FBD2355

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2355 TAPE '(&01)' ON DEVICE '(&00)' NOT USABLE FOR RELOAD

### Meaning

The tape mounted on device (&00) cannot be identified as FDDRL save tape
- It is not a FDDRL save tape
- Important tape labels are not readable
- The tape is a copy of a FDDRL save tape, but the copy was not created
with a filename beginning with 'FDDRL...'.

### Response

Check tape labels
Perhaps create a new copy of tape(s) with a correct filename beginning
with 'FDDRL...' and use this copy for RELOAD.

## FBD2358

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2358 DISK DEVICE TYPE '(&00)' NOT SUPPORTED. RELOAD NOT POSSIBLE

### Meaning

The tape cannot be reloaded because the device type of disk is not
supported by this BS2000 version or FDDRL version.

### Response

(&00): device type code: device type is unknown to BS2000 version
device type: device type is not supported by FDDRL version
Reload tape under suitable BS2000 and FDDRL version!

## FBD2359

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD2359 UNIT (MN) OF ORIGINAL DISK NOT SAVED. RESTORE WITH OPERAND VALUE *SAME-UNIT NOT POSSIBLE

### Meaning

The unit name (MN) of the original disk was not stored during save runs
of older FDDRL versions.
The restore with operand OVERWRITE-DISK=*UNIT(UNIT=*SAME-UNIT) is not
possible.

## FBD2381

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 10

Warranty : YES

FBD2381 FDDRL RLOD TAPE (&01) DISK (&00)

### Meaning

Insert for mount message NKVT013.
(&00): VSN of the disk saved
(&01): reel number of the tape

## FBD2382

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 10

Warranty : NO

FBD2382 OUTPUT DISK FOR FDDRL RELOAD OF '(&00)'

### Meaning

Insert for mount message NKVD013.
(&00): VSN of the disk saved.

## FBD3001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD3001 I/O ERROR '(&01)' ON DISK DEVICE '(&00)'. ABNORMAL TERMINATION WITH DUMP

### Meaning

(&00): mnemonic name (MN) of disk device
(&01): PPAM return code

## FBD3002

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD3002 I/O ERROR '(&01)' ON DISK DEVICE '(&00)'. ABNORMAL JOB TERMINATION

### Meaning

(&00): mnemonic name (MN) of disk device
(&01): PPAM return code
022E : volume lost

## FBD3004

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD3004 I/O ERROR '(&01)' ON DISK DEVICE '(&00)'. CONTINUE PROCESSING? REPLY (R=RESTART; T=TERMINATE; D=TERMINATE WITH SYSTEM DUMP)

### Meaning

(&00): mnemonic name (MN) of disk device
(&01): PPAM return code or logical return code (LRC)
0224 : request memory error
0226 : i/o termination with logical error
0227 : i/o termination with error (without LRC)
C801 : data check error (on output disk)
xxxx : other unexpected errors

### Response

R: Restart disk processing after a new disk assignment.
T: Terminate FDDRL job.
D: Terminate FDDRL job after SYSTEM DUMP.

## FBD3005

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD3005 I/O ERROR '(&01)' ON DISK DEVICE '(&00)'. CONTINUE PROCESSING? REPLY (C=CONTINUE; A=CONTINUE ALWAYS; R=RESTART; T=TERMINATE)

### Meaning

(&00): mnemonic name (MN) of disk device
(&01): logical return code (LRC) or PPAM return code
C801 : data check error (on input disk)
0227 : i/o termination with error (without LRC)

### Response

C: Continue disk processing, ignore defective data blocks of this i/o;
data is lost
A: Continue disk processing, ignore all defective data blocks of the disk;
data is lost
R: Restart disk processing after a new disk assignment.
T: Terminate FDDRL job.

## FBD3101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD3101 (&00) HPS LOST ON DISK '(&01)'

### Meaning

(&00): number of lost halfpages (2K units)
(&01): mnemonic name (MN) of disk device

## FBD3104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD3104 DALTA REPORTED ERROR CAUSE (&00)

### Meaning

(&00): error code:
X'8000' operand error
X'4000' alternate track pool exhausted
X'2000' homeaddress/record0 inconsistent
X'1000' read error on SVL
X'0800' read error on homeaddress/record0
X'0400' read error on data to be restored
X'0200' device access error
X'0100' internal error
X'0080' block access inhibited
X'0040' SVL update not completed
X'0020' not a BS2000 volume
X'0010' $REQM error
X'0008' page fixing error
X'0002' device status error ($DSTATUS)
X'0001' disk not support.

## FBD3106

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD3106 HPS FROM '(&00)' UP TO '(&01)' LOST ON DISK '(&02)'

### Meaning

(&00): first PHP (physical halfpage) in the range of lost HPs
(&01): last PHP in the range of lost HPs
(&02): VSN of the disk

## FBD3107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD3107 ALL HPS FROM '(&00)' LOST ON DISK '(&01)'

### Meaning

The last halfpages (2k units) of the restored disk are lost
(from PHP number (&00) up to the end of the disk).

## FBD3108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD3108 PHP '(&00)' LOST ON DISK '(&01)'

### Meaning

The answer 'C' (CONTINUE) was given.
PHP: physical half page
(&00): lost PHP (physical halfpage)
(&01): mnemonic name (MN) of disk device

## FBD3109

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD3109 '(&00)' BYTES LOST AT END OF DISK '(&01)'

### Meaning

The end of disk is out of PHP boundary, therefore the specified number of
bytes at the end of disk may not be saved.
(&00): number of lost bytes
(&01): mnemonic name (MN) of disk device

## FBD3153

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD3153 I/O ERROR '(&01)' ON DISK '(&00)'

### Meaning

An unrecoverable i/o error (&01) occurred on disk device (&00).
Cause: See previous console messages.
Dependent on the error condition following actions are possible:
- a disk restart is performed, thereby the disk device is released and
reallocated, the last i/o is repeated (LRC=A8..)
- the FDDRL run is terminated abnormally
(&00): mnemonic name (MN) of disk device
(&01): logical return code (LRC) (significant only for diagnoses)

## FBD3154

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD3154 I/O ERROR '(&01)' ON DISK '(&00)'. CONTINUE PROCESSING? REPLY (TSN.=RETRY; R=RESTART; C=CONTINUE; A=CONTINUE ALWAYS; T=TERMINATE)

### Meaning

Either an 'undefined unrecoverable error' or a 'parity error' occurred
on device (&00).
(&00): mnemonic name (MN) of disk device
(&01): logical return code (LRC)
meaning: see previous console message EXC0857

### Response

TSN.: Repeat last i/o.
R : Release and allocate disk device; repeat last i/o.
C : Continue disk processing after defective data block; data are lost.
A : Continue disk processing after defective data block for all
subsequent defective data blocks; data are lost.
T : Terminate FDDRL job.

## FBD3155

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD3155 I/O ERROR '(&01)' ON DISK '(&00)'. CONTINUE PROCESSING? REPLY (TSN.=RETRY; R=RESTART; T=TERMINATE)

### Meaning

An unrecoverable i/o error (&01) occurred on disk device (&00).
The error cannot be bypassed.
(&00): mnemonic name (MN) of disk device
(&01): logical return code (LRC)
meaning: see previous console message EXC0857

### Response

TSN.: Repeat last i/o.
R : Release and allocate disk device; repeat last i/o.
T : Terminate FDDRL job.

## FBD3156

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD3156 I/O ON DISK '(&00)' WAS DELAYED (LRC='(&01)')

### Meaning

A waiting state has occurred several times for the disk device (&00).
The waiting time has accumulated up to 10 seconds and
the FDDRL run was delayed accordingly.
(&00): mnemonic name (MN) of disk device
(&01): logical return code (LRC) (significant only for diagnoses)

## FBD3201

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD3201 DISK RESTART ACTIVATED

### Meaning

After an i/o error has occurred and the disk gets released and
reallocated.
Afterwards the processing continues.

## FBD4001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4001 I/O ERROR '(&01)' ON TAPE DEVICE '(&00)'. ABNORMAL TERMINATION WITH DUMP AND ERROR ADDRESS

### Meaning

(&00): mnemonic name (MN) of tape device
(&01): PTAM return code or LRC (for diagnoses only)
0771 : system error
0772 : invalid DAR
0775 : illegal operation
0778 : not allowed commission
A0xx : logical error, wait and retry
A4xx : logical error, correct and retry
ACxx : logical program error
C806 : i/o program error
C80A : tape identifier error
D003 : block shorter than count
D004 : block longer than count

## FBD4002

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4002 I/O ERROR '(&01)' ON TAPE DEVICE '(&00)'. ABNORMAL JOB TERMINATION

### Meaning

(&00): mnemonic name (MN) of tape device
(&01): PTAM return code
0779 : volume lost

## FBD4003

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4003 I/O ERROR '(&01)' ON TAPE DEVICE '(&00)'. TAPE RESTART NECESSARY

### Meaning

(&00): mnemonic name (MN) of tape device
(&01): PTAM return code or logical return code (LRC)
0776 : logical error return code
0779 : volume lost
077B : blocks lost
077C : blocks lost but saved
A8xx : logical error, no correction possible
C800 : undefined unrecoverable error
C802 : not found condition
C803 : path not available
C804 : device inoperable
C805 : device busy
C807 : write inhibit
C808 : tape and device not compatible
C809 : empty tape
C80C : reset key
C80E : device assigned elsewhere
C810 : command retry request
C812 : reset notification
C813 : volume fenced
C819 : XF-feature not available (MBK4)
C81A : tape length error, tape too short
C81C : tape length error, tape too long
D1xx : ATL (automated tape library) error (xx=ERA code)

## FBD4004

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD4004 I/O ERROR '(&01)' ON TAPE DEVICE '(&00)'. CONTINUE PROCESSING? REPLY (R=RESTART; T=TERMINATE)

### Meaning

(&00): mnemonic name (MN) of tape device
(&01): logical return code (LRC)
C800 : undefined, unrecoverable error
C801 : data check error
C809 : empty tape
C811 : block id sequence error
C81B : block id sequence error in space file
C824 : cryption error

### Response

R: Restart tape processing at begin of tape.
T: Terminate FDDRL job.

## FBD4005

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

FBD4005 I/O ERROR '(&01)' ON TAPE DEVICE '(&00)'. CONTINUE PROCESSING? REPLY (C=CONTINUE; A=CONTINUE ALWAYS; R=RESTART; T=TERMINATE)

### Meaning

(&00): mnemonic name (MN) of tape device
(&01): logical return code (LRC)
C801 : data check error

### Response

C: Continue tape processing after the defective data block;
data is lost
A: Continue tape processing after the defective data block for all
subsequent defective data blocks; data is lost
R: Restart tape processing at begin of tape
T: Terminate FDDRL job.

## FBD4010

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4010 TAPE RESTART ACTIVATED

### Meaning

The routine for the release and reallocation of a tape device has been
activated.

## FBD4011

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4011 (&02) DATA ERROR(S) DETECTED ON TAPE '(&00)', DEVICE '(&01)'

### Meaning

The number of detected data errors on tape is shown.
(&00): tape VSN
(&01): mnemonic name (MN) of tape device
(&02): number of detected data errors

## FBD4012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD4012 UNLOAD OF TAPE ON DEVICE '(&00)' STARTED

## FBD4013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD4013 SUBSYSTEM MAREN NOT AVAILABLE

### Meaning

The specification TAPE-DEVICE-TYPE=*BY-VOLUME-CATALOG is not possible
without MAREN

## FBD4014

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4014 MAREN FUNCTION '(&00)' REPORTS ERROR '(&01)' FOR TAPE/FILE '(&02)'

### Meaning

(&00): MAREND function (VS,F0,F1,O1,O2,C1)
(&01): MAREN message key or error code
(&02): VSN of tape or MAREN filename

## FBD4015

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

FBD4015 PREPARE TAPE '(&00)' FOR FDDRL RUN (ACCESS='(&01)', DISK/DISK-SET='(&02)')

### Meaning

This messsage supports 'pre-restore' of volumes by ROBAR and CentricStor.

## FBD4016

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4016 JV FUNCTION '(&00)' REPORTS ERROR '(&01)' FOR JV '(&02)'

### Meaning

(&00): JV function (GETJV, SETJV)
(&01): JV error code or JV message key
(&02): JV name

## FBD4017

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD4017 DMS ERROR '(&01)' WITH MACRO '(&00)' ON FILE '(&02)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

Unexpected error during execution of DMS macro

## FBD5000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD5000 FDDRL JOB HAS NOT BEEN EXECUTED

### Meaning

For the 'FDDRL JOB PROTOCOL' there is no termination code (TERMCODE)
present. Causes:
- the FDDRL job has not been executed
- the FDDRL job has been very early abnormally terminated

### Response

Repeat FDDRL job

## FBD5001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5001 REQUEST MEMORY ERROR. ABNORMAL TERMINATION

### Meaning

The request was not successfully processed, the memory not allocated.

## FBD5002

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5002 RELEASE MEMORY ERROR. ABNORMAL TERMINATION

### Meaning

The request was not successfully processed.

## FBD5016

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5016 UPDATE OF SVL NOT POSSIBLE. ABNORMAL JOB TERMINATION

### Meaning

During a RELOAD or COPY job, a dummy VSN is set in the SVL of the output
disk. After the data had been saved it was not possible to write the
original VSN in the SVL. Possible causes:
- device was detached
- command UNLOCK-DISK at a foreign system
SVL: standard volume label

## FBD5023

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5023 I/O ERROR '(&01)' ON DISK '(&00)'. ABNORMAL TERMINATION WITH DUMP

### Meaning

The i/o error may be the result of an incorrect i/o program.
(&00): mnemonic name (MN) of disk device
(&01): logical return code (LRC)
meaning: see previous console message EXC0857

### Response

Take system dump

## FBD5024

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5024 ABNORMAL TERMINATION REQUESTED BY USER OR INITIATED BY PROGRAM AFTER DEVICE ERROR RECOVERY

## FBD5034

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5034 DISK NOT SUPPORT BY DALTA, CONTINUATION NOT POSSIBLE. ABNORMAL JOB TERMINATION

## FBD5036

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5036 FDDRL INTERNAL ERROR. ABNORMAL TERMINATION WITH DUMP AND ERROR ADDRESS

## FBD5037

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5037 (&00) MACRO PROCESSED WITH ERROR. ABNORMAL TERMINATION WITH DUMP AND ERROR ADDRESS

## FBD5038

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

FBD5038 (&00) MACRO PROCESSED WITH ERROR CODE '(&01)'. ABNORMAL TERMINATION WITH DUMP AND ERROR ADDRESS

## FBD5039

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD5039 TASK CANCELED. ABNORMAL TERMINATION

## FBD5040

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FBD5040 ABNORMAL PROGRAM TERMINATION (ABEND)

### Meaning

The routine for abnormal program termination was activated
(STXIT event class 'ABEND').
Causes:
- system error, connection lost
- commands: START-PROGRAM, LOAD-PROGRAM, ABEND, LOGOFF, CANCEL-JOB
- hardware error
- forced unload of a subsystem

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages