# KVP

## KVP0000

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0000 7.500 KVP VERSION (&00) INITIALISED ON (&01) AT (&02)

## KVP0001

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0001 KVP PARAMETER FILE ERROR

### Meaning

&00 = KVP version number, &01 = Date, &02 = Time
The KVP parameter file kvpparam contains a syntax error, the file no longer exists or the
system has no further available storage space.
1. On starting up KVP:
If the file is present and sufficient storage space is available, the file is renamed to
/opt/SMAWL/conf/kvpparam.defect. A new parameter file with the default
parameter content is then written and used by KVP.
2. When a new KVP parameter file is activated:
KVP continues to use the old parameter records.

### Response

1. Rename the file kvpparam.defect to kvpparam. and correct the
defective entry in the file or modify the new file
kvpparam. using the KVP configuration.
To do this it is necessary to rewrite the logging options and all the records.
You must then activate the new configuration.
2. Correct the defective entry in the file. Then activate the corrected configuration.

## KVP0002

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0002 NEW KVP PARAMETER FILE ACTIVATED

## KVP0005

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0005 CURRENT TRANSLATION TABLES: (&00)

### Meaning

&00 = Designation of the line code or the conversion tables
The BS2000 console messages are converted from EBCDIC and ASCII and vice versa on
the basis of the specified standards. The default setting is Euro/International ISO 8859-1
(ASCII) to BS2000 EBCDIC.DF.04-1 and vice versa.

## KVP0006

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0006 LANGUAGE TRANSLATION FILE ERROR (&00)

### Meaning

&00 = Designation of the line code or the conversion tables
The international character translation file inter.atoe or inter.etoa is not present and
the system has no further available storage space in which to create such a file. KVP terminates.

### Response

Make storage space available under /opt.

## KVP0007

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0007 EVENTING IMPOSSIBLE BECAUSE (&00) FINISHED WITH ERROR

### Meaning

&00 = Reason (CALL or INITIALISATION)
Because the call or initialisation with error finished, eventing is impossible.
The event CPU STOPPED or CPU RUNNING cannot reported to SEM.
The functionality of KVP is not affected.

### Response

If the message is irritating, start KVP again.
If that does not help, contact the service.

## KVP0008

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0008 OPEN ERROR NODE=(&00) (&01)

### Meaning

&00 = Node, &01 = Reason
A device node or a necessary device node cannot be opened by the KVP. In general the working with this KVP is not possible.

### Response

Correct the erroneous file or device configuration.

## KVP0009

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0009 LIVE MIGRATION COULD NOT BE ACTIVATED IN KVP

### Meaning

KVP was not able to activate Live Migration. After a Live Migration, the KVP must therefore
be restarted on the new system via the SEM or using the kvpSid command. Normal
work with this KVP is not affected when the message appears.

## KVP0010

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0010 CONNECTION REQUEST REJECTED: USERID (&00) IS LOCKED

### Meaning

&00 = User-ID (Login name)
1. The specified user ID has been locked.
2. The user ID has been declared invalid because it has not been used for the specified
number of days.
3. The expiry date of the specified user ID has been reached.
After this date it is no longer possible to access the system under this user ID.

### Response

It remains locked until the password of the specified user ID is defined via the SEM authorization.

## KVP0013

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0013 STATION (&00) REJECTED BY SYSTEM: CONSOLE (&01) IS UNKNOWN

### Response

&00 = User ID, &01 = Mnemonic name of console
The specified mnemonic name of the console must either be entered in the BS2000
parameter file SYSPAR.BS2.... (the precise file name depends on the version) or must be
modified in the KVP parameter file.

## KVP0014

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0014 STATION (&00) REJECTED BY SYSTEM: CONSOLE (&01) IS ALREADY ASSIGNED

### Meaning

&00 = User ID, &01 = Mnemonic name of console
Another station is already logged on at the BS2000 system with the specified mnemonic
console name. This mnemonic console name is not currently available.

## KVP0018

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0018 SYSTEM IS NOT READY FOR INPUT; PROBABLY NEW IPL NECESSARY

### Meaning

BS2000 is not active, the IPL has not terminated or still has to be started. The message is
output if console I/O traffic (read path) is disrupted (system/hardware error).

### Response

You must wait for the end of the current IPL or perform a new IPL.

## KVP0019

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0019 SYSTEM IS NOT READY FOR INPUT

### Meaning

BS2000 is not active, the IPL has not terminated or still has to be started. The message is
output if console I/O traffic (read path) is disrupted (system/hardware error).

### Response

You must wait for the end of the current IPL or perform a new IPL.

## KVP0020

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0020 SYSTEM INPUT FROM CONSOLE (&00) TIMED OUT

### Meaning

&00 = Mnemonic name of console
BS2000 has not accepted an input.

### Response

Repeat the input. If it is rejected again, perform a new IPL.

## KVP0021

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0021 SYSTEM INPUT FROM CONSOLE (&00) TIMED OUT; PROBABLY NEW IPL NECESSARY

### Meaning

BS2000 has not accepted an input.

### Response

Repeat the input. If it is rejected again, perform a new IPL or activate the KTT devices.

## KVP0041

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0041 COMMENCING BS2000 SHUTDOWN - (&00)

### Meaning

&00 = Explanatory text
An extraordinary BS2000 shutdown has been initiated. The text specifies the cause.

## KVP0042

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0042 COMMENCING SYSTEM SHUTDOWN - STOP OF KVP IN MAXIMUM (&00) MINUTES

### Meaning

&00 = Maximum wait time
BS2000 is termited. KVP is then terminated. LINUX is terminated at the latest on expiry of
the specified time.
This message may also be issued if an environment fault has occurred.
– Fan fault
– Temperature monitoring
– Power supply fault

### Response

In the case of an environment fault: identify and eliminate the cause. If necessary, inform
the service staff.

## KVP0054

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0054 INPUT TO (&00) REJECTED UNTIL LOGGING IS POSSIBLE

### Response

&00 = partner (SYS, SVP)
The original error must be eliminated (see the preceding messages). You can then repeat
the input. If it is not possible to eliminate the original error, logging may also be deactivated.

## KVP0070

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0070 NO WORKING-STORAGE AVAILABLE FOR (&00) - ENTER INPUT AGAIN

### Response

&00 = KVP name (HV0, VM1, VM2, etc.)
You must repeat the input. If this does not help either, you must terminate KVP via the “KVP
Administration” menu and then restart it.

## KVP0071

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0071 INPUT LOCKED - PRESS F2 KEY

### Response

Input is currently locked. You can press the F2 key to open a selection screen in which you
can unlock input. To do this, you must enter the password.
If the LINUX login is locked, access to the console is aborted. Use of the login remains
locked until the password corresponding to the login is defined via the LINUX user
administration.

## KVP0000

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0072 'LAST MESSAGES' CAN NOT BE DISPLAYED - NO MEMORY AVAILABLE

### Meaning

The menu function “LAST MESSAGES” cannot be executed because the file system is full.

### Response

Delete any unnecessary files.

## KVP0074

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0074 WIDES OF THE FRAME IS TOO SMALL

### Meaning

The xterm window for kvpbs2 is not at least 80 characters wide. kvpbs2 is terminated.

### Response

Widen the window.

## KVP0075

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0075 INPUT CANNOT BE LOCKED

### Meaning

The screen cannot be locked for local accounts.

### Response

Terminate bs2console and log in again later.

## KVP0080

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0080 INVALID PFKEYS - NOT LOADED

### Meaning

An invalid pfkey file has been specified.

### Response

Try again and enter a correct pfkey file name.

## KVP0111

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0111 STATION (&00) CONNECTED FROM TERMINAL ((&01)) AS CONSOLE (&02)

### Meaning

&00 = User ID, &01 = Terminal device name, &02 = Mnemonic name of console or SVP device

## KVP0112

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0112 STATION (&00) DISCONNECTED FROM TERMINAL ((&01)) AS CONSOLE (&02)

### Meaning

&00 = User ID, &01 = Terminal device name, &02 = Mnemonic name of console or SVP device

## KVP0120

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0120 INVALID BS2000 MESSAGE TO CONSOLE (&00)

### Meaning

&00 = Mnemonic name of console
The specified length of a BS2000 message does not correspond to the received length. The
message is also output if console I/O traffic is disrupted.
Inform the Customer Support staff because a system/hardware error or an internal
overwrite error has occurred.

## KVP0801

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0801 FILE-LOGGING FAILE

### Response

The access rights of the file structure /var/opt/SMAW/X2000/log and of the file
/var/opt/SMAW/X2000/log/log_info should be checked and, if necessary, corrected.
This message is also output if archiving is set to REQUIRED and none of the existing logging
files could be archived. The system administrator must make sure that the archiving
command can be terminated without errors or the files must be deleted.

## KVP0802

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP0802 (&00) ARCHIVING FAILED

### Meaning

&00 = Archive file name
The archiving command terminated with an error. If Archiving required is set then the
oldest logging file is deleted when the configured number of logging files is reached. If
Archiving required is set then the attempt to archive the file is repeated at periodic
intervals.

### Response

Check the archiving command for errors. If you are archiving to tape you may need to insert
a new tape and perform a manual backup.

## KVP5000

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP5000 KVP MESSAGE FILE COULD NOT BE OPENED

### Meaning

The message file kvp.cat under /opt/SMAW/X2000/lib/nls/de or
/opt/SMAW/X2000/lib/nls/en no longer exists or the access rights are set incorrectly.
KVP continues to run but uses English message texts.

### Response

You should check the file access rights and correct them if necessary. The file can be read
in again from the backup volume or the installation volume. You must then restart KVP.

## KVP5001

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

KVP5001 INVALID KVP PARAMETER (&00)

### Meaning

&00 = Parameter
KVP was called with invalid parameters. KVP terminates.

### Response

Call KVP with valid parameters.
– The system designation must consist of three alphanumeric characters.
– The channel parameter must be a number from 0 through 127.
– The unit parameter must be a number from 0 through 254.
– The line parameter contains the letter B (bus) or C (channel).
– The trace parameter must be a number from 1 through 255.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages