## ARCCOPY

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARCCOPY Copyright (C) (&01) (&00) All Rights Reserved

## ARCD003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARCD003 DIRCONV STATEMENT COMPLETED

### Meaning

Processing of the current statement has terminated.
DIRCONV is ready to accept further commands.

## ARCD006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARCD006 DIRCONV STATEMENT NOT COMPLETED

### Meaning

Processing of the current statement was aborted since some errors
were found. DIRCONV is ready to accept further statements.

## ARCLOAD

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARCLOAD Program '(&00)', version '(&01)' of '(&02)' loaded from file '(&03)'

## ARC0000

Destination: CONSOLE Routing code: U Weight: 50

Warranty : NO

ARC0000 ARCHIVE SUBTASK STARTED BY TSN '(&00)'

### Meaning

An ARCHIVE subtask has been created by the task with TSN (&00).

## ARC0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0001 ARCHIVE READY

### Meaning

ARCHIVE is loaded and is waiting for a statement.

## ARC0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0002 STATEMENT ACCEPTED. ARCHIVE SEQUENCE NUMBER '(&00)', VERSION '(&01)'

### Meaning

The statement syntax was correct and the statement is accepted.
(&00): the 15 character identifier of this ARCHIVE process
(&01): version number of the privileged part (TPR) of ARCHIVE.

## ARC0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0003 ARCHIVE STATEMENT COMPLETED

### Meaning

Processing of the current statement has terminated.
ARCHIVE is ready to accept further commands.

## ARC0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0004 ARCHIVE STATEMENT COMPLETED WITH WARNINGS

### Meaning

Processing of the current statement has terminated, although some warnings
were given. ARCHIVE is ready to accept further statements.

## ARC0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0005 ARCHIVE STATEMENT COMPLETED WITH ERRORS

### Meaning

Processing of the current statement has terminated although some errors
were given. ARCHIVE is ready to accept further statements.

## ARC0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0006 ARCHIVE STATEMENT NOT COMPLETED

### Meaning

Processing of the current statement was aborted since some errors
were found. ARCHIVE is ready to accept further statements.

## ARC0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0007 ARCHIVE STATEMENT REJECTED, VERSION '(&00)'

### Meaning

An error was detected during syntax analysis of the ARCHIVE statement.
(&00): version number of the TPR part of ARCHIVE.

### Response

For detailed informations please notice preceding messages.

## ARC0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0008 SVID IS ALREADY ASSIGNED

### Meaning

The given SVID is already assigned to another ARCHIVE run.

### Response

Retry with a greater SVID.

## ARC0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0009 ARCHIVE TERMINATED

### Meaning

The END statement is encountered. ARCHIVE is terminated.

## ARC001F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC001F '(&00)'

## ARC0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0010 VOLUME '(&00)' OF TYPE '(&01)' ADDED TO THE POOL

### Meaning

The volume whose volume type is (&01) and whose VSN is (&00) has been
added to the pool of the specified directory.

## ARC0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0011 VOLUME '(&00)' OF VOLUME TYPE '(&01)' REMOVED FROM THE POOL

### Meaning

The volume whose VSN is (&00) and whose volume type is (&01) has been
removed from the pool in the directory specified in the POOL statement.

## ARC0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0012 ARCHIVE-PROCESS '(&00)' PROCESSED FROM QUEUE FILE

### Meaning

The specified sequence of statements has been removed from the queue file
and entered for running.
(&00): the ARCHIVE sequence number (yymmdd.hhmmss) of the statements.

## ARC0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0013 ARCHIVE PROCESS '(&00)' DELETED FROM QUEUE FILE

### Meaning

The specified sequence of statements has been removed from the queue
file and can never be run.

## ARC0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0014 ARCHIVE-PROCESS '(&00)' RESTARTED FROM CHECKPOINT FILE

### Meaning

The specified statement on the checkpoint file is about to be restarted
and any further messages will refer to this restarted statement.
(&00): the ARCHIVE sequence number (yymmdd.hhmmss) of the statement.

## ARC0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0015 ARCHIVE PROCESS '(&00)' DELETED FROM CHECKPOINT FILE

### Meaning

The specified statement on the checkpoint file has been removed and can
never be restarted.
(&00): the ARCHIVE sequence number (yymmdd.hhmmss) of the statement.

## ARC0016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0016 PARAM STATEMENT ERROR '(&00)'

### Meaning

The PARAM statement input has been rejected with invalid operand(s).
(&00): character string of invalid operand(s).

### Response

Enter corrected PARAM statement.

## ARC0017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0017 PARAM STATEMENT ACCEPTED

### Meaning

The PARAM statement input has been accepted by ARCHIVE.
ARCHIVE is ready to accept further commands.

## ARC0018

Destination: CONSOLE Routing code: U Weight: 50

Warranty : NO

ARC0018 ARCHIVE SUBTASK TERMINATED

### Meaning

The ARCHIVE subtask has terminated processing.

## ARC0019

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0019 END OF FILE ON SYSDTA

### Meaning

ARCHIVE has detected an end of file condition while reading
from SYSDTA. The text of the current statement will be analysed as
though complete. After all processing for this statement has
terminated, an END statement is simulated.

## ARC0020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0020 TOO MANY ERRORS OR WARNINGS. FURTHER MESSAGES SUPPRESSED

### Meaning

Statement analysis in ARCHIVE has reached its limit of errors
and/or warnings. No further error or warning messages will be
output during statement analysis.

## ARC0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0021 MORE THAN ONE PASSWORD OPERAND. PASSWORDS ARE ADDED TO THOSE ALREADY SPECIFIED

### Meaning

More than one PASSWORD operand has been given. The effect is as if all
the passwords were supplied in a single operand.

## ARC0022

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0022 MORE THAN ONE '(&00)' OPERAND. PREVIOUS VALUE IS IGNORED

### Meaning

An operand type has been repeated or there was an equivalent operand
before (BLKSIZE and TAPE-BLOCK-SIZE are equivalent, also TAPES and VOLUME
and DISKS and VOLUME).
The later value is the one which will be used.
(&00): the keyword of the operand which has been repeated.

## ARC0023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0023 'INQUIRE' and 'LIST' MUST HAVE A LISTING DEVICE. 'LIST=SYSOUT' ASSUMED

### Meaning

A LIST=NONE operand has been specified for the INQUIRE or LIST
statement. LIST=SYSOUT will be used instead.

## ARC0024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0024 DEFAULT VALUE OF 'CHANGED' OPERAND REQUIRES A 'DIRECTORY'. 'CHANGED=NO' IS ASSUMED

### Meaning

The default value of the CHANGED operand is YES, but this is not
compatible with a DIRECTORY=NONE operand.
Therefore a value of NO is assumed for the CHANGED operand.

## ARC0025

Destination: CONSOLE Routing code: U Weight: 50

Warranty : NO

ARC0025 VOLUME '(&01)' CONTAINS '(&00)' PAM PAGES

### Meaning

&00: the total number of PAM pages that were written until now on the
output volume by ARCHIVE.
&01: output volume

## ARC0026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0026 NUMBER OF DRIVES REDUCED TO NUMBER OF VOLUME GROUPS IN 'CONTINUE' OR 'FROM' OPERAND

### Meaning

A DRIVES operand specifies more volume drives than are implicitly
given by a CONTINUE or FROM operand. The value will be reduced
accordingly.

## ARC0027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0027 FILES COPIED FROM TAPE WILL NOT BE ERASED

### Meaning

For a save from tape the operand ERASE=YES has been specified.
For the tape files of the FILES statement, the operand ERASE=YES
will have no effect.

## ARC0028

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0028 '(&00)' IS NOT FOLLOWED BY '='. '(&00)=' IS ASSUMED

### Meaning

An operand keyword, which should be separated from its value by '=',
has been given without following '='. Processing continues as if the
'=' has been given, and the characters following the keyword are
taken as the operand value.
(&00): the keyword of the operand.

## ARC0029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0029 'CONTINUE' DEVICE TYPE NOT CONSISTENT. VALUE IGNORED

### Meaning

The device type specified in the CONTINUE operand for a save or export
type statement is not the same as that specified in the TAPES or DISKS
operand. The former is ignored.

## ARC0030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0030 DMS ERROR '(&00)' ON OUTPUT VSN '(&01)'. VOLUME REJECTED

### Meaning

The DMS error (&00) has occurred on the output volume (&01) during
open processing. A new output volume is requested and processing continues
If there is a DIRECTORY, the volume record is updated to show that the
volume is unusable.

## ARC0031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0031 'DEVICE' OPERAND IGNORED BECAUSE 'TO=PUBLIC' SPECIFIED

### Meaning

The DEVICE operand is not taken in account in FILES statement when
TO=PUBLIC is specified.

## ARC0032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0032 'DIRECTORY' CANNOT BE USED WHEN 'CATONLY=YES'. 'DIRECTORY=NONE' IS ASSUMED

### Meaning

It is not allowed to give a DIRECTORY name when CATONLY=YES.
The statement will be executed without DIRECTORY.

## ARC0033

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0033 ARCHIVE SUBTASK TSN '(&00)' GENERATED

### Meaning

Display of subtask TSN on the terminal.

## ARC0034

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0034 CLOSE ERROR '(&00)' ON INPUT VSN '(&01)'. RUN CONTINUES

### Meaning

When issuing a CLOSE for the input volume with VSN (&01)
the DMS error (&00) occurred. The run continues.

## ARC0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0035 FILE TO BE RESTORED ALREADY EXISTS. FILE NOT REPLACED

### Meaning

The RESTORE statement did not specify REPLACE=YES so the existing file
is not replaced.
The message is associated with the file in error on SUMMARY report
(HSMS) or parameter SNR=*NO (ARCHIVE). For another files this message
will be suppressed.
Processing continues.

## ARC0036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0036 *** WARNING: FGG-INDEX FOR THIS FILE HAS NOT BEEN SAVED ***

### Meaning

No FGG index has been saved for this file (which is a generation).
This may cause errors when trying to restore this file.
FGG: file generation group

## ARC0037

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0037 SPECIFIED FILE NAME '(&00)' NOT PROCESSED

### Meaning

This message is issued for every name in the NAME operands in the FILES
statements, which did not cause at least one file to be saved or
restored, that means, that the result of the run would have been the same
also if these names had been omitted.
This message is also issued when the same filename was given twice in
the statement.

## ARC0038

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0038 SPECIFIED JOB VARIABLE '(&00)' IN JOBVAR STATEMENT NOT PROCESSED

### Meaning

This message is issued for every name in the NAME operands of the JOBVAR
statements, which did not cause at least one job variable to be saved or
restored, that means, that the result of the run had been the same also if
these names had been omitted.

## ARC0039

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0039 JOB VARIABLE TO BE RESTORED ALREADY EXISTS. JOB VARIABLE NOT REPLACED

### Meaning

The RESTORE statement did not specify REPLACE=YES, therefor the existing
job variable is not replaced.
The message is associated with the job variable in error on SUMMARY report
(HSMS) or parameter SNR=*NO (ARCHIVE). For another job variable this
message will be suppressed.
Processing continues.

## ARC0040

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0040 FILE / JV IS ALREADY PROCESSED IN A SVID GREATER THAN OR EQUAL TO THE CONTINUED SVID. FILE / JV NOT SAVED

### Meaning

This file or job variable has an entry in the directory with a SVID
greater or equal the continued one. The file or job variable is not saved
in order to keep the directory consistent.

## ARC0041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0041 MORE THAN ONE OF THE ALTERNATIVE OPERANDS 'FILES'/'JOBVAR' 'SV' OR 'POOL' SPECIFIED. LAST OPERAND WILL BE EXECUTED

### Meaning

In the INQUIRE statement more than one of the alternative operands is
given. Processing continues by analyzing the rest of the statement.
Only the last one of the given alternative operands will be executed.

## ARC0042

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0042 SPECIFIED ELEMENT (TYPE '(&00)', NAME '(&01)' (VERSION '(&02)') NOT PROCESSED

### Meaning

No library element has been restored due to this specification in
the element list. For instance this message will be issued if there is
no matching element in the library.

### Response

Hint: With //RLE ELEMENT=LIST-ALL-TO-REPORT one gets a list of all
existing library elements.

## ARC0043

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0043 FILE OR JOB VARIABLE RESTORED MORE THAN ONCE

### Meaning

File or job variable restored more than once.
When the file is restored under the same sub save number the last reported
has replaced the preceding one. For different sub saves the report
does not say which file is restored latest.

## ARC0044

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0044 CNS FILE OR FGG WITH CNS GENERATIONS OR CNS INDEX IS NOT ERASED

### Meaning

The file or the FGG was not erased, because the file or at least a
generation or the index of the FGG was not saved (because it was not
changed).
FGG: file generation group

## ARC0045

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0045 PUBSET '(&00)' NOT ACCESSIBLE

### Meaning

The public volume set with explicitly specified cat ID (&00) is not
accessible. The affected files are not saved.

### Response

Check state of the MPVS-System.

## ARC0046

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0046 NOT ENOUGH CLASS 5 SPACE FOR 'STREAM=YES'. 'STREAM=NO' ASSUMED

### Meaning

If there is not enough free class 5 address space STREAM=NO is assumed.

## ARC0047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0047 DIRECTORY FOR RUNS WITH 'PARAM-CATID=YES'

### Meaning

PARAM-CATID=YES had been set during the first SAVE run with this
directory.
With that PARAM-CATID=YES has become necessary for every further SAVE and
RESTORE run with this directory.

## ARC0048

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0048 REQM ERROR DURING SCAN OF '(&00)'. ERROR RECOVERY STARTED

### Meaning

Request for class 5 memory failed during scan of catalog partition
(&00). The error routine will issue a $RDCT for each single file instead
of
a scan of the whole partition. This will lead to decrease the performance.

### Response

Check the affected user ID: probably there is an extreme number of files
catalogued in this catalog partition so that a class 5 memory overflow
occurred. In this case it is recommended to split up the user ID into
several user IDs or to spread it into several public volume sets.

## ARC0049

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0049 END OF FILE NOT FOUND

### Meaning

File is not completely saved on the specified tapes.

## ARC0050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0050 VOLUME '(&00)' IS ALREADY IN THE POOL. REQUEST IGNORED

### Meaning

The volume with VSN (&00) is already in the pool in the
directory specified in the statement. The same VSN cannot be
added to the pool, even if another device is specified.
The request to add the volume is ignored.

## ARC0051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0051 VOLUME '(&00)' IS NOT IN THE POOL. REQUEST IGNORED

### Meaning

The volume whose VSN is (&00) is not in the pool of the directory
specified in the POOL statement. The request to remove is ignored.

## ARC0052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0052 VOLUME '(&00)' CONTAINS VALID INFORMATION. REQUEST REJECTED

### Meaning

The user wants to remove a volume from the POOL which belongs
to SVID that is not yet purged.

### Response

Either purge the SVID or leave the volume in the POOL.

## ARC0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0053 HSMS RUNS ARE ALSO PRESENT

### Meaning

The ARCHIVE checkpoint file contains data for HSMS.

### Response

Do not erase file $TSOS.ARCHIVE.CHKPT.

## ARC0054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0054 'PARAM SNR=YES' IS ASSUMED BECAUSE OF 'LIST = ..,ALL'

## ARC0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0055 OPERAND '(&00)' DIFFERS FROM THAT OF INITIAL RUN

### Meaning

An operand of the current statement is different to that given in the
statement being continued.
(&00): - ERASE, LIST or DIRSAVE; new value is used.
- DEVICE, SHARE; the value of the statement being continued will
be used.

## ARC0056

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0056 PUBLIC FILE SAVED WITH 'CATONLY=YES'. FILE NOT RESTORED

### Meaning

The save run that is actually read in was done with CATONLY=YES but the
affected file resides on public volumes. The catalog entry of this file
is not restored.

## ARC0057

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0057 '(&00)' ERRORS DURING PROCESSING OF INPUT TAPE OR DISC SAVE FILE '(&01)'

### Meaning

Errors occurred during processing an input tape / tape-cartridge / disk
save file.
(&00): number of errors
(&01): tape / tape-cartridge / disk VSN.
Any files affected and to be copied will be indicated in the ARCHIVE
Report.

## ARC0058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0058 OUTPUT TO SYSOUT FOR 'INQUIRE' REPORT CANCELLED BY K2 KEY

### Meaning

The output of the ARCHIVE INQUIRE report to SYSOUT is cancelled by
the k2 key. Report output to SYSLST continues (if specified).

## ARC0059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0059 FILE HAS BEEN SAVED 'ON LINE'

### Meaning

If the statement is a SAVE/EXPORT, an opened file has been
saved/exported (i.e ON LINE).
If the statement is a RESTORE/IMPORT, an online saving file
has been restored/imported.
The file consistency is not guaranteed.

### Response

In the case of data base files the data base consistency must be
considered:
- after SAVE/EXPORT it may be necessary to additionally save logging
files,
- after RESTORE/IMPORT the consistency of the data base must be ensured
before further use. Depending on the data base system, this may require
logging files, which must be saved separately.

## ARC0060

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0060 EOF NOT FOUND ON OUTPUT VOLUME '(&00)' DURING RESTART

### Meaning

Volume (&00) contains an abnormally terminated save run. Correct restore
from this volume can be guaranteed only when the run is done with
DIRECTORY.
Restore runs from this volume without DIRECTORY in general will have
unpredictable results. They work correctly only if all files to be
restored are specified fully qualified in the NAME operand and no file
generation groups are among them.

### Response

When saving without DIRECTORY, repeat save for the files on volume (&00).

## ARC0061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0061 FILE GREATER THAN 32GB. FILE NOT PROCESSED

### Meaning

Files with a file size greater than 32GB can not be processed
with this ARCHIVE Version or in this environment.

### Response

Processing of this file is possible in an environment with
following features:
- >= BS2000 OSD V5.0a
- >= ARCHIVE V6.0a
- In case of a restoration the destination pubset must allow
- files larger than 32GB.

## ARC0062

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0062 FILE GREATER THAN 32GB. FILE NOT SAVED

### Meaning

Saving of files with file size greater than 32GB not
supported with CATALOG-FORMAT=*BEFORE-OSD-V1.

### Response

Saving of this files is possible using
CATALOG-FORMAT=*KEEP.

## ARC0063

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0063 THERE ARE NO JOB VARIABLES SAVE RECORDS IN THE DIRECTORY-FILE FOR USER ID '(&00)'

### Meaning

The user ID (&00) has no job variables save records in the directory file
given in the INQUIRE statement.
Processing of the statement continues.

## ARC0064

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0064 JOB VARIABLE '(&00)' NOT IN DIRECTORY FILE. PROCESSING CONTINUES

### Meaning

The job variable name (&00) does not exist in the directory file give in
the INQUIRE statement. Processing continues.

## ARC0065

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0065 THERE ARE NO JOB VARIABLES SAVE RECORDS IN DIRECTORY FILE

### Meaning

An INQUIRE statement with a JOBVAR operand has been given for a directory
file with no job variables save records.
Processing of the statement continues.

## ARC0066

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0066 OUTPUT VSN '(&00)' GIVEN IN STATEMENT CANNOT BE USED. VOLUME IS REJECTED

### Meaning

The output VSN (&00) given in statement is already in use or has
a volume type different to the output volume type of the actual run.
The specified volume is rejected.

## ARC0067

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0067 POOL DOES NOT CONTAIN TAPES

### Meaning

An INQUIRE statement with a POOL operand has specified a directory
which has no tapes in its pool.
Processing of the statement continues.

## ARC0068

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0068 FILE '(&00)' IS NOT IN DIRECTORY FILES

### Meaning

The file name (&00) does not exist in the directory given in the
INQUIRE statement.
Processing continues with the next file name in the FILES statement.

## ARC0069

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0069 NO FILE OR JV SAVE RECORDS IN DIRECTORY FILE

### Meaning

An INQUIRE statement with a FILES operand has been given for a directory
file with no file save records.
Processing of the statement continues.

## ARC007A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC007A SAVE VERSION '(&00)' NOT OR INCONSISTENT IN DIRECTORY FILE

### Meaning

The Save Version specified for Purge with FORCE has no correct entry.
References to this Save Version - if there are any in other records -
will be removed.

## ARC0070

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0070 NO SAVE VERSION RECORDS IN DIRECTORY

### Meaning

An INQUIRE statement with a SV operand has been given for a directory
file with no save versions.
Processing of the statement continues.

## ARC0071

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0071 NO FILE SAVE RECORDS IN DIRECTORY FILE FOR USER ID '(&00)'

### Meaning

The user ID (&00) has no file save records in the directory file given
in the INQUIRE statement.
Processing continues with the next file name in the FILES operand.

## ARC0072

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0072 NO FILES WITH MATCHING BACKUP LEVEL WERE SAVED BEFORE OR EQUAL THE SPECIFIED DATE AND TIME

### Meaning

A PURGE or INQUIRE statement has been given but no files with matching
backup level were saved before or at the specified date and time.
Processing of the statement continues.

## ARC0073

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0073 SAVE VERSION '(&00)' IS NOT IN DIRECTORY FILE

### Meaning

A PURGE or INQUIRE statement with a specific save version identifier
has been given, but the version does not exist on the directory.
Processing continues with the next save version identifier specified.

## ARC0074

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0074 THERE ARE NO OBSOLETE SAVE VERSIONS IN DIRECTORY FILE

### Meaning

An INQUIRE statement with a SV=OBSOLETE operand or a PURGE statement has
been given, but there are no obsolete save versions on the directory.
Processing of the statement continues.

## ARC0075

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0075 ONLY OBSOLETE SAVE VERSIONS CAN BE PURGED

### Meaning

A PURGE statement with a specific save version identifier has been
given, but the save version is not obsolete and will not be purged.
Processing of the statement continues with the next save version
identifier.

## ARC0076

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0076 ERASE OF FILE '(&00)' NOT POSSIBLE. RUN CONTINUES

### Meaning

While processing a PURGE statement an I/O error has occurred when
trying to erase the disk save file (&00).
Processing continues.

### Response

Erase disk save file with /DELETE-FILE.

## ARC0077

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0077 *** FILE HAS IDCERPI SET - USE 'REPAIR-DISK-FILES' TO REPAIR IT ******

### Meaning

The file is not orderly closed, for instance due to a system crash while
it was opened in write mode. The value of LAST-PAGE-POINTER may be
incorrect.
If the file is an ISAM file it may be in an inconsistent status.

### Response

Repair the file with REMOVE-FILE-ALLOCATION-LOCKS and save it again or
repair the file with REMOVE-FILE-ALLOCATION-LOCKS after RESTORE or IMPORT.

## ARC0078

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0078 TOO MANY DRIVES SPECIFIED FOR 'FROM/CONTINUE'

### Meaning

More drives have been specified than are appropriate for the save
version being continued.
Processing continues with the correct number of drives.

## ARC0079

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0079 OVERFLOW OF GENERATION NUMBER IN 'THRU' STATEMENT

### Meaning

The relative value for a file generation number in a THRU statement causes
an overflow of the generation number (value must be 1 - 9999). The
generation number is increased or lowered by 9999.
As the THRU statement is valuated alphabeticly, maybe generations of a
group are not saved.

## ARC0080

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0080 MISSING FULL SAVE. FILE '(&00)' RESTORED FROM AN EARLIER SVID

### Meaning

LATEST or a date (and time of day) has been specified in the FROM operand
of the RESTORE statement. The youngest save for file (&00) before the
specified time is a partial save. During the current restore the
corresponding full save has not been found in the directory. Therefore the
file has been restored from the youngest full save before the rejected
partial save and perhaps another partial save.

## ARC0081

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0081 MISSING FULL SAVE. FILE '(&00)' NOT RESTORED

### Meaning

A partial or an incremental save cannot be restored.
Possible reasons:
- PARTIAL save: similar situation as labeled by message ARC0080.
However there is no full save earlier than the rejected partial save
in the directory.
- INCREMENTAL save: only the CNS entry exists in the directory.
The full save has been erroneously purged by the user.
- for NET-STORAGE file only: there is only a CATL and/or CNS entry
in the directory while *DATA-AND-CATALOG required a save-type FULL.

## ARC0082

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0082 ERROR DURING WRITE OF 'FULL-RESTORE-CHECKPOINT' RECORD FOR FILE '(&00)'

### Meaning

The restore of the full save of the affected file could be completed
successfully but the checkpoint record indicating this fact for the
following restore of a partial save could not be written. The partial save
will not be restored.

### Response

Restore the partial save in another run.

## ARC0083

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0083 ERROR DURING WRITE OF INDEX RESTORE CHECKPOINT FOR GROUP '(&00)'. INDEX WILL NOT BE RESTORED

### Meaning

The index of the affected file generation group (&00) could be restored
correctly from the actual first SVID, but the checkpoint record
indicating this fact for the restore of the index from the following
SVIDs could not be written. Therefore as REPLACE=NO is specified
the index will not be restored from the following SVIDs.

### Response

Restore index and generations in another run.

## ARC0084

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0084 'ERASE=NO' IS ASSUMED WITH 'RENAME' AT EXPORT

### Meaning

The operand ERASE is ignored for renamed FILES/JOBVAR.
Processing continues.

## ARC0085

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0085 FILE GENERATION MAY NOT BE RENAMED AT EXPORT

### Meaning

A file generation may not be renamed at EXPORT. The whole file
generation group must be renamed. Processing continues with the next
FILES/JOBVAR statement.

## ARC0086

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0086 NOT ABLE TO SAVE THE DIRECTORY

### Meaning

In a SAVE type of run with a DIRSAVE=YES operand, the directory cannot be
saved either because no subtask is still active or because the directory
can not be saved completely on the same output device. The processing
of the statement will continue.

## ARC0087

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0087 VALUE OF 'BLOCK-SIZE' OPERAND TOO LOW FOR THIS SAVE RUN. MINIMUM VALUE IS TAKEN

### Meaning

The minimum value is taken :
- if SAVE-ACL=YES, the minimum value is 3
- if TARGET-ARCHIVE-VERSION=FROM-V26B (default) and
SAVE-ACL=NO, the minimum value is 2
- BLOCK-SIZE=1 is only possible with TARGET-ARCHIVE-VERSION=BEFORE-V26B.

## ARC0088

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0088 FILE '(&00)' PARTIALLY SAVED IN LATEST SAVED VERSION; SKIPPED DURING THIS RUN

### Meaning

Files partially saved in latest save version are not backed up in the
frame of a backup run FROM=*ONLY-LATEST-BACKUP

## ARC0089

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0089 CONTINUE-TAPE '(&00)' ALREADY FULL. CONTINUE WILL BE STARTED ON NEXT TAPE

### Meaning

The continue tape is already full. Continue will be started on the next
tape.

## ARC0090

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0090 FILE NAME INDICATES A TEMPORARY FILE. FILE NOT PROCESSED

### Meaning

Name of file to be processed begins with a character which in the actual
session indicates temporary files; so the file is considered as temporary.
Temporary files will not be saved/restored.

### Response

Use the RENAME operand in the FILES statement to rename the file. Use
a name which does not indicate temporary files.

## ARC0091

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0091 MIGRATED FILE NOT SAVED / EXPORTED

### Meaning

Only TSOS is allowed to SAVE a migrated file. EXPORT of a
migrated file is not allowed.

## ARC0092

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0092 SUBSYSTEM 'SRPMFACL' NOT CREATED. FILE RESTORED WITH DMS DEFAULT PROTECTIONS

### Meaning

The full access control list was required to be restored for this file,
but the subsystem SRPMFACL was not created.
The file is restored without ACL protection.
SRPMFACL and FACS is not supported with SECOS from Version V4.0.

### Response

Create the subsystem SRPMFACL and retry.

## ARC0093

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0093 RENAME OF MIGRATED FILE NOT ALLOWED. FILE NOT PROCESSED

### Meaning

Possible reasons:
1. Rename of migrated files is not allowed if only the CE is
restored to disk;
2. In the selected save version the file to be restored
has save type MIGF, which means that the CE of a migrated
file was saved. Rename of a migrated file
is not allowed if only the CE can be restored.

## ARC0094

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0094 OPERAND 'COMPRESS' RESET TO 'NO' BECAUSE OF HARDWARE COMPRESSION

### Meaning

The device performs a hardware compression. This one has priority over
the software compression. The COMPRESS operand is reset to NO.

## ARC0095

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0095 FILE/JV NOT ACCESSIBLE AND NOT PROCESSED. ACCESS MONITOR RETURN CODE: '(&00)'

### Meaning

The return code corresponds to following situations:
X'0001': FILE/JV not share
X'0002': FILE/JV read only
X'0003': FILE/JV protected by password
X'0004': FILE/JV protected by expiration date
X'0005': FILE cannot be renamed
X'0006': the owner is not the caller
X'0007': FILE/JV protected by ACL
X'0008': FILE inconsistent
X'0009': PLAM library is in protected mode
X'000A': FILE protected by GUARDS
X'000B': the given GUARD is not found
X'000C': the file owner is not authorized to use the given GUARD
X'000D': the subsystem GUARDS is not active
X'000E': terminate task
X'0015': monitor internal error
X'0016': parameter error
X'0017': invalid file name
X'0018': file does not exist
X'0019': no lock present
X'001A': PVS not accessible
X'001B': no access right to PVS.

## ARC0096

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0096 MIGRATED FILE '(&00)' NOT COPIED

### Meaning

The file (&00) is no more migrated. It has been erased, recalled or
changed since the migration and it will not be copied
If the file is member of several-SVIDs, this message is used for the
older SVID.

## ARC0097

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0097 CATALOG ACCESS ERROR '(&00)' FOR FILE (&01). CATALOG CHECK SKIPPED

### Meaning

An error occurred during access of the system catalog.
Processing of the file continues without check of the catalog.
(&00): error code and secondary return code (if present).
(&01): file name.

## ARC0098

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0098 ERROR '(&00)' IN MACRO '(&01)' DURING MIGRATION / RECALL. FILE SPECIFIC PROCESSING CONTINUES IF POSSIBLE OTHERWISE RUN IS TERMINATED

### Meaning

During migration / recall support for HSMS the error (&00) occurred.
Possible errors:
- connect/disconnect subsystem HSMS (ESM) error,
- file specific catalog access (CMS) error,
- file specific erase (DMS) error,
- file specific lock (DMS) error,
- ARCHIVE (ARC) error (more information in the SERSLOG file).
File specific processing continues, otherwise run is terminated.

## ARC0099

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0099 ONLY '(&00)' SUBTASK(S) WILL BE USED

### Meaning

Processing of the statement will only use (&00) drives though more
were specified in the DRIVES operand.

## ARC0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0100 INPUT TEXT DOES NOT START WITH A STATEMENT KEYWORD

### Meaning

At the beginning of the statement analysis, a statement keyword was
expected but not found.
The analyse of input text is continued.
The statement will not be executed.

## ARC0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0101 '(&00)' NO KEYWORD OR NOT ALLOWED

### Meaning

(&00) is no ARCHIVE keyword
or - if ARC0134 has been displayed before -
a statement keyword in a wrong context.
The execution of the statement will be aborted.

### Response

Enter corrected statement.

## ARC0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0102 '(&00)' OPERAND IS NOT VALID FOR THIS STATEMENT. STATEMENT NOT EXECUTED

### Meaning

An operand has been given which is not appropriate to this statement.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.

## ARC0103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0103 A 'TO' OPERAND HAS OCCURRED BEFORE THIS 'FROM' OPERAND. STATEMENT NOT EXECUTED

### Meaning

A FROM operand, implying a RESTORE type of run, has been found but
a TO operand, implying a SAVE type of run, has already been given.
Processing continues after this error by analyzing the rest of the
statement.

## ARC0104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0104 A 'FROM' OPERAND HAS OCCURRED BEFORE THIS 'TO' OPERAND. STATEMENT NOT EXECUTED

### Meaning

A TO operand, implying a SAVE type of run, has been found but a
FROM operand, implying a RESTORE type of run, has already been given.
Processing continues after this error by analyzing the rest of
the statement.

## ARC0105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0105 VALUE OF '(&00)' OPERAND SHOULD BE 'YES' OR 'NO'. STATEMENT NOT EXECUTED

### Meaning

The value of the specified operand should be YES or NO.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.

## ARC0106

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0106 VALUE OF '(&00)' OPERAND SHOULD BE A POSITIVE INTEGER. STATEMENT NOT EXECUTED

### Meaning

Value of the (&00) operand should be a positive integer.
Processing continues after this error by analyzing of statement.

## ARC0107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0107 THIS DIRECTORY MAY NOT BE USED FOR THIS ARCHIVE RUN. STATEMENT NOT EXECUTED

### Meaning

A directory has been specified which may only be accessed by privileged
users. Processing continues after this error by analyzing the rest of
the statement.

## ARC0108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0108 A NEW DIRECTORY CANNOT BE SPECIFIED FOR THIS STATEMENT. STATEMENT NOT EXECUTED

### Meaning

A NEW operand has been specified with the directory operand.
This is not permitted for the statement being processed.
Processing continues after this error by analyzing the rest of the
statement.

## ARC0109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0109 ILLEGAL 'LIST' OPERAND VALUE. STATEMENT NOT EXECUTED

### Meaning

An illegal value has been given for the LIST operand.
Only SYSLST, SYSOUT, BOTH or NONE are valid.
Processing continues after this error by analyzing the rest of
the statement.

## ARC0110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0110 STATEMENT INCOMPLETE. STATEMENT IGNORED

### Meaning

The text supplied does not form a complete statement.
Processing continues after this error by analyzing the rest of
the statement, but the statement will not be executed.

### Response

Reenter correct statement.

## ARC0111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0111 ERROR IN '(&00)' OPERAND: VSN NOT VALID. STATEMENT NOT EXECUTED

### Meaning

A VSN was expected with the specified operand keyword.
Processing continues after this error by analyzing the rest of
the statement.
(&00): the keyword of the operand in error.

## ARC0112

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0112 ERROR IN '(&00)' OPERAND: INVALID OR MISSING VSN LIST. STATEMENT NOT EXECUTED

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.
Possible reasons:
- A VSN of a private disk is specified when a VSN of a Net-Storage
volume is expected.
- A VSN of a Net-Storage volume is specified when VSN of a
private disk is expected.

## ARC0113

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0113 ERROR IN '(&00)' OPERAND: INVALID OR MISSING PASSWORD. STATEMENT NOT EXECUTED

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.

## ARC0114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0114 ERROR IN '(&00)' OPERAND: INVALID OR MISSING SAVE VERSION IDENTIFIER. STATEMENT NOT EXECUTED

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.

## ARC0115

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0115 ERROR IN '(&00)' OPERAND: DATE NOT FOUND. STATEMENT NOT EXECUTED

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.

## ARC0116

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0116 ERROR IN '(&00)' OPERAND: BACKUP LEVEL IS NOT 'A' OR 'B' OR 'C' OR 'D'. STATEMENT NOT EXECUTED

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of
the statement, but the statement will not be executed.
(&00): the keyword of the operand in error.

## ARC0117

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0117 ERROR IN '(&00)' OPERAND. STATEMENT NOT EXECUTED

### Meaning

The value of the operand (&00) is invalid or missing.
The data type is 'alphanum-name 1..8'.
Processing continues after this error by analyzing the rest of the
statement.
(&00): operand name

## ARC0118

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0118 'FORCE=YES' REQUIRES FULLY QUALIFIED SVIDS

## ARC0119

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0119 ERROR IN '(&00)' OPERAND: INVALID OR MISSING FILE/JV/ELEMENT NAME

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of the
statement.
(&00): the keyword of the operand in error.

## ARC0120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0120 ERROR IN '(&00)' OPERAND: 'LATER' OR 'ACTIVE' NOT FOUND. STATEMENT NOT EXECUTED

### Meaning

Specified operand for keyword (&00) invalid or missing.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.
(&00): the keyword of the operand in error.

## ARC0121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0121 FILE IS NOT ERASED

### Meaning

The file is not erased because
- not all generations belonging to it are saved yet
- or files on userid SYSHSMS was not erased

## ARC0122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0122 ERROR '(&00)' DURING MIGRATION / RECALL. FILE SPECIFIC PROCESSING CONTINUES IF POSSIBLE OTHERWISE RUN IS TERMINATED

### Meaning

During migration / recall support for HSMS the following error (&00)
occurred:
- File specific DMS error
- File specific ARCHIVE error
- DSSM error ($ESMCONI) during access to subsystem HSMS
- CMS error ($DFMFLMI) during lock/unlock of a file
- HSMS error ($DMAHSMI) during access to a file
If possible, file specific processing continues, otherwise run is
terminated.

### Response

Enter in system mode /HELP-MSG for corresponding message key:
- DMS error: /HELP-MSG DMS(&00)
- ARCHIVE error ((&00)=Annn): /HELP-MSG ARC0nnn
Evaluate SERSLOG for other errors.

## ARC0123

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0123 PRECEDING 'FILES' OR 'JOBVAR' STATEMENT MISSING. STATEMENT NOT EXECUTED

### Meaning

A statement has been given which requires a preceding FILES or JOBVAR
statement.
The statement will not be executed.
The analyse of input text is continued.

## ARC0124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0124 A 'FROM' OPERAND MUST BE SPECIFIED FOR 'IMPORT' OR 'LIST' COMMANDS

### Meaning

A FROM operand must be specified for IMPORT or LIST commands.
Processing continues after this error by analyzing the rest of
the statement, but the statement will not be executed.

## ARC0125

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0125 FILES CANNOT BE RENAMED WITH THIS STATEMENT. STATEMENT NOT EXECUTED

### Meaning

A RENAME operand has been specified, but is invalid for the statement
being analysed.
Processing continues after this error by analyzing the rest of the
statement. The statement will be not executed.

## ARC0126

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0126 ANOTHER USER'S FILES OR JOB VARIABLES CAN ONLY BE SPECIFIED BY PRIVILEGED USERS. A NORMAL USER CAN EXPORT OTHER USER'S FILES OR JOB VARIABLE WITH THE PARAMETER FILE-ATTRIBUTES=*RESET-TO-STD. STATEMENT IGNORED

### Meaning

Another user's files or job variables can only be specified with this
statement by privileged users. Processing continues after this error
by analyzing the rest of the statement, but the statement will not be
executed.

## ARC0127

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0127 VALUE OF '(&00)' OPERAND REQUIRES A DIRECTORY. STATEMENT NOT EXECUTED

### Meaning

Value of (&00) operand requires a directory.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.
(&00): DUPLICATE or DIRSAVE or FROM or FROM=SVID.

## ARC0128

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0128 DIRECTORY REQUIRED WITH THE 'POOL', 'PURGE', 'INQUIRE' STATEMENT. STATEMENT NOT EXECUTED

### Meaning

Directory required with the POOL, PURGE, INQUIRE statement.
Processing continues after this error by analyzing the rest of the
statement. The statement will not be executed.

## ARC0129

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0129 'POOL' STATEMENT HAS NO 'ADD' OR 'REMOVE' OPERANDS. STATEMENT NOT EXECUTED

### Meaning

POOL statement has no ADD or REMOVE operands.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.

## ARC0130

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0130 A CONTINUE SAVE RUN WITHOUT DIRECTORY FILE MUST SPECIFY VSN(S). STATEMENT NOT EXECUTED

### Meaning

In a continue save run no directory file has been specified. In this case
the CONTINUE operand must specify tape or disk VSNs. Processing continues
after this error by analyzing the rest of the statement. But the
statement will not be processed.

## ARC0131

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0131 ERROR IN 'FROM' OPERAND: TIME SPECIFIED MUST NOT BE EARLIER THAN THAT OF THE SAVE VERSION. STATEMENT NOT EXECUTED

### Meaning

Error in FROM operand: time specified must not be earlier than that
of the save version. Processing continues after this error by analyzing
the rest of the statement, but the statement will not be executed.

## ARC0132

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0132 'FILES' STATEMENT CANNOT HAVE A 'TO' OPERAND WITH THIS STATEMENT. STATEMENT NOT EXECUTED

### Meaning

A FILES statement cannot have a TO operand with this statement.
Processing continues after this error by analyzing the rest of
the statement, but the statement will not be executed.

## ARC0133

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0133 A 'FILES' OR 'JV' STATEMENT CANNOT HAVE A 'FROM' OPERAND WITH THIS STATEMENT. STATEMENT NOT EXECUTED

### Meaning

A FILES or JV statement cannot have a FROM operand with this statement.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.

## ARC0134

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0134 STATEMENT KEYWORD MISPLACED. STATEMENT IGNORED

### Meaning

A statement keyword has been found during the analysis of another
statement. Processing continues after this error by analyzing the rest
of the original statement, but neither of the commands will be executed.

## ARC0135

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0135 ERROR DURING ON LINE SAVING OF AN DATA BASE. FILE NOT PROCESSED

### Meaning

The database online saving authorization has been modified during the
run.

### Response

Try to save this file with another run.

## ARC0136

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0136 ARCHIVE SEQUENCE NUMBER NOT SPECIFIED. STATEMENT NOT PROCESSED

### Meaning

An ARCHIVE sequence number (yymmdd.hhmmss preceded by 'A.' or 'L.')
was expected but not found.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.

## ARC0137

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0137 INVALID ARCHIVE SEQUENCE NUMBER OR SAVE VERSION IDENTIFIER. STATEMENT NOT EXECUTED

### Meaning

Invalid ARCHIVE sequence number or save version identifier.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.

## ARC0138

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0138 INVALID '(&00)' OPERAND VALUE. STATEMENT NOT EXECUTED

### Meaning

Invalid (&00) operand value.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.
(&00): the keyword of the operand in error.

## ARC0139

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0139 'DRIVES' OPERAND OUT OF RANGE. STATEMENT NOT EXECUTED

### Meaning

The DRIVES operand value is not a positive integer.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.

## ARC0140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0140 SYSDTA READ ERROR. STATEMENT ABORTED

### Meaning

SYSDTA read error.
Processing of the current statement is aborted.

## ARC0141

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0141 ARCHIVE STATEMENT EXCEEDS BUFFER SIZE OR HAS LENGTH ZERO. STATEMENT ABORTED

### Meaning

The text of the statement supplied to ARCHIVE is too long or has the
length zero. Processing of the current statement is aborted.

## ARC0142

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0142 INSUFFICIENT CLASS 6 MEMORY. STATEMENT IGNORED

### Meaning

ARCHIVE cannot obtain enough class 6 memory to hold the text of the
statement which has been input.
Processing of the statement is aborted.

## ARC0143

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0143 WRLST OR WROUT ERROR OR NO FURTHER OUTPUT FOR INQUIRE DUE TO K2 KEY. STATEMENT ABORTED

### Meaning

An error has occurred during writing to SYSLST or SYSOUT,
or ARCHIVE INQUIRE report to SYSOUT is cancelled by K2 key and
report output to SYSLST is not specified.
Further printing is suppressed and processing of the current statement
terminates.

## ARC0144

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0144 'SAVE' OR 'EXPORT' WITH 'CONTINUE' OR 'DIRSAVE' IS NOT POSSIBLE WITH SPECIFIED DEVICE TYP

## ARC0145

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0145 ERROR IN '(&00)' OPERAND: INVALID DATE OR SAVE VERSION IDENTIFIER. STATEMENT NOT EXECUTED

### Meaning

Error in (&00) operand: Invalid date or save version identifier.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.
(&00): the keyword of the operand in error.

## ARC0146

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0146 FILE '(&00)' NOT COMPLETELY SAVED ON '(&01)' AND CANNOT BE FOUND DURING RESTART. STATEMENT ABORTED

### Meaning

A file was partially saved on a tape and the file cannot be found
during a restart of the statement.
Processing of the current statement is aborted.
(&00): the name of the file.
(&01): the VSN of the tape.

## ARC0147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0147 NOTHING FOUND TO RESTORE OR TO LIST

### Meaning

ARCHIVE has found out, that there is no suitable SVID in the directory, or
that the specified files / job variables have not been saved into the
specified SVIDs.

## ARC0148

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0148 '(&00)' FILE DOES NOT EXIST. CONTACT THE SYSTEM ADMINISTRATOR

### Meaning

An ARCHIVE system file does not exist.
Processing of the statement terminates. The system administrator should
be informed that the file is missing in order that he can create it.
(&00): the file identifier CHKPT or LATER.

### Response

The file must be created by an ARCHIVE run under TSOS.

## ARC0149

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0149 SHARUPD CONFLICT ON DIRECTORY HAS LASTED TOO LONG. STATEMENT ABORTED

### Meaning

ARCHIVE, after retrying the OPEN of the directory for a
certain length of time since giving message ARC0805 has aborted
processing of the current statement since the SHARUPD conflict persists.

## ARC0150

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0150 BLOCK LOCK ERROR ON '(&00)' FILE. STATEMENT ABNORMALLY TERMINATED

### Meaning

An I/O operation on a file has had a lock error.
Processing of the statement terminates. The statement should be reissued
when the necessary file is free.
(&00): the file identifier CHKPT or LATER or DIRECTORY.

## ARC0151

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0151 '(&00)' IS ALLOWED FOR PRIVILEGED USERS ONLY

### Meaning

Reject invalid operand or value of an operand.

## ARC0152

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0152 DIRECTORY SPECIFIED FOR A CONTINUE SAVE DIFFERS FROM THAT OF THE ORIGINAL SAVE. SUBSAVE TERMINATED

### Meaning

The directory specified for a CONTINUE save differs
from that of the original save. Subsave is terminated.

## ARC0153

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0153 A SAVE CANNOT BE CONTINUED BY A USER OTHER THAN THE ONE WHO MADE THE ORIGINAL SAVE

### Meaning

A save cannot be continued by an user other than the one who made the
original save. In particular, a normal user may not continue an HSMS save.
The (sub)save is terminated.

## ARC0154

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0154 SAVE VERSION IDENTIFIER SPECIFIED (IN A 'CONTINUE' OR 'SAME SVID' RUN) DIFFERS FROM THAT OF THE ORIGINAL RUN. SUBSAVE TERMINATED

### Meaning

CONTINUE run:
The save version identifier specified by the CONTINUE operand
differs form that of the original save.
SAME SVID run:
Different input save versions have been specified, or the input
save version identifier differs from the one to be continued.

## ARC0155

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0155 OPERAND '(&00)' DIFFERS FROM THAT OF INITIAL RUN. STATEMENT ABORTED

### Meaning

An operand to the current statement is different to that given in the
statement of the run being continued. The current statement is aborted.
(&00): the operand of the statement which is different.

## ARC0156

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0156 SAVE VERSION '(&00)' IS NOT IN THE DIRECTORY. STATEMENT ABORTED

### Meaning

The save version (&00), specified in the statement, cannot be found in
the directory. Processing of the statement is aborted.
(&00) : save version (S.YYMMDD.HHMMSS)

## ARC0157

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0157 DIRECTORY FILE IS NOT IN THE CATALOG. STATEMENT ABORTED

### Meaning

The directory file is not in the catalog. Statement aborted.

## ARC0158

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0158 FILE IS NOT EMPTY AND CANNOT BE USED AS A NEW DIRECTORY. STATEMENT ABORTED

### Meaning

The file specified as a new directory in the statement already exists
and is not empty. It cannot, therefore, be used as a new directory.
Processing of the current statement is aborted.

## ARC0159

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0159 SPECIFIED FILE HAS NOT APPROPRIATE FILE ATTRIBUTES OR IT IS NOT IN THE EXPECTED FORMAT FOR A '(&00)' FILE. STATEMENT ABORTED

### Meaning

The file whose type is given by (&00) does not have the correct
characteristics.
(&00): DIRECTORY or CHECKPOINT or LATER or PRINT.

### Response

In the case of CHECKPOINT or LATER, the system administrator should
be consulted about the error. For the other types of file, the user
should correct the file characteristics and reissue the statement.
See 'Work Files' section of the ARCHIVE User Guide.

## ARC0160

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0160 FILE GENERATION GROUP IS NOT ERASED BECAUSE NOT ALL GENERATIONS BELONGING TO IT ARE SAVED

### Meaning

The file generation group is not erased because not all generations
belonging to it are saved.

## ARC0161

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0161 WRONG USAGE WITH THIS TYPE OF DIRECTORY. STATEMENT ABORTED

### Meaning

The directory specified was wrongly used.
Possible reasons:
- The directory was created for archiving with SAVE/EXPORT and is
being used for archiving with DSAVE/DEXPORT (or DRESTORE/DIMPORT)
or vice versa.
- The directory has been created via HSMS (e.g for migration and
archival). Only ARCHIVE IMPORT/LIST runs can work.
The statement is aborted.

## ARC0162

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0162 VOLUME '(&00)' IS NOT IN THE POOL OR NOT USED BY ANY SVID

### Meaning

For a run with DIRECTORY VSN (&00) has been specified as data medium of
an ARCHIVE save file by a FROM or CONTINUE operand.
- But either the directory tape pool does not contain VSN (&00),
- or VSN is marked as not used by any SVID,
- or a disk VSN is specified for an ARCHIVE save file
on tape or tape cartridge,
- or a disk VSN is specified without SVID.

## ARC0163

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0163 SAVE VERSION OF TAPE '(&00)' IS NOT CONSISTENT WITH THE PREVIOUS TAPES. STATEMENT ABORTED

### Meaning

In checking the consistency of tape VSNs supplied in the statement,
tape VSN (&00) has been found to have a save version identifier
on the directory which is inconsistent with that of previous tapes.
Processing of the current statement is aborted.

## ARC0164

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0164 SVID '(&00)' FOR TAPE '(&01)' IS DIFFERENT TO THAT IN THE 'CONTINUE' OR 'FROM' OPERAND

### Meaning

For a run with DIRECTORY both a SVID and one or more tape VSNs have
been specified by a FROM or CONTINUE operand. But directory
information proves, that VSN (&01) belongs to SVID (&00).

## ARC0165

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0165 THERE ARE NO SAVE VERSION RECORDS IN THE DIRECTORY. STATEMENT ABORTED

### Meaning

No save versions can be found in the directory file.
Processing of the current statement is aborted.

## ARC0166

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0166 SPECIFIED 'STATE' SAVE VERSION IS OLDER THAN ANY SAVE VERSION IN THE DIRECTORY. STATEMENT ABORTED

### Meaning

A RESTORE type of statement cannot restore any files to the specified
state since all save versions in the directory are younger than the
specified one.
Processing of the current statement is aborted.

## ARC0167

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0167 DISK VSN MUST BE SPECIFIED. STATEMENT ABORTED

### Meaning

At least one disk VSN must be specified for saving to volume type disk.
Specification POOL or OPERATOR is not allowed.
The statement is aborted.

## ARC0168

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0168 PUBLIC DISKS CANNOT BE USED FOR A EXPORT STATEMENT. STATEMENT ABORTED

### Meaning

A public disk VSN specified in VOLUME operand may not be used to create
disk save files for export.
The statement is aborted.

## ARC0169

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0169 NOT PERMITTED RENAME OF A CATALOG ENTRY. CATALOG ENTRY NOT RESTORED

### Meaning

When restoring a catalog entry only the cat ID can be renamed.
The catalog entry was not restored.
Processing continues with the next file.

## ARC0170

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0170 DIRECTORY FILE COULD NOT BE SAVED ON VSN '(&00)'. DIRECTORY NOT SAVED

### Meaning

There is not enough space on the volume (&00) to save the directory
file. With DIRSAVE=YES it is not possible to use more than one
volume for saving the directory. The directory file is not saved.

### Response

Save the directory file with another ARCHIVE run.

## ARC0171

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0171 DMS ERROR '(&00)' ON '(&01)' FILE. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&00): DMS error code
(&01): PRINT or DIRECTORY or CHECKPOINT or LATER or PARAMETER.

## ARC0172

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0172 DIRECTORY NAME NOT FULLY QUALIFIED. STATEMENT REJECTED

### Meaning

The directory name must be specified fully qualified.

### Response

Retry statement with correct directory name.

## ARC0173

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0173 PRINT FILE ALREADY IN CATALOG. STATEMENT ABORTED

### Meaning

The print file, which is created at the beginning of certain file
archiving commands, already exists in the catalog.
Processing of the current statement is aborted.

### Response

The statement should be reissued, then a different print file name is
generated.

## ARC0174

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0174 DMS ERROR '(&00)' DURING ERASE OF PRINT FILE. PROCESSING CONTINUES. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

At the end of a statement which generates printing, ARCHIVE
attempts to erase the print file for the reports.
Processing of statement continues.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&00): error code from the ERASE macro.

### Response

The user has to erase the print file himself.

## ARC0175

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0175 WRONG ARCHIVE TAPE FORMAT. SVID CANNOT BE CONTINUED

### Meaning

The tapes, or the save files on disk, which have been specified by the
CONTINUE operand, have been created by an ARCHIVE version, which writes
the blocks on tape or on disk in a format, which differs from the format
of the ARCHIVE version of the current run. This makes this CONTINUE
impossible.

### Response

Convert the tape, or the disk save files by the current ARCHIVE version
into the actual format (save tape from tape) and start the CONTINUE run
again.

## ARC0176

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0176 ERROR DURING DIRECTORY UPDATE. DIRECTORY NOT UPDATED FOR THIS FILE/JOB VARIABLE

### Meaning

The directory records for this file or job variable are probably damaged
or cannot be extended.
The directory has not been updated for this file / job variable.

### Response

In case of restore: The file / job variable can be restored
from this SVID only without directory.
In case of a save run: try to reorganize the directory
by means of DIRCONV and retry the save run.

## ARC0177

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0177 DIRECTORY FILE COULD NOT BE SAVED ON ONE VOLUME. FILE IS NOT SAVED

### Meaning

There is not enough space on one volume to save the directory
file. With DIRSAVE=YES it is not possible to use more than one
volume for saving the directory. The directory file is not saved.

### Response

Save the directory file with another ARCHIVE run.

## ARC0178

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0178 UNABLE TO FIND SAVE FILE ON VOLUME '(&00)' FOR SAVE VERSION '(&01)'

### Meaning

The save file containing the required files for a restore statement
or for a save statement with continue does not exist.
Processing of the statement continues with the next save version,
if there is any more to process.
A save statement with continue is aborted.

## ARC0179

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0179 CHECKPOINT OF STATEMENT NOT FOUND. STATEMENT ABORTED

### Meaning

During a restart of an ARCHIVE statement, the statement cannot be
found on the checkpoint file.
Processing of the current statement is aborted.

## ARC0180

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0180 NO FILES OR JOB VARIABLES FOUND TO PROCESS. STATEMENT ABORTED

### Meaning

In the statement, none of the FILES or JV specifications
has yielded any files or job variables to be processed.
Processing of the current statement is aborted.

## ARC0181

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0181 ERROR DURING PRINT FILE ACCESS. STATEMENT ABORTED

### Meaning

An error occurred during access of the print file
ARCHIVE.P.SVID. The ARCHIVE run is terminated.

### Response

Depends on error occurred. This error is indicated by another ARCHIVE
message which is given before.

## ARC0182

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0182 CURRENT DATE AND TIME LESS THAN THE TIMESTAMP OF THE LAST SAVE VERSION IN THE DIRECTORY OR LESS THAN THE LAST ASN IN CHECKPOINT FILE. STATEMENT ABORTED

### Meaning

There is already a save version in the directory or
an archive sequence number in the checkpoint file with a date or time
higher than the current date or time of the machine.
Probably the system was loaded with a wrong date or time.

### Response

SHUTDOWN and load system again with the correct date and time.
Repeat HSMS/ARCHIVE run.

## ARC0183

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0183 ANOTHER USER'S FILES OR JOB VARIABLES CAN ONLY BE SPEC. WITH THIS STATEMENT BY PRIV. USERS OR THEY MUST BE RENAMED INTO THE OWN USER ID

### Meaning

Another user's files or job variables can only be specified with this
statement by privileged users. Processing continues after this error by
analyzing the rest of the statement, but the statement will not be
executed. A RENAME into the own userid may be specified.

## ARC0184

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0184 SUBTASK TERMINATED ABNORMALLY

### Meaning

An ARCHIVE subtask has terminated without notifying the main
task. Processing of the current statement is aborted.
You can find the cause of the abnormal termination in the console
report. The cause may be:
- /CANCEL-JOB
- system error

## ARC0185

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0185 A RENAME AT EXPORT IS NOT ALLOWED WITH 'CATONLY=YES' OR 'FROM=PRTAPE'

### Meaning

It is not allowed to give a rename in FILES/JOBVAR at EXPORT with
CATONLY=YES or FROM=PRTAPE.

## ARC0186

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0186 'TARGET-ARCHIVE-VERSION=BEFORE-V26B' INCOMPATIBLE WITH OTHER OPERANDS

### Meaning

Operand TARGET-ARCHIVE-VERSION=BEFORE-V26B cannot be used
in case of compression or EXPORT to disk.

## ARC0187

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0187 ERASE ERROR '(&00)' ON FILE '(&01)'. STATEMENT ABORTED

### Meaning

In processing a DELETE statement to remove a statement from the
checkpoint file, an erase error has occurred.
Processing of the current statement is aborted.
(&00): error code from the ERASE macro.
(&01): file name
- ARCHIVE.P.YYMMDD.HHMMSS: the print file for the statement.
- ARCHIVE.SAVE.FILE(YYMMDD-HHMMSS-.): the save file for tape saves
- ARCHIVE.SAVE.FILE.YYMMDD.HHMMSS.VSN: the save file for disk
saves.

### Response

Erase file with /DELETE-FILE.

## ARC0188

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0188 ARCHIVE SEQUENCE NUMBER '(&00)' IS RUNNING. STATEMENT REJECTED

### Meaning

The statement with ARCHIVE sequence number (&00) is running at the
moment. A statement to PROCESS or DELETE it is rejected.

## ARC0189

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0189 USER DOES NOT HAVE THE PRIVILEGE TO ACCESS ARCHIVE SEQUENCE NUMBER '(&00)'

### Meaning

A PROCESS or DELETE statement has been given for ARCHIVE sequence
number (&00), which is for another user, and the current
user does not have the privilege to access this ARCHIVE sequence number.
The statement is aborted.

## ARC0190

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0190 ARCHIVE SEQUENCE NUMBER '(&00)' NOT FOUND. STATEMENT REJECTED

### Meaning

A PROCESS or DELETE statement has been given for ARCHIVE sequence
number (&00) which is not in the checkpoint or LATER file, as
appropriate.
The statement is aborted.

## ARC0191

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0191 ERROR IN 'NAME' OPERAND: 'RENAME' FILE NAME IS NOT COMPATIBLE WITH ORIGINAL FILE NAME. STATEMENT NOT EXECUTED

### Meaning

Either the original or the renamed file name ends with '.'. But the other
file name does not.
Processing continues after this error by analyzing the rest of the
statement, but the statement will not be executed.

## ARC0192

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0192 'FROM SV' NOT VALID FOR THIS STATEMENT. STATEMENT ABORTED

### Meaning

The SV alternative in the FROM operand is not allowed for
volume type disk. The statement is aborted.

## ARC0193

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0193 ERROR IN '(&00)' OPERAND: PUBLIC VOL SPECIFIED. STATEMENT ABORTED

### Meaning

Save/restore type commands using public disk VSNs in (&00) operand may
only be issued by privileged users. Specification of public disk VSNs in
ORIGIN operand however is inadmissible. The statement is aborted.

## ARC0194

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0194 ERROR IN '(&00)' OPERAND: INVALID DEVICE. STATEMENT ABORTED

### Meaning

The device specified in the (&00) operand is not alphanumeric.
The statement is aborted.

## ARC0195

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0195 ERROR IN '(&00)' OPERAND: DEVICE REQUIRED. STATEMENT ABORTED

### Meaning

DEVICE is not optional for the (&00) operand and must be
specified. The statement is aborted.

## ARC0196

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0196 ERROR IN '(&00)' OPERAND: VSN REQUIRED. STATEMENT ABORTED

### Meaning

VSNs are not optional with this statement and must be specified in
(&00) operand. The statement is aborted.

## ARC0197

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0197 SUBTASKS CANNOT BE CREATED. STATEMENT ABORTED

### Meaning

The subtasks required by ARCHIVE cannot be created.
Processing of the current statement is aborted.

## ARC0198

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0198 INDEX-DATA-SEPARATION NOT POSSIBLE. FILE NOT RESTORED

### Meaning

An ISAM file with separated volumes for index and data could not be
restored, because a suitable allocation on different disks was not
possible.

### Response

Restore the file with a statement, that allows right allocation for this
file.

## ARC0199

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0199 DISC DEALLOCATION ERROR: RETURN CODE '(&00)'. RUN CONTINUES

### Meaning

This is a diagnostic error message.
Disc deallocation will occur at subtask termination.

## ARC0200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0200 DMS ERROR '(&00)' ON DISK FILE. FILE NOT COPIED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The DMS error (&00) has occurred.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
The message is associated with the file in error on SUMMARY report
(HSMS) or parameter SNR=*NO (ARCHIVE). For another files this message
will be suppressed.
Processing continues.

## ARC0201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0201 DMS ERROR '(&00)' ON DISK FILE. IN SYSTEM-MODE: /HELP-MSG DMS(&00)

### Meaning

The DMS error (&00) has occurred while attempting to restore the
catalog entry of a file or a FGG index or a JV for with only the catalog
entry was saved.
The message is associated with the file in error on the ARCHIVE report.
Processing continues with the next file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
FGG: file generation group

## ARC0202

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0202 DMS ERROR '(&00)' ON DISK FILE. FILE NOT CORRECTLY COPIED. IN SYSTEM-MODE: /HELP-MSG DMS(&00)

### Meaning

The DMS error (&00) has occurred during I/O on a disk file, the file has
not been fully copied. The message is associated with the file in error on
the ARCHIVE report.
Processing continues with the next file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## ARC0203

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0203 DMS/JVS ERROR '(&00)' WHEN TRYING TO ERASE FILE OR JV. IN SYSTEM-MODE: /HELP-MSG DMS(&00) OR /HELP-MSG JVS(&00)

### Meaning

An error occurred when ARCHIVE tried to erase a file or a JV
(&00): DMS or JVS error code.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## ARC0204

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0204 GENERATION CANNOT BE RESTORED: GROUP INDEX DOES NOT EXIST OR IS INCORRECT

### Meaning

A generation cannot be restored, because the group index does not exist
or is incorrect.
The message is associated with the file in error on the ARCHIVE report.
Processing continues with the next file.

## ARC0205

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0205 FILE TO BE RESTORED FROM A PARTIAL SAVE DOES NOT EXIST ON DISK OR IS INCOMPATIBLE WITH TYPE OF SAVED FILE. FILE NOT RESTORED

### Meaning

File to be restored from a partial save does not exist on disk or is
incompatible with the type of the saved file. File not restored.
The message is associated with the file in error on the ARCHIVE report.
Processing continues with the next file.

## ARC0206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0206 DMS ERROR '(&00)' WHILE ACCESSING FGG INDEX. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

Following the RESTORE of a generation file a DMS error has been given
while attempting either to read, write or acquire private disk
for, its FGG Index. The FGG Index Access and/or EXPIRATION DATE and/or
WRITE PASSWORD may be incorrect.
The message is associated with the file in error on the ARCHIVE report.
Processing continues with the next file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
FGG: file generation group

## ARC0207

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0207 RECORD IN DIRECTORY FOR FILE '(&00)' OR SAVE VERSION '(&01)' DESTROYED

### Meaning

An error in the directory was found during restore or save from tape.
A record for a file or for a save version has wrong contents.

### Response

The save from tape or restore can probably be processed if the file
or save version can be excluded.
The directory file will be necessary for diagnosis.

## ARC0208

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0208 LOGICAL HALFPAGE NUMBER BEHIND BLOCK '(&00)' NOT IN ASCENDING ORDER. REST OF FILE NOT COPIED

### Meaning

The order of the PAM pages which belong to the file is not correct.
The block behind block (&00) has a wrong PAM page number.
Saving of this file is immediately stopped, when this error is recognized.
(&00): block number (hexadecimal)

### Response

This file is destroyed! It has to be analysed and repaired immediately.
In this SAVE run it was saved only incompletely.
When a RESTORE run without directory is done from
this save run, this file has to be excluded explicitly!

## ARC0209

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0209 JV ERROR (&00). JOB VARIABLE NOT RESTORED

### Meaning

The JVS or DMS error (&00) has occurred while attempting to restore
a job variable. The message is associated with the job variable in error
on the ARCHIVE report.
Processing continues.

## ARC0210

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0210 DMS ERROR '(&00)' ON INPUT VSN '(&01)'. VOLUME REJECTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The DMS error (&00) has occurred at the start of the input VSN (&01).
Processing continues with the next volume.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

For DMS error "0D77 or 0DD8" repeat run under user ID TSOS
with OPERATOR=YES operand.

## ARC0211

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0211 NO CONVERSION FOR THE FILE. FILE NOT RESTORED

### Meaning

The conversion necessary to restore a key file on non key disk is
rejected.
Possible reasons:
- conversion operand equals NO
- STANDARD conversion and restore from
a partial save (only possible in CONV format)
- the file already exists (no replace is made in case of conversion).
- the file is encrypted and cannot be converted by ARCHIVE.
File is not restored. Processing continues with next file.

## ARC0212

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0212 STANDARD CONVERSION (KEY TO NON KEY) NOT (ENTIRELY) POSSIBLE. FILE NOT (FULLY) RESTORED

### Meaning

The standard conversion is not (entirely) possible for this file. The file
is not (fully) copied.
Possible reasons are:
- RECORD-FORMAT = FIXED and RECORD-SIZE too long (file not restored),
- RECORD-FORMAT = VARIABLE and a too long record is encountered during
conversion (file partially restored).
The processing continues with next file.

### Response

The file can be converted in CONV format.

## ARC0213

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0213 DMS ERROR '(&00)' ON INPUT VSN '(&01)'. SUBSAVE TERMINATED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The DMS error (&00) has occurred while processing the input VSN (&01).
The subtask is unable to continue.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## ARC0214

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0214 CONNECTION ERROR WITH SUBSYSTEM PAMINT. FILE NOT (FULLY) RESTORED

### Meaning

An error occurred when ARCHIVE tried to connect to PAMINT: subsystem
is not created.
The file is not (fully) restored.

### Response

Ask the system administrator to make a START-SUBSYSTEM for PAMINT, and
reenter the ARCHIVE statement.

## ARC0215

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0215 RELATIVE FILE GENERATION NUMBER MUST NOT BE USED WITH THIS STATEMENT

### Meaning

A relative generation number for a file generation can be used only
with SAVE and EXPORT commands.
Processing continues after this error by analyzing the rest
of the statement, but the statement will not be executed.

## ARC0216

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0216 SAVE VERSION IDENTIFIER ON INPUT VSN '(&00)' DIFFERS FROM THAT SPECIFIED. VOLUME IS OMITTED

### Meaning

Either the user had specified a particular save version identifier and
this does not correspond with that in the save file header block of VSN
(&00), or the save version identifier of the first input volume was
different from that of VSN (&00).
Processing continues with the next volume.
This message can also occur when files are saved via HSMS and imported,
specifying an input volume, but without specifying a save-version-id.

## ARC0217

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0217 INPUT VSN '(&00)' DOES NOT BELONG TO THE SAME SUBSAVE VERSION AS THE FIRST INPUT VOLUME. VOLUME IS OMITTED

### Meaning

The user has not correctly grouped VSNs in the ARCHIVE statement according
to the subsave version to which each belongs, or a wrong volume has been
mounted on the drive.
Processing continues with the next volume.
(&00): VSN of volume in error.

## ARC0218

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0218 INPUT VSN '(&00)' IS OUT OF SEQUENCE AND IS REJECTED. PROCESSING CONTINUES WITH NEXT VOLUME

### Meaning

Input volumes have not been mounted in the order in which they were
written. VSN (&00) is out of sequence.
Processing continues with the next volume.

## ARC0219

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0219 DEVICE TYPE OF VOLUME TO BE CONTINUED IS NOT KNOWN

### Meaning

In the ARCHIVE statement the operand DEVICE is not specified.
The value of the DEVICE operand could not be evaluated for the statement
to be continued.

### Response

Specify device type (tape) or save version identifier (disk) in the
ARCHIVE statement and retry.

## ARC0220

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0220 DMS ERROR '(&00)' ON OUTPUT VSN '(&01)'. VOLUME CANNOT BE CONTINUED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

During a CONTINUE run, the DMS error (&00) occurs on volume with
VSN (&01). The saving cannot continue and the subsave terminates.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## ARC0221

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0221 DMS ERROR '(&00)' ON OUTPUT VSN '(&01)'. SUBTASK TERMINATED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

Error (&00) on output VSN (&01).
The subsave is terminated.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&00): DMS error code.
(&01): VSN of volume or ' ' if no volume was given by the operator.

## ARC0222

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0222 INTERNAL ERROR '(&00)' DURING ACCESS ON ARCHIVE-DIRECTORY FOR FILE '(&01)'

### Meaning

'(&00)': error code
0001: end of file
0002: end of record type
0003: begin of file
0004: record not found
0005: read error
0006: next error
0007: previous error
0008: write error
0009: eliminate error
0010: open error
0011: close error
0012: error in FAUTPF
0013: other error
0014: DMS open error
0017: lock/unlock error

## ARC0223

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0223 MAREN-ERROR '(&00)' WHEN REQUESTING A FREE TAPE. SUBSAVE TERMINATED. IN SYSTEM MODE /HELP-MSG MAR(&00)

### Meaning

(&00): message key of MAREN.

### Response

Enter /HELP-MSG-INFORMATION for MAREN message MAR(&00).

## ARC0224

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0224 NOT ENOUGH 'DISKS' OR 'VOLUMES' SPECIFIED. SUBSAVE TERMINATED

### Meaning

A SAVE or EXPORT run has terminated because another output disk
volume is needed and no more are given in the DISKS or VOLUME operand.

### Response

The intended saving of files may be completed by a subsequent SAVE
or EXPORT run. With this the remaining files and a sufficient number
of disks have to be specified.

## ARC0225

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0225 ERROR '(&00)' REPORTED BY SUBSYSTEM SRPMFACL. FILE NOT SAVED

### Meaning

Possible errors are:
2 internal error in SRPMFACL (SERSLOG entry created).
3 ACL not found.
5 no ACL entry.
FFFF Subsystem SRPMFACL not created or not available.
SRPMFACL and FACS is not supported with SECOS from Version V4.0.

### Response

Contact the system administrator or
perform save run with parameter SAVE-ACL=NO.

## ARC0226

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0226 PAM BLOCK NO. '(&00)' IN SAM/ISAM FILE HAS WRONG CFID. FILE NOT COMPLETELY SAVED

### Meaning

Block (&00) of the actual file has an incorrect CFID (coded file id).
Saving of the file is stopped.
Check of the CFID for blocks in ISAM files is performed only for those
ISAM files which must be without a hole.
(&00): block number (hexadecimal)

### Response

The affected file is destroyed and must be reconstructed.

## ARC0227

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0227 PASSWORD ROUTINE REJECTS FURTHER PASSWORD INTRODUCTION (RETURN CODE '(&00)'). STATEMENT REJECTED

### Meaning

Possible reasons:
- the maximum number of pages for password is reached (RC = 4);
- the maximum number of possible passwords for the task has been
reached (RC = 5);
- the maximum number of possible passwords for the password table
has been reached (RC = 6).

### Response

Analyse the return code (&00) of the passwords processor and take
the appropriated action.

## ARC0228

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0228 END OF FILE NOT FOUND: FILE NOT COMPLETELY COPIED

### Meaning

The file was either saved with errors or written on two or more tapes
which were not given in the RESTORE statement.

### Response

Check the save report whether the file was saved correctly or not. If the
file was saved correctly repeat the RESTORE with the complete tape list.

## ARC0229

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0229 '(&00)' CANNOT BE USED AS SUBSEQUENT DISK FOR CONTINUE SAVE FOR THIS SUBTASK (USER ERROR)

### Meaning

Reaction on user error.

### Response

Doing SAVE with CONTINUE, the VSNs of the preceding subsaves with the same
SVID must not be used as subsequent disks. That means: this disks must not
be specified in the DISK/VOLUME operand.

## ARC0230

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0230 FILE/JV SAVED MORE THAN ONCE UNDER THIS SVID. RESTORE VERSION IS UNPREDICTABLE

### Meaning

During a save type of run, the file/jobvariable concerned has
specified more than once in the FILES commands. It is
impossible to predict what version of this file will
be restored from that SVID.

## ARC0231

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0231 FILE NOT COMPLETELY COPIED DUE TO SKIPPED INPUT TAPE

### Meaning

The file was saved on two tapes. The second tape could not be read in
due to DMS error or because checks proved an inconsistency.

### Response

If the continuation tape could not be opened due to DMS error try to
restore the file again, use other devices. If the tape was rejected
because of an inconsistency, run the restore again with the correct tapes.

## ARC0232

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0232 INPUT VSN '(&00)' IS NOT AN ARCHIVE TAPE BUT A HSMS BACKUP SERVER TAPE.

### Meaning

The input tape VSN (&00) was not written by ARCHIVE but by HSMS.
Tape is rejected. Please use HSMS product.

## ARC0233

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0233 DMS ERROR '(&00)' ON OUTPUT DISK. SUBSAVE TERMINATED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For RESTORE to disk volumes with VSNs given in TO operand: when DMS
error (&00) during restore of a file, the RESTORE run is terminated,
because same DMS error is expected to occur for any further file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

- DMS error "D541 or D54A" shows that there is no or insufficient space
available. Erase files you need no more from volumes and restore further
files, or restore further files to other volumes.
- DMS error "D53A" shows erase or change error for F1-label on private
volume. See message D53A.

## ARC0234

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0234 INTERNAL ERROR IN SUBSYSTEM 'PAMINT'. FILE NOT (FULLY) RESTORED

### Meaning

An internal error occurred in PAMINT during KEY-to-NONKEY conversion of
the file. The file is not (fully) restored.

## ARC0235

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0235 INVALID PARAMETER IN /ENTER-JOB COMMAND

### Meaning

/ENTER-JOB command cannot be done due to an invalid parameter,
(by example a wrong password).

## ARC0236

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0236 REQM ERROR DURING SCAN OF JOB VARIABLES FOR '(&00)'. JOB VARIABLES NOT COMPLETELY SAVED

### Meaning

Request for class 5 memory failed during scan of catalog partition (&00)
for job variables. Only this part of the job variables is saved, which was
already read in when the error occurred.

## ARC0237

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0237 CATALOG ACCESS ERROR '(&00)' FOR USER ID '(&01)'. STATEMENT ABORTED

### Meaning

An error occurred during reading of the system catalog.
The save run is terminated
(&00): error code and secondary return code (if present)
(&01): affected user ID and cat ID (if present).

## ARC0238

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0238 DMS ERROR '(&00)' DURING POSITIONING FOR CONTINUE SAVE. SUBSAVE TERMINATED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

When positioning after the already saved data on tape or on disk save file
the DMS error with error code (&00) occurred.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Try save run again.

## ARC0239

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0239 INPUT TAPES IN WRONG SEQUENCE. FILE NOT COMPLETELY COPIED

### Meaning

During reading in of a file that was saved over several tapes, it has
been discovered, that a wrong continuation tape was given.
The affected file will not be completely copied.

### Response

Give ARCHIVE statements again with all tapes in correct order.

## ARC0240

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0240 READ ERROR DURING RESTORE/COPY OF FILE. DUMMY BLOCK WRITTEN

### Meaning

While reading the saved file an I/O error happened.
A dummy block was written instead of the not readable ARCHIVE block.
If the ARCHIVE block contained more than one PAM page of data, the blocks
behind the dummy block will have another CFID than the file itself in the
restored file.

### Response

Repair the file or erase it and restore it from another save version.

## ARC0241

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0241 READ ERROR DURING RESTORE OR COPY OF FILE. FILE NOT COMPLETELY WRITTEN

### Meaning

This message is output in the ARCHIVE report beneath the affected file.
During reading of this file a read error occured. The file is only written
up to the last block which could be read.

### Response

- For RESTORE run: Restore the file with REPLACE=ALL from another save
version.
- For save from tape run: It will not be possible, to restore this file
from this copy of the original save version.

## ARC0242

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0242 RESTORE OR COPY OF FILE STOPPED DUE TO MORE THAN '(&00)' ERRORS IN INPUT VSN

### Meaning

Processing of the tape, on which the affected file was saved, is
terminated, because more than the permitted maximum number of read errors
occurred. The file is not completely restored or copied.
The message is associated with the file in error on the ARCHIVE report.
(&00): number of errors (hexadecimal)

### Response

- For RESTORE runs: Restore the file with REPLACE=ALL from another save
version.
- For save from tape runs: It will not be possible to restore the file
from this copy!

## ARC0243

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0243 FORMAT ERROR DURING RESTORE/COPY OF FILE. DUMMY BLOCK WRITTEN

### Meaning

During check of the ARCHIVE blocks which were read a format error was
detected.
A dummy PAM block was written in the file instead of the inconsistent
ARCHIVE block. If the ARCHIVE block contains more than one PAM PAGE of
data, the following PAM blocks of the file may have another CODED FILE ID
than the rest of the reconstructed file.

### Response

Repair file (i.e. add the missing PAM blocks with DPAGE) or erase the file
and reconstruct it from another save version id. If the file remains not
repaired, it might be impossible to save it again with ARCHIVE.

## ARC0244

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0244 FORMAT ERROR OR WRONG BLOCK NUMBER FOUND DURING RESTORE OR COPY OF FILE. FILE NOT COMPLETELY WRITTEN

### Meaning

This message is output in the ARCHIVE report beneath the line for the
affected file. When reading a tape during a RESTORE respectively
a save from tape run a format error was detected on a tape block.
Writting of the affected file is stopped.

### Response

- RESTORE run: restore the file from another save version or repeat run
with PARAM OPERATOR=YES.
- save from tape run: this file cannot be restored from this save
version! Copy this file from another save version or first restore the
file on disk (look also for message ARC0292).

## ARC0245

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0245 ERROR DURING POSITIONING OF TAPE AFTER READ ERROR. FILE NOT COMPLETELY WRITTEN

### Meaning

This message is output in the ARCHIVE report beneath the line for the
affected file. Processing of the file and the tape is stopped, because
it was not possible, to bring the tape into correct position again after
a read error occurred.

### Response

Retry the run on another device. If the same error happens again, read
file from another save version.

## ARC0246

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0246 ERROR DURING READ OF FULL RESTORE CHECKPOINT RECORD. PARTIAL SAVE NOT RESTORED

### Meaning

The information whether the according full save could be restored
successfully could not be read. The partial save is not restored for this
reason.

### Response

Restore the partial save in an extra run.

## ARC0247

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0247 FULL RESTORE CHECKPOINT RECORD NOT FOUND. PARTIAL SAVE NOT RESTORED

### Meaning

There is no record in the checkpoint file that indicates, that the restore
of the full save of this file was completed successfully. The partial save
is not restored for this reason.

### Response

Restore the affected file in an extra run.

## ARC0248

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0248 UNEXPECTED ARCHIVE DATA BLOCK NUMBER FOUND INSTEAD OF '(&00)'. FILE NOT COMPLETELY COPIED

### Meaning

During reading of the affected file a block with wrong ARCHIVE data block
number was found. The expected number was (&00). The file was not
read in completely.
(&00): block number (hexadecimal)

### Response

See message ARC0777.

## ARC0249

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0249 INPUT VSN '(&00)' IS NOT AN ARCHIVE TAPE. TAPE REJECTED

### Meaning

The input tape VSN (&00) was not written by ARCHIVE. Tape rejected.

## ARC0250

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0250 SYSTEM ERROR CAUSED ABNORMAL TERMINATION OF SUBTASK TSN# (&00)

### Meaning

After a system error, the specified subtask is pended indefinitely.
The subsave was not terminated.

## ARC0251

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0251 RELEASE FOR CLASS 5 MEMORY POOL ERROR '(&00)'

### Meaning

(&00): secondary indicator and return code of RELMP macro.

## ARC0252

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0252 CATALOG IDENTIFIER MUST NOT BE SPECIFIED IN THE 'CATID=NO' MODE

### Meaning

In the CATID=NO mode the specification of a catalog identifier is
forbidden:
1. In any file name of a NAME, EXCEPT, THRU, RENAME operand of a SAVE,
EXPORT, RESTORE, IMPORT or LIST statement;
2. In the name of the directory in runs with DIRSAVE=YES.
Exceptions: A specification of a catalog identifier is always allowed at
the RENAME operand in RESTORE, IMPORT or LIST runs. The (redundant)
specification of the default catalog identifier for the directory file is
always allowed too.

### Response

Try again without catalog identifier qualification or switch to CATID=YES
mode and try again.

## ARC0253

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0253 TAPE DEVICE ALLOCATION FOR DEVICE TYPE '(&01)' AND LOCATION '(&02)' FAILED WITH ERROR '(&00)'.

### Meaning

During a reservation at the beginning of a run there may exist following
causes:
- The device typ or the location have been specified invalid.
- The operator has not attached any tape device for the required type.
- All tape devices at the specified location are occupied.
At the end of a run the error may occure during the re-establish of a
suspended device reservation. In this case a subtask has not regularily
released the device access.
'(&00)': error code
1: device temporarily not available
2: device permanent not available
3: allocation not allowed
4: device not defined
5: others
'(&01)': device type
'(&02)': location

## ARC0254

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0254 VALUE OF 'PARAM CATID' DIFFERS FROM MODE ON VSN '(&00)'. VOLUME IS NOT PROCESSED

### Meaning

The value of PARAM CATID in the actual run differs from the CATID mode
of the run in which VSN (&00) was written.

### Response

Set correct value for PARAM CATID and retry statement.

## ARC0255

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0255 RANGE OF FILES SPECIFIED WITH 'THRU' OPERAND EXCEEDS ONE PVS

### Meaning

Range of files specified with THRU operand exceeds one PVS. Remark the
default regulation for missing catalog identifier.

## ARC0256

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0256 IMPOSSIBLE TO SEARCH THE SPECIFIED DIRECTORY FOR CAT IDS

### Meaning

Cat IDs can only be specified in the FILES or JOBVAR operands of an
INQUIRE statement, if the specified directory belongs to SAVE runs with
PARAM CATID=YES.

## ARC0257

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0257 WRONG LAST BLOCK ON VOLUME '(&00)'. VOLUME CANNOT BE CONTINUED

### Meaning

The consistency check of the last block of the ARCHIVE save file
on volume (&00) detected an error. This makes CONTINUE impossible.
The cause for this error can be for instance a damage on the
save file itself or a hardware error during positioning in case
of a tape volume.

### Response

Check the rejected volume with a LIST run. Check tape devices.

## ARC0258

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0258 CATALOG ACCESS ERROR '(&00)' FOR FILE (&01). USERID NOT COMPLETELY SAVED

### Meaning

An error occurred during access of the system catalog.
The run continues but the affected userid is not completely saved.
(&00): error code.
(&01): file name.

## ARC0259

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0259 CONTINUE TAPE '(&00)' IS UNUSABLE. SVID CANNOT BE CONTINUED

### Meaning

The tape with VSN (&00) that should be continued is marked as unusable in
the directory. That means that an I/O error occurred during writing on
this tape in the preceding save run. Continue for this SVID is not
allowed.

### Response

Save files/job variables into a new save version instead of the continue.

## ARC0260

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0260 EXPECTED EOF LABELS NOT FOUND BEHIND BLOCK '(&00)' ON VSN '(&01)'. VOLUME ABANDONED

### Meaning

The end of an ARCHIVE tape file consists of a TAPE MARK, three EOF LABELS
and a TRAILER LABEL. In this case ARCHIVE found a TAPE MARK
but not the EOF labels. Reasons for this situation are: TAPE MARK was
detected because of a device error or the tape was not correctly closed.
See also ARC0280, ARC0281, ARC0283 and ARC0284.
(&00): block number (hexadecimal)

### Response

Try another run on another device and check the ARCHIVE SAVE REPORT for a
CLOSE error.

## ARC0261

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0261 DIRECTORY FILE MUST NOT BE A FILE GENERATION. STATEMENT REJECTED

## ARC0262

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0262 MISSING CATALOG ENTRY EXTENSION. FILE NOT PROCESSED

### Meaning

As the CATALOG ENTRY EXTENSION is missing, the file is defect.
Therefore the file is not processed.

## ARC0263

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0263 SAVE VERSION CREATED WITH 'PARAM CATID=NO' CANNOT BE CONTINUED WITH 'PARAM CATID=YES'

### Meaning

The save version that has to be continued was created with PARAM CATID=NO
(the directory file was later converted into CATID=YES format).
Therefore the save version must not be continued with PARAM CATID=YES.

### Response

Start new save version instead of CONTINUE or convert affected tape(s)/
disk file(s) into CATID=YES format by copy save version and continue
converted save version.

## ARC0264

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0264 TASK MANAGEMENT REPORTS A TASK CREATION ERROR '(&00)'

### Meaning

During creation of a subtask the error (&00) occurs.
The subtask could not be created.

## ARC0265

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0265 FILE NAME TOO LONG OR INVALID. FILE NOT PROCESSED

### Meaning

Possible reasons:
- the name of the file to be saved/restored is longer than 41
characters.
- the name of the file generation group to be saved is longer than
34 characters.
- there is not enough space in the catalog entry to rename the file.

### Response

Use RENAME operand to give a correct file name.

## ARC0266

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0266 A 'FILES' CANNOT HAVE AN 'ORIGIN' OPERAND WITH THIS STATEMENT

### Meaning

A FILES cannot have an ORIGIN operand with this statement.
Processing continues after this error by analyzing the rest
of the statement, but the statement will not be executed.

## ARC0267

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0267 DEVICE TYPE 'WORK' MUST NOT BE USED WITH DIRECTORY

## ARC0268

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0268 INVALID OPTION FOR ENCRYPTED FILE. FILE NOT PROCESSED

### Meaning

The file is encrypted.
An invalid option for encrypted files has been requested:
HSMS-Run : EXPORTED-ENVIRONMENT is not *KEEP
ARCHIVE-RUN: T-A-V=BEFORE-V26B or LOCATION=RESET or ATTRIBUTES=RESET
The file will be not saved. The statement will be continued.

## ARC0269

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0269 MAREN-ERROR '(&01)' WITH VSN '(&00)'. VOLUME REJECTED. IN SYSTEM MODE /HELP-MSG MAR(&01)

### Meaning

The VSN (&00) was rejected by the subsystem MAREN with error code (&01)
Processing of the current statement is continued.

### Response

Enter /HELP-MSG-INFORMATION for MAREN message MAR(&01).

## ARC0270

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0270 ON VOLUME '(&00)' EXISTS A SAVE FILE WITH SAME SVID, THAT IS NOT WRITTEN FROM THIS ARCHIVE RUN

### Meaning

During restart processing on volume (&00) an ARCHIVE save file is found,
that cannot be overwritten. This file is written from an ARCHIVE run
on another CPU and this run possibly was not the original run of
the restarted ARCHIVE run.
Processing of the current statement is aborted.

### Response

If the restart is started from another CPU as the original run,
start the restart from the same CPU. If this is not possible
or restart was performed on the same CPU as the original run,
start the original run again.

## ARC0271

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0271 RECORDS WITH SAME KEY FOUND: '(&00)'. STATEMENT ABORTED

### Meaning

Though the directory file must not have double keys two records with the
same key were detected. The directory is in no consistent state.
(&00): printable part of the double record key.

### Response

Inform diagnosis.

## ARC0272

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0272 FILE '(&00)' NOT COMPLETELY PROCESSED

### Meaning

The processing of the file (&00) is cancelled (especially by /CANCEL-JOB
statement). Therefore the output file is incomplete.

## ARC0273

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0273 ERROR '(&00)' IN SHOW-FILE-ATTRIBUTES ON FGG INDEX

### Meaning

During replacing a relative generation number an SHOW-FILE-ATTRIBUTES
error (&00) occurred on the FGG index of the generation group.
Processing continues after this error by analyzing the rest of
the statement, but the statement will not be executed.
FGG: file generation group

## ARC0274

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0274 INVALID BACKUP LEVEL IN CATALOG. FILE NOT PROCESSED

### Meaning

The consistency check of the file's BACKUP level in the catalog
has detected an invalid value. The file was not saved.

### Response

Change BACKUP-level.

## ARC0275

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0275 PLAM ERROR '(&00)' AT PARTIAL SAVE/RESTORE OF A PLAM LIBRARY WITH 'BLOCK-CONTROL=NO'

### Meaning

The PLAM error (&00) occurred during handling of a PLAM library with
BLOCK-CONTROL=NO.
Possible reasons:
- either at partial SAVE. In this case, the library is not saved.
- or at RESTORE from partial SAVE. In this case, the restored library can
contain informations about elements deleted with DESTROY=YES between the
full SAVE and the partial SAVE.
If the library is security relevant, erase it.

## ARC0276

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0276 JOB VARIABLE '(&00)' NOT COMPLETELY PROCESSED

### Meaning

The processing of the job variable (&00) is cancelled (especially
by cancel statement).

## ARC0277

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0277 'CATID' TYPE OF DIRECTORY DIFFERS FROM MODE OF ACTUAL RUN. STATEMENT REJECTED

### Meaning

The value for PARAM CATID in the current run differs from that of the
other SAVE runs that were done with the specified directory file.

### Response

Set correct value for PARAM CATID and retry statement.

## ARC0278

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0278 ERROR CONCERNING VOLUME TYPE. FILE NOT PROCESSED

### Meaning

Possible reasons:
- NDM error (system dump produced by ARCHIVE),
- volume type unknown to the system.

### Response

If this is no NDM error:
- check catalog entry.

## ARC0279

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0279 ERROR CONCERNING VOLUME-TYPE OF FILE '(&00)'. STATEMENT ABORTED

### Meaning

Possible reasons:
- NDM error (system dump produced by ARCHIVE),
- volume type unknown to the system,
- file (&00) already existing with unfit volume type.

### Response

If this is no NDM error:
- check catalog entry,
- rename or erase file and try again.

## ARC0280

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0280 ERROR '(&00)' DURING EOF LABEL CHECK ON VSN '(&01)'. VOLUME ABANDONED

### Meaning

ARCHIVE got an internal oder DMS error behind the TAPE MARK during EOF
label check. The TAPE MARK could be detected because of a device error.
See also Messages ARC0260, ARC0281, ARC0283 and ARC0284.

### Response

Repeat the ARCHIVE run on another device.

## ARC0281

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0281 TRAILER LABEL NOT FOUND ON TAPE '(&00)'. SVID CANNOT BE CONTINUED

### Meaning

ARCHIVE expects a trailer label behind the EOF labels.
The trailer label is used to check whether the svid can be continued or
not.
In this case the trailer label is missing. The reason could be a device or
close error. See also ARC0260, ARC0280, ARC0283 and ARC0284.

### Response

Repeat the run on another device.

## ARC0282

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0282 CONTINUE TAPE '(&00)' HAD AN ERROR DURING LAST SAVE RUN. SVID CANNOT BE CONTINUED

### Meaning

The continue tape had an error during last save run. The SVID cannot be
continued.

## ARC0283

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0283 END OF SAVE NOT FOUND ON TAPE '(&00)'. SVID CANNOT BE CONTINUED

### Meaning

End of save not found. The reasons could be an error during last save run
or a device error. See also ARC0260, ARC0280, ARC0281 and ARC0284.

### Response

Check the ARCHIVE save report and repeat the run on another device.

## ARC0284

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0284 ERROR '(&00)' DURING TRAILER LABEL CHECK ON VSN '(&01)'. VOLUME ABANDONED

### Meaning

ARCHIVE got an internal or DMS error behind the TAPE MARK during TRAILER
label check. See also Messages ARC0260, ARC0280, ARC0281 and ARC0283.

### Response

Repeat the run on another device.

## ARC0285

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0285 VOLUME '(&00)' IS NOT LAST VOLUME OF A COMPLETE SAVE RUN. SUBSAVE TERMINATED

### Meaning

The continue volume is full and the last data block on volume is not the
last block of a file ARCHIVE saved. This message will be given if the
volume to be continued is not the last volume or the last volume of an
aborted run.

### Response

Repeat the run with the last volume of this SVID if you have not done
before.

## ARC0286

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0286 TRAILER BLOCK ON TAPE '(&00)' INDICATES AN UNKNOWN TAPE STATE. SUBSAVE TERMINATED

### Meaning

The TRAILER label indicates an unknown tape state. Reasons could be an
error during last save run or a read error.

### Response

Check the ARCHIVE report and repeat the run on another device.

## ARC0287

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0287 ERROR DURING READ OF INDEX RESTORE CHECKPOINT RECORD. INDEX NOT RESTORED

### Meaning

The information whether the index could be restored from the according
previous SVID could not be read. Therefore as REPLACE=NO is specified
the index is not restored.

### Response

Restore index and generations in another run.

## ARC0288

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0288 INDEX RESTORE CHECKPOINT RECORD NOT FOUND. INDEX NOT RESTORED

### Meaning

There is no record in the checkpoint file that indicates, that the index
can replace the existing one although REPLACE=NO is specified. The index
is not restored for this reason.

### Response

Restore the affected group in another run.

## ARC0289

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0289 WRONG BLOCK NUMBER FOUND INSTEAD OF '(&00)' ON INPUT VSN '(&01)'. OPERATOR HAS TO ANSWER IF PROCESSING OF VOLUME SHALL BE CONTINUED

### Meaning

The position of input VSN (&01) got lost. A block with ARCHIVE data block
number (&00) was expected but the block just read in has another number.
(&00): block number (hexadecimal)

### Response

If any device errors have occurred before this message try to read in
the tape from another device. If no device errors have occurred, print
the blocks around the specified block and check,
whether all blocks were saved correctly on this tape.
The operator now gets the message ARC0906.
Answer .0: the volume can be aborted.
Answer .1: the processing of the volume is continued.
If the processing of the volume is continued, and the readed block and
the preceeding one belongs to a file just in process, the operator will
get the message ARC0902.
Answer .0: skip file.
Answer .1: continue processing of file.
If the processing of the file is continued, in this file maybe blocks
are missing. To get the logical block numbers of the surroundings
of the error print the surroundings of the ARCHIVE block on tape.

## ARC0290

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0290 WRONG BLOCK NUMBER FOUND INSTEAD OF '(&00)' ON INPUT VSN '(&01)'. START OF FILE '(&02)' NOT FOUND. FILE NOT PROCESSED

### Meaning

In spite of detection of an unexpected ARCHIVE data block number
the processing of the input tape was continued. The next block read
belongs to another file, but beginning of file could not be found.
This file is not processed.
(&00): block number (hexadecimal)

## ARC0291

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

ARC0291 NOT ENOUGH SPACE AVAILABLE FOR '(&00)' MEMORY REQUEST. NO MEMORY ALLOCATED

### Meaning

Insufficient (&00) memory to satisfy the request. No memory
is allocated. Space limit exceeded.

### Response

Contact the system service.
Increase MEMORY-POOL-SIZE in ARCHIVE parameter file SYSPAR.ARCHIVE.xxx

## ARC0292

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0292 PROCESSING OF FILE CONTINUED IN SPITE OF WRONG BLOCK NUMBER. POSSIBLY BLOCKS ARE MISSING

### Meaning

In spite of getting an ARCHIVE block with wrong block number the
processing of the file was continued. Possibly some blocks are missing in
the file.

### Response

Print the tape blocks in the surrounding and repair file (especially with
DPAGE) or read the file from another save version.
Look also for message ARC0289 and ARC0778.

## ARC0293

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0293 INSUFFICIENT SPACE FOR MEMORY POOL

### Meaning

There is not sufficient contiguous space for allocation
inside the MEMORY POOL or class 6 memory. Perhaps, there
are too many files declared.

### Response

Try again with reduced number of files.

## ARC0294

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0294 SUBSYSTEM ARCHIVE NOT ENABLED BY DSSM

### Meaning

DSSM was not able to load or connect the TPR-Part of ARCHIVE.
Possible reasons:
- SYSLNK.ARCHIVE.version not existing or not usable,
- user has disabled subsystem ARCHIVE by command
/RELEASE-SUBSYSTEM-SPACE,
- other DSSM errors.

### Response

Contact the system administrator.

## ARC0295

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0295 FILE IS ALREADY SAVED UNDER THIS SVID. CNS DIRECTORY UPDATE REJECTED

### Meaning

During a save type of run, the file concerned has been specified more than
once in the FILES commands. The file was already saved under this SVID.
The directory update with CNS is rejected, even if this time an error
occured.

## ARC0296

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0296 SAVE FILE ON SUPPORT '(&00)' IS NOT READABLE BY THIS ARCHIVE VERSION

### Meaning

The save file on support (&00) is not readable by this ARCHIVE version.
Processing continues with the next volume.

## ARC0297

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0297 PARTIAL SAVE OF LIBRARY '(&00)' IS REPLACED BY A FULL SAVE

### Meaning

The BITMAP space required for partial SAVE of the PLAM library
(&00) could not be allocated.
The library is fully saved.

## ARC0298

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0298 TWO 'EXCEPT' OPERANDS MUST BE SEPARATED BY AT LEAST A 'NAME' OPERAND

### Response

Separate the operands EXCEPT by a NAME. This NAME operand may be
empty: F EXCEPT=...,NA=,EXCEPT=...

## ARC0299

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0299 'MODIFY-ARCHIVE' REQUESTED FOR A NON EXISTING 'SVID-EXTENSION-RECORD'

### Meaning

There is no SVID extension record corresponding to the SVID
specified in the MODIFY-ARCHIVE statement.

## ARC0300

Destination: CONSOLE Routing code: U Weight: 70

Warranty : NO

ARC0300 ARCHIVE INTERNAL ERROR IN '(&00)'

### Meaning

An internal ARCHIVE error or a system error has occured which should be
investigated by the support group for the product.
With this message the operator is offered as system dump.
Any error between ARC0301 and ARC0399 will also generate this message.
(&00): module name and location where the error was detected.

### Response

Send system dump, console report and ARCHIVE report to diagnosis team.

## ARC0301

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0301 ARCHIVE INTERNAL ERROR DURING UFS ACCESS. STATEMENT ABORTED

## ARC0305

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0305 USER TABLE ACCESS ERROR. STATEMENT ABORTED

### Meaning

USER TABLE access error.
ARC0300 is sent to the operator's console to inform him of an error.
The statement is aborted.

## ARC0306

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0306 MRS CATALOG ACCESS ERROR '(&00)' FOR PUBSET '(&01)'. STATEMENT ABORTED

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR) is sent to the
console with a (&00)-code for the location, where the error occurred
in the program.

### Response

Eventually take system dump.

## ARC0307

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0307 MRS CATALOG ACCESS ERROR '(&00)'. STATEMENT ABORTED

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR) is sent to the
console with a (&00)-code for the location, where the error occurred
in the program.

### Response

Eventually take system dump.

## ARC0308

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0308 MAINTASK COULD NOT ENABLE MEMORY POOL. STATEMENT ABORTED

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR)
is sent to the console with a (&00)-code for the
location, where the error occurred in the program.

### Response

Eventually take system dump.

## ARC0309

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0309 TSN '(&00)' UNABLE TO CONNECT TO MEMORY POOL. STATEMENT ABORTED

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR)
is sent to the console with a (&00)-code for the
location, where the error occurred in the program.

### Response

Eventually take system dump.

## ARC0310

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0310 ERROR DURING ACCESS TO ENTER FILE. STATEMENT ABORTED

### Meaning

The PROCESS statement starts jobs by ENTER files.
An ENTER file could not be processed due to an error.
The statement is aborted
ARC0300 is sent to the operator's console to inform him of the error.

## ARC0311

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0311 MEMORY POOL REQUEST ERROR. RETURN CODE '(&00)'. STATEMENT ABORTED

### Meaning

A request for memory pool store failed.
(&00): secondary indicator and return code of REQM call.
Additionally message ARC0300 is sent to console
and a system dump is offered.

### Response

Send system dump, console report and ARCHIVE report to diagnosis team.

## ARC0312

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0312 CATALOG ACCESS ERROR '(&00)' FOR '(&01)'. STATEMENT ABORTED

### Meaning

An error occurred during reading of the system catalog. Message ARC0300 is
sent to the operator and a system dump is offered. The save run is
terminated.
If this error occurs inside the error recovery routine for Cl 5 memory
overflow (see MSG ARC0048) the save run is not terminated but continued
with the next user ID.
(&00): error code and secondary indicator (if present).
(&01): user ID and cat ID (if present) of the affected catalog partition.

### Response

Take system dump and inform diagnosis.

## ARC0315

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0315 MEMORY POOL NOT DESTROYED OR NOT ENABLED

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR)
is sent to the console with a (&00)-code for the
location, where the error occurred in the program.

### Response

Eventually take system dump.

## ARC0320

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0320 ARCHIVE INTERNAL ERROR. STATEMENT ABORTED

### Meaning

An error has occurred within ARCHIVE which should be investigated
by the support group for the product.
The user should not re-attempt the statement until the reason for the
error has been ascertained.
Message ARC0300 is sent to the operator's console to inform him of an
error.

### Response

System dump, console report, statement and SYSOUT must sent to the
diagnose center.

## ARC0332

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0332 TAPE ALLOCATION ERROR: RETURN CODE '(&00)'. SECONDARY RETURN CODE '(&01)'. RUN CONTINUES

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR) is sent to the
console.

### Response

Eventually take system dump.

## ARC0333

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0333 TAPE DEALLOCATION ERROR: RETURN CODE '(&00)'. SECONDARY RETURN CODE '(&01)'. RUN CONTINUES

### Meaning

Additionally the message ARC0300 (ARCHIVE INTERNAL ERROR) is sent to the
console.

### Response

Eventually take system dump.

## ARC0400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0400 RUN IS ABORTED. SOME FILES ARE PROBABLY NOT PROCESSED

### Meaning

The processing of some files is aborted.
Therefore the output file is incomplete.

## ARC0401

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0401 ERROR '(&00)' ON GUARDS FILE. PROCESSING CONTINUES

### Meaning

GUARDS was called to lock or unlock a GUARDS file.
The processing continues with the next file.

### Response

/HELP-MSG-INFORMATION PRO(&00) gives the meaning of the GUARDS message.

## ARC0402

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0402 RESTORE TO NK4 DISK NOT POSSIBLE. FILE NOT PROCESSED

### Meaning

NK4 native disks do not support the format of the file to be restored.
NK4 disks support only:
1. NK-ISAM files with BLOCK-CONTROL=*DATA4K, and
2. NK-PAM/SAM files with BLOCK-CONTROL=*NO/*DATA
and BLOCK-SIZE=(*STD,even value).
ARCHIVE is not able to restore other NK files to a NK4 disk.
K-files: the standard conversion K-to-NK is possible only for PAM/SAM
files with BLOCK-SIZE=(*STD,even value).
Other K-files can be restored only with conversion in CONV format.
In this case, they are converted in NK-files with
BLOCK-CONTROL=*NO and BLOCK-SIZE=(*STD,2).
Processing continues with next file.

### Response

1) Before ARCHIVE save, convert the file with PAMCONV into a format
supported by NK4-disk and save the converted file.
2) Make the restore to a NK2-disk and convert the restored file with
PAMCONV to NK4-disk.

## ARC0403

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0403 PLAM ERROR '(&00)' DURING K-TO-NK CONVERSION. FILE NOT ENTIRELY CONVERTED

### Meaning

The PLAM error (&00) has occurred during K-TO-NK conversion by PAMINT.
The file was not entirely converted/restored.
Processing continues with the next file.

## ARC0404

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0404 TO COPY A 'CATONLY=YES' SAVE IS ONLY ALLOWED WITH 'CATONLY=YES' IN CURRENT STATEMENT

### Meaning

It was tried, to copy a save tape which was produced
with CATONLY=YES without declaration of CATONLY=YES
in the current statement.

### Response

Repeat the run with CATONLY=YES.

## ARC0405

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0405 CONTINUATION MARK IN COLUMN 72 IS NOT BLANK OR '-'. STATEMENT ABORTED

### Meaning

Reading an ARCHIVE statement out a file, another character than blank
or '-' was found in column 72. The analyse of the rest of the statement
continues but the statement will not be executed.

## ARC0406

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0406 CMS ERROR '(&00)' ON PVS '(&01)'

### Meaning

The CMS error (&00) occurred during the MRSCAT entry access for PVS (&01).

## ARC0407

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0407 'BLOCK-SIZE' VALUE TOO HIGH. MAXIMUM VALUE '(&00)'

### Meaning

The BLOCK-SIZE value cannot be used to process the run on the
specified VSN/PVS.

### Response

Reduce the BLOCK-SIZE value.

## ARC0408

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0408 SECURE ERROR '(&00)' DURING SECURE OF OUTPUT VOLUME '(&01)'. IN SYSTEM MODE: HELP-MSG NKS(&00)

### Meaning

ARCHIVE did a SECURE-RESOURCE-ALLOCATION TAPE=(VOLUME=(&01)).
This secure was not successful.
Possible reasons:
- the volume is not defined in MAREN catalog.
- no device is defined or available for requested volume type.
- the volume is already used by another task.

### Response

Check the volume status in MAREN or its usage by a SHOW-TAPE-STATUS.

## ARC0409

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0409 MIGRATED FILE NOT PROCESSED

## ARC0410

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0410 READ ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. AFFECTED FILE COULD NOT BE IDENTIFIED AND CANNOT BE RESTORED OR COPIED

### Meaning

Block (&00) of VSN (&01) could not be read due to read error.
This block contains the very first block of a saved file.
This file is not restored or copied.
(&00): block number (hexadecimal)

### Response

Find out which file is missing with help of the
ARCHIVE save report of the proper save run.
Restore the file from another save version
(for save from tape append the file with CONTINUE).

## ARC0411

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0411 READ ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. PROCESSED FILE IS '(&02)'. DUMMY BLOCK WRITTEN

### Meaning

ARCHIVE block number (&00) on VSN (&01) could not be read. The name of the
affected file is (&02). A dummy PAM page was written instead of the not
readable ARCHIVE block. The following PAM pages of the reconstructed file
may have a different CFID than the rest of the file, They don't belong to
the file and there content is undefined.
(&00): block number (hexadecimal)

### Response

Erase file, mount volume into another device and try to read in the file
separately. If this does not work, either read in file from another save
version or repair it with help of a program like DPAGE.

## ARC0412

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0412 READ ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. PROCESSED FILE IS '(&02)'. FILE IS NOT PROCESSED FURTHER

### Meaning

During restore or copy of file (&02) a read error happens.
Location of the read error: Block (&00) of VSN (&01).
(&00): block number (hexadecimal)

### Response

Restore the file from another save version with REPLACE=ALL.
For a save from tape runs: It is not possible, to restore this file from
this copy!

## ARC0413

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0413 FORMAT ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. AFFECTED FILE COULD NOT BE IDENTIFIED AND CANNOT BE RESTORED

### Meaning

A format error was detected on block (&00) of VSN (&01).
The affected block contains the beginning of a new file.
This file cannot be identified and restored.
(&00): block number (hexadecimal)

### Response

Check ARCHIVE report against statement or against appertaining
save report to see, which file is missing (if any). Restore
this file from another save version.

## ARC0414

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0414 FORMAT ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. PROCESSED FILE IS '(&02)'. DUMMY BLOCK WRITTEN

### Meaning

When checking the format of ARCHIVE block number (&00) on input VSN (&01)
an inconsistency was detected. The name of the affected file is (&02).
The restored file will have at least one dummy PAM page.
(&00): block number (hexadecimal)

### Response

See message ARC0243. Additionally check the HERS file of the save run.
Possibly there have been hardware problems during writing of the tape.

## ARC0415

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0415 FORMAT ERROR OR WRONG BLOCK NUMBER INSTEAD OF '(&00)' ON VSN '(&01)'. PROCESSED FILE IS '(&02)'. FILE SKIPPED

### Meaning

When checking the format of ARCHIVE block number (&00) on input
VSN (&01) an inconsistency or a wrong block number was detected.
The reconstruction or copy of the file is terminated.
(&00): block number (hexadecimal)
(&01): VSN of input volume
(&02): affected file name

### Response

Try to read in this tape / disk save file again. If the error occurs again
for another block, check HERS file of the save run.
Probably there have been hardware problems during writing of the
tape/disk. Read in the files from another save version in this case or
repeat run with PARAM OPERATOR=YES.
For copy save file runs: It is not possible, to restore this file from
this copy. Copy this file from another save version od firts restore the
file on disk (look also for message ARC0292).

## ARC0416

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0416 ERROR DURING POSITIONING OF VSN '(&00)' AFTER READ ERROR. TAPE ABANDONED

### Meaning

When trying to bring the tape (&00) into correct position
after a read error happens, another error occurred.

### Response

Retry the run with another device.

## ARC0417

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0417 DMS ERROR '(&00)' ON INPUT VSN '(&01)' DURING POSITIONING AFTER OPEN ERROR. VOLUME ABANDONED

### Meaning

The operator had given .1 (skip labels) as reply to message ARC0903
after OPEN error on tape (&01).
During the following attempt to position to the ARCHIVE header block
the error (&00) occurred. The tape is skipped and the run is continued
with the next tape.

### Response

Mount the tape on another device and try to read it separately.
If this attempt fails too, read the affected files from another
save version.

## ARC0418

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0418 ARCHIVE HEADER BLOCK NOT FOUND AFTER OPEN ERROR '(&00)' ON INPUT VSN '(&01)'. VOLUME ABANDONED

### Meaning

An I/O error with code (&00) occurred during label checking for input
tape (&01) and the operator had given .1 (skip labels) as reply to the
then appearing message ARC0903. During the following attempt to read the
tape in spite of the error the ARCHIVE header block could also not be
read. The tape is skipped and the run is continued with the next tape.

### Response

Mount the tape on another device and try to read it in separately. If this
attempt fails too, read the affected files from another save version.

## ARC0419

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0419 WRONG BLOCK NUMBER INSTEAD OF '(&00)' ON VSN '(&01)'. PROCESSING OF FILE '(&02)' IS CONTINUED

### Meaning

In spite of getting an ARCHIVE block with wrong block number
the processing of the file is continued.
Look as for message ARC0292.
(&00): block number (hexadecimal)

## ARC0420

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0420 INTERNAL ERROR IN SUBTASK. STATEMENT ABORTED

### Meaning

A severe internal error was detected in a subtask. The subtask has
terminated.

### Response

Send system dump, console report and ARCHIVE report (if present) to the
diagnosis team.

## ARC0421

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0421 DISC ALLOCATION ERROR: RETURN CODE '(&00)'. RUN CONTINUES

### Meaning

Additionally the message ARC0900 is sent to console to offer to
the operator to take a system dump.

### Response

Send system dump, console report and ARCHIVE report (if present)
to the diagnosis team.

## ARC0422

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0422 TOO MANY FILES/JVS TO PROCESS; STATEMENT ABORTED

### Meaning

There is insufficient memory to generate the meta information
of all files/jvs.

### Response

Split the statement in some smaller parts and retry.
A possible solution for a COPY-SAVE-FILE statement which
concerns a complete save file is to enter several
COPY-SAVE-FILE statements with the operand SAVE-FILE=*CONTINUE
which concerns only some SVIDs of the save file.

## ARC0423

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0423 PVS '(&00)' NOT ACCESSIBLE. STATEMENT ABORTED

### Meaning

The Pubset (&00) is not in an accessible state.

### Response

Contact the system administrator.

## ARC0424

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0424 RENAME IS NOT ALLOWED FOR A FILE/JV EXPORTED WITH A RESET OF ITS LOCATION. FILE/JV IS NOT PROCESSED

### Meaning

The RENAME at IMPORT is not allowed when the reset of file location
has been requested at EXPORT time.

## ARC0425

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0425 'LOCATION=RESET' OR 'ATTRIBUTES=RESET' IS NOT ALLOWED. STATEMENT REJECTED

### Meaning

The reset of the location or attributes is requested with incompatible
operands: DIRECTORY specified and/or CATONLY=YES operand.

## ARC0426

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0426 RESTORE IS NOT ALLOWED FOR A FILE/JV EXPORTED WITH 'LOCATION=RESET'. FILE/JV IS NOT PROCESSED

### Meaning

A file/jv exported with LOCATION=RESET can only be processed by
the IMPORT statement.

## ARC0427

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0427 NO 'FULL' SAVE EXISTS FOR THIS FILE. RUN CONTINUES

### Meaning

The file was saved with an CNS entry, although no full save for
this file was found in the directory.
Possible causes:
- The corresponding full save was purged or not copied into
this archive.

## ARC0428

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0428 SVID/SFID ERROR DURING DUPLICATION. RUN IS ABORTED

### Meaning

The SVID/SFID to be duplicated is older than the youngest SVID/SFID
in the output directory file. The duplication is not possible.

## ARC0429

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0429 DMS ERROR '0331' WITH SECONDARY RETURN CODE '(&00)'. FILE IS NOT PROCESSED

### Meaning

Due to DMS error DMS0331, the file is not (completely) processed.
The processing continues with the next file.

### Response

Issue /HELP-MSG-INFORMATION for DMS0331.
Contact the system administrator to take the appropriate action
according to the meaning of the secondary RC mentioned in the DMS0331
message help.

## ARC0430

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0430 ERROR '(&00)' DURING ACCESS VALIDATION FOR THIS FILE/JV

### Meaning

The return code corresponds to following situations:
0001: FILE/JV not share
0002: FILE/JV read only
0003: FILE/JV protected by password
0004: FILE/JV protected by expiration date
0005: FILE cannot be renamed
0006: the owner is not the caller
0007: FILE/JV protected by ACL
0008: FILE inconsistent
0009: PLAM library is in protected mode
0010: FILE protected by GUARDS
0011: the given GUARD is not found
0012: the file owner is not authorized to use the given GUARD
0013: the subsystem GUARDS is not active
0014: terminate task
0015: cannot access system file
0016: file not erasable
0017: call $DMAPWD Action=*PUNISH

## ARC0431

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0431 SECURE ERROR '(&00)' DURING SECURE OF OUTPUT DEVICE. IN SYSTEM MODE: HELP-MSG NKS(&00)

### Meaning

ARCHIVE executed the command SECURE-RESOURCE-ALLOCATION DEVICE=(TYPE=...).
The output device could not be reserved.

## ARC0432

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0432 PATHNAME '(&00)' TOO LONG. FILE NOT PROCESSED

### Meaning

The pathname resulting from the renaming is too long. The processing
goes on with the next file to process.

### Response

The user has to rename the file in such a way that the resulting pathname
is not too long.

## ARC0433

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0433 INVALID VALUE '(&00)' FOR PARAMETER '(&01)' IN ARCHIVE PARAMETER FILE. ANALYSIS CONTINUES

### Meaning

An invalid value is proposed for the specified parameter.
Parameter file not accepted.
Processing continues to analyse the rest of the input text.

## ARC0434

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0434 DMS ERROR '(&00)' DURING POSITIONING ON INPUT VSN '(&01)'

## ARC0435

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0435 DESTINATION SVID '(&00)' FOR SOURCE SVID '(&01)' ALREADY CATALOGED. RUN IS ABORTED

### Meaning

The destination SVID is generate depending on the source SVID.
If the destination SVID is already cataloged in the directory,
a MOVE-SAVE-FILE is not possible.

## ARC0436

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0436 INVALID ARCHIVE PARAMETER FILE. ARCHIVE LOADING ABORTED

### Meaning

Error(s) in ARCHIVE parameter file.
ARCHIVE loading aborted.

## ARC0437

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0437 NO WRITE-PASSWORD ON ARCHIVE PARAMETER FILE. ARCHIVE LOADING ABORTED

### Meaning

The ARCHIVE parameter file is not protected by a password.
The loading of ARCHIVE is aborted.

## ARC0438

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0438 UNKNOWN PARAMETER '(&00)' IN ARCHIVE PARAMETER FILE. ANALYSIS CONTINUES

### Meaning

Unknown parameter in the ARCHIVE parameter file
(maybe blanks in the expression).
Parameter file not accepted.
Processing continues to analyse the rest of the input text.

## ARC0439

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0439 D-STATEMENTS NO LONGER SUPPORTED. ENTER A CORRECT STATEMENT

## ARC0440

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0440 UFS ERROR '(&00)' DURING OPERATION '(&01)' ON FILE '(&02)' ON HOST '(&03)'

### Meaning

- The file or directory does not exist (any more)
- the user has no permission on this file for backuping or archiving
- the file also appears in the except list
- the file is in the restricted file (for Unix only)
- the files from bs2fs mounted in POSIX are not saved
with BACKUP-NODE-FILES

### Response

Correct the error and retry.
Note on saving BS2000 files available in bs2fs under POSIX: these
files can be backed up with BACKUP-FILES only.

## ARC0441

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0441 ONE SUBSYSTEM IS NOT AVAILABLE. RUN ABORTED

### Meaning

A subsystem that is needed for NFS or POSIX is not available.
Run aborted.

### Response

Check the subsystems that are needed for NFS or POSIX.
Restart the run after correction.

## ARC0442

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0442 INVALID LOCALIZATION OF A FILE, - FILE NOT PROCESSED

## ARC0443

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0443 FILE OF ANOTHER TYPE ALREADY EXISTS.

## ARC0444

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0444 VOLUME '(&00)' ALREADY CONTAINS SAVE FILE WITH SAME IDENTIFIER. RUN ABORTED

### Meaning

A new save file must be created on volume '(&00)', though a save
file with same identification already exists and may not be
overwritten.

### Response

The user must use another volume or purge the existing save version.

## ARC0445

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0445 DMS ERROR '(&00)' ON SAVE FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The DMS error '(&00)' has occurred on the save file '(&01)'.
The subtask processing is terminated.
For more detailed information about the DMS error code, enetr /HELP-MSG
in system mode or consult the BS2000 manual 'SYSTEM MESSAGES'.

## ARC0446

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0446 DMS ERROR '(&00)' DURING CONCURRENT-COPY SAVE FILE ACCESS. RUN ABORTED

### Meaning

During a concurrent copy backup, the DMS error '(&00)' occurred for
the save file access. Run aborted.

### Response

In system mode: /HELP-MSG-INFORMATION DMS(&00)

## ARC0447

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0447 ERROR DURING CONCURRENT-COPY PROCESSING OF FILE/JV '(&00)'. THE RUN CONTINUES WITH NEXT FILE/JV

## ARC0448

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0448 GUARDS FILE IGNORED BY CONCURRENT COPY PROCESSING

## ARC0449

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0449 UFS ERROR '(&00)' DURING OPERATION '(&01)'

### Response

Correct the error and retry

## ARC0450

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0450 BIND TO ARCHIVE UNSUCCESSFULLY. RETURNCODE=X'(&00)'

## ARC0451

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0451 CMX ERROR CODE '(&00)' OCCURRED WHEN ISSUING CMX COMMAND '(&01)' FOR WORKSTATION '(&02)'

### Meaning

No further processing is performed. A system dump is issued and the
ARCHIVE task is terminated.

## ARC0452

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0452 INTERNAL ERROR OCCURRED IN MODULE '(&00)' WHEN ISSUING CMX COMMAND '(&01)'

### Meaning

No further processing is performed. A system dump is issued and the
ARCHIVE task is terminated.

## ARC0453

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0453 NOT ENOUGH BUFFER DATA AREA CAN BE ALLOCATED TO GET DATA FROM WORKSTATION '(&00)'

### Meaning

No processing is performed for the concerned workstation.

## ARC0454

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0454 WORKSTATION '(&00)' PREMATURELY DISCONNECTED DUE TO EXTERNAL EVENT

### Meaning

The processing is aborted for the concerned workstation.

## ARC0455

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0455 UNEXPECTED CMX EVENT '(&00)' HAS BEEN RECEIVED FOR THE WORKSTATION '(&01)'

### Meaning

No further processing is performed. A system dump is issued and the
ARCHIVE task is terminated

## ARC0456

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0456 CMX NAME ERROR FOR WORKSTATION '(&00)'

### Meaning

No processing is performed for the concerned workstation.

## ARC0457

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0457 NODE '(&00)' CAN NOT/NO MORE BE REACHED.

### Meaning

Node (&00) can not/no more be reached. The NFS network access
method is involved to continue the processing.

### Response

Contact the system administrator. More information can be found in
the server conslog file.

## ARC0458

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0458 ERROR DURING CO-OWNING CHECK OF FILE/JV '(&00)'.

### Meaning

An error happens during the co-owning check for file/jv
(&00), the processing continues with the next file(jv)name.

## ARC0459

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0459 SYNTAX ERROR IN HSMS-SV SYSDAT FILE '(&01)' FOR NODE '(&00)'

### Meaning

Concerned node '(&00)' is not correctly entered in SYSDAT.

### Response

Delete node entry in SYSDAT for NFS processing or correct entry
as client. Contact the system administrator.

## ARC0460

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0460 AT LEAST ONE INPUT VOLUME IS MISSING. FILE NOT COMPLETELY PROCESSED

## ARC0461

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0461 FILE SYSTEM NOT MOUNTED. FILE NOT PROCESSED

### Response

Please contact the system administrator

## ARC0462

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0462 ARCHIVE RUN ALREADY IN PROGRESS FOR THIS USERID CATALOG. FILE NOT PROCESSED

## ARC0463

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0463 ERROR '(&00)' ON SYSSRPM FILE. PROCESSING CONTINUE

### Meaning

SRPM was called for the process of a SRPM file. The process continues with
the next file.

### Response

/HELP-MSG-INFORMATION SRM(&00) gives the meaning of the SRPM message.
SRM0001 means "PARAMETER ERROR". This is so in case of invalid rename
of the Users Catalog.

## ARC0464

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0464 ARCHIVE DOES NOT PROCESS FILES LOCATED ON SM-PUBSET '(&00)'

### Meaning

ARCHIVE does not process files that are located on a SM pubset to preserve
the consistency of the SM pubset.

### Response

Files located on a SM pubset must be processed by HSMS.

## ARC0465

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0465 ERROR DURING CONCURRENT COPY PROCESSING. FURTHER DIAGNOSE WITH CCOPY ERROR CODE '(&00)' FROM '(&01)'

### Meaning

Errors possible in normal operation: 000C - CCOPY Session
cancelled, 000D - CCOPY Session deleted

## ARC0466

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0466 HARDLINKED FILE NOT FOUND. DATA LOCALISATION IS UNKNOWN

## ARC0467

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0467 BEGIN OF FILE NOT FOUND AFTER READ OR FORMAT ERROR ON INPUT VOLUME

## ARC0468

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0468 DMS ERROR '(&00)' ON INPUT VOLUME '(&01)'. RUN IS TERMINATED

## ARC0469

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0469 THE ERROR '(&00)' OCCURRED FOR THE WORKSTATION '(&01)'

### Meaning

No further processing is performed. A system dump is issued and the
ARCHIVE task is terminated

## ARC0470

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0470 FIRST VOLUME CONTAINING FILE IS MISSING. FILE ATTRIBUTES ARE UNKNOWN

## ARC0471

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0471 FILE NOT COMPLETELY WRITTEN ON VOLUME. END OF FILE IS MISSING

## ARC0472

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0472 INTERFACE '(&01)' REPORTS ERROR '(&00)' AT LOCATION '(&02)'

### Meaning

Errors from Interface FARAM:
01 file not empty,
02 file not catalogued,
03 file is not a repository or is not accessable,
04 internal Low-Key invalid,
05 internal High-Key missing,
06 internal Low-Key missing,
07 Sharupd Conflict,
08 Request-Memory-Error,
09 DMS-Error,
10 internal error,

## ARC0473

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0473 ERROR '(&00)' REPORTED BY '(&01)' IN '(&02)'

## ARC0474

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0474 SRPM CANNOT ACCESS PUBSET FOR SRPM BACKUP. PROCESSING CONTINUES.

### Meaning

SRPM provides main returncode 0002, pubset not accessible or in slave
mode as shared pubset with master osd version lower than 6.0B.

## ARC0475

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0475 ERROR CODE '(&02)' OCCURRED WHEN ISSUING SOCKETS COMMAND '(&01)' FOR WORKSTATION '(&00)'

## ARC0476

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0476 SAVE FILE CREATED WITHOUT SPECIFICATION OF A DIRECTORY; PROCESSING ABORTED.

## ARC0477

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0477 ERROR: '(&00)'

## ARC0478

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0478 PLAM ERROR '(&00)' ON DISK FILE. FILE NOT COPIED. IN SYSTEM MODE: /HELP-MSG PLA(&00)

### Meaning

The PLAM error (&00) has occurred. The message is associated with the
file in error on the ARCHIVE report.
Processing continues with the next file.
For more detailed information about the PLAM error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## ARC0479

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0479 SRMUTC ERROR '(&00)' WHILE UPDATING USER TABLE

### Meaning

An error occured when attempting to update the HSMS fields in the USER
table.

## ARC0480

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0480 REMOTE WORKSTATION UNREACHABLE. OBJECT NOT PROCESSED

### Response

Please contact your system administrator.

## ARC0481

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0481 OBJECT COULD NOT BE SAVED DUE TO AN EXTERNAL EVENT ON WORKSTATION

### Response

Please contact your workstation administrator.

## ARC0482

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0482 OBJECT COULD NOT BE RESTORED DUE TO AN EXTERNAL EVENT ON WORKSTATION

### Response

Please contact your workstation administrator.

## ARC0483

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0483 OBJECT IS COMPRESSED AND COULD NOT BE RESTORED DUE TO A CONFIGURATION ERROR ON WORKSTATION

### Meaning

The object (file or directory) could not be restored. It had to be
decompressed on the client workstation as network compression was
enabled during backup, but this is not possible due to a configuration
error of HSMS-CL on the workstation.
Possible configuration errors:
- the path name for the control file for network compression is
missing in the system-wide configuration data of HSMS-CL
- the control file for network compression is not accessible
- the section Compression Methods of the control file has no entry
for the compression method used during backup
- the path for the decompression program is missing in the entry
for the right compression method
- the decompression program is not accessible

### Response

Please contact your workstation administrator. After elimination of the
error cause, a new restore request must be issued.

## ARC0484

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0484 SECURE ERROR '(&00)' DURING SECURE OF OUTPUT DEVICE

### Meaning

The output device could not be reserved.
(&00): $NKSSEC return code
0004: wait time too short
0005: device not available in the system
0006: secure was aborted by request (CANCEL/SHUTDOWN)
0008: device currently not available
0009: waiting period over

## ARC0485

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0485 SECURE ERROR '(&00)' DURING SECURE OF DEVICES. IN SYSTEM MODE: /HELP-MSG NKS(&00)

### Meaning

ARCHIVE executed the command SECURE-RESOURCE-ALLOCATION DEVICE=(TYPE=...).
The input and output devices could not be reserved at the same time.

## ARC0486

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0486 SECURE ERROR '(&00)' DURING SECURE OF INPUT DEVICE

### Meaning

The input device could not be reserved.
(&00): $NKSSEC return code
0004: wait time too short
0005: device not available in the system
0006: secure was aborted by request (CANCEL/SHUTDOWN)
0008: device currently not available
0009: waiting period over

## ARC0487

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0487 SECURE ERROR '(&00)' DURING SECURE OF OUTPUT VOLUME '(&01)'

### Meaning

The output volume could not be reserved.
(&00): $NKSSEC return code
0004: wait time too short
0005: volume not available or protected
0006: secure was aborted by request (CANCEL/SHUTDOWN)
0007: mount impossible
0009: waiting period over

## ARC0488

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0488 SECURE ERROR '(&00)' DURING SECURE OF INPUT AND OUTPUT VOLUME '(&01)'. IN SYSTEM MODE: /HELP-MSG NKS(&00)

### Meaning

ARCHIVE executed the cmd SECURE-RESOURCE-ALLOCATION TAPE=(VOLUME=(&01)).
The input and output tape could not be reserved at the same time.
Possible reasons:
- one volume is not defined in MAREN catalog.
- no device is defined or available for requested volume type.
- one volume is already used by another task.

### Response

Check the volume status in MAREN or its usage by a SHOW-TAPE-STATUS.

## ARC0489

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0489 SECURE ERROR '(&00)' DURING SECURE OF INPUT VOLUME '(&01)'

### Meaning

The input tape could not be secured.
(&00): $NKSSEC return code
0004: wait time too short
0005: volume not available or protected
0006: secure was aborted by request (CANCEL/SHUTDOWN)
0007: mount impossible
0009: waiting period over

## ARC0490

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0490 DEVICE MANAGEMENT ERROR. RUN STOPS

## ARC0491

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0491 HSMS-CL INCOMPATIBILITY DETECTED. FILE NOT RESTORED

### Meaning

The file to be restored is not compatible with the HSMS-CL version.

## ARC0492

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0492 CONNECTION REFUSED BY THE CLIENT VERSION '(&01)' ON THE WORKSTATION '(&00)'. REASON '(&02)'

## ARC0493

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0493 FILE SYSTEM INCOMPATIBILITY DETECTED. FILE NOT RESTORED

### Meaning

The file to be restored is not compatible with the filesystem mounted on
the client workstation.

## ARC0494

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0494 PLAM ERROR '(&00)' DURING RESTORE-LIBRARY-ELEMENT

### Meaning

A PLAM error (&00) has occurred. The processing for restoring of
information on the elements is aborted. Run stops.

## ARC0495

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0495 RESTORE-LIBRARY-ELEMENT FAILURE. ERROR '(&00)'

### Meaning

An error has occurred. The processing for restoring of information on the
elements is aborted. Run stops.
(&00): Errors:
1: PLAM error
2: DMS error
3: Report error
others: not defined

### Response

Try the statement RESTORE-FILES for restoring the completed libary.

## ARC0496

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0496 STMT //RESTORE-LIBRARY-ELEMENTS NOT POSSIBLE. REASON '(&00)'

### Meaning

The RESTORE-LIBRARY-ELEMENTS statement is not possible because the
save-version does not contain the save-plam-information.
Possible reasons:
1: the file is not a library or the library has not a good status
2: the library has not been saved with SAVE-PLAM-INFO=*YES
3: the library does not exist (//RLE only possible in an existing library)
4: the existing library has been migrated

## ARC0497

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0497 CLIENT '(&00)' ERROR: '(&01)'

## ARC0498

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0498 CLIENT ERROR: '(&00)' FOR FILE '(&01)'

## ARC0499

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0499 INVALID TAG SIZE FOR HOST '(&00)'

### Meaning

The maximal size of data contained in a tag has been reached.
Possible reasons are:
- The FROM-FILE of the workstation specified in the statement is too big
(greater than 100 KB).
- The except list is too big (greater than 100 KB).

## ARC0501

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0501 INVALID SAVE BLOCK SIZE; PROCESSING OF SAVE FILE ABORTED

### Meaning

Possible reasons:
1. The block size of the save file exceeds the limit of 32kB.
Block sizes greater than 32kB are supported from OSD V6.0.
To restore a save file created by BS2000 OSD V6.0 or later
in previous BS2000 version, you have to specify in the save run
BLOCKING-FACTOR = 15 instead of *MAX.
2. The block size of the disc save file exceeds the limit for
current ARCHIVE version. To make continuation of a disc save file
created in ARCHIVE/HSMS V9.0B or later in previous ARCHIVE/HSMS
version possible, you have to specify BLOCK-SIZE-DISK=STD instead
of MAX in the file SYSPAR.ARCHIVE.<ver> before the original
save run.

## ARC0502

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0502 INVALID SAVE BLOCK SIZE; PROCESSING OF TAPE '(&00)' ABORTED

### Meaning

The block size of the save file on tape exceeds the limit of 32KB.
Block sizes greater than 32KB are supported from OSD V6.0.
To process a save file created by BS2000 OSD V6.0 or later
in previous BS2000 version, you have to specify in the save run
BLOCKING-FACTOR = 15 instead of *MAX.

## ARC0503

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0503 NET-STORAGE VOLUME '(&00)' NOT ASSIGNED TO A PUBSET. SUBTASK TERMINATED.

### Meaning

The specified Net-Storage volume is not assigned to a pubset.
The ARCHIVE subtask is unable to continue.

### Response

Check status of the Net-Storage volume. A Net-Storage volume can be
assigned to a pubset by /ADD-NET-STORAGE-VOLUME.

## ARC0504

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0504 RESTORE TO NET-STORAGE VOLUME NOT POSSIBLE FOR THIS BS2000 VERSION.

### Meaning

It is not possible to restore files to Net-Storage in BS2000 version
lower than V9.0.

### Response

Use NEW-SUPPORT=*PUBLIC-DISK(STORAGE-TYPE=*PUBLIC-SPACE) or
NEW-SUPPORT=*SYSTEM-MANAGED-PUBSET(STORAGE-TYPE=*PUBLIC-SPACE) operand to
direct Net-Storage files being restored to public space.
To choose Net-Storage files only use
ORIGINAL-SUPPORT=*PUBLIC-DISK(STORAGE-TYPE=*NET-STORAGE).

## ARC0505

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0505 MISSING SAVE OF SAVE-TYPE FULL, PART OR CATL FOR NET-STORAGE FILE '(&00)'. CATALOG ENTRY NOT RESTORED

### Meaning

There are only CNS entries in the directory for the specified file.

## ARC0506

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0506 RESTORE TO NET-STORAGE VOLUME NOT POSSIBLE FOR FGG

### Meaning

It is not possible to restore FGGs to a Net-Storage volume.

### Response

Restore FGG to public space of a pubset or to a private disk.

## ARC0507

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0507 RESTORE OF DATA-AND-CATALOG WAS SPECIFIED BUT LATEST SAVE-VERSION CONTAINS SAVE-TYPE CATL FOR FILE '(&00)'. FILE NOT RESTORED

### Meaning

The youngest file version in the selected range of save-versions has
the save-type CATL and has a newer file version or different CFID
than the last save-type FULL of the file.
The Net-Storage file has not been restored.

### Response

Select a range of save versions that exclude this file
with save-type 'CATL'.

## ARC0508

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0508 UNABLE TO FIND SAVE FILE ON PUBSET '(&00)' FOR SAVE VERSION '(&01)'

### Meaning

The save file containing the required files for a restore statement
or for a save statement with continue does not exist.
Processing of the statement continues with the next save version,
if there is any more to process.
A save statement with continue is aborted.

## ARC0509

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0509 DEVICE-TYPE NETSTOR IS NOT POSSIBLE WITH CURRENT SETTINGS.

### Meaning

It is not possible to use device-type NETSTOR if STORAGE-TYPE=
PUBLIC-SPACE is specified in the parameter file SYSPAR.ARCHIVE.

### Response

Use STORAGE-TYPE=ANY in the parameter file SYSPAR.ARCHIVE
to be able to use device of any type.

## ARC0510

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0510 RESTORE OF NET-STORAGE FILES NOT POSSIBLE. FILE NOT RESTORED.

### Meaning

It is not possible to restore Net-Storage files if STORAGE-TYPE=
PUBLIC-SPACE is specified in the parameter file SYSPAR.ARCHIVE.

### Response

Use STORAGE-TYPE=ANY in the parameter file SYSPAR.ARCHIVE
to process any storage type of files.

## ARC0511

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0511 RESTORE OF NET-STORAGE NODE-FILES NOT POSSIBLE TO THIS TYPE OF DISK. FILE NOT RESTORED.

### Meaning

It is not possible to restore Net-Storage node-files to public space
or private disk.

## ARC0512

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0512 RESTORE OF NET-STORAGE NODE FILES NOT POSSIBLE. FILE NOT PROCESSED.

### Meaning

Net-Storage node files cannot be restored with this ARCHIVE version
or the current BS2000 version does not support node files.

### Response

For restore of PAM node files following versions are required:
- BS2000 OSD/BC >= V10.0
- ARCHIVE >= V10.0A
For restore of SAM node files following versions are required:
- BS2000 OSD/BC >= V11.0
- ARCHIVE >= V11.0A

## ARC0513

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0513 IT IS IMPOSSIBLE TO CONVERT FILES WITH NONZERO LAST BYTE POINTER WITH CURRENT VERSION OF PAMINT. FILE NOT (FULLY) RESTORED.

### Meaning

Converting files with LBP <> 0 is not possible
with PAMINT version installed on this system.

### Response

Contact system administrator to make PAMINT up-to-date.

## ARC0514

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0514 RESTORE OF FILES WITH LAST BYTE POINTER NOT POSSIBLE TO PRIVATE DISK. FILE NOT RESTORED.

### Response

Restore the file on public disk or Net-Storage.

## ARC0515

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

ARC0515 WRONG BLOCK NUMBER '(&00)' ON VSN '(&01)'. STATEMENT ABORTED

### Meaning

The position of output VSN (&01) got lost. A block with ARCHIVE data block
number (&00) was expected but the block just written out has another
number.
(&00): block number (hexadecimal)
(&01): output VSN

## ARC0516

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0516 THE NEXT SAVE WITHIN THE DIRECTORY MUST BE INTO A NEW SAVE FILE.

### Meaning

Continuation of the actual save file will not be possible because the
SFID/SVID is not consistent due to a DMS error and cannot be continued.

## ARC0517

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0517 SAVING ON S1 LEVEL DEFINED BY ALL HSMS-CONTROLLED VOLUME SETS IS NOT POSSIBLE IN CURRENT BS2000 VERSION.

### Meaning

Saving on S1 level defined by all HSMS-CONTROLLED volume sets is only
possible in BS2000 OSD/BC V11.0A and higher.
In case of a shared SM pubset, the master system also must have
BS2000 OSD/BC version V11.0A or higher.

## ARC0518

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0518 THE VOLUME SET '(&01)' CAN NOT BE USED AS S1 STORAGE LEVEL. REASON '(&00)'. SUBTASK TERMINATED.

### Meaning

Due to internal error inappropriate volume set has been
selected by system as S1 level in SM pubset environment
when it is defined by *ALL-HSMS-CONTROLLED in the SM pubset parameters.
(&00): Identification of a possible reasons:
0001: Error in STAMI;
0002: the volume set is not HSMS-CONTROLLED;
0003: maximal I/O length of the volume set is not suitable.
(&01): Catalog ID of the volume set

## ARC0519

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0519 SAM NODE FILE SAVED WITH 'SAVE-SAM-STRUCTURE=*NO'. FILE NOT RESTORED.

### Meaning

It is not possible to restore SAM node files to
public space, private disk, or Net-Storage with FILE-TYPE=*BS2000,
if the files have been saved with the save option
SAVE-SAM-STRUCTURE=*NO.

### Response

Restore the specified files on Net-Storage with FILE-TYPE=*NODE-FILE.

## ARC0521

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0521 RESTORE OF FILE ON NET-STORAGE NOT POSSIBLE. FILE NOT RESTORED. ERROR CODE '(&00)'.

### Meaning

Meaning of the error code:
- 01 : It is not possible to restore ISAM files on Net-Storage as
node files (user specified FILE-TYPE=*NODE-FILE).
- 02 : It is not possible to restore PAM files with the attribute
BLKCTRL=DATA on Net-Storage as node files (user specified
FILE-TYPE=*NODE-FILE).
- 03 : It is not possible to restore SAM files with the attribute
BLKCTRL=PAMKEY on Net-Storage as node files (user specified
FILE-TYPE=*NODE-FILE).

### Response

ISAM files, PAM files with BLKCTRL=DATA and SAM files with
BLK-CONTR=PAMKEY can only be restored on Net-Storage as of type BS2000.
Specify FILE-TYPE=*BS2000 during restore of these files on Net-Storage.

## ARC0522

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0522 FILE NOT SAVED

### Meaning

A file was not saved during the incremental save run, because it was
already saved with the current version. Nevertheless an inconsistency
was found that indicates, that the file was saved inadequately during
a previous run.E.g. splitted mirrored disks have been saved without
the usage of CCOPY, or EXPORT or EXPORT-FILES was used for backup
instead of SAVE or BACKUP-FILES.

### Response

E.g. save mirrored disks by HSMS with usage of CCOPY. For data backup use
the statements SAVE or BACKUP-FILES.Contact the system administrator.

## ARC0523

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0523 ERROR '(&00)' DURING ACCESS TO MANAGEMENT CLASS '(&01)' OF SM-PUBSET '(&02)'

### Meaning

The error (&00) occurred when accessing the management class catalog.
All the files assigned to the management class are skipped.
Possible reasons according to the error code:
- 03 - the management class (&01) not defined in generic catalog
of pubset
- 04 - access to the object (&01) locked by another task
- 05 - subsystem GCF not available
- 07 - the SM pubset (&02) not under HSMS control
- 08 - the pubset (&02) not available on the processing system
- 09 - the pubset (&02) not available on the processing system

### Response

Contact the system administrator to solve the problem
and try again to save the skipped files.

## ARC0554

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0554 DIRECTORY FILE CONTAINS INCONSISTENT INFORMATION ON NEW/OLD SVID. PROCESSING CONTINUES

### Meaning

Inconsistencies have been introduced between the HSMS processing and
the ARCHIVE processing (e.g via PURGE function). The processing continues.

## ARC0556

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0556 FILE TO BE MIGRATED IS NOT THE SAME AS THE FILE THAT WAS SAVED BY ARCHIVE

### Meaning

Between the copy of the file in an ARCHIVE save version and the update of
its catalog entry (migrate), the CFID or the version number was changed.
The file is not migrated.

## ARC0557

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0557 INVALID MIGRATION TO S2

### Meaning

The migration to S2 is only possible for files that were already migrated
to S1. The migration is not done.

## ARC0558

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0558 FILE TO BE PROCESSED IS NOT MIGRATED

### Meaning

A exchange / recall was done for a file that is not migrated.
The exchange / recall is not done.

## ARC0559

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0559 FILE TO BE RECALLED IS NOT REALLY MIGRATED

### Meaning

A recall was done for a file that has the migrated indicator in its
catalog entry but for which public space is already allocated.
The migrated indicator is reset in the catalog entry and the file
is not recalled.

## ARC0560

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0560 CONTINUE OF THIS HSMS SAVE FILE NOT ALLOWED. RUN TERMINATED

### Meaning

Only HSMS can continue a save file/save version created by HSMS which
either contains several save versions or is a save file on S1-level or
is a save file with the same SVID.

## ARC0561

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0561 SAVE VERSION CANNOT BE CONTINUED AFTER A MODIFICATION OF THE SAVE-FILE-STRUCTURE . RUN TERMINATED

### Meaning

A save version can not be continued after the statement:
//MODIFY-ARCHIVE-ATTRIBUTES ...,SAVE-FILE-STRUCTURE=*SEVERAL-SVID

### Response

Create a new save version with //BACKUP-FILES ...,SAVE-FILE=*NEW

## ARC0562

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0562 CONTINUE OF A SAVE VERSION WHICH IS PART OF A HSMS SAVE FILE IS NOT ALLOWED. RUN TERMINATED

### Meaning

The specified save version is contained in a save file generated by
HSMS. This save file contains several save versions and it is not allowed
to continue them.

## ARC0563

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0563 WRONG STATEMENT USED FOR A SAVE FILE WITH 'SEVERAL-SVID-OPTION'. RUN TERMINATED

### Meaning

To create or continue a save file which contains several save versions
HSMS must use the EXPORT statement.
For read access one has to use IMPORT.

## ARC0564

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0564 CATALOG ENTRY OF MIGRATED FILE HAS WRONG FORMAT

### Meaning

The ARCHIVE-HSMS part of the catalog entry has a format before
BS2000/OSD V1.0.
But the statement assumes a format of BS2000/OSD V1.0.
The migration/exchange has not been processed.

## ARC0565

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0565 CATALOG ENTRY OF MIGRATED FILE CONTAINS UNKNOWN OR WRONG INFORMATION

### Meaning

The HSMS-ARCHIVE part of the catalog entry has an unknown version.
The migration/exchange has not been processed.

## ARC0566

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0566 CATALOG ENTRY OF THE MIGRATED FILE IS NOT CONSISTENT

### Meaning

The catalog entry of the migrated file contains wrong lengthes.
The migration/exchange has not been processed.

## ARC0567

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0567 INSUFFICIENT SPACE IN THE CATALOG ENTRY

### Meaning

The migration/exchange has not been processed because of insufficient
space in the catalog.

## ARC0568

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0568 ERROR '(&00)' FOR OPERAND '(&01)'

### Meaning

An error was detected for the specified operand in the SDF-transfer-area.

### Response

Correct the operand.

## ARC0569

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0569 OFFLINE COPY OF MULTIPLEXED TAPES TO DISK IS NOT ALLOWED. STATEMENT ABORTED

### Response

Retry the statement specifying TO-STORAGE=*S2-STORAGE-LEVEL.

## ARC0570

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0570 ERROR '(&00)' IN COMMAND '(&01)'

### Meaning

An error was detected for the specified command in the SDF-transfer-area.

## ARC0571

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0571 ERROR DETECTED DURING OPEN OR CLOSE OPERATION ON DIRECTORY/REPOSITORY FILE

### Meaning

An error occured during open or close operation on the directory file,
the run was aborted.
An automatic check of the file was done by ARCHIVE to try to correct the
problem.

## ARC0572

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0572 ANOTHER TRACE COMMAND IS CURRENTLY BEING TREATED

## ARC0573

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0573 THE PREPROCESSING HAS FAILED ON WORKSTATION '(&00)'. BACKUP-NODE-FILES OR RESTORE-NODE-FILES PROCESSING IS ABORTED FOR THAT WORKSTATION

## ARC0574

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ARC0574 ERROR '(&00)'; SFID NOT FOUND FOR SVID '(&01)'. CONTACT THE SYSTEM ADMINISTRATOR

## ARC0575

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0575 CLIENT ERROR

## ARC0576

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

ARC0576 NOT ENOUGH SPACE AVAILABLE FOR MEMORY REQUEST AT '(&00)'.

### Meaning

Insufficient (&00) memory to satisfy the request. No memory
is allocated. Space limit exceeded.

### Response

Contact the system service.

## ARC0577

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0577 MAREN-ERROR '(&00)' WITH RETURN CODE '(&01)'. IN SYSTEM MODE /HELP-MSG (&00)

### Meaning

(&00): message key of MAREN.
(&01): return code of MARENFA.

### Response

Enter /HELP-MSG-INFORMATION for MAREN message (&00).

## ARC0578

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0578 SUBSYSTEM '(&00)' NOT AVAILABLE (RETURN CODE='(&01)')

### Meaning

(&00): subsystem (e.g. MAREN)
(&01): return code of subsystem interface

### Response

Contact the system administrator.

## ARC0701

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0701 DMS ERROR '(&00)' ON OUTPUT VSN '(&01)'. ARCHIVE ERROR RECOVERY STARTED

### Meaning

During SAVE or copy of a file or save version a write error occurred on
tape (&01) with DMS error code (&00). ARCHIVE is trying to avoid negative
consequences of the error or at least to keep them as small as possible.

### Response

Check the ARCHIVE report after the run thoroughly, to see
if any errors occurred in consequence.

## ARC0702

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0702 DMS ERROR '(&00)' ON OUTPUT VSN '(&01)'. SUBSAVE TERMINATED

### Meaning

During writing the save file on volume (&01) an error with error code
(&00) occurred. The affected subtask is terminated.

### Response

Repeat save run.

## ARC0703

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0703 ERROR RECOVERY ON VSN '(&00)' NOT SUCCESSFUL. SUBSAVE TERMINATED

### Meaning

The attempt to write EOF-labels on a defined position of output tape (&00)
failed. The save run is terminated.
Eventually there are already some correctly saved files on the affected
VSN (see ARCHIVE report. Last file is perhaps not correct even if
inicated FULL).

### Response

Do the save run again, do not use the affected volume or device again.

## ARC0704

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0704 DMS ERROR '(&00)' DURING ERROR RECOVERY AFTER WRITE ERROR ON VSN '(&01)'. SUBSAVE TERMINATED

### Meaning

During error recovery after a write error on output tape with VSN (&01)
another DMS error with error code (&00) happened. Error recovery cannot be
continued successfully. The save run is terminated.

### Response

Check condition of device/tape material. Do save run again with other
devices/tapes.

## ARC0705

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

ARC0705 MORE THAN '(&00)' ERRORS ON INPUT VSN '(&01)'. VOLUME ABANDONED

### Meaning

Maximum of allowable read or format errors for one volume is (&00).
This maximum is exceeded for VSN (&01). Processing of this volume is
terminated and run continues with the next volume.
(&00): number of errors (hexadecimal)

### Response

Check conditions of the affected device. Try to read in the volume
separately from another device. If this attempt fails too, read in
the affected files from another save version.

## ARC0706

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0706 ARCHIVE ERROR RECOVERY PROBLEM DUE TO THE OUTPUT DEVICE TYPE. SUBSAVE TERMINATED

## ARC0707

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0707 DEADLOCK RECOVERY FAILURE

### Meaning

A deadlock was detected and the recovery started.
Due to an error the recovery processing is aborted.

### Response

Read the report to find out the reason of the recovery processing failure.

## ARC0708

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0708 RESTART POINT NOT FOUND ON INPUT TAPE AFTER ERROR RECOVERY FOR OUTPUT TAPE

## ARC0777

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

ARC0777 WRONG BLOCK NUMBER FOUND INSTEAD OF '(&00)' ON INPUT VSN '(&01)'. VOLUME ABANDONED

### Meaning

The position of input VSN (&01) got lost. A block with ARCHIVE data block
number (&00) was expected but the block just read in has another number.
For tape run with PARAM OPERATOR=YES: the operator terminated processing
of this volume (look for message ARC0906) or the block number of the block
is lower than that of the preceding one, that means the block does not
belong to the same ARCHIVE save file.
(&00): block number (hexadecimal)

### Response

If any tape device errors have occurred before this message try to read
in the tape from another device. Otherwise, print the blocks around the
specified block and check, whether all blocks were saved correctly.
In case of tape run, repeat it with PARAM OPERATOR=YES.

## ARC0778

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

ARC0778 WRONG BLOCK NUMBER FOUND INSTEAD OF '(&00)' ON INPUT VSN '(&01)'. PROCESSING OF VOLUME CONTINUES

### Meaning

The position of input VSN (&01) got lost. A block with ARCHIVE data block
number (&00) was expected but the block just read in has another number.
Processing of volume continues.
(&00): block number (hexadecimal)

### Response

If any device errors have occurred before this message try to read in
the tape from another device. If no device errors have occurred, print
the blocks around the specified block and check,
whether all blocks were saved correctly on this tape.

## ARC0800

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0800 THE RETENTION PERIOD FOR SOME FULL BACKUPS SHOULD BE UPDATED

### Meaning

A partial or a differential backup has been issued, and one ore more
referred full backups will be obsolete before this new backup.

## ARC0801

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0801 ALIAS FILE NAME SUBSTITUTION: '(&00)' BECOMES '(&01)'. PROCESSING CONTINUES

### Meaning

The specified alias file name (&00) has been translated into the
real file name (&01).

## ARC0802

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0802 COMPUTED BLOCK-SIZE VALUE IS '(&00)'

### Meaning

From the present disk configuration, the maximum possible value has been
computed and will be used.

## ARC0803

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0803 CE OF MIGRATED FILE '(&00)' ('(&01)','(&02)','(&03)') RESTORED

### Meaning

Internal message. Processed by HSMS internally.

## ARC0804

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0804 LOCALISATION INFORMATION OF THE MIGRATED FILE '(&00)' IS INVALID. PROCESSING CONTINUES

### Meaning

The localization information of the migrated file is invalid.
(&00): file name.

## ARC0805

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0805 SHARUPD CONFLICT ON DIRECTORY. PROCESSING SUSPENDED

### Meaning

Another task has the directory open for updating and the task issuing
this message will suspend itself until directory access is possible.
After expiration of a maxium time intervall the message ARC0149 will be
given. Processing continues normally if the directory becomes available.

## ARC0806

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0806 VOLUME '(&00)' BELONGS TO DIRECTORY '(&01)'

## ARC0807

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0807 SAVE FILE '(&00)' RETENTION PERIOD UPDATED

## ARC0808

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0808 MIGRATED FILE '(&00)' ERASED. PROCESSING CONTINUES

### Meaning

No valid data for the catalog entry of a migrated file.
File has been erased.
(&00): file name.

## ARC0809

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0809 NO DEVICE DEPOT FOR LOCATION '(&00)'. RUN CONTINUES WITHOUT LOCATION

## ARC0810

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0810 THE RETENTION PERIOD OF SOME BACKUPS WILL BE MODIFIED

### Meaning

A partial or a differential backup has been issued, and one ore more
referred backups would be obsolete before this new backup.
The retention period will be updated automatically.

## ARC0811

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0811 THE SAVE VERSION OF THE LIBRARY CONTAINS SAVE-PLAM-INFORMATION

### Meaning

The library has been saved with SAVE-PLAM-INFO=*YES.
The stmt RESTORE-LIBRARY-ELEMENTS can be used.

## ARC0812

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0812 ARCHIVE TAPE DRIVER TASK TSN '(&00)' GENERATED

### Meaning

Display of tape driver TSN on the terminal.

## ARC0813

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0813 CLIENT '(&00)' INFORMATION: '(&01)'

## ARC0814

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0814 CLIENT INFORMATION: '(&00)' FOR FILE '(&01)'

## ARC0815

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0815 SUBTASK '(&00)' HAS TRANSFERRED '(&01)' PAM PAGES FOR '(&02)' FILES AND '(&03)' JVS IN '(&04)' SECONDS

### Meaning

&00: number of the subtask (0..9, A..F)
&01: number of transferred PAM-pages
&02: number of saved or restored files
&03: number of saved or restored jobvariables
&04: number of seconds during which the ARCHIVE.SAVE.FILE was open

## ARC0816

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0816 SUBTASK '(&00)' HAS TRANSFERRED '(&01)' MEGABYTES FOR '(&02)' FILES IN '(&04)' SECONDS

### Meaning

&00: number of the subtask (0..9, A..F)
&01: number of transferred megabytes
&02: number of saved or restored files
&04: number of seconds during which the ARCHIVE.SAVE.FILE was open

## ARC0817

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0817 ORDER '(&00)' IS ACCEPTED ON THE WORKSTATION '(&01)'

### Meaning

The workstation '(&01)' has accepted the order '(&00)'
coming from the server.
(&00): order (PREPROCESSING, POSTPROCESSING, PRE/POST PROCESSING)

## ARC0818

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0818 PRE/POST PROCESSING IS REFUSED BY THE WORKSTATION '(&00)'. PRE/POST PROCESSING WILL NOT BE PERFORMED

### Meaning

The workstation '(&00)' has refused the Pre/post processing order
coming from the server.

### Response

The client on workstation '(&00)' is not smart enough to perform the
pre/post processing, or the pre/post processing is not defined in the
client configuration file on that workstation.

## ARC0819

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0819 FILES SAVED MODIFIED SINCE '(&00)'

### Meaning

All files will be saved were changed since '(&00)'.

## ARC0820

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0820 DIRECTORY '(&00)' SAVED ON VSN '(&01)'

## ARC0821

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0821 'SAVE-PLAM-INFO=*YES' WILL BE IGNORED FOR MIGRATED FILES

### Meaning

SAVE-PLAM-INFO=*YES will be ignored for currently migrated files.

## ARC0822

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0822 ALIAS JV NAME SUBSTITUTION: '(&00)' BECOMES '(&01)'. PROCESSING CONTINUES

### Meaning

The specified alias jv name (&00) has been translated into the
real jv name (&01).

## ARC0825

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0825 SUBTASK '(&00)' HAS TRANSFERRED '(&01)' PAM PAGES FOR '(&02)' FILES AND '(&03)' JVS WITH 256K-BLOCKING IN '(&04)' SECONDS

### Meaning

&00: number of the subtask (0..9, A..F)
&01: number of transferred PAM-pages
&02: number of saved or restored files
&03: number of saved or restored jobvariables
&04: number of seconds during which the ARCHIVE.SAVE.FILE was open

## ARC0826

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0826 SUBTASK '(&00)' HAS TRANSFERRED '(&01)' MB FOR '(&02)' FILES WITH 256K-BLOCKING IN '(&04)' SECONDS

### Meaning

&00: number of the subtask (0..9, A..F)
&01: number of transferred megabytes
&02: number of saved or restored files
&04: number of seconds during which the ARCHIVE.SAVE.FILE was open

## ARC0830

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0830 SAVE/EXPORT TO A NK4 DISK IS MADE. THE VALUE OF 'BLOCK-SIZE' OPERAND IS INCREMENTED BY 1

### Meaning

In case of SAVE/EXPORT to a native NK4 disk, the value of BLOCK-SIZE
operand must be odd. The given value has been incremented by 1.

## ARC0831

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0831 SECURE RELEASE PROBLEM. RUN CONTINUES

## ARC0832

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0832 ERROR '(&00)' ON FILE '(&01)' DURING 'EXCHANGE'. PROCESSING CONTINUES

### Meaning

The error (&00) occurs during the EXCHANGE processing of file (&01).
The EXCHANGE processing continues with the next file.
(&00): DMS code or ARCHIVE message number.
(&01): file name.

## ARC0833

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0833 INTERNAL ERROR '(&00)' DURING HSMS-API PROCESSING

### Meaning

An error has been detected during the processing of a HSMS-API run
More information are available in the SERSLOG file.

## ARC0834

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0834 VOLUME '(&00)' ALREADY IN DIRECTORY. VOLUME CONTENTS WILL NOT BE USED

## ARC0836

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0836 MEMORY POOL SATURATION DETECTED BY '(&00)'

## ARC0837

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0837 NO DEVICE DEPOT FOR LOCATION '(&00)'. RUN CONTINUES WITH DEFAULT LOCATION

## ARC0838

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0838 SAVE-PLAM-INFO PARAMETER NOT AVAILABLE FOR A ILAM VERSION LOWER THAN V03.2A

### Meaning

Normal processing continues but the RESTORE-LIBRARY-ELEMENTS will not be
possible on this library.

### Response

Change the SAVE-PLAM-INFO parameter in the parameter file of ARCHIVE.

## ARC0839

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0839 TAPE INITIALISATION IS IGNORED FOR VOLUME '(&00)'

### Meaning

During a COPY-SAVE-FILE or COPY-NODE-SAVE-FILE with SAVE-FILE = *NEW(...),
the vsn (&00) given to ARCHIVE for output is marked to be initialized.
The tape initialization is ignored by ARCHIVE and the run continues.
This tape can be rejected if the user has not the TSOS privilege.

## ARC0840

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0840 A BACKUP BY CATALOG MODIFICATION DATE IS NOT SUPPORTED BY THE CLIENT VERSION ON WORKSTATION '(&00)' A FULL SAVE IS EXECUTED INSTEAD.

### Meaning

This client software version on workstation '(&00)' is not able
to perform backup by catalog modification date.

### Response

Please upgrade this client software to a newer one or use full or
partial backups.

## ARC0841

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0841 RETENTION PERIOD POSSIBLY NOT UPDATED. REASON '(&00)'

### Meaning

Error during retention period update, the process is not completed.
Risk of inconsistency between different values
The reasons are:
01: MAREN not present
02: bad MAREN version. At least MAREN V7.0B is needed
03: MAREN error
04: DISK error. The catalog entry of your save file is not updated
05: Update problem
06: SFID does not exist
07: directory read problem
08: directory write problem

### Response

Try a new //MODIFY-ARCHIVE with RETPD-EXTENSION = 0

## ARC0842

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0842 SAVE FILE '(&00)' RETENTION PERIOD IS OBSOLETE

### Meaning

The retention period of the SFID '(&00)' was obsolete.
For RETPD-EXTENSION > 0 the retention period has been increased
but the value is still obsolete.
For RETPD-EXTENSION < 0 the retention period has not been changed.

### Response

If needed, change the retention period again.

## ARC0843

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0843 ERROR '(&00)' WHEN TRYING TO CONNECT SUBSYSTEM HSMS. NO ACCOUNTING POSSIBLE

## ARC0844

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0844 WARNING '(&00)' DETECTED AT LOCATION '(&01)'

## ARC0845

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0845 INVALID REPAIRED REPOSITORY FILE '(&00)'

### Meaning

Some invalid records remain in the directory file.

### Response

Check missing VSN(S) to complete "SAVE_VERSION / SAVE_FILE",
erase the repository file and retry LIST statement with all VSNS

## ARC0846

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0846 RENAMING PROCESSING DOES NOT APPLY ON THIS OBJECT

### Meaning

For some objects, the renaming is useless or not applicable.
For Informix objects, Exchange and SQL-Server V7.0 the restore is aborted

## ARC0847

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0847 VSN '(&00)' GIVEN BY MAREN IS REJECTED BY ARCHIVE. RUN CONTINUES

### Meaning

Inconsistency between MAREN catalog and ARCHIVE directory detected:
A free tape is proposed by MAREN althought it is already registrated in
ARCHIVE directory. Following causes results in refusal of the tape:
- the tape is already assigned to a save version
- the tape is marked as 'UNUSABLE'
- the expiration date of the tape has not been expired until now
Run continues with a new volume.
The run is aborted after several wrong tape proposals.

### Response

Please clarify the inconsistency.
Repair the inconsistency with DIRCONV (//UPDATE-VOLUME-CATALOG).

## ARC0848

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0848 PLAM ERROR '(&00)' DURING PLAM INFORMATION SAVE

### Meaning

A PLAM error (&00) has occurred. The processing for saving of information
on the elements of the library is aborted.
Normal processing continues but the RESTORE-LIBRARY-ELEMENTS will not be
possible on this library.

## ARC0849

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0849 ERROR DURING PLAM INFORMATION SAVE

### Meaning

The processing for saving of information on the elements of the library is
aborted.
Normal processing continues but the RESTORE-LIBRARY-ELEMENTS will not be
possible on this library.

## ARC0850

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0850 PREPARE TAPE '(&00)' FOR ARCHIVE RUN (ACCESS='(&01)')

### Meaning

This message supports 'pre-restore' of volumes by ROBAR and CentricStor.

## ARC0851

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0851 END OF S0 ONLINE BACKUP. BACKUP FROM S2 LEVEL BEGINS

## ARC0852

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

ARC0852 SHARUPD CONFLICT ON DIRECTORY '(&00)' HAS LASTED TOO LONG. REPLY (T=TERMINATE; C=CONTINUE)?

### Meaning

ARCHIVE has retried the opening of the directory for the maximum time
limit since giving message ARC0805. The operator is asked to terminate
the archive run or to continue (for the same time limit).

### Response

Depending on the reason of the sharupd conflict, the operator may
try to unlock the directory and continue (.C) or terminate (.T) the
ARCHIVE run.

## ARC0853

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0853 SHARUPD CONFLICT ON CHECKPOINT FILE '(&00)'. PROCESS WAITS

### Meaning

The process has to wait until the checkpoint file becomes free.

## ARC0854

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : NO

ARC0854 ARCHIVE LOGGING FILE '(&00)' OPENED

### Meaning

(&00): file name.

## ARC0855

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : NO

ARC0855 ARCHIVE LOGGING FILE '(&00)' CLOSED

### Meaning

(&00): file name.

## ARC0856

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ARC0856 ARCHIVE TAPE DRIVER TASK STARTED BY TSN '(&00)'

### Meaning

An ARCHIVE tape driver task has been created by the task with TSN (&00).

## ARC0857

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ARC0857 ARCHIVE TAPE DRIVER TASK TERMINATED

### Meaning

The ARCHIVE tape driver task has terminated processing.

## ARC0859

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ARC0859 TAPE INITIALISATION WAS NOT DONE FOR VOLUME '(&00)'

### Meaning

The volume (&00) given to ARCHIVE for output is marked to be initialized
but the init processing has failed.
The run continues but the volume can be rejected if the user has not the
TSOS privilege.

## ARC0860

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0860 DEADLOCK DETECTED. RECOVERY PROCESS STARTED

## ARC0861

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0861 DEADLOCK SUSPECTED. RECOVERY PROCESS STARTED

## ARC0862

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0862 DEADLOCK RECOVERY SUCCESSFULL

## ARC0869

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0869 NODE-ID '(&00)' NOT PRESENT IN SYSDAT '(&01)', PROCESSING CONTINUES WITH NFS

### Meaning

Without node entry in SYSDAT, processing switches to NFS.

## ARC0870

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0870 CLIENT '(&00)' WARNING: '(&01)'

## ARC0871

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0871 CLIENT WARNING: '(&00)' FOR FILE '(&01)'

## ARC0872

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0872 COPY-SAVE-FILE SINGLE-TO-SEVERAL WAS IMPOSSIBLE. SINGLE-TO-SINGLE IS USED INSTEAD

### Meaning

The parameter SINGLE-TO-SEVERAL=*YES was specified for a COPY-SAVE-FILE
where the destination save-file is not several svids.

## ARC0873

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0873 THE POSTPROCESSING HAS FAILED ON WORKSTATION '(&00)'

## ARC0874

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0874 A POSIX OR NFS FILE SYSTEM IS FULL. RUN ABORTED

### Meaning

A POSIX or NFS file system is full.
Run aborted.

### Response

Check the concerned POSIX and NFS file systems.
Restart the run after correction.

## ARC0875

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0875 WARNING: USERID OF CALLER '(&00)' DOES NOT EXIST.

### Meaning

A HSMS request was processed by the master host.
The caller userid doesn't exist at the home pubset.
Files/JVs are not processed for those coowning is required.

### Response

Add userid to the home pubset at the master host.
Repeat the run in case of errors.

## ARC0876

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0876 WARNING: RESTORED DIRECTORY CONTAINS NOT THE LATEST SAVE VERSION!

### Meaning

ARCHIVE has found additional files on the specified tape behind the
restored directory. This additional files are not registered in
the restored directory.
Hence it is not possible to restore all files with its latest
version.

### Response

Please check if you have specified the tape containing the
latest save version of the directory. If there is a newer save
version of the directory on another tape, repeat the run with
this one.

## ARC0877

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0877 WARNING: '(&00)'

## ARC0878

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0878 WARNING: FILE CANNOT BE PROCESSED BECAUSE OF COMPATIBILITY PROBLEMS

## ARC0879

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0879 FILE TO BE RESTORED IS PROTECTED. FILE NOT REPLACED

### Meaning

The RESTORE statement specified REPLACE=*YES(PROTECTION-RESPECTED=*ALL)
and the file is protected. The file is not replaced.
The message is associated with the file in error on parameter
SNR=*NO (ARCHIVE). For another files this message will be
suppressed.
Processing continues.

## ARC0880

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0880 PLAM-INFO CANNOT BE OBTAINED FOR ENCRYPTED LIBRARY

### Meaning

Library is saved without PLAM-INFO.
Full save is executed instead of partial save.

## ARC0881

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0881 SAVE VERSION IN ARCHIVE HAS EARLIER EXPIRATION DATE THAN FILE '(&00)'

### Meaning

The save version in the archive has an earlier FILE-EXPIRATION-DATE
than the file (&00) that was archived.

### Response

Increase FILE-EXPIRATION-DATE of the save version
to protect against early deletion.

## ARC0882

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ARC0882 SAVE VERSION IN ARCHIVE HAS EARLIER EXPIRATION DATE THAN JV '(&00)'

### Meaning

The save version in the archive has an earlier FILE-EXPIRATION-DATE
than the job variable (&00) that was archived.

### Response

Increase FILE-EXPIRATION-DATE of the save version
to protect against early deletion.

## ARC0883

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ARC0883 WARNING: REPORT WAS SHORTENED DUE TO LACK OF MEMORY SPACE

### Meaning

Due to lack of memory space the report was shortened by
the list of the saved PLAM library elements.

### Response

If a full output report is needed
Please reduce number of LMS files to be saved per run or
inform system administrator to increase MEMORY-POOL-SIZE in
parameter file SYSPAR.ARCHIVE.xxx.

## ARC0900

Destination: CONSOLE Routing code: U Weight: 70

Warranty : NO

ARC0900 INTERNAL ARCHIVE SUBTASK ERROR IN '(&00)'

### Meaning

A severe internal error was detected in a subtask. A system dump is
offered to the operator.
(&00): location of the error.

### Response

Take system dump and send it together with console report and ARCHIVE
report to diagnosis team.

## ARC0901

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0901 READ ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. FILE IN PROCESS IS '(&02)'. REPLY (0=SKIP FILE; 1=SKIP BLOCK)?

### Meaning

ARCHIVE block number (&00) on input VSN (&01) could not be read. The name
of the affected file is (&02).
(&00): block number (hexadecimal)

### Response

.0: the file is skipped and the run continues with the next file.
.1: a dummy PAM page is written instead of the not readable ARCHIVE block.
Processing of the file continues in spite of the error.

## ARC0902

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0902 FORMAT OR BLOCK NUMBER ERROR FOR BLOCK '(&00)' ON VSN '(&01)'. FILE IN PROCESS IS '(&02)'. REPLY (0=SKIP FILE; 1=CONTINUE FILE)?

### Meaning

The ARCHIVE block number (&00) on input volume with VSN (&01) is not of
the expected format, or the block number was wrong (in this case the
message ARC0778 preceeds this message).
(&00): block number (hexadecimal)
(&01): VSN of volumes
(&02): The name of the file just read.

### Response

.0: processing of this file is terminated. The run continues with the next
file.
.1: processing of this file is continued in spite of the error.

## ARC0903

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0903 OPEN ERROR '(&00)' ON INPUT VSN '(&01)'. REPLY (0=SKIP TAPE; 1=SKIP LABEL)?

### Meaning

During checking of the labels of input tape (&01) the I/O-error
with error code (&00) happened.

### Response

.0: the tape is skipped and the ARCHIVE run continues with the next tape.
.1: it is tried to read the tape in spite of this error. Label checks may
be incomplete. In this case one or more device error messages will
appear on the operator's console. They have to be answered.

## ARC0904

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

ARC0904 VSN (&00) IS NO MORE FREE IN ARCHIVE POOL. PLEASE ASSIGN ANOTHER VSN

### Meaning

The VSN (&00) which the operator entered to message DMS0591, is marked
as not available in the ARCHIVE pool or is already reserved by another
subtask.

### Response

Enter any other VSN to the following message DMS0591.

## ARC0905

Destination: CONSOLE Routing code: U Weight: 70

Warranty : NO

ARC0905 $REQM OR ENAMP ERROR IN MODULE 'FAFE'

### Meaning

Request memory or enable memory pool error occurred.
Therefore the subtask is terminated abnormally.

## ARC0906

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0906 WRONG BLOCK NUMBER FOUND INSTEAD OF '(&00)' ON INPUT VSN '(&01)'. REPLY (0=ABANDON VOLUME; 1=CONTINUE PROCESSING)?

### Meaning

The position of input VSN (&01) got lost. A block with ARCHIVE data block
number (&00) was expected but the block just read in has another number.
(&00): block number (hexadecimal)

### Response

.0: processing of this volume is terminated. The run continues
with the next tape.
.1: processing of this volume is continued in spite of the error.

## ARC0907

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0907 DMS ERROR '(&00)' DURING MOUNT OF TAPE FOR ARCHIVE. REPLY (T=TERMINATE ARCHIVE WITH ERROR; C=CONTINUE WITH ANOTHER VSN)?

### Meaning

During mount of an ARCHIVE tape DMS error (&00) occurred.

### Response

.T: terminate ARCHIVE with error
.C: continue ARCHIVE with another VSN.

## ARC0908

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0908 DMS ERROR '(&00)' DURING MOUNT OF INPUT VSN '(&01)' FOR ARCHIVE. REPLY (T=TERMINATE ARCHIVE WITH ERROR; C=CONTINUE WITH NEXT VSN; R=RETRY)?

### Meaning

DMS error (&00) occurred during mount of volume (&01) for ARCHIVE.

### Response

.T: terminate ARCHIVE with error
.C: continue ARCHIVE with the next input VSN
.R: retry with same VSN; volume is ready

## ARC0909

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

ARC0909 SYSTEM ERROR DURING INITIALISATION OF ARCHIVE SUBTASK ENVIRONMENT

### Meaning

A system error has occurred during the creation of the environment
for the ARCHIVE subtask. The subtask terminated abnormally.

## ARC0910

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ARC0910 LENGTH OF FAF3 NOT CORRECT OR FAF3 HAS BEEN OVERWRITTEN

### Meaning

A system error has occurred during the creation of the environment
for the ARCHIVE subtask. The subtask terminated abnormally.

## ARC0911

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ARC0911 DMS ERROR '(&00)' DURING '(&01)'-ACCESS TO FILE '(&02)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The file cannot be processed due to the specified error or the recalled
file cannot be unlocked.

### Response

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## ARC0912

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ARC0912 ERROR '(&00)' WHEN CALLING '(&01)' IN MODULE '(&02)'

### Meaning

The specified system interface reports the specified error to a module
of the ARCHIVE control program.

### Response

Interpret the error code according to the interface documentation.
If necessary, pass statement report and SYSLST log for diagnosis.

## ARC0913

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ARC0913 TASK IS WAITING '(&02)' SECONDS FOR INPUT TAPE '(&01)' BECAUSE OF DMS ERROR '(&00)'.

### Meaning

DMS error (&00) occurred during mount of input volume (&01).
Task is waiting until tape is available, the maximum waiting time is
(&02) seconds.
If the tape is not available until the waiting time is exceeded,
the operator may destinate the further proceeding by reply to the
message ARC0908.
This behaviour should facilitate the automatic processing
(&00): DMS error (055F: Volume could not be allocated)
(&01): VSN of input tape
(&02): maximum waiting time (DIALOG-/BATCH-REQUEST-TIME but
at most 7200 seconds)

### Response

Wait until tape is available or make tape accessible.
Response to the message ARC0908 after time out.

## ARC0914

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

ARC0914 ARCHIVE REPORTS:'(&00)'.

### Meaning

This is a general ARCHIVE message.
It will be given only in those special cases where no specific
ARCHIVE message number exists.
The meaning depends on the insert.

## ARC0999

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

ARC0999 MORE THAN (&00) WRONG REPLIES. '0' OR 'T' IS ASSUMED

### Meaning

An ARCHIVE message with expected reply had been issued.
The operator has given more than (&00) times an incorrect
answer. The ARCHIVE run is continued as if the operator
had given '0' or 'T' as answer.

## ARC9900

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ARC9900 ERROR X'(&00)' DURING EXECUTION OF MACRO CMD

### Response

See the manual 'Executive Macros' for explanation of the
return code.

## ARC9901

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ARC9901 INSERT-TEXT = '(&00)'

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages