## GPR0100

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

GPR0100 INTERNAL ERROR IN PRNGD-SUBSYSTEM-INITIALIZATION; ERROR CODE (&00)

### Meaning

Some operating resources aren't available. These resources are
according to the error code:
0000 - No memory space for subsystem object available.
0001 - No memory space for PRNGD error trace available.
0002 - No memory space for PRNGD event trace available.
0003 - No memory space for task lock object available.
0004 - Task lock can't be created.
0005 - Server bourse can't be created.
0006 - No memory space for file object available.
0007 - No memory space for PRNG object available.
0008 - Error at reading configuration file.
0009 - Error at initialization of PRNG.
0010 - Error at accessing seed file.
0011 - Error at connection of holder task with SDF.
0012 - Error at notification of DSSM.

### Response

None.

## GPR0105

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

GPR0105 ERROR IN DSSM-PRNGD-INTERFACE; ERROR CODE (&00)

### Meaning

The cause for this message is according to the error code:
0001 - A notification of DSSM failed.
0002 - Some internal error occurred during restart of PRNGD subsystem.

### Response

None.

## GPR0110

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

GPR0110 THE SUBSYSTEM PRNGD IS READY

### Meaning

The subsystem PRNGD is as far initialized that it can fulfill
requests for (pseudo) random numbers.

### Response

None.

## GPR0150

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

GPR0150 THE FOLLOWING SYSTEM DUMP OF TASK GPR1 SERVES AS DIAGNOSTIC AID

### Meaning

If the reason for the occurred problem isn't already clear from the
previous message, then take the dump please and send it to your support.

### Response

None.

## GPR9999

Destination: USER-TASK Routing code: Weight: 09

Warranty : NO

GPR9999 ENGLISH

### Meaning

Identifier for selected message language in BS2000.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages