## OMYCCXX

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMYCCXX DCAM RETURN CODE X'CCXX....': CALL REJECTED BY THE SYSTEM EXIT ROUTINE

### Meaning

Selfexplanatory.

### Response

Ask the system administrator for the meaning of the second byte.

## OMYCC00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMYCC00 DCAM RETURN CODE X'CC00....': CALL REJECTED BY THE SYSTEM EXIT ROUTINE

### Meaning

Selfexplanatory.

### Response

Not given.

## OMYFFFF

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMYFFFF DCAM LOSCON CONTINGENCY RETURN CODE

### Meaning

Meaning of the right byte of register 6:
00, Connection cleared down by partner.
08, Processing error (e.g. X.25 malfunction).
0C, Partner no longer available or data station failure.
10, Connection aborted by network administrator.
14, Connection interrupted in network.
18, Network error.
20, Warning before connection loss.
28, Connection closed by system administration.
2C, Error in connection element of station services.

### Response

34: Error in station service protocol.
38, Error in transport system.
40, Error in connection message from station service for user.
50, Proposed transport services class not accepted by partner.
54, Proposed priority in data network not accepted by partner.
58, Disconnection due to shortage of DCM memory (too many negative
transport acknowledges not fetched).
5C, VTSU of partner not active.
60, Transport connection closed due to protocol error of partner.
1C/24/30/3C/44/48/4C, Reserved.
Reestablish the connection; if necessary inform the network
administrator.

## OMY0CAC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CAC DCAM RETURN CODE X'0CAC....': APPLICATION NAME DOES NOT START WITH '$'

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CA0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CA0 DCAM RETURN CODE X'0CA0....': DISCONNECTION BY PARTNER DUE TO PROTOCOL ERROR OR INCONSISTENCY

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CA4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CA4 DCAM RETURN CODE X'0CA4....': OPTCD=EXPRESS NOT ALLOWED SINCE NOT AGREED UPON WITH PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CA8

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CA8 DCAM RETURN CODE X'0CA8....': UNRECOVERABLE UCON ERROR

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CBC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CBC DCAM RETURN CODE X'0CBC....': INTERNAL UCON ERROR (AUTHENTICITY CHECK NOT POSSIBLE)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CB0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CB0 DCAM RETURN CODE X'0CB0....': PROCESSOR NAME DOES NOT DESIGNATE THE OWN (HOME) PROCESSOR

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CB4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CB4 DCAM RETURN CODE X'0CB4....': SUPERVISOR TASK CAN NOT BE CREATED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CB8

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CB8 DCAM RETURN CODE X'0CB8....': WRONG CONNECTION IDENTIFIER (CID) FOR THIS OPERATION IDENTIFIER (OPID)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CCC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CCC DCAM RETURN CODE X'0CCC....': PROTOCOL INCONSISTENCY

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CC0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CC0 DCAM RETURN CODE X'0CC0....': NO FREE ENTRY IN CONSOLE NAME TABLE AVAILABLE

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CC4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CC4 DCAM RETURN CODE X'0CC4....': DCAM VERSION LESS THAN 10

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CC8

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CC8 DCAM RETURN CODE X'0CC8....': PARTNER IS NO CHIP CARD TERMINAL

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CD0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CD0 DCAM RETURN CODE X'0CD0....': SUBSYSTEM FOR CHIP CARD CHECK NOT AVAILABLE

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0CD4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0CD4 DCAM RETURN CODE X'0CD4....': ERROR IN KVP PROTOCOL

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C0C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C0C DCAM RETURN CODE X'0C0C....': A CONNECTION REQUEST FROM THIS PARTNER IS ALREADY ENQUEUED (NO YOPNCON OPTCD=ACQUIRE POSSIBLE)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C00 DCAM RETURN CODE X'0C00....': CALL REJECTED DUE TO CURRENT STATE OF PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C04 DCAM RETURN CODE X'0C04....': PARTNER IS NOT CONNECTED TO THE DCAM APPLICATION (INVALID CID)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C08

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C08 DCAM RETURN CODE X'0C08....': PARTNER IS ALREADY CONNECTED TO THE DCAM APPLICATION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C1C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C1C DCAM RETURN CODE X'0C1C....': FORCED DISCONNECTION RESP. DISCONNECTION REQUESTED BY PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C10

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C10 DCAM RETURN CODE X'0C10....': DIP CONTROL BLOCK NOT ACTIVE (INVALID DID)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C14

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C14 DCAM RETURN CODE X'0C14....': INVALID LID

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C18

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C18 DCAM RETURN CODE X'0C18....': DISCONNECTION DUE TO USER REQUEST OR YCLSCON

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C2C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C2C DCAM RETURN CODE X'0C2C....': PARTNER IS IN STATE CA. YRECEIVE OPTCD=SPEC NOT ALLOWED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C20

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C20 DCAM RETURN CODE X'0C20....': PARTNER IS IN STATE CS AND THE TRANSITION TO STATE CA IS NOT YET COMPLETED (OR VICE VERSA)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C24

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C24 DCAM RETURN CODE X'0C24....': PARTNER IS IN STATE CS WITH OUTSTANDING YRECEIVE CALLS. THE REQUESTED TRANSITION TO STATE CA IS NOT ALLOWED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C28

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C28 DCAM RETURN CODE X'0C28....': PARTNER IS IN STATE CS FOR ANOTHER PROCESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C3C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C3C DCAM RETURN CODE X'0C3C....': OPTCD=EXPRESS NOT ALLOWED WITH EDIT=SYSTEM

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C30

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C30 DCAM RETURN CODE X'0C30....': MESSAGE TOO LONG (GREATER THAN MAXLN=)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C34

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C34 DCAM RETURN CODE X'0C34....': POSITION OF THE DISTRIBUTIONCODE EXCEEDS THE MAXIMUM MESSAGE LENGTH

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C38

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C38 DCAM RETURN CODE X'0C38....': SEQUENCE NUMBER ALREADY IN USE AND ACKNOWLEDGE PROCESSING NOT COMPLETED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C4C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C4C DCAM RETURN CODE X'0C4C....': PARTNER NOT ACCESSIBLE (THE APPLICATION IS NOT OPENED)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C40

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C40 DCAM RETURN CODE X'0C40....': CONNECTION REQUEST REJECTED BY PARTNER WITHOUT SPECIFICATION OF A REASON

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C44

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C44 DCAM RETURN CODE X'0C44....': INVALID COMBINATION OF DEPROT= AND EDIT=

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C48

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C48 DCAM RETURN CODE X'0C48....': SYSTEM TIMEOUT FOR CONNECTION REQUEST

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C5C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C5C DCAM RETURN CODE X'0C5C....': CONNECTION REQUEST REJECTED BY PARTNER (YREJLOG)

### Meaning

Meaning of the third byte (only for ISO connection):
18, Erroneous connection request.
2C, Partner rejects connection request.
40, Connection request rejected.

### Response

Not given.

## OMY0C50

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C50 DCAM RETURN CODE X'0C50....': PARTNER DOES NOT PROCESS CONNECTION REQUESTS (THE APPLICATION IS IN STOP STATE)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C54

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C54 DCAM RETURN CODE X'0C54....': PARTNER DOES NOT ACCEPT CONNECTION REQUESTS (THE APPLICATION IS CREATED WITH ATTR=NLOGON)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C58

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C58 DCAM RETURN CODE X'0C58....': INVALID LOGON-PASSWORD (LOGPW=)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C6C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C6C DCAM RETURN CODE X'0C6C....': ERROR IN ACTIVATION OF VTSU SUPPORT OF PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C60

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C60 DCAM RETURN CODE X'0C60....': PARTNER CHARACTERICS NOT ACCEPTED BY PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C64

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C64 DCAM RETURN CODE X'0C64....': ERROR IN STATION SERVICE PROTOCOL

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C68

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C68 DCAM RETURN CODE X'0C68....': PARTNER DOES NOT PROCESS CONNECTION REQUESTS. A CONNECTION REQUEST BY PARTNER FOLLOWS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C7C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C7C DCAM RETURN CODE X'0C7C....': RESERVED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C70

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C70 DCAM RETURN CODE X'0C70....': PARTNER BELONGS TO ANOTHER DCAM-APPLICATION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C74

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C74 DCAM RETURN CODE X'0C74....': DIP CONTROL BLOCK DOES NOT ADDRESS A DCG CONTROL BLOCK

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C78

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C78 DCAM RETURN CODE X'0C78....': CONNECTION TERMINATED BY PARTNER OR SYSTEM IMMEDIATELY AFTER COMPLETION OF CONNECTION REQUEST

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C8C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C8C DCAM RETURN CODE X'0C8C....': INVALID PASSWORD (UCON)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C80

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C80 DCAM RETURN CODE X'0C80....': SYNTAX ERROR IN CONNECTION LETTER (UCON)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C84

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C84 DCAM RETURN CODE X'0C84....': UNKNOWN AUTHORIZATION NAME (UCON)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C88

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C88 DCAM RETURN CODE X'0C88....': AUTHORIZATION NAME ALREADY IN USE (UCON)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C9C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C9C DCAM RETURN CODE X'0C9C....': CONNECTION REQUEST REJECTED BY THE SYSTEM ADMINISTRATION

### Meaning

Selfexplanatory.

### Response

Ask the system administrator.

## OMY0C90

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C90 DCAM RETURN CODE X'0C90....': PROPOSED TRANSPORT SERVICE CLASS REJECTED BY PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C94

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C94 DCAM RETURN CODE X'0C94....': PROPOSED NET PRIORITY REJECTED BY PARTNER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0C98

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0C98 DCAM RETURN CODE X'0C98....': GENERAL ERROR (E.G. X.25 FAILURE)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0000 DCAM RETURN CODE X'0000....': CALL COMPLETED OR ACCEPTED

### Meaning

Meaning of the third byte:
00, Message fitts in buffer resp. calling task is the primary process.
04, Message too long resp. calling task is the secondary process.
08, Message too long; remainder is kept.
10, VTSU control block not transferred; connection works without VTSU
control block.
40, State of TD9763 not completely transferred.
80, State of TD9763 completely transferred.
In the forth byte the single bits have the following meaning:
01, Message is a letter.
02, GO signal.

### Response

04/08: Transport acknowledge positive/negative.
10, An express message has arrived.
20/40/80, Element/Subgroup/Group of message arrived (NEA connection).
20, More data of message follows (ISO connection).
80, No more data of message follows (ISO connection).
Not given.

## OMY0400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0400 DCAM RETURN CODE X'0400....': CALL COMPLETED WITH WARNING

### Meaning

Meaning of the third byte:
04, Contradiction in code specifications.
08, No letter has arrived (OPTCD=NQ).
0C, No LOGON request in queue.
10, Time out (TOVAL=).
14/18, System time out (/BCTIMES).
20, Connection letter truncated.
24, Error in VTSU.
28, Partner characteristic truncated.
2C, Edited message too long.

### Response

30: Invalid edit options.
34, Call terminated by YRESET.
44, No printer operable for output.
48, Invalid control character (NL) entered in extended line mode.
The meaning of the forth byte see under 'OMY0000'.
Not given.

## OMY080C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY080C DCAM RETURN CODE X'080C....': DCAM APPLICATION ALREADY OPENED AND ONLY USABLE BY ONE TASK

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0800

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0800 DCAM RETURN CODE X'0800....': CALL REJECTED DUE TO CURRENT STATE OF THE DCAM APPLICATION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0804

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0804 DCAM RETURN CODE X'0804....': DCAM APPLICATION NOT OPENED BY THE CALLING TASK (INVALID AID)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0808

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0808 DCAM RETURN CODE X'0808....': DCAM APPLICATION ALREADY OPENED AND ATTR=NSHARE SPECIFIED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY081C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY081C DCAM RETURN CODE X'081C....': DISTRIBUTION NAME OR DISTRIBUTION CODE ALREADY USED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0810

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0810 DCAM RETURN CODE X'0810....': DCAM APPLICATION ALREADY OPENED BY THE CALLING TASK

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0814

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0814 DCAM RETURN CODE X'0814....': DCAM APPLICATION ALREADY OPENED AND VERIFY=PRIMARY SPECIFIED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0818

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0818 DCAM RETURN CODE X'0818....': DCAM APPLICATION NOT OPENED AND VERIFY=SECONDARY SPECIFIED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY082C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY082C DCAM RETURN CODE X'082C....': FORCED TERMINATION OF DCAM APPLICATION DUE TO INVALID CONTINGENCY OR EVENT ITEM SPECIFIED BY THE PRIMARY PROCESS.

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0820

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0820 DCAM RETURN CODE X'0820....': FORCED TERMINATION OF DCAM APPLICATION (WARNING)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0824

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0824 DCAM RETURN CODE X'0824....': FORCED TERMINATION OF DCAM APPLICATION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0828

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0828 DCAM RETURN CODE X'0828....': FORCED TERMINATION OF DCAM APPLICATION DUE TO DCAM ERROR

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY083C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY083C DCAM RETURN CODE X'083C....': TERMINATION OF THE DCAM APPLICATION DUE TO REQUEST OF THE SECONDARY PROCESS.

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0830

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0830 DCAM RETURN CODE X'0830....': FORCED TERMINATION OF DCAM APPLICATION DUE TO INVALID CONTINGENCY OR EVENT ITEM SPECIFIED BY THE SECONDARY PROCESS.

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0834

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0834 DCAM RETURN CODE X'0834....': FORCED TERMINATION OF DCAM APPLICATION DUE TO TERMINATION OF THE PRIMARY PROCESS.

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0838

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0838 DCAM RETURN CODE X'0838....': TERMINATION OF THE DCAM APPLICATION DUE TO REQUEST OF THE PRIMARY PROCESS.

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY084C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY084C DCAM RETURN CODE X'084C....': TOO MANY DCAM APPLICATIONS OPENED BY THIS TASK

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0840

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0840 DCAM RETURN CODE X'0840....': TOO MANY SIMULTANEOUS CALLS OF THE SAME TYPE FOR THIS TASK

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0844

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0844 DCAM RETURN CODE X'0844....': DCAM APPLICATION NOT ACTIVE

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0848

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0848 DCAM RETURN CODE X'0848....': INVALID PASSWORD (USEPW=)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY085C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY085C DCAM RETURN CODE X'085C....': TOO MANY NOT PREDEFINED DCAM APPLICATIONS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0850

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0850 DCAM RETURN CODE X'0850....': TOO MANY NOT PREDEFINED DCAM APPLICATIONS FOR A TASK

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0854

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0854 DCAM RETURN CODE X'0854....': INVALID PASSWORD WHEN PASSWORD IN RDF GIVEN

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0858

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0858 DCAM RETURN CODE X'0858....': DCAM APPLICATION OPENED BY OTHER SUBSYSTEM

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0860

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0860 DCAM RETURN CODE X'0860....': TOO MANY CONNECTIONS FOR NOT PREDEFINED DCAM APPLICATION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY0864

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY0864 DCAM RETURN CODE X'0864....': DCAM VERSION DIFFERENT FROM THE SPECIFICATION OF THE PRIMARY PROCESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY100C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY100C DCAM RETURN CODE X'100C....': DCM TERMINATION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1000 DCAM RETURN CODE X'1000....': CALL REJECTED DUE TO CURRENT STATE OF THE DATA COMMUNICATION SYSTEM (DCM)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1004 DCAM RETURN CODE X'1004....': DCM MEMORY SHORTAGE

### Meaning

Meaning of the third byte:
04, BCAM: Retry i/o later.
08, BCAM: Memory shortage.
0C, DCAM: Wait for GO signal.
20, DCAM: No control block available.
24, DCAM: No ID entry available.
28, DCAM: No memory available ($REQM).
2C, DCAM: Overload in partner system.
30, DCAM: Too many events not fetched.

### Response

Not given.

## OMY1008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1008 DCAM RETURN CODE X'1008....': DCM TERMINATION (WARNING)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1010 DCAM RETURN CODE X'1010....': DCM NOT ACTIVE

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1014 DCAM RETURN CODE X'1014....': DCM ERROR

### Meaning

Meaning of the third byte:
04, BCAM: Unknown BCINF return code.
08, BCAM: Unknown APINF return code.
0C, BCAM: Unknown STINF return code.
10, BCAM: Unknown return code.
The forth byte contains the unknown BCAM return code.

### Response

Not given.

## OMY1020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1020 DCAM RETURN CODE X'1020....': DCAM TEMPORARY LOCKED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY140C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY140C DCAM RETURN CODE X'140C....': CALL MAY NOT BE GIVEN FROM APPLICATIONS WITH ATTR=NLOGON

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1400 DCAM RETURN CODE X'1400....': A CALL WAS USED IMPROPER

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1404

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1404 DCAM RETURN CODE X'1404....': CALL MAY NOT BE GIVEN FROM A SECONDARY PROCESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1408

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1408 DCAM RETURN CODE X'1408....': CALL MAY NOT BE GIVEN FROM APPLICATIONS WITH ATTR=NSHARE OR ATTR=(SHARE,NDISCO)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1410

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1410 DCAM RETURN CODE X'1410....': EQUAL CALLS WITH OPTCD=(ACQUIRE,ASY) OR OPTCD=(ACCEPT,ASY,SPEC) ARE ALREADY IN PROCESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1414

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1414 DCAM RETURN CODE X'1414....': DCAM APPLICATION HAS NO RIGHT FOR THIS CALL

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1418

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1418 DCAM RETURN CODE X'1418....': A SYNCHRONOUS CALL IS ALREADY ENQUEUED FOR THIS PROCESS (OPTCD=(Q,SYN))

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY180C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY180C DCAM RETURN CODE X'180C....': INVALID DCG CONTROL BLOCK ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1800

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1800 DCAM RETURN CODE X'1800....': CALL REJECTED DUE TO ERRONEOUS OPERANDS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1804

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1804 DCAM RETURN CODE X'1804....': INVALID APPLICATION CONTROL BLOCK ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1808

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1808 DCAM RETURN CODE X'1808....': INVALID CONNECTION CONTROL BLOCK ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY181C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY181C DCAM RETURN CODE X'181C....': INVALID DISNAME ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1810

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1810 DCAM RETURN CODE X'1810....': INVALID DIP CONTROL BLOCK ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1814

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1814 DCAM RETURN CODE X'1814....': INVALID EVENT NOTIFICATION CONTROL BLOCK ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1818

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1818 DCAM RETURN CODE X'1818....': INVALID APPNAME ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY182C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY182C DCAM RETURN CODE X'182C....': INVALID AREA ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1820

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1820 DCAM RETURN CODE X'1820....': INVALID PTNNAME ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1824

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1824 DCAM RETURN CODE X'1824....': INVALID CONTINGENCY IDENTIFIER ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1828

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1828 DCAM RETURN CODE X'1828....': INVALID EVENT ITEM IDENTIFIER ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY183C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY183C DCAM RETURN CODE X'183C....': INVALID PARTNER NAME

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1830

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1830 DCAM RETURN CODE X'1830....': INVALID AAREA ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1834

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1834 DCAM RETURN CODE X'1834....': INVALID DCAM APPLICATION NAME

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1838

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1838 DCAM RETURN CODE X'1838....': INVALID DISTRIBUTION CODE NAME

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY184C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY184C DCAM RETURN CODE X'184C....': AAREALN LESS THAN 8 OR AREALN IS 0

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1840

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1840 DCAM RETURN CODE X'1840....': INVALID PROCESSOR NAME

### Meaning

Possible reasons for the invalid processor name are:
a) processor name syntactical wrong.
b) processor not activated (/BCDAC or no /BCACT given).
c) processor unknown resp. not generated (/BCOUT or no /BCIN given).
d) route(s) to processor not activated (/BCDAC or no /BCACT given).
e) route(s) to processor unknown resp. not generated (/BCOUT or no
/BCIN given).

### Response

Not given.

## OMY1844

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1844 DCAM RETURN CODE X'1844....': CONNECTION CONTROL BLOCK ALREADY USED FOR ASYNCHRONOUS CALL

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1848

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1848 DCAM RETURN CODE X'1848....': SEQUENCE NUMBER EXCEEDS UPPER LIMIT

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY185C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY185C DCAM RETURN CODE X'185C....': UNRECOVERABLE ERROR IN VTSU

### Meaning

Meaning of the third byte:
00: EDIT parameter error (user buffer may be too small for the message
header with EDITIN=PHYS).
04, Invalid device header.
08, Message length is 0.
0C, VTSU not available.
10, Error in VTSU control block.
14, Message with error in NEABT protocol received.

### Response

Not given.

## OMY1850

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1850 DCAM RETURN CODE X'1850....': INVALID SUBFUNCTION

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1854

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1854 DCAM RETURN CODE X'1854....': INVALID PRONAME ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1858

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1858 DCAM RETURN CODE X'1858....': AREALN IS NEGATIVE

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY186C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY186C DCAM RETURN CODE X'186C....': CONTRADICTION BETWEEN ACB CONTROL BLOCK PARAMETERS AND ISO=Y

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1860

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1860 DCAM RETURN CODE X'1860....': INVALID DISTRIBUTION CODE LENGTH (CODELN=)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1864

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1864 DCAM RETURN CODE X'1864....': RESERVED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1868

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1868 DCAM RETURN CODE X'1868....': RESERVED

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY187C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY187C DCAM RETURN CODE X'187C....': INCONSISTENCY BETWEEN ROUTL= AND ROUTN=

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1870

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1870 DCAM RETURN CODE X'1870....': NO VTSU CONTROL BLOCK EXISTS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1874

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1874 DCAM RETURN CODE X'1874....': VTSU CONTROL BLOCK NOT ALLOWED (EDIT=USER)

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1878

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1878 DCAM RETURN CODE X'1878....': INVALID VCB ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY1880

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY1880 DCAM RETURN CODE X'1880....': INVALID ROUTL ADDRESS

### Meaning

Selfexplanatory.

### Response

Not given.

## OMY2000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY2000 DCAM RETURN CODE X'2000....': ILLEGAL ADDRESS

### Meaning

Possible reasons for the illegal address are:
a) invalid application control block (ACB) address.
b) invalid request control block (RPB) address.
c) request control block (RPB) used by asynchronous call.
d) invalid address or invalid contents of the parameter list.
e) invalid register number.

### Response

Not given.

## OMY2400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMY2400 DCAM RETURN CODE X'2400....': THE SUBSYSTEM DCAM IS NO (MORE) AVAILABLE

### Meaning

The Subsystem DCAM is not created or in HOLD resp. DELETE
state and the task has not yet executed any DCAM calls.

### Response

Not given.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages