## OMP0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0000 DEVICE NOT FOUND. COMMAND WAS NOT EXECUTED

### Meaning

No additional information.

### Response

Define the printer or use the correct device name.

## OMP0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0001 DEVICE LIMIT EXCEEDED. COMMAND WAS NOT EXECUTED

### Meaning

Printer limit exceeded for the current processor. Command could
not be executed.

### Response

Delete another printer or generate a new printer table.

## OMP0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0002 WRONG DUMP ADDRESS. MESSAGE COULD NOT BE TREATED BY THE STANDARD PROP

### Meaning

The standard PROP had found an error in the message. The message will be
sent to the operator.

### Response

None.

## OMP0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0003 ERROR ENTRY WITH ADDRESS (&00) COULD NOT BE FOUND

### Meaning

No additional information.

### Response

Correct the address.

## OMP0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0004 (&00) ERROR (&01) OCCURRED AT ADDRESS (&02) IN MODULE (&03)

### Meaning

An internal call to PROP or a call to the operating system
contains an error. The name of the call is (&00). (&01) is
the error code from R15, (&02) is the address of the call
and (&03) the module name.

### Response

Notify the PROP or the system administrator.

## OMP0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0005 NO MODIFICATION PARAMETER DEFINED. EVENT TABLE DEACTIVATED

### Meaning

No modification parameter list defined for the event table
(see operand SDTPAR in the OPTAB macro). Event table deactivated.

### Response

Correct the event table.

## OMP0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0006 "(&00)" EXECUTED

### Meaning

Command (&00) successfully executed.

### Response

None.

## OMP0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0007 MEMORY FILE IS EMPTY

### Meaning

There is no error entry in the memory file PROP.MEMORY.

### Response

None.

## OMP0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0008 NO DEVICE DEFINED

### Meaning

The printer table contains no printer for the current processor.

### Response

Define a printer or generate a new printer table.

## OMP0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0010 DEVICE TABLE WRONG OR NOT DEFINED. SPS PACKET COULD NOT BE ACTIVATED

### Meaning

Printer table not defined or an error occurred during
compilation of the new printer table. The SPS packet
could not be activated without a printer table.

### Response

Define a printer table or correct the current printer table.

## OMP0012

Destination: USER-TASK, CONSOLE Routing code: X Weight: 99

Warranty : NO

OMP0012 WARNING: THE VERSION OF SPOOL USED IS NOT SUPPORTED BY STANDARD PROP.

### Meaning

- Standard PROP has not been adapted for the SPOOL version used.
- Errors may occur in SPOOL message processing.

### Response

- Notify the PROP or system administrator.

## OMP0400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0400 LENGTH OF TSN-SPECIFIC AREA INCORRECT. EVENT TABLE DEACTIVATED

### Meaning

The length of the TSN area specified with the TSNAREA operand in
the OPTAB macro is less than 16 or greater than 4096. The event
table has been ignored.

### Response

Correct the OPDEF entry. Recompile the event table and load it
again.

## OMP0401

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0401 ILLEGAL EVENT TABLE ENTRY. EVENT TABLE DEACTIVATED

### Meaning

An event table contains an invalid entry (e.g. POS > 2999).

### Response

Correct the OPDEF entry. Recompile the event table and load it
again.

## OMP0402

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0402 MEMORY MANAGEMENT ERROR. PROP DEACTIVATED

### Meaning

An error occurred during the PROP management of TSN-specific areas.
PROP has been deactivated.

### Response

Notify OMNIS administrator. Reload OMNIS and PROP.

## OMP0403

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0403 NO COMMAND PROCEDURE DEFINED. "/PROP" COMMAND IGNORED

### Meaning

The PROP command cannot be processed because no command procedure
was defined in the event table assigned to the partner.

## OMP0404

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

OMP0404 INCORRECT EVENT TABLE HEADER. EVENT TABLE DEACTIVATED

### Meaning

A illegal event table header was detected. Possible reasons:
the module is not an event table or another
module (with the same entry name) was loaded.

### Response

Load the correct event table or correct the event table.

## OMP0405

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0405 WRONG EVENT TABLE VERSION. EVENT TABLE DEACTIVATED

### Meaning

No additional information.

### Response

Recompile event table using the current PROP macro library.

## OMP0406

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0406 TSN-SPECIFIC AREA IS TOO BIG. EVENT TABLE DEACTIVATED

### Meaning

Another event table has already been loaded with a TSN-Specific
area smaller than the current TSN-Specific area.

### Response

Use the same length in all event tables.

## OMP0407

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0407 INCORRECT PROCEDURE HEADER. EVENT TABLE DEACTIVATED

### Meaning

An illegal procedure header was detected when all the administration
procedures associated with the current event table were validated.
An event table entry points to an address not containing a procedure.

### Response

Correct the event table.

## OMP0408

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0408 WRONG PROCEDURE VERSION. EVENT TABLE DEACTIVATED

### Meaning

No additional information.

### Response

Recompile the procedure using the current macro library.

## OMP0409

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0409 LENGTH OF THE PROCESSOR-SPECIFIC AREA INCORRECT. EVENT TABLE DEACTIVATED

### Meaning

The length specified with the PROAREA operand in the
OPTAB macro ist less than 16 or greater than 4096. The event table
has been ignored.

### Response

Correct the event table.
load it again.

## OMP0410

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0410 PROCESSOR-SPECIFIC AREA IS TOO BIG. EVENT TABLE DEACTIVATED

### Meaning

An event table has already been loaded with a processor-specific
area smaller than that of the current event table.

### Response

Use the same length in all event tables.

## OMP0411

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0411 ERRORS HAVE OCCURRED WHILE PROCESSING DADM MESSAGES FROM PARTNER (&00)

### Meaning

The length of the DADM messages cannot be determined by PROP.
This can lead to errors in messages that are defined in event tables.
At occurrence of a DADM message that does not end in X'0F'
this message is issued.

### Response

Use NTAC2-version greater than V3.0.
Increase the UCON Buffer of the specified partner.
Notify system service.

## OMP0412

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0412 (&00) ERROR (&01) AT ADDRESS (&02)

### Meaning

System call (EXEC, DMS) contains an error.
The name of the call is (&00). (&01) is the error code from R15
and (&02) is the address of the call.

### Response

Depends on the error code (&01). If necessary notify the OMNIS
administrator or system administrator.

## OMP0413

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0413 SDF SYNTAX FILE NOT FOUND. COMMAND IGNORED

### Meaning

The SDF syntax file SYSSDF.OMNIS-PROP.<ver> is not cataloged.

### Response

Catalog the file SYSSDF.OMNIS-PROP.<ver>.

## OMP0414

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0414 (&00) COMMAND IS NOT DEFINED OR DEACTIVATED IN THE EVENT TABLE. COMMAND IGNORED

### Meaning

The command could not be assigned to an active event table entry.
The command has been ignored.

### Response

Correct the command or reactivate the event table entry.

## OMP0415

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0415 MEMORY MANAGEMENT ERROR (&00) OCCURRED IN MODULE (&01) AT ADDRESS (&02)

### Meaning

An error occurred during the PROP management of a TSN- or processor-
specific area.

### Response

Notify the PROP administrator. Reload OMNIS and PROP.

## OMP0416

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0416 "(&00)" EXECUTED

### Meaning

Command (&00) successfully executed.

### Response

None.

## OMP0417

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0417 INCORRECT EVENT TABLE. COMMAND IGNORED

### Meaning

The current event table contains an error. The command
has not been executed.

### Response

Correct, recompile and reload the event table.

## OMP0418

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0418 INCORRECT OPERATOR TABLE. COMMAND IGNORED

### Meaning

The current operator table contains an error. The command
has not been executed.

### Response

Correct, recompile and reload the operator table.

## OMP0419

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0419 WRONG PASSWORD. COMMAND IGNORED

### Meaning

No additional information.

### Response

Use the right password and enter the command again.

## OMP0420

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0420 TABLE ENTRY (&00) NOT FOUND. COMMAND IGNORED

### Meaning

No additional information.

### Response

Use the right name and enter the command again.

## OMP0421

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0421 ERROR IN SDF SYNTAX FILE (&00). INPUT IGNORED

### Meaning

An error occurred in the SDF syntax file (&00). See previous
message OMP0422. The current input was ignored.

### Response

Correct or catalog the syntax file and load OMNIS and
PROP again.

## OMP0422

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0422 (&00) ERROR (&01) OCCURRED FOR SDF SYNTAX FILE (&02)

### Meaning

A call to SDF (OPNCALL, TRCMD) contains an error.
The name of the call is (&00). (&01) is the error code from
R15 and (&02) is the current syntax file.
Error code:
X'04' Unrecoverable error
X'08' Parameter error
X'0C' Treansfer area to small
X'10' EOF
X'1C' Incorrect command
X'28' Protocol area to small
X'30' Time expired
X'38' SDF not available
X'44' Syntax file not found
X'48' SDF command executed
X'54' Maximum context number reached

### Response

Depends on the error code (&01). If necessary notify the SDF developer.

## OMP0423

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0423 NO SDF SYNTAX FILE, OR ONLY THE GLOBAL SDF SYNTAX FILE WITH "CHECK=NO", WAS DEFINED IN THE OPERATOR TABLE FOR THIS PARTNER. COMMAND IGNORED.

### Meaning

The command could not be checked syntactically.
The command was not executed.

### Response

Define the SDF syntax file necessary for this partner in
the operator table. Notify the PROP administrator.

## OMP0600

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0600 PLEASE ENTER COMMAND

### Meaning

No additional information.

### Response

Enter a command.

## OMP0601

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0601 OUTPUT ERROR. NO MESSAGE GENERATED

### Meaning

No additional information.

### Response

Reenter the MSG command.

## OMP0602

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0602 SYNTAX ERROR. COMMAND WAS NOT EXECUTED

### Meaning

No additional information.

### Response

Correct the command.

## OMP0603

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0603 RDATA ERROR. COMMAND WAS NOT EXECUTED

### Meaning

No additional information.

### Response

Reenter the command.

## OMP0604

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0604 WRONG MESSAGE KEY. COMMAND IGNORED.

### Meaning

The 4-byte message key is wrong.

### Response

Correct the message key.

## OMP0605

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0605 GENMSG VERSION (&00) READY.

### Meaning

No additional information.

## OMP0700

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0700 PROPTEST VERSION (&00) READY.

### Meaning

No additional information.

## OMP0701

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0701 SYNTAX ERROR. COMMAND WAS NOT EXECUTED.

### Meaning

No additional information.

### Response

Correct the command.

## OMP0702

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0702 PROPTEST NORMALLY TERMINATED.

### Meaning

No additional information.

## OMP0703

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0703 (&00) ERROR (&01) AT ADDRESS (&02).

### Meaning

A call to the operating system (EXEC, DMS) contains an error.
The name of the call is (&00). (&01) is the error code from R15
and (&02) is the address of the call.
The meaning of the error code is given in the BS2000 manuals.

### Response

Depends on the error code (&01). If necessary notify the OMNIS
administrator or system administrator.

## OMP0704

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0704 UNEXPECTED END OF FILE. PROPTEST TERMINATED.

### Meaning

EOF was detected while the next command was being read. PROPTEST
was terminated.

## OMP0705

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0705 NO TERMINAL DEFINED. COMMAND WAS NOT EXECUTED.

### Meaning

No additional information.

### Response

Define a terminal.

## OMP0706

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0706 PAC (&00) NOT FOUND. COMMAND WAS NOT EXECUTED.

### Meaning

No additional information.

### Response

Correct the partner address code.

## OMP0707

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0707 WRONG MESSAGE-KEY LENGTH. COMMAND IGNORED

### Meaning

Only 4- and 7-byte message keys are allowed.

### Response

Correct the message key.

## OMP0708

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0708 EXIT GROUP '(&00)' IS NOT DECLARED

### Meaning

No additional information.

### Response

Correct the 'EXIT' operand or declare a new exit group.

## OMP0709

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0709 EXIT GROUP '(&00)' DECLARED

### Meaning

No additional information.

### Response

None.

## OMP0710

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0710 EXIT GROUP '(&00)' IS ALREADY DECLARED

### Meaning

No additional information.

### Response

None.

## OMP0711

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0711 EXIT MODULE (&00) CANNOT BE LOADED. OPERAND "EXIT" IS IGNORED

### Meaning

The exit module was not loaded. The error
code is given in the preceding message OMS0703.

### Response

Correct the name of the exit routine or make the exit routine
available in the module library.

## OMP0712

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0712 OUTPUT TO TERMINAL (&00)/(&01):

### Meaning

No additional information.

## OMP0713

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0713 MESSAGE TO PARTNER (&00)/(&01):

### Meaning

No additional information.

## OMP0714

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0714 COMMAND TO OMNIS:

### Meaning

No additional information.

## OMP0715

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

OMP0715 INVALID VERSION OF EXIT MODULE (&00). EXIT MODULE NOT LOADED

### Meaning

No additional information.

### Response

Recompile the exit module using the correct macro library.

## OMP0716

Destination: USER-TASK, CONSOLE Routing code: X Weight: 99

Warranty : NO

OMP0716 MESSAGE FILE (&00) IS NOT ASSIGNED TO PARTNER (&01)

### Meaning

No additional information.

## OMP0717

Destination: USER-TASK, CONSOLE Routing code: X Weight: 99

Warranty : NO

OMP0717 (&00) ERROR (&01) OCCURRED FOR MESSAGE FILE (&02)

### Meaning

An internal call to PROPTEST or a call to the operating system
contains an error. The name of the call is (&00). (&01) is the
error code from R15 and (&02) is the current message file.

### Response

Check the message file.

## OMP0718

Destination: USER-TASK, CONSOLE Routing code: X Weight: 99

Warranty : NO

OMP0718 MESSAGE (&00) WAS NOT FOUND IN THE ASSIGNED MESSAGE FILES

### Meaning

No additional information.

## OMP0719

Destination: USER-TASK, CONSOLE Routing code: X Weight: 99

Warranty : NO

OMP0719 FILE (&00) IS NOT A MESSAGE OUTPUT FILE. FILE WAS IGNORED

### Meaning

No additional information.

### Response

Check the file.

## OMP0720

Destination: USER-TASK, CONSOLE Routing code: X Weight: 99

Warranty : NO

OMP0720 NO MESSAGE FILE ASSIGNED TO PARTNER (PAC=(&00)). MESSAGE WAS NOT GENERATED

### Meaning

No additional information.

### Response

Assign a message file with the ASSIGN-MESSAGE-FILE command.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages