## IDAS072

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDAS072 A BREAKPOINT IS ALREADY PRESENT AT THIS LOC

## IDA0C11

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0C11 USER PROGRAM NOT LOADED. CMD IGNORED

### Meaning

The specified command cannot be executed unless a program
has been loaded.

## IDA0N43

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0N43 DUMP WRITTEN TO $SYSUSER FOR DATA SECURITY REASONS

### Meaning

A user dump or an area dump has been written to $SYSUSER.
The dump contains READPASS-protected data.

### Response

Contact the system administrator. He has to decide whether or not the
dump can be passed on to the user whose ID is part of the dump file name.

## IDA0N44

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

IDA0N44 NO VALID AREA SPECIFIED FOR AREA DUMP; DUMP NOT TAKEN

### Meaning

Only invalid areas have been specified.

## IDA0N45

Destination: USER-TASK, CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N45 DUMP DESIRED? REPLY (Y=USER-/AREADUMP TO DISK; Y, <VOLUMETYPE>=USER-/AREADUMP TO TAPE; Y,SYSTEM=SYSTEMDUMP; N=NO)

### Meaning

If DUMP=STD was specified in the MODIFY-TEST-OPTIONS command
(default value), a reply
is requested in case of a program error, when the command /CREATE-DUMP
is entered or when calling one of the
macros CDUMP2, TERMD, TRMJD, or in the case of TERM DUMP=YES,
whether a dump is to be taken. If 'Y' is entered, a USER/AREA DUMP is
written to disk.
If 'Y,<VOLUMETYPE>' is entered, a USER/AREA DUMP is written to tape.
If 'Y,SYSTEM' is entered, a USER/AREA DUMP can be rerouted to a
SYSTEM DUMP output (in case of READ-PRIVILEGE>=3).
If the reply is invalid, this message is displayed until a valid reply is
entered. If the message display is terminated with a negative return code
(e.g. due to an incorrect I/O) this message is repeated twice by CDUMP.
If these repeats are unsuccessful as well, a USER/AREA DUMP is taken.
Message IDA0N45 is suppressed for transaction tasks, in case of
/CANCEL DUMP=NO and in case of /MOD-TEST-OPTIONS DUMP=*NO/*YES/*SYSTEM.

### Response

Y: USER/AREA DUMP is written to disk.
Y,<VOLUMETYPE>: USER/AREA DUMP is written to tape.
Y,SYSTEM: SYSTEM DUMP is output.
N: No dump is taken.

## IDA0N46

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

IDA0N46 CDUMP OPERAND LIST INCORRECT OR NOT AVAILABLE

### Meaning

Dump output was rejected because the CDUMP operand list is invalid or
unavailable.

### Response

Correct the CDUMP call.

## IDA0N47

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

IDA0N47 DUMP PROHIBITED BY /MODIFY-TEST-OPTIONS COMMAND

### Meaning

Dump output is suppressed because the DUMP=NO operand was specified in
the /MODIFY-TEST-OPTIONS command or the maximal dump-number is limited
by MAXIMUM-NUMBER.

## IDA0N48

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

IDA0N48 TASK/SYSTEM SETTINGS PROHIBIT DUMP

### Meaning

No user dump is taken, as the task is in batch or procedure mode and
/MODIFY-TEST-OPTIONS DUMP=STD was specified or SHUTDOWN has been
initiated.

## IDA0N49

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

IDA0N49 INSUFFICIENT TEST PRIVILEGE FOR DUMP

### Meaning

The test privilege is not sufficient do dump the requested task.

## IDA0N50

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

IDA0N50 SYSTEMDUMP CALLED AT LOCATION '(&00)'

### Meaning

CDUMP is called at address '(&00)' to output a SYSTEM DUMP.

## IDA0N51

Destination: USER-TASK, CONSOLE Routing code: R Weight: 70

Warranty : NO

IDA0N51 PROGRAM INTERRUPT AT LOCATION '(&00)'

### Meaning

This message is sent to SYSOUT in the case of a user error or to the
operator console in the case of a system error.
(&00) provides the location of the interrupt and diagnostic information.
For a description of the system event codes (if EC=STD in CDUMP call)
see the section 'STXIT procedure with contingency processing'
(table 'STXIT event classes and associated interrupt events') in the
BS2000 manual 'Executive Macros'.
The event code X'06' was added to the table, indicating that the maximum
nesting depth has been exceeded (see the description of STXIT operands).
The insert (&00) has the format <a>, <b>, <c>, <d> and can assume
the following values:
a) in the case of a USER/AREA DUMP
<a> hexadecimal error address (modulename) or hex. err. addr. (NO NAME)
<b> EC=eventcode or (CDUMP) or (ADUMP) or (TERM)
or (SVC X'nn').
If the CDUMP-call was caused by entering the command /CREATE-DUMP
and if there was loaded a program then EC contains the number of
the programs last executed SVC.
<c> not applicable
<d> CODE=nnnnnnn or INSERT=insert or not applicable
b) in the case of a SYSTEM DUMP
<a> hexadecimal error address (modulename+nnnnn)
or hex. err. addr. (ABSOLU)
<b> EC=eventcode
<c> ELSN=nnnn or not applicable
<d> CODE=nnnnnnnn or INSERT=insert or not applicable
For EC=..., ELSN=..., CODE=..., INSERT=... see the manual 'Executive
Macros'.

## IDA0N52

Destination: CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N52 SYSTEM DUMP DESIRED? REPLY: (EOT=OUTPUT TO DISK; <VOLUMETYPE>=OUTPUT TO TAPE; N=NO)

### Meaning

After a CDUMP message on the cause of the SYSTEM DUMP has been displayed
(messages IDA0N50 or IDA0N51) the operator is asked whether
or not the SYSTEM DUMP is to be taken and to which device it is to
be written. If the reply is invalid (e.g. invalid device type), message
IDA0N52 is repeated. If the specified device type is valid but the
requested device not available, message IDA0N58 is displayed.
repeated. Any device type can again be selected.
In unattended operation, which is indicated by system parameter
DUMPCTRL, the message is suppressed.

### Response

EOT : SYSTEM DUMP is written to disk.
<VOLUMETYPE>: SYSTEM DUMP is written to a serial device
of the specified type.
N : No SYSTEM DUMP is taken.

## IDA0N53

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0N53 DUMP BEING PROCESSED. PLEASE HOLD ON

### Meaning

This informs the user that dump output has been initiated.
This message is displayed only on terminal, i.e. only for a USER/AREA
DUMP or for a SYSTEM DUMP requested by replying 'Y,SYSTEM' to the
IDA0N45 message.

## IDA0N54

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

IDA0N54 '(&00)' WRITTEN TO FILE '(&01)'

### Meaning

After the dump has been taken, the type of dump and the name of the
dump file are displayed for the user/operator.
(&00): USER DUMP or AREA DUMP or SYSTEM DUMP
(&01): name of the dump file.

## IDA0N55

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

IDA0N55 TITLE: '(&00)'

### Meaning

This message is displayed subsequent to message IDA0N54 for a
USER/AREA DUMP to inform the user about the header line (&00).

## IDA0N56

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0N56 CURRENT SYSTEM DUMP SUPPRESSED (DUPLICATE)

### Meaning

A SYSTEM DUMP with an identical interrupt address and an identical
event code already exists on $SYSDUMP.

## IDA0N57

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

IDA0N57 INSUFFICIENT DISK SPACE. NO DUMP OUTPUT

## IDA0N58

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

IDA0N58 TAPE DEVICE TYPE NOT AVAILABLE? REPLY: (EOT=OUTPUT TO DISK; <VOLUMETYPE>=OUTPUT TO TAPE; N=NO)

### Meaning

No tape device of the specified type is free or exists.

### Response

EOT: Dump is written to disk.
<VOLUMETYPE>: Dump is written to a serial device of the specified type.
NO: No Dump is taken.

## IDA0N59

Destination: CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N59 DMS IS NOT YET AVAILABLE. (REPLY: EOT=TERMINATE DUMP)

### Meaning

This message is displayed i.e during startup if a dump is called while
the BS2000 functions required by CDUMP (Data Management System) are not
yet available. CDUMP returns to the caller with return code X'3C'
after EOT has been entered.

### Response

A SLED should be initiated after this message because system
startup should be performed without errors.

## IDA0N60

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

IDA0N60 DUMP TASK CREATED FOR TSN '(&00)'

### Meaning

A dump task has been created to output a dump for TSN '(&00)'.

## IDA0N61

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

IDA0N61 DUMP PROCESSING ABORTED DUE TO '(&00)' ERROR AT PC='(&01)'. RC='(&02)'

### Meaning

The detailed error cause may be obtained from the CONSLOG listing if
output of message IDA0N61 was successful.
The following values are possible at present:
$CREATE... error when creating a CDUMP task
$PNUP ... error at PEND/UNPEND of dump task
CL4REQM... no class 4 memory available
CMF-CREA.. $ECMF error: CREATE
CMF-MOVE.. $ECMF error: MOVE
DMS ... DMS error
$NVYPGA... error RC from $NVYPGA interface
$RMMDIV... error RC from $RMMDIV interface
NO_SPACE.. no more space on disk for this dump
NSPINDH .. error RC from NSPINDH module
RECOVERY.. system error during CDUMP error recovery
SYSTEM ... unspecified system error
VALIDATE.. $VALID error: an essential page was not allocated
ZEROPAGE.. an essential page was deleted (e.g. TCB)
DUMPxxxx.. the CDUMP internal error <xxxx> occurred:
0001 no TTSAV memory available
0002 no memory available
0003 no CLASS 3 memory available
0004 no CLASS 4 memory available
0005 no CLASS 5 memory available
0006 no CLASS 6 memory available
0007 DUMPTASK execution aborted
0013 inconsistency between ITEM# and PAGE#
0014 error in DMS processing
0015 insufficient disk space available
0019 recursive CDUMP call
001A second CDUMP call in errored task
001B Userdump canceled by *CANCEL-RUNNING-DUMP
(&01): Program counter where the (&00) error occurred.
(&02): Return code specifying the (&00) error more precisely.
The inserts (&01) and (&02) are not always provided. This depends on
the error (&00).

## IDA0N62

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0N62 DUMP NOT COMPLETED DUE TO INCONSISTENT TABLES

### Meaning

The message ID IDA0N62 is displayed without message text as an
insert in the termination message if dump processing cannot
be completed due to inconsistent tables (e.g. missing JCB).

## IDA0N63

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0N63 DMS(&00) ERROR OCCURRED. DUMP PROCESSING CONTINUED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter the
command /HELP-MSG DMS(&00) in system mode or see the 'BS2000 System
Messages' manual.
(&00): DMSnnnn ... DMS error with error code nnnn.

## IDA0N64

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

IDA0N64 SNAP INITIATED BY CDUMP

### Meaning

Due to a request of the CDUMP caller CDUMP initiated a $SNAP-call
so that SNAP creates a snapdump.
This snapdump is used to create a more consistent systemdump and
is deleted at the end of the dump processing.

## IDA0N65

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

IDA0N65 CDUMP USES SNAPDUMP '(&00)'

### Meaning

The systemdump created by this task is built with the use of the
snapdump (&00).

## IDA0N66

Destination: USER-TASK, CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N66 CURRENT USERDUMP IS SUPPRESSED (DUPLICATE).

### Meaning

An Userdump with an identical interrupt address, an identical
$CPROG-counter and an identical event code already exists.

## IDA0N67

Destination: USER-TASK, CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N67 SUPPRESS-DUPLICATE-USERDUMP NOT POSSIBLE BECAUSE OF REQM-ERROR.

## IDA0N68

Destination: USER-TASK, CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N68 OUTPUT OF AN USERDUMP TO A SPECIAL CATID NOT POSSIBLE.

### Meaning

It will be tried to give out the userdump to the default catid.

## IDA0N98

Destination: CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N98 CDUMP WAS CALLED BEFORE DMS-READY

### Meaning

The availability of the data management system (DMS) is a precondition
for creating a dump via CDUMP.

### Response

For generation of diagnostic data, a 'crash' is initiated by CDUMP.
Please take a SLED.

## IDA0N99

Destination: CONSOLE Routing code: R Weight: 90

Warranty : NO

IDA0N99 TASK OF SYSTEM DUMP IN HOLD STATE. REPLY (EOT=PEND TASK; T=TERMINATE DUMP)

### Meaning

During CDUMP processing a system error occurred which prevents dump
output. The error cause might be specified in more detail in the
preceding message IDA0N61 (only if there was an IDA0N61).
Diagnostic material can be produced by pending the task and taking
a SLED after SHUTDOWN or an attempt can be made to analyze the error
by means of online diagnostic utilities.
Otherwise the dump processing can be terminated which means that the
error is ignored and the concerned task(s) is (are) activated again.

### Response

EOT: The task will be PENDED INDEFINITELY for later SLED.
T : The dump processing will be terminated and the concerned task(s)
is (are) activated.

## IDA0SAA

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SAA ERROR LOGGING ENTRY FOR 'IDIAS' FOREIGN TASK TRACE

### Meaning

Message for documentation only.

## IDA0SBA

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SBA DIAGNOSTIC SNAPSHOT DUMP CAUSED BY 'IDIAS' EXIT

### Meaning

Message for documentation only.

## IDA0SBB

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SBB DIAGNOSTIC SETS CAUSED BY 'IDIAS' EXIT

### Meaning

Message for documentation only.

## IDA0SIA

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SIA NO MEMORY SPACE AVAILABLE FOR WRITE-STOP TABLE

### Meaning

IDIAS cannot request any class 3 or class 4 memory
(class 3 or class 4 memory saturation).

### Response

Enter /START-SUBSYSTEM again later.

## IDA0SIB

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SIB NO MEMORY SPACE AVAILABLE FOR NUCLEUS LOCK TRACE TABLE

### Meaning

IDIAS cannot request any class 3 memory (class 3 memory saturation).

### Response

Enter /START-SUBSYSTEM again later.

## IDA0SIC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SIC WRITE-STOP SIH ROUTINE ALREADY ACTIVE

### Meaning

SIH routine for write-stop is already loaded.

## IDA0SID

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SID SUBSYSTEM 'IDIAS' CANNOT BE DELETED BECAUSE MEMORY AREAS ARE STILL MONITORED FOR WRITE ACCESS

### Meaning

Some write-stops still exist in the system.

### Response

Remove write-stops by means of /REMOVE-WRITE-STOP and retry
/STOP-SUBSYSTEM IDIAS.

## IDA0SIE

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SIE SUBSYSTEM 'IDIAS' CANNOT BE DELETED BECAUSE DEFAULT WRITE-STOP ROUTINE CANNOT BE ACTIVATED

## IDA0SI0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI0 NO MEMORY SPACE AVAILABLE FOR PROCESSOR-LOCAL DATA

### Meaning

IDIAS cannot request any class 3 memory (class 3 memory saturation).

### Response

Reenter /START-SUBSYSTEM later.

## IDA0SI1

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI1 NO MEMORY SPACE AVAILABLE FOR STOP TABLE

### Meaning

IDIAS cannot request any class 3 memory (class 3 memory saturation).

### Response

Repeat /START-SUBSYSTEM later.

## IDA0SI2

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI2 NEW 'DIAG-SVC' ROUTINE ALREADY ACTIVE

### Meaning

The SIH part of IDIAS has already been loaded.

## IDA0SI3

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI3 SUBSYSTEM 'IDIAS' CANNOT BE DELETED BECAUSE AN IDIAS NO-EDIT-DUMP IS ACTIVE

## IDA0SI4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI4 'DIAG-SVC' ROUTINE COULD NOT BE ACTIVATED

### Meaning

The SIH part of IDIAS cannot be activated.

## IDA0SI5

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI5 SUBSYSTEM 'IDIAS' LOADED

## IDA0SI6

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI6 SUBSYSTEM 'IDIAS' NOT DELETED BECAUSE SOME INSTRUCTION-STOPS ARE STILL ACTIVE

### Meaning

Some Instruction-Stops are still contained in the system.

### Response

Remove the stops by means of /REMOVE-INSTRUCTION-STOP and repeat
/STOP-SUBSYSTEM IDIAS.

## IDA0SI7

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI7 SUBSYSTEM 'IDIAS' CANNOT BE DELETED BECAUSE 'DIAG-SVC' ROUTINE CANNOT BE ACTIVATED

## IDA0SI8

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI8 SUBSYSTEM 'IDIAS' DELETED

## IDA0SI9

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0SI9 SUBSYSTEM 'IDIAS' CANNOT BE DELETED BECAUSE THE TRACE COMMUNICATION BOURSES ARE STILL IN USE

## IDA0S0A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S0A SYNTAX ERROR '(&00)' IN IDIAS COMMAND

## IDA0S0B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S0B TASK NOT IN USER TABLE. ENTER /BEGIN-IDIAS

### Meaning

A stop can only be set by IDIAS users.

## IDA0S0C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S0C TASK ALREADY IN IDIAS-TABLE

### Meaning

The TID of the task has been found in the IDIAS protection table.

## IDA0S0D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S0D MORE THAN 31 TASKS IN USER TABLE. TRY COMMAND AGAIN LATER

### Meaning

Every IDIAS user occupies one of 31 entries in the user table.

### Response

Reenter the command when IDIAS is used less frequently.

## IDA0S0E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S0E MAXIMUM PERMISSIBLE NUMBER OF INSTRUCTION- OR WRITE-STOPS REACHED. STOP CANNOT BE SET

### Meaning

The systemwide upper limit of active Instruction- or Write-Stops
is imposed by the system administrator.

### Response

Ask the system administrator to provide for more stops.

## IDA0S0F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S0F NAME ALREADY EXISTS FOR ANOTHER STOP

### Meaning

The name of an IDIAS-Stop must be unique.

### Response

Enter /SHOW-IDIAS-STATUS to see who has already used this name.

## IDA0S06

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S06 ADDRESS AND NAME DO NOT DESIGNATE THE SAME INSTRUCTION- OR WRITE-STOP

### Meaning

Address and name of an Instruction- and Write-Stop must be unique.

### Response

Enter /SHOW-IDIAS-STATUS to see which name belongs to the stop.

## IDA0S07

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S07 'TASK' OR 'SUBSYSTEM' OPERAND CANNOT BE OMITTED FOR AN INSTRUCTION-STOP IN CLASS 5/6 MEMORY

### Meaning

If the stop address is in class 5 or class 6 memory, the task or
subsystem has to be specified unambiguously.

### Response

Reenter the command with the TASK or SUBSYSTEM operand.

## IDA0S08

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S08 MEMORY NOT AVAILABLE OR FOREIGN MEMORY NOT ACCESSIBLE. FUNCTION ABORTED

### Meaning

An error was reported by $REQM or $CMF.

### Response

Try to reduce the class 5 memory without impairing the foreign task.

## IDA0S09

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S09 USER ID NOT AUTHORIZED TO USE THE IDIAS COMMAND

## IDA0S1A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S1A MORE THAN FOUR TASKS PER INSTRUCTION-STOP MAY NOT BE SPECIFIED EXPLICITLY

### Meaning

In the TASK operand one TID or a list of up to 4 TIDs can be specified.
If the TID of the test task is not known, the following entries are
permissible:
- F-D: the first dialog task encountering the stop is halted
- F-B: the first batch task encountering the stop is halted
- F-I: the first interrupt-driven task encountering the stop
is halted.

### Response

Reduce the number of TIDs or enter one of the specifications listed above.
A combination of these specifications is also permissible.

## IDA0S1B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S1B THIS INSTRUCTION- OR WRITE-STOP CANNOT BE REMOVED OR CHANGED

### Meaning

The user attempted to access an Instruction- or Write-Stop set by
another user.
The Instruction- or Write-Stop can, however, only be changed or
removed by the user who set it.

## IDA0S1C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S1C SPECIFIED INSTRUCTION-STOP DOES NOT EXIST. ENTER /SHOW-INSTRUCTION-STOPS

### Meaning

A command has been entered for a nonexisting instruction-stop.

### Response

Enter /SHOW-INSTRUCTION-STOPS NAME=*ALL in order to obtain a
list of all instruction-stops.

## IDA0S1D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S1D 'TASK' OPERAND CANNOT BE OMITTED

### Meaning

1. More than one task is in the Instruction- or Write-Stop-List,
but the TASK operand has been omitted.
If ACTION=*INCREMENT-COUNTER is specified, the task in question must
be unique.
2. TASK-ID operand may not be omitted when the
/TRACE-INSTRUCTIONS command is issued for the first time for a task.
3. TASK operand may not be omitted when the
/ADD-WRITE-STOP command is issued for the first time for a task.
4. TASK-ID operand may not be omitted when the
/CREATE-SYSTEM-DUMP command is issued.

## IDA0S1E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S1E SEVERAL TASKS NOT FOUND. ENTER /SHOW-IDIAS-STATUS

### Meaning

Some of the specified TIDs could not be found, the others have been
released.

### Response

Enter /SHOW-IDIAS-STATUS to see which tasks have not yet been released.

## IDA0S1F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S1F SYNCHRONIZATION PROBLEMS. TRY COMMAND AGAIN LATER

### Meaning

The Instruction- or Write-Stop table could not be locked even
after 30 attempts.

### Response

If the repetition of the command is not successful, contact the
maintenance staff.

## IDA0S10

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S10 INSTRUCTION-STOP-ADDRESS HAS TO BE SPECIFIED FOR A NEW INSTRUCTION-STOP

### Meaning

When setting a new Instruction-Stop the Instruction-Stop-address has
to be specified in the form <module> + <reladd> or ABSOLUTE + <absadd>.

### Response

Enter the corrected command.

## IDA0S11

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S11 SPECIFIED MODULE OR ENTRY NOT FOUND IN (&00) (&01).

### Meaning

The specified module or entry don't exist in given context/subsystem.

### Response

Reenter the command with an existing module or with another context/
subsystem.

## IDA0S12

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S12 DISPLACEMENT VALUE HIGHER THAN MODULE LENGTH

### Meaning

If <module> + <distance> is specified, the Instruction-Stop or
CONTINUE-AT-MODULE-ADDRESS-address
can be located only within the module.

### Response

Ensure that the Instruction-Stop is set at the correct location.

## IDA0S13

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S13 ODD ADDRESS INVALID FOR /ADD-INSTRUCTION-STOP

### Meaning

All instructions have to be aligned on a halfword or word boundary.

### Response

Enter the corrected command.

## IDA0S14

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S14 INSTRUCTION-STOP ILLEGAL FOR A 'DIAG-SVC'

### Meaning

Double Instruction-Stops are not permitted.

### Response

Enter /SHOW-INSTRUCTION-STOPS to see if a stop is already
set at this location.

## IDA0S15

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S15 UNALLOCATED ADDRESS. COMMAND REJECTED

### Meaning

Error when validation was performed for the Instruction-Stop- or
CONTINUE-AT-... -address.

### Response

Check if the address lies next to an unallocated page.

## IDA0S17

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S17 INSTRUCTION-STOPS OR CONTINUE-AT-...-ADDRESSES IN CLASS 1 MODULES REQUIRE 'OPTION=*SUPPRESS-STATIC-CHECK'

### Meaning

Most class 1 modules run in processor state SIH and may not be stopped.

### Response

If really desired, repeat the command at your own risk with
OPTION=*SUPPRESS-STATIC-CHECK.

## IDA0S18

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S18 INVALID OPERATION CODE AT INSTRUCTION-STOP- OR CONTINUE-AT-...-ADDRESS. OPERAND 'OPTION=*SUPPRESS-STATIC-CHECK' REQUIRED

### Meaning

Such an Instruction-Stop should be used only in very special cases.

### Response

If really desired, repeat the command at your own risk with
OPTION=*SUPPRESS-STATIC-CHECK.

## IDA0S19

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S19 OWN OR PROTECTED TASK CANNOT BE TESTED WITH 'IDIAS'

### Meaning

After a /BEGIN-IDIAS a task is protected against IDIAS.

## IDA0S2A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S2A (&00) INSTRUCTION-STOPS REMOVED. (&01) ARE CURRENTLY IN THE SYSTEM

### Meaning

This message is displayed on terminal and console for revision purposes.

## IDA0S2B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S2B INTERNAL DIAGNOSTIC TRACE IS ALREADY RUNNING

## IDA0S2C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S2C INTERNAL DIAGNOSTIC TRACE HAS ALREADY BEEN SWITCHED OFF

## IDA0S2D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S2D POSSIBLY RECURSIVE INSTRUCTION-STOP IN TESTTASK

### Meaning

Remove Instruction-Stop from testtask.

### Response

none

## IDA0S2E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S2E RESUME-CMD ILLEGAL AT FOREIGN INSTRUCTION-STOP

### Meaning

Observer-Task is not owner of this instruction-stop

### Response

/SHOW-INSTRUCTION-STOPS NAME=*ALL,SELECT-TASK=*ANY to see
the owner of of this Instruction-Stop

## IDA0S20

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S20 COMMAND WITHDRAWN BY USER. NO INSTRUCTION-STOP SET

## IDA0S21

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S21 (&00) + (&01) : (&02)

### Meaning

The statements at the Instruction-Stop- or CONTINUE-AT-...-location
are displayed.

### Response

Check if the right location was found.

## IDA0S22

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

IDA0S22 ADDRESS OK? REPLY (Y=YES; N=NO)

### Meaning

Confirmation is requested for setting the Instruction-Stop.
Y: the displayed statements agree with the expectations.

## IDA0S23

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S23 SPECIFIED USER EXIT PROCEDURE NOT YET LOADED

### Meaning

The name of the exit is unknown to IDIAS.

### Response

Use /LOAD-IDIAS-EXIT in order to load the EXIT module.

## IDA0S24

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S24 INSTRUCTION-STOP SET AT (&00) + (&01)

### Meaning

This message informs the operator about the user's activities.

## IDA0S25

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S25 OLD CODING DOES NOT MATCH PREVIOUS CODING

### Meaning

The old code was changed after it had been saved before (re)setting the
Instruction-Stop.

### Response

Analyze the error cause.

## IDA0S26

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S26 /WAIT-IDIAS-EVENT COMMAND TERMINATED WITHOUT EVENT DUE TO TIME-LIMIT

### Meaning

The command /WAIT-IDIAS-EVENT was terminated after the specified wait
time <s> had elapsed without an event occurring for the specified
Instruction- or Write-Stop.

## IDA0S27

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S27 NO TASK SPECIFIED FOR THIS INSTRUCTION-STOP. INSTRUCTION-STOP IS DORMANT

### Meaning

An Instruction-Stop for which no task has been specified is ineffective.

### Response

Enter the command /ADD-INSTRUCTION-STOP STOP=...,TASK=*ADD-TASK(...),
if the stop is to be activated.

## IDA0S28

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S28 INSTRUCTION-STOP AND CONTINUE-AT-...-ADDRESS MAY NOT RESIDE IN DIFFERENT SUBSYSTEMS

### Meaning

The only permissible combinations are:
- Instruction-Stop and CONTINUE-AT-...-address in the same
subsystem (same class 5 memory), or
- Instruction-Stop in class 5 and CONTINUE-AT-...address
in class 2 or class 4 memory.
No other combinations are technically possible.

## IDA0S29

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S29 INVALID SUBSYSTEM

### Meaning

The specified operands do not unambiguously identify a
Instruction-Stop in a subsystem.
Possible reasons:
- A stop with the same address already exists within another subsystem.
(The address of a stop must be unique even if the stops reside in
different address spaces.)
- The specified stop resides within the CP part of the operating system
(subsystem is CP).
- The stop with the specified address resides within another subsystem.
- The stop with the specified name resides within another subsystem.
For more detailed information see the manual.

### Response

Repeat the command with the correct subsystem.

## IDA0S3A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S3A NO 'IDIAS' TRACE IN TASK '(&00)' POSSIBLE. COMMAND REJECTED

### Meaning

In the specified task another trace is already performed by another
monitoring task.

## IDA0S3B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S3B TASK WITH (&00) '(&01)' DOES NOT EXIST. COMMAND REJECTED

### Meaning

The task specified in an IDIAS-command does not exist.

## IDA0S3C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S3C TRACE NOT POSSIBLE IN ONE'S OWN TASK OR IN A PROTECTED TASK. COMMAND REJECTED

### Meaning

IDIAS users or protected tasks cannot be specified in an IDIAS-command.

## IDA0S3D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S3D 'IDIAS' TRACE RUNNING IN IDIAS MODULE

### Meaning

The current trace task enters, with activated FTT, an IDIAS module.

## IDA0S3E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S3E TASK '(&00)' STOPPED BY DIAGNOSTIC STOP

### Meaning

The test task has been stopped by a diagnostic stop in the trace path.

## IDA0S3F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S3F CHANGE OF MAXIMUM NUMBER OF INSTRUCTION- OR WRITE-STOPS NOT POSSIBLE

### Meaning

The maximum permissible number of Instruction- or Write-Stops
cannot be changed because there are still stops in use
or there was an error when releasing memory space.

### Response

Remove the Instruction- or Write-Stops and try the command again.

## IDA0S30

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S30 INTERNAL 'IDIAS' ERROR. SERSLOG ENTRY CREATED

## IDA0S31

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S31 'IDIAS' TRACE RUNNING IN TASK LOCK '(&00)'

### Meaning

The current trace task enters a task lock path.
(&00): name of the module.

## IDA0S32

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S32 'IDIAS' TRACE LEAVING A TASK LOCK PATH

### Meaning

The current trace task leaves a task lock path.

## IDA0S33

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S33 IMPLICIT 'RESUME' FOR TASK '(&00)'

### Meaning

The current trace task entered a task or system lock path. The value
*RESUME-TASK was specified for the LOCK-HANDLING operand, or a trace was
attempted within an IDIAS module.

## IDA0S34

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

IDA0S34 TMI WAIT TIME IN TASK '(&00)' EXCEEDED. REPEAT WAITING? REPLY (Y=YES; N=NO)

### Meaning

The time specified in the WAIT-TIME-LIMIT operand as the wait time
for a TMI event to occur has been exceeded.

### Response

Enter another /TRACE-INSTRUCTIONS command with an increased value in
the WAIT-TIME-LIMIT operand.

## IDA0S35

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S35 TASK '(&00)' NOT AT OWN INSTRUCTION-STOP OR WITHIN A TRACE PATH. COMMAND REJECTED

### Meaning

In the specified task no IDIAS trace is possible at present, as
the task is not at an Instruction-Stop nor within an IDIAS trace path.

### Response

Insert an Instruction-Stop before the routine to be tested. Let the
test task run to that stop and repeat the /TRACE-INSTRUCTIONS command.

## IDA0S36

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S36 NO FURTHER TEST TASK POSSIBLE. COMMAND REJECTED

### Meaning

The maximum permissible number of 5 parallel test tasks has been reached.
No further trace task can be created.

### Response

Enter /RESUME-IDIAS-TEST-TASK for a test task no longer required and
repest /TRACE-INSTRUCTIONS for the new test task.

## IDA0S37

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S37 'IDIAS' TRACE FOR TASK '(&00)' COMPLETED

## IDA0S38

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S38 TRACE TASK '(&00)' TERMINATED

### Meaning

The trace task has been terminated due to an error or by an explicit
termination request.

## IDA0S39

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S39 UNKNOWN PC '(&00)' IN TASK '(&01)' AT ADDRESS '(&02)'

### Meaning

The last instruction processed in the test task with TID (&01) was an
unknown operation code.

## IDA0S4A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S4A NO TASK SPECIFIED. COMMAND REJECTED

## IDA0S4B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S4B 'IDIAS' TRACE ACTIVE. NO GLOBAL WRITE-STOP POSSIBLE

### Meaning

A global write-stop is only possible if no IDIAS trace is active
in the entire system.

### Response

Terminate the IDIAS trace by means of /RESUME-IDIAS-TEST-TASK and retry
command.

## IDA0S4C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S4C GLOBAL WRITE-STOP ACTIVE. NO 'IDIAS' TRACE POSSIBLE

### Meaning

An IDIAS trace is only possible if no global write-stop is set.

### Response

Remove write-stop by means of /REMOVE-WRITE-STOP and retry trace command.

## IDA0S4D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S4D WRITE-STOP IN TASK '(&00)' IS SET. NO 'IDIAS' TRACE POSSIBLE

### Meaning

IDIAS trace and write-stop cannot not be used in parallel in a task.

### Response

Remove write-stop by means of /REMOVE-WRITE-STOP and retry trace command.

## IDA0S4E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S4E TEST TASK IS NEITHER AT OWN INSTRUCTION-STOP NOR AT OWN WRITE-STOP NOR WITHIN A TRACE PATH. COMMAND REJECTED

## IDA0S4F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S4F /RESUME-IDIAS-TEST-TASK FOR TASKS AT FOREIGN WRITE-STOP IMPERMISSIBLE. COMMAND REJECTED

## IDA0S40

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S40 NO RESPONSE FROM TASK '(&00)' SINCE LAST TRACE STEP

### Meaning

Unknown condition of test task.
Some possible reasons:
- system error
- permanent loop
- deadlock situation
- wait for a requested lock.

### Response

Check condition of test task.
Try a further /TRACE-INSTRUCTIONS command.

## IDA0S41

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S41 'IDIAS' TRACE ILLEGAL AT A FOREIGN INSTRUCTION-STOP

### Meaning

Tracing can only be started from own instruction stops.

### Response

Enter /SHOW-INSTRUCTION-STOPS,NAME=*ALL,SELECT-TASK=*ANY to see
the owner of this Instruction-Stop.

## IDA0S42

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S42 RECURSIVE 'IDIAS' TRACE NOT POSSIBLE

### Meaning

An attempt was made to trace within a module which is called by
IDIAS FITT processing.

### Response

Enter /RESUME-IDIAS-TEST-TASK or /REMOVE-INSTRUCTION-STOP for
the Instruction-Stop to continue the trace.
IDIAS trace.

## IDA0S43

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S43 CONNECTION TO SUBSYSTEM 'IDIAS' CANNOT BE ESTABLISHED. IDIAS TRACE NOT POSSIBLE

### Meaning

The function 'CONNECT-SUBSYSTEM' cannot be processed.

### Response

Please contact the maintenance staff.

## IDA0S44

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S44 NO MEMORY AVAILABLE FOR INSTRUCTION- OR WRITE-STOP-TABLE

### Meaning

IDIAS cannot request any class 3 memory (class 3 memory saturation).

### Response

Reenter command later.

## IDA0S45

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S45 SPECIFIED USER EXIT PROCEDURE CANNOT BE LOADED

### Meaning

Error during loading of the exit procedure.
Some possible reasons:
- 8 exit procedures already loaded
- specified exit procedure already loaded
- invalid library name
- invalid module name
- error in BINDER/LOADER system.

### Response

Check the possible error reasons. In case of BLS error a message
is issued directly by BLS.

## IDA0S46

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S46 MORE THAN 512 INSTRUCTION- OR WRITE-STOPS REQUESTED

### Meaning

The maximum number of stops managed by IDIAS is the listed number.

### Response

Correct and reenter the command.

## IDA0S47

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S47 NO 'IDIAS' TRACE ACTIVE

## IDA0S48

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S48 NO WRITE-STOP ON THIS HSI POSSIBLE

### Meaning

A write-stop can only be set on processors with CFCS3 HSI.

## IDA0S49

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S49 'IDIAS' TRACE IN TASK '(&00)' ACTIVE. NO WRITE-STOP POSSIBLE

### Meaning

IDIAS trace and write-stop cannot be used in parallel in one task.

### Response

Terminate IDIAS trace by means of /RESUME-IDIAS-TEST-TASK
and reenter /ADD-WRITE-STOP command.

## IDA0S5A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S5A CDUMP RUNNING IN TASK '(&00)'. /REMOVE-WRITE-STOP COMMAND IMPERMISSIBLE

### Meaning

As long as the CDUMP function is active in the test task the corresponding
write-stop cannot be removed.

### Response

Enter /SHOW-SYSTEM-DUMP-STATUS to see when the CDUMP function
is terminated.

## IDA0S5B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S5B GLOBAL WRITE-STOP SET FROM '(&00)'+'(&01)' TO '(&02)'+'(&03)'

### Meaning

This message is displayed on terminal and console.

## IDA0S5C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S5C LOCAL WRITE-STOP SET IN TASK '(&00)' FROM '(&01)+(&02)' TO '(&03)+(&04)'

## IDA0S5D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S5D IDIAS-NO-EDIT-DUMP NOT POSSIBLE

### Meaning

NO-EDIT dump is not possible for the specified test task.
Possible reasons:
- specified task does not exist.
- a NO-EDIT dump is already active in the specified task.
- the task is just in the last termination step.
- no bourse slot can be requested.
- the task is in state 'pended indefinitely'.

## IDA0S5E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S5E OPTION=*SUPPRESS-DYNAMIC-CHECKS NECESSARY FOR A IDIAS-NO-EDIT DUMP IN THIS TASK. COMMAND REJECTED

### Meaning

The specified test task is a system task or it is in one of the
'inactive queues' Q5 - Q13.

## IDA0S5F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S5F LENGTH OF WRITE-STOP CONTROL AREA MAY NOT BE CHANGED. COMMAND REJECTED

## IDA0S50

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S50 INVALID TASK SPECIFICATION FOR GLOBAL WRITE-STOP

### Meaning

The global write-stop is already active for another task.

### Response

Enter /SHOW-WRITE-STOP to see for which task the global write-stop
is active.

## IDA0S51

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S51 INVALID NAME OR START ADDRESS FOR WRITE-STOP. COMMAND REJECTED

### Meaning

Possible reasons:
- a write-stop already exists with the specified name
- a write-stop already exists with the specified address (possibly in
another subsystem)
- the specified address does not exist.

### Response

Enter /SHOW-WRITE-STOPS to get a list of all write-stops.

## IDA0S52

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S52 NO FURTHER OPERANDS PERMITTED IF WILDCARDS SPECIFIED IN NAME. COMMAND REJECTED

## IDA0S53

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S53 GLOBAL WRITE-STOP REMOVED

### Meaning

This message is displayed on terminal and console for revision purposes.

## IDA0S54

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S54 (&00) WRITE-STOPS REMOVED. (&01) ARE CURRENTLY IN SYSTEM

## IDA0S55

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S55 NAME ALREADY EXISTS

### Meaning

The name is already used for an Instruction- or Write-Stop.

### Response

Enter /SHOW-IDIAS-STATUS to see which names are already in use.
Reenter /ADD-...-STOP with a new name.

## IDA0S56

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S56 INVALID LENGTH FOR WRITE-STOP. COMMAND REJECTED

## IDA0S57

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S57 ONLY ONE TPR WRITE-STOP EVENT PERMITTED PER ADDRESS SPACE. COMMAND REJECTED

## IDA0S58

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S58 CDUMP RUNNING IN TASK '(&00)'. NO MODIFICATION OF TPR WRITE-STOP EVENT PROCESSING POSSIBLE

### Meaning

As long as the CDUMP function is active in the test task the TPR event
processing cannot be modified.

### Response

Enter /SHOW-SYSTEM-DUMP-STATUS to see when the CDUMP function
is terminated.

## IDA0S59

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S59 'IDIAS' WRITE-STOP RANGE CONFLICT. COMMAND REJECTED

### Meaning

No task-local write-stop is possible, because a system-global write-stop
is set or no system-global write-stop is possible because a task-local one
is set.

### Response

Enter /SHOW-WRITE-STOPS to obtain a list of all write-stops set.

## IDA0S6B

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0S6B DIAGNOSIS-STOP ON A RDPC-INSTRUCTION OR RDPC-INSTRUCTION IN DELAY-SLOT FORBIDDEN.

### Meaning

Setting of a diagnosis stop on a RDPC instruction or executing
of a RDPC instruction in a delay-slot is not allowed.

### Response

Try it again on another address.

## IDA0S6C

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0S6C TMI WAIT TIME IN OBSERVER-TASK EXCEEDED. IDIAS-AREA-TRACE POSSIBLY FINISHED.

### Meaning

The specified wait time for a TMI event to occur has been exceeded.
Because it is an Area-Trace, Trace-End is assumed.

## IDA0S6D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S6D AREA-TRACE: MODULE NOT FOUNFD OR TRACE-BEGIN GREATER TRACE-END

### Meaning

Repeat command with correct operands.

## IDA0S60

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S60 SPECIFIED WRITE-STOP DOES NOT EXIST. ENTER /SHOW-WRITE-STOPS

### Meaning

A command has been entered for a nonexisting write-stop.

### Response

Enter /SHOW-WRITE-STOPS NAME=*ALL to obtain a list of all
write-stops.

## IDA0S61

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S61 NO INSTRUCTION-STOP SET

## IDA0S62

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S62 NO WRITE-STOP SET

## IDA0S63

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S63 TASK (&00) REMOVED FROM STOPLIST.

### Meaning

Corresponding Instruction-Stop not more available for this task.

### Response

none

## IDA0S64

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S64 USER WANTS TO SET AN INSTRUCTION-STOP WITHIN AN IDIAS-MODULE. COMMAND REJECTED.

### Meaning

It is not allowed to set an Instruction-Stop into an IDIAS-module.

### Response

Reenter the command with a Non-IDIAS-Module.

## IDA0S65

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S65 NO MEMORY SPACE AVAILABLE FOR SAVING WATCHING-AREA.

### Meaning

IDIAS cannot request any Class-3-memory (Cl-3-memory saturation).

### Response

Repeat command without Rewrite-function.

## IDA0S66

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S66 TASK IS NOT OWNER OF THE/AN INSTRUCTION-STOP.

### Meaning

For this (Beobachter-)Task an Instruction-Stop does not exist.

### Response

Enter /SHOW-INSTRUCTION-STOPS NAME=*ALL,SELECT-TASK=*ALL.

## IDA0S67

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S67 TASK IS NOT OWNER OF THE/A WRITE-STOP.

### Meaning

For this (Observer-)Task a Write-Stop does not exist.

### Response

Enter /SHOW-WRITE-STOPS NAME=*ALL,SELECT-TASK=*ALL.

## IDA0S70

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S70 (&00) IS AN ENTRY IN MODULE (&01).

## IDA0S71

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0S71 SPECIFIED USER EXIT PROCEDURE CANNOT BE LOADED

### Meaning

Error during loading of the exit procedure.
Some possible reasons:
- 8 exit procedures already loaded
- specified exit procedure already loaded
- invalid library name
- invalid module name
- error in BINDER/LOADER system.

### Response

Check the possible error reasons. In case of BLS error a message
is issued directly by BLS.

## IDA0S72

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0S72 INSTRUCTION-STOP ALREADY PRESENT AT SAME ADDRESS

### Meaning

The user attempted to set an instruction-stop which is
already set for same address.

### Response

Enter /SHOW-INSTRUCTION-STOPS NAME=*ALL,SELECT-TASK=*ALL
to get a list of all instruction-stops.

## IDA0S73

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0S73 WRITE-STOP ALREADY PRESENT AT SAME START ADDRESS

### Meaning

The user attempted to set a write-stop which is already set
for same start address.

### Response

Enter /SHOW-WRITE-STOPS NAME=*ALL,SELECT-TASK=*ALL
to get a list of all write-stops.

## IDA0001

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0001 HARDWARE-AUDIT NOT RUNNING. COMMAND REJECTED

### Meaning

HOLD-HA-A (ISP: ACTION=DISC) is only possible with active AUDIT

## IDA0002

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0002 HARDWARE-AUDIT ALREADY RUNNING. COMMAND REJECTED

### Meaning

HARDWARE-AUDIT-mode already activated, either by
a foreign task AUDIT request or by an ALL-JOBS(ISP:ALLTASK)-
AUDIT request.

## IDA0003

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0003 HARDWARE-AUDIT TABLE NOT ASSIGNED. COMMAND REJECTED

### Meaning

As HARDWARE-AUDIT was not switched on, no tables can be edited by
SHOW-HA-A (ISP: AUDIT DISPLAY=YES)

### Response

switch on HARDWARE-AUDIT.

## IDA0004

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0004 HARDWARE AUDIT RUNNING WITH 'SCOPE=OWN-JOB'. 'SCOPE=PROGRAM-LEVEL' REJECTED

### Meaning

A PCB-specific HARDWARE-AUDIT request (SCOPE=PROGRAM-LEVEL; ISP:
SCOPE=FUNCT) is rejected if a task-specific HARDWARE-AUDIT (SCOPE=
OWN-JOB; ISP: SCOPE=TASK) is running

### Response

Switch off task-specific HARDWARE-AUDIT and reenter command.

## IDA0006

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0006 ISP-CMD: HARDWARE-AUDIT OPERAND 'SAVE' IGNORED

### Meaning

Operand SAVE is not allowed in connection with:
- ACTION = OFF
- ACTION = DISC
- DUMP = YES
- DISPLAY= YES.

## IDA0007

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0007 HARDWARE-AUDIT-TABLE EMPTY, NO OUTPUT

### Meaning

The HARDWARE-AUDIT table is empty and cannot be edited for that reason.

## IDA0008

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0008 ISP-CMD: SYNTAX ERROR IN HARDWARE-AUDIT OPERAND. COMMAND REJECTED

### Response

Reenter command with correct syntax.

## IDA0009

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0009 HARDWARE-AUDIT SAVE TABLE LENGTH NOT ALLOWED. 'BUFFER-SIZE = (&00)' ASSUMED

### Meaning

1.) For STATE=USER (Usercommand):
The operand BUFFER-SIZE (ISP: SAVE) must have a value within the
range 0 through 16. processing continues with a 16-page save table.
2.) For STATE=SYS (Systemadministratorcommand):
The operand BUFFER-SIZE (ISP: SAVE) may only have the values 0 or 1.
processing continues with a one-page save table.

## IDA0010

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0010 ISP-CMD: OPERAND COMBINATION INVALID. HARDWARE-AUDIT-COMMAND REJECTED

### Meaning

1) If SCOPE=ALLTASK, the following operands are not allowed:
ACTION=DISC
STATE = USER or
DUMP = YES or
DISPLAY= YES.
2) If SCOPE=FUNCT, the following operands are not allowed:
ACTION = OFF or
ACTION = DISC or
DUMP = YES or
DISPLAY= YES.
3) In the case of TID= or TSN=, the following operands are not allowed:
SCOPE = ALLTASK or
SCOPE = FUNCT or
DUMP = YES or
DISPLAY= YES.

### Response

Repeat HARDWARE-AUDIT command with correct operand combination.

## IDA0011

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0011 ISP-CMD: PRIVILEGE ERROR. HARDWARE-AUDIT COMMAND REJECTED

### Meaning

1) The user does not have the privilege to use a TPR-HARDWARE-AUDIT
2) The user does not have the privilege to use a TU-HARDWARE-AUDIT
for a foreign task which does not run under the own user-ID.

## IDA0012

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

IDA0012 INTERNAL ERROR IN HARDWARE-AUDIT ROUTINE. SYSTEM DUMP GENERATED

## IDA0014

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0014 (&00) MEMORY SATURATION. NO HARDWARE-AUDIT PROCESSING

### Meaning

Memory saturation for
class 3 original tables;
class 4 management area;
class 4 table management;
class 5 save tables;
class 5 work area.
(&00): CL3 or CL4 or CL5.

### Response

Release memory and repeat the HARDWARE-AUDIT-command

## IDA0015

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0015 TASK WITH (&00) (&01) DOES NOT EXIST. HARDWARE-AUDIT COMMAND REJECTED

### Meaning

The task does not exist.
(&00): TSN or TID,
(&01): Task number.

### Response

Check the task numbers and repeat the HARDWARE-AUDIT command.

## IDA0016

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0016 NO PROGRAM LOADED. HARDWARE-AUDIT COMMAND REJECTED BECAUSE OF MISSING (&00) PCB

### Meaning

TU or TPR-PCB not existing. SCOPE=PROGRAM-LEVEL (ISP: SCOPE=FUNCT) cannot
be processed.
(&00): TU or TPR.

### Response

Repeat HARDWARE-AUDIT command with a loaded program.

## IDA0017

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

IDA0017 'ALL-JOBS-HARDWARE-AUDIT' SWITCHED OFF FOR ALL TASKS DUE TO CL3 OR CL4 MEMORY SATURATION

### Meaning

ALL-JOBS (ISP: ALLTASK) -HARDWARE-AUDIT SWITCHED OFF, BECAUSE NO MORE
AUDIT-INTERNAL TABLES CAN BE REQUESTED

## IDA0018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0018 INTERNAL HARDWARE-AUDIT ERROR. HARDWARE-AUDIT-TABLE-OUTPUT REJECTED

### Meaning

Because of an error in module AUDEDIT it is not possible to display the
HARDWARE-AUDIT table.

### Response

Contact the maintenance staff.

## IDA0019

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0019 START-HARDWARE-AUDIT COMMAND REJECTED. REPEAT COMMAND LATER

### Meaning

The command-sequence START-HA-A/ STOP-HA-A/ START-HA-A for a foreign Task
in TPR causes the MSG mentioned above always, if the foreign Task did not
run in the meantime. This has the consequence, that the second START-HA-A
command has to be repeated later, because the STOP-HA-A command is not
yet finished, as it is still waiting in a queue.
Using the ISP-format the corresponding commands are:
AUDIT ACTION=ON or AUDIT ACTION=OFF

### Response

Repeat START-HA-A command later

## IDA0020

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0020 HARDWARE-AUDIT NOT AVAILABLE ON THIS HSI. COMMAND REJECTED

### Meaning

HARDWARE-AUDIT is only available on processors with CFCS3 HSI.

## IDA0021

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0021 ABNORMAL TASK TERMINATION DUE TO INTERNAL HARDWARE-AUDIT I/O ERROR

### Meaning

Abnormal task termination caused by an HARDWARE-AUDIT-internal
not repairable WROUT/WRLST error

## IDA0022

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0022 NO FURTHER MEMORY AVAILABLE FOR HARDWARE-AUDIT-OUTPUT ON SYSLST

### Meaning

No further memory available for file assigned to SYSLST.
HARDWARE-AUDIT-table-output stopped.

## IDA0023

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0023 TU-HARDWARE-AUDIT FOR ALL TASKS OF CHOSEN USER-ID NOT AVAILABLE AT THIS TIME DUE TO SYSTEM-ADMINISTRATOR-RESTRICTION.

### Meaning

System-Administrator prevented TU-HARDWARE-AUDIT-Commands for active
USER-ID by command MODIFY-USER-ATTRIBUTES.

### Response

Call System-Administrator.

## IDA0024

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0024 TU-HARDWARE-AUDIT NOT AVAILIBLE AT THIS TIME FOR TASK IN CONTROL DUE TO USER-RESTRICTION.

### Meaning

User prevented TU-HARDWARE-AUDIT-Commands for Task In Control
by command MODIFY-TEST-OPTIONS.

### Response

Switch AUDIT-privilege by command MODIFY-TEST-OPTIONS and repeat command.

## IDA0030

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0030 LINKAGE-AUDIT NOT RUNNING. COMMAND REJECTED

### Meaning

LINKAGE-AUDIT mode was not switched on.

## IDA0031

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0031 LINKAGE-AUDIT ALREADY RUNNING. COMMAND REJECTED

### Meaning

LINKAGE-AUDIT mode already activated, either by another task
due to a foreign task AUDIT request or by an ALL-JOBS
AUDIT request.

## IDA0032

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0032 LINKAGE-AUDIT TABLE NOT ASSIGNED. COMMAND REJECTED

### Meaning

As LINKAGE-AUDIT was not switched on, no tables can be edited

### Response

switch on LINKAGE-AUDIT.

## IDA0033

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0033 LINKAGE-AUDIT RUNNING WITH 'SCOPE=OWN-JOB'. 'SCOPE=PROGRAM-LEVEL' REJECTED

### Meaning

A PCB-specific LINKAGE-AUDIT request is rejected when a task-specific
LINKAGE-AUDIT is running.

### Response

If required, switch off task-specific LINKAGE-AUDIT and then repeat
command.

## IDA0034

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0034 LINKAGE-AUDIT-TABLE EMPTY, NO OUTPUT

### Meaning

The LINKAGE-AUDIT table is empty and cannot be edited for that reason
with SHOW-LI-A.

## IDA0035

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0035 LINKAGE-AUDIT-PRIVILEGE ERROR. COMMAND REJECTED

### Meaning

The user does not have the privilege to request a TU LINKAGE-AUDIT
for a foreign task which does not run under the own user ID.

## IDA0036

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0036 INTERNAL ERROR IN LINKAGE-AUDIT ROUTINE. SYSTEM DUMP GENERATED

## IDA0037

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0037 (&00) MEMORY SATURATION. NO LINKAGE-AUDIT PROCESSING

### Meaning

Memory saturation for
class 3 original tables;
class 4 management area;
class 5 save tables;
class 5 work area.
(&00): CL3 or CL4 or CL5.

### Response

Release memory. Reenter LINKAGE-AUDIT command.

## IDA0038

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0038 TASK WITH (&00) (&01) DOES NOT EXIST. LINKAGE-AUDIT-COMMAND REJECTED

### Meaning

(&00): TSN or TID
(&01): task number.

### Response

Check task numbers and repeat LINKAGE-AUDIT command.

## IDA0039

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0039 NO PROGRAM LOADED. LINKAGE-AUDIT COMMAND REJECTED BECAUSE OF MISSING (&00) PCB

### Meaning

TU or TPR-PCB not existing. SCOPE=PROGRAM-LEVEL cannot
be processed.
(&00): TU or TPR.

### Response

Repeat LINKAGE-AUDIT command with a loaded program.

## IDA0040

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0040 CL3 OR CL4 MEMORY SATURATION. 'ALL-JOBS-LINKAGE-AUDIT' SWITCHED OFF

## IDA0042

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0042 PROCESSOR-LOCAL LINKAGE-AUDIT ALREADY RUNNING. COMMAND REJECTED

### Meaning

A processor-local LINKAGE-AUDIT was already activated with
SCOPE=INTERRUPT-HANDLING or SCOPE=SYSTEM-LEVEL.

## IDA0043

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0043 LINKAGE-AUDIT WITH 'STATE=SYSTEM' NOT POSSIBLE DUE TO ACTIVE PROCESSOR-LOCAL LINKAGE-AUDIT WITH SCOPE=SYSTEM-LEVEL. COMMAND REJECTED

### Meaning

During an active LINKAGE-AUDIT with STATE=PROCESSOR (SCOPE=SYSTEM-LEVEL)
no task-local TPR LINKAGE-AUDIT is possible.

### Response

Switch off processor-local LINKAGE-AUDIT with STOP-LINKAGE-AUDIT
STATE=PROCESSOR(SCOPE=SYSTEM-LEVEL) and switch on task-local
TPR LINKAGE-AUDIT with STATE=SYSTEM

## IDA0044

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0044 PROCESSORLOCAL LINKAGE-AUDIT WITH 'SCOPE=SYSTEM-LEVEL' NOT POSSIBLE DUE TO ACTIVE TPR LINKAGE-AUDIT. COMMAND REJECTED

### Meaning

During an active LINKAGE-AUDIT with STATE=SYSTEM a processor-
local LINKAGE-AUDIT with SCOPE=SYSTEM-LEVEL is not possible.

### Response

Switch off TPR LINKAGE-AUDIT with STOP-LINKAGE-AUDIT STATE=SYSTEM for all
tasks and then switch on processorlocal LINKAGE-AUDIT
with SCOPE=SYSTEM-LEVEL

## IDA0045

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0045 CENTRAL LINKAGE-AUDIT ADMINISTRATION CURRENTLY LOCKED. RETRY COMMAND LATER

### Meaning

To ensure consistency of the LINKAGE-AUDIT management tables, the tables
were locked during processing.

### Response

Retry LINKAGE-AUDIT command later.

## IDA0046

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0046 ABNORMAL TASK-TERMINATION BECAUSE OF INTERNAL I/O-ERROR IN LINKAGE-AUDIT; OUTPUT ABORTED

### Meaning

Because of a WROUT- or WRLST-error in LINKAGE-AUDIT the task is
terminated.

## IDA0047

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0047 LINKAGE-AUDIT OPERAND 'BUFFER-SIZE' IGNORED

### Meaning

LINKAGE-AUDIT was in HOLD state. A save table already exists.

## IDA0048

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0048 LINKAGE-AUDIT-TABLE OF A FOREIGN TASK NOT DISPLAYED

### Meaning

The LINKAGE-AUDIT-Table of a foreign task cannot be displayed because
of an internal system error.

### Response

Contact the maintenance staff.

## IDA0049

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0049 TASK IN TERMINATION. LINKAGE-AUDIT COMMAND REJECTED

### Meaning

The task concerned is being terminated.

## IDA0050

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0050 LINKAGE-AUDIT START-COMMAND REJECTED. REPEAT COMMAND LATER

### Meaning

The command-sequence START-LI-A/ STOP-LI-A/ START-LI-A for a foreign Task
in TPR causes the MSG mentioned above always, if the foreign Task did not
run in the meantime. This has the consequence, that the second START-LI-A
command has to be repeated later, because the STOP-LI-A command is not
yet finished, as it is still waiting in a queue.

### Response

Repeat START-LI-A command later

## IDA0051

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0051 LINKAGE-AUDIT SAVE TABLE LENGTH NOT ALLOWED. 'BUFFER-SIZE=(&00)' ASSUMED

### Meaning

The operand BUFFER-SIZE must have a value within the range
0 through 16. processing continues with a 16-page save table.

## IDA0052

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0052 TU-LINKAGE-AUDIT FOR ALL TASKS OF CHOSEN USER-ID NOT AVAILABLE AT THIS TIME DUE TO SYSTEM-ADMINISTRATOR-RESTRICTION.

### Meaning

System-Administrator prevented LINKAGE-AUDIT-Commands for active
USER-ID by command MODIFY-USER-ATTRIBUTES.

### Response

Call System-Administrator.

## IDA0053

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0053 TU-LINKAGE-AUDIT NOT AVAILIBLE AT THIS TIME FOR TASK IN CONTROL DUE TO USER-RESTRICTION.

### Meaning

User prevented TU-LINKAGE-AUDIT-Commands for Task In Control
by command MODIFY-TEST-OPTIONS.

### Response

Switch AUDIT-privilege by command MODIFY-TEST-OPTIONS and repeat command.

## IDA0054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0054 INVALID CALL OF A SYSTEM FUNCTION IN AUDIT

## IDA0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0055 INTERNAL ERROR IN AUDIT

## IDA0056

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0056 AUDALLOW-PARAM DURING STARTUP NEITHER 'YES' NOR 'NO': YES' ASSUMED.

### Meaning

System-Administrator gave no or a wrong value for param AUDALLOW in
Startup-Parameter-Service: AUDALLOW=YES assumed.

## IDA0057

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0057 PROCESSOR-LOCAL LINKAGE-AUDIT SWITCHED OFF AT END OF STARTUP.

### Meaning

Processor-local LINKAGE-AUDIT was switched off at end of STARTUP close
before SYSTEM READY, as AUDALLOW=NO was given in parameter-service

## IDA0058

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0058 PROCESSOR-LOCAL LINKAGE-AUDIT NOT ACTIVE

### Meaning

the processorlocal LINKAGE-AUDIT was switched off successfully during
startup-processing, or the switch-off-attempt failed because processor-
local LINKAGE-AUDIT had not been switched on.

## IDA0059

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0059 PROCESSOR-LOCAL LINKAGE-AUDIT ACTIVE

### Meaning

The processorlocal LINKAGE-AUDIT was switched on by startup-parameter
service.

## IDA0060

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0060 NO AUDIT-COMMANDS POSSIBLE IN THIS SESSION DUE TO SYSTEM-ADMINISTRATOR-RESTRICTION.

### Meaning

System-Administrator prevented all AUDIT-Commands by giving AUDALLOW=NO
in Startup-Parameter-Service.

## IDA0061

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0061 ERRORLOGGING ENTRY

### Meaning

error occurrred during a TPR-LINKAGE-AUDIT contingency

## IDA0104

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0104 USER PROGRAM NOT LOADED

### Meaning

The user has issued an AID command without loading a program before.

### Response

Load program and repeat command.

## IDA011D

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA011D CONNECT-SUBSYSTEM FOR AID ALREADY PERFORMED IN THIS TASK. NO TASK-LOCAL LOAD POSSIBLE. COMMAND NOT PROCESSED

### Meaning

If AID has been loaded as a subsystem in a task, no task-local
loading is possible.
AID can only be loaded either as a subsystem or task-locally.

## IDA0113

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0113 AIDSYS: NO MEMORY AVAILABLE

### Meaning

There is no more class 5 memory available for AIDSYS. AIDSYS cannot work
or only work with restrictions.

### Response

a) Reenter the command later.
b) Reload the program.

## IDA0119

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0119 AID COULD NOT BE LOADED

### Meaning

Invalid CSECT operand or specified file is not an OML.

### Response

Specify another library or contact the system administrator.

## IDA0122

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0122 AIDSYS: TRAPCODE SVC IN CODING THAT WAS NOT SET BY AIDSYS

### Meaning

The interrupted program encountered a trapcode SVC
(SVC 129) though AIDSYS does not hold any information about
this SVC in its internal tables (e.g., SVC 129 was used
without the appropriate authorization or SVC 129 was set
by another task).

### Response

Remove SVC 129 from the program.

## IDA0123

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

IDA0123 ***** AID REP AT LOCATION (&00), LENGTH = (&01) *****

### Meaning

Using AID, a user changed coding or data in the address space of the
system.

## IDA0124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0124 INVALID CALL OF A SYSTEM FUNCTION IN AIDSYS

## IDA0125

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0125 A SITUATION WHERE AN ABSOLUTE TEST PROTECTION IS NECESSARY EXISTS. IN THIS CASE THE PROGRAM CAN ONLY BE PROCESSED, BUT MUST NOT BE TESTED

### Meaning

The only AID commands that may be specified in such a situation are
%R(ESUME) and %REMOVE.
AID is informed by the $CHKEXO macro whether a
situation where an absolute test protection is necessary exists. Such a
situation exists, for example, if a (part of a) program was loaded from
a file which is protected by a read password.

### Response

Eliminate the situation described above, for example by declaration of
the read password, or enter the %R(ESUME) command.

## IDA0127

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0127 AID NOT AVAILABLE. CONTACT SYSTEM ADMINISTRATOR

### Meaning

AID is not available at the moment (not bound to the system).

### Response

Contact the system administrator for loading AID.

## IDA0128

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0128 INTERNAL ERROR IN ASTRACE

## IDA013A

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA013A TASK-LOCAL LOAD OF AID NOT SUPPORTED FOR THIS USER-ID

## IDA0130

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0130 STRINGS WITH LEADING '%' ARE TREATED AS AID COMMANDS

### Meaning

A character string with a leading % has been entered.
This string is interpreted as an AID command by the command
processor although AID is not available.

## IDA0140

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0140 AID TRAP WITH INCONSISTENT HSI CONTEXT

### Meaning

An AID trap interrupt has occured. AIDSYS can not handle this interrupt,
since the current PMode does not match the PMode, expected for the
interrupt location.

### Response

Take a dump and report the error.

## IDA015A

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA015A SUBSYSTEM AIDSYS COULD NOT BE INITIALIZED

### Meaning

The initialization of AIDSYS could not be processed completely.

### Response

Another try later could be successful.

## IDA015B

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA015B DECOUPLED PART OF SUBSYSTEM AIDSYS COULD NOT BE INITIALIZED

### Meaning

The initialization of AIDSYS could not be processed completely.

### Response

Another try later could be successful.

## IDA015C

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA015C ERROR IN AID VERSION INDICATOR

### Meaning

The current subsystem AID is not able to run in the current BS2000
version.

### Response

Contact the system administrator.

## IDA015D

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA015D SUBSYSTEM AID COULD NOT BE INITIALIZED

### Meaning

The initialization of AID by AIDSYS could not be processed completely.

### Response

Another try later could be successful.

## IDA015E

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA015E AID TRAP NOT ALLOWED IN FUNCTIONAL LEVEL TPR

### Meaning

An AID trap interrupt has occured in the functional level TPR. But AIDSYS
does not support the corresponding trap code handling in TPR.

### Response

Remove the SVC 129 from the program.

## IDA0151

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0151 SUBSYSTEM AIDSYSA COULD NOT BE INITIALIZED

### Meaning

The initialization of AIDSYSA could not be processed completely.

### Response

Another try later could be successful.

## IDA0152

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0152 AIDSYS ERROR IN PARSING OF AID COMMAND

### Meaning

During the analysis of an AID command by AIDSYS, an internal error
has occured.

## IDA0153

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0153 AID IN ERRORNEOUS STATE

### Meaning

An unrecoverable error in AID has occured.

### Response

In the current task, AID is no longer available.

## IDA0154

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0154 COMMAND PRIVILEGE MISSING

### Meaning

The necessary command privilege for AID commands is missing in the
current task.

## IDA0155

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0155 CONNECT TO SUBSYSTEM AIDSYS FAILED

### Meaning

At the moment, the task can not be connected to the subsystem AIDSYS.

### Response

Contact the system administrator.

## IDA0157

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0157 INTERNAL ERROR IN AIDSYS

## IDA0158

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0158 SUBSYSTEM AIDSYSA NOT LOADED

### Meaning

The subsystem AIDSYSA must be permanently available.

## IDA0159

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0159 UNEXPECTED EVENT FOR AIDSYS

### Meaning

An event has been reported to AIDSYS. However, caused by inconsistencies
within the AIDSYS data context, a treatment of the event is not possible.

## IDA0160

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0160 THE SVC 130 IS RESTRICTED TO INTERNAL USAGE

## IDA0161

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0161 AID TRAP IN PAGE PROTECTED AREA NOT ALLOWED

## IDA0162

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0162 UNRECOVERABLE ERROR DURING OUTPUT TO SYSOUT

## IDA0163

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0163 ERROR DURING ACCESS TO SYSOUT

## IDA0164

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0164 ERROR DURING CLOSE OF DUMP FILE '(&00)'. DMS ERROR CODE (&01)

## IDA0165

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0165 CHANGE OF PAGE PROTECTED AREA NOT SUPPORTED FOR FOREIGN TASK ACCESS

## IDA0166

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

IDA0166 MAXIMUM PCB NUMBER REACHED

## IDA0167

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0167 A SITUATION WHERE AN ABSOLUTE TEST PROTECTION IS NECESSARY EXISTS IN THE SELECTED TASK.

### Meaning

AID is informed by the $CHKEXO macro whether a
situation where an absolute test protection is necessary exists. Such a
situation exists, for example, if a (part of a) program was loaded from
a file which is protected by a read password.

## IDA0171

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0171 INTERNAL ERROR FOR CURRENT LIVE MIGRATION STATE

## IDA0172

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0172 INTERNAL ERROR FOR PREVIOUS LIVE MIGRATION STATE

## IDA0173

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0173 INTERNAL ERROR FOR SOME LIVE MIGRATION STATE

## IDA0174

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0174 NO LIVE MIGRATION OCCURRED

## IDA0175

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0175 BUFFER OVERFLOW FOR LIVE MIGRATION HISTORY

## IDA0176

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0176 INVALID LM-COUNTER SPECIFICATION '(&00)'

## IDA0180

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0180 ASINUS : TASK TERMINATION AFTER UNSUCCESSFUL CALL OF $TANC.

### Meaning

ASINUS cannot access it's own data via the anchor in the TCB.

## IDA0181

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

IDA0181 ASINUS : TASK TERMINATION AFTER UNSUCCESSFUL CALL OF $GETMEM.

### Meaning

ASINUS cannot create diagnosis data.

## IDA0198

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0198 BREAK IN SYSTEM PROGRAM AT LOCATION X'(&00)', AMODE=(&01)

### Meaning

A system program attempts to read a command.
(&00): address following the BKPT call
(&01): addressing mode (should be 31).

### Response

If you do not work under the system administrator ID, enter 'R'.

## IDA0199

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

IDA0199 PROGRAM BREAK AT ADDRESS X'(&00)', AMODE=(&01)

### Meaning

In the program, a BKPT system call was performed, e.g. to offer a
possibility for entering system commands.
(&00): address immediately following the system call
(where the program will continue)
(&01): addressing mode at the time of interruption (24 or 31).

### Response

If the program did not issue any messages and the break is not desired,
enter 'R'.

## IDA030F

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA030F CHANGE OF HARDWARE OR LINKAGE AUDIT MODE NOT GRANTED

### Meaning

A change of the Linkage or Hardware AUDIT mode is forbidden in the
user catalogue entry.

## IDA0300

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

IDA0300 SYNTAX ERROR IN MODIFY-TEST-OPTIONS OR SHOW-TEST-OPTIONS OR SHOW-SYMBOL-INFORMATION OR SHOW-MAP-INFORMATION OR SHOW-LIVE-MIGRATION-HISTORY OR SHOW/MODIFY-LIVE-MIGRATION-DEFAULTS COMMAND

### Meaning

Message number of command return code for the commands
MODIFY-TEST-OPTIONS and SHOW-TEST-OPTIONS and
SHOW-SYMBOL-INFORMATION and SHOW-MAP-INFORMATION and
SHOW-LIVE-MIGRATION-HISTORY and
SHOW-LIVE-MIGRATION-DEFAULTS and MODIFY-LIVE-MIGRATION-DEFAULTS.
Possible additional message for MODIFY-TEST-OPTIONS: EXC0926

## IDA0301

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

IDA0301 SEMANTICAL ERROR IN MODIFY-TEST-OPTIONS OR SHOW-TEST-OPTIONS OR SHOW-SYMBOL-INFORMATION OR SHOW-MAP-INFORMATION OR SHOW-LIVE-MIGRATION-HISTORY OR SHOW/MODIFY-LIVE-MIGRATION-DEFAULTS COMMAND

### Meaning

Message number of command return code for the commands
MODIFY-TEST-OPTIONS and SHOW-TEST-OPTIONS and
SHOW-SYMBOL-INFORMATION and SHOW-MAP-INFORMATION and
SHOW-LIVE-MIGRATION-HISTORY and
SHOW-LIVE-MIGRATION-DEFAULTS and MODIFY-LIVE-MIGRATION-DEFAULTS.
Possible additional messages for MODIFY-TEST-OPTIONS: EXC0930, EXC0927.

## IDA0302

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0302 NO MEMORY AVAILABLE IN CDUMP

## IDA0303

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0303 TASK '(&00)' NOT AVAILABLE

### Meaning

The specified task is not available.
(&00): TSN of the specified task.

### Response

Select another task.

## IDA0304

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0304 PRIVILEGE MISSING FOR ACCESS TO TASK '(&00)'

### Meaning

The specified task does not belong to the own user ID and the current
task has not the command privileg TSOS.
(&00): TSN of the specified task.

### Response

Select another task.

## IDA0305

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0305 SPECIFIED PASSWORD IGNORED FOR TSOS

## IDA0306

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0306 PRIVILEGE MISSING FOR PASSWORD ACCESS

## IDA0307

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0307 SPECIFIED TASK NOT ACCESSIBLE

## IDA0308

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IDA0308 NO MATCH FOR SPECIFIED PASSWORD

## IDA0310

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0310 TASK LOCK 'LKASHOOK' NOT GOT

### Meaning

The task lock is not created or is held by another task.

### Response

Contact the system administrator or reenter the command.

## IDA0311

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0311 NO MEMORY AVAILABLE TO PROCESS THE COMMAND

### Response

Contact the system administrator.

## IDA0312

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0312 SYSTEM HOOK TABLES NOT ASSIGNED

## IDA0313

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0313 'COMPARE' VALUE CONTAINS ODD NUMBER OF HEX CHARACTERS

## IDA0314

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0314 'DATA' VALUE CONTAINS ODD NUMBER OF HEX CHARACTERS

## IDA0315

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0315 SPECIFIED MODULE NOT FOUND

## IDA0316

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0316 DISPLACEMENT EXCEEDS MODULE BOUNDARY

## IDA0317

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0317 MISALIGNED SYSTEM HOOK ADDRESS

### Meaning

The hook address must be halfword aligned on /390 HSI.

## IDA0318

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0318 RESERVED MODULE SPECIFIED

### Meaning

System hooks must not be set within reserved modules.

### Response

The system hook might be set via address specification nevertheless.
But there will be a risk for system damage in this case.

## IDA0319

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0319 SYSTEM HOOK ADDRESS NOT WITHIN SYSTEM ADDRESS SPACE

## IDA032A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA032A SYNTAX ERROR IN A SYSTEM HOOK COMMAND

### Meaning

Message number of command return code for system hook commands.

## IDA032B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA032B SEMANTICAL ERROR IN A SYSTEM HOOK COMMAND

### Meaning

Message number of command return code for system hook commands.

## IDA032C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA032C INVALID CPU NUMBER SPECIFICATION

### Meaning

CPU numbers must be within the range 0..31 .

## IDA0320

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0320 SYSTEM HOOK ADDRESS NOT ALLOCATED

## IDA0321

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0321 SYSTEM HOOK '(&00)' NOT FOUND

## IDA0322

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0322 ACCESS ERROR FOR SYSTEM HOOK ADDRESS

## IDA0323

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0323 UNSUPPORTED INSTRUCTION AT SYSTEM HOOK ADDRESS

### Meaning

There must be no branch instruction or SVC at the hook address.

## IDA0325

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0325 RESERVED SYSTEM HOOK NAME SPECIFIED

### Meaning

The names C'$SYSSHxx' cannot be assigned explicitly by the user.

## IDA0326

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0326 LACK OF INTERNAL RESOURCES

### Meaning

Too much system hooks have been set.

### Response

Remove some system hooks.

## IDA0327

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0327 SYSTEM HOOK NAME ALREADY EXISTS

## IDA0328

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0328 INCONSISTENT 'CONDITION' SPECIFICATION

### Meaning

The specified register offset exceeds the length of the register.

## IDA0329

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0329 INCONSISTENT 'ACTION' SPECIFICATION

### Meaning

For writing into a register the data must specify exactly 4 bytes.

## IDA033A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA033A SYSTEM INTERFACE '(&00)' DELIVERS RETURN CODE '(&01)'

## IDA033B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA033B $VSVAID INTERFACE YIELDS UNEXPECTED RECORD TYPE '(&00)'

## IDA033C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA033C Command not allowed in execute-only situation

## IDA0330

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0330 NO SYSTEM HOOKS FOUND FOR SPECIFIED INPUT

## IDA0331

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0331 ERROR IN REMOVING SYSTEM HOOK '(&00)'

## IDA0332

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0332 NO OUTPUT FOUND FOR SPECIFIED INPUT

## IDA0333

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0333 UNRECOVERABLE ERROR DURING CPU SYNCHRONIZATION

### Meaning

A call of $SYNCPU yields an unexpected return code.

## IDA0334

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0334 (&00)+(&01)=(&02): (&03)

### Meaning

The instruction at the hook address is dislpayed.

### Response

Check if the right address was found.

## IDA0335

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0335 ADDRESS OK? REPLY (Y=YES; N=NO)

### Meaning

Confirmation is requested for setting the system hook.

### Response

Y: the displayed instruction agrees with the expectations.
N: the hook shall not be set.

## IDA0336

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0336 COMMAND WITHDRAWN BY USER. NO SYSTEM HOOK SET

## IDA0337

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0337 COMMAND NOT POSSIBLE DUE TO SYSTEM-ADMINISTRATOR-RESTRICTION

### Meaning

The system parameter 'SYSTHOOK' does not have the required value.

## IDA0338

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0338 COMMAND NOT POSSIBLE DUE TO AN EXISTING EXCLUSIVE RIGHT FOR SYSTEM HOOKS

### Meaning

Another task has the exclusive right for system hooks.

## IDA0339

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0339 EXCLUSIVE RIGHT FOR SYSTEM HOOKS NOT GOT

### Meaning

In the moment, another task has the exclusive right for system hooks.

### Response

Through specification of the operand FORCE=*YES the exclusive
right can be got nevertheless.

## IDA034A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA034A SYSTEM HOOK IN WRONG STATE

### Response

Deactivate Hook via DEACTIVATE-SYSTEM-HOOK before.

## IDA034B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA034B INVALID POSITION SPECIFICATION

### Meaning

The specified position within the action list is invalid.

## IDA034C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA034C SYNTAX ERROR IN SYSTEM HOOK PROGRAM LINE '(&00)' OF ACTION '(&01)'

## IDA034D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA034D SYSTEM HOOK PROGRAM OF ACTION '(&00)' TOO LARGE

## IDA034E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA034E DMS ERROR '(&00)' FOR FILE '(&01)'

## IDA034F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA034F BLOCK SIZE OF FILE '(&00)' IS NOT STD(1)

## IDA0340

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0340 EXCLUSIVE RIGHT FOR SYSTEM HOOKS NOT PRESENT

### Meaning

The task does not have the exclusive right for system hooks.

## IDA0341

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0341 SPECIFIED LOCK NOT HELD

## IDA0342

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0342 INVALID TASK SPECIFICATION

### Meaning

Besides leading blanks, only the characters (0..9,A..Z) are allowed.
A digit must not succeed a leading blank.

## IDA0343

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0343 OUTPUT ABORTED DUE TO REQUESTED LIMITATION

### Meaning

The number of output records was limited by the operand RECORDS.

## IDA0344

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0344 DIFFERENT SIZE FOR EXISTING LOGGING BUFFER NOT SUPPORTED

## IDA0345

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0345 VERIFICATION ERROR IN SYSTEM HOOK PROGRAM LINE '(&00)' OF ACTION '(&01)'

## IDA0346

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0346 SYSTEM HOOK PROGRAM OF ACTION '(&00)' EMPTY

## IDA0347

Destination: USER-TASK, CONSOLE Routing code: 1 Weight: 99

Warranty : NO

IDA0347 THE EXCLUSIVE RIGHT FOR SYSTEM HOOKS WAS ASSIGNED TO THIS TASK

### Meaning

In the moment, this task has the exclusive right for special
system hook commands.

## IDA0348

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

IDA0348 '(&00)' SYSTEM HOOKS REMOVED. '(&01)' ARE CURRENTLY IN THE SYSTEM

## IDA0349

Destination: USER-TASK, CONSOLE Routing code: 1 Weight: 99

Warranty : NO

IDA0349 SYSTEM HOOK '(&00)' SET

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages