## SCDCOPY

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

SCDCOPY Copyright (C) (&00) (&01) All Rights Reserved

## SCDLOAD

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

SCDLOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## SCD0001

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0001 '(&00)' NO INTERRUPT

### Meaning

An input/output operation by SCDM was started to the System Connection
Director (&00) without an I/O interruption.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0002

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0002 '(&00)' CHANNEL STATUS BYTE ERROR , EFB='(&01)' , CSB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) was terminated with channel status byte error.
(&01) = Executive Flag Byte, (&02) = Channel Status Byte.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0003

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0003 '(&00)' PATH NOT OPERATIONAL , EFB='(&01)' , CHPID='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed, because the channel path (&02) was not operational.
(&01) = Executive Flag Byte.

### Response

Check SCD (&00) and channel path (&02), call maintenance if necessary.

## SCD0004

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0004 '(&00)' COMMAND REJECT , USB='(&01)' , SB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&01) = Unit Status Byte , (&02) = Sense Bytes.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0005

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0005 '(&00)' BUS OUT CHECK , USB='(&01)' , SB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&01) = Unit Status Byte , (&02) = Sense Bytes.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0006

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0006 '(&00)' EQUIPMENT MALFUNCTION , USB='(&01)' , SB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&01) = Unit Status Byte , (&02) = Sense Bytes.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0007

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0007 '(&00)' SCD DISKETTE NOT READY , USB='(&01)' , SB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&01) = Unit Status Byte , (&02) = Sense Bytes.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0008

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0008 '(&00)' BUFFER OVERRUN , USB='(&01)' , SB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&01) = Unit Status Byte , (&02) = Sense Bytes.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0009

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0009 '(&00)' UNDEFINED ERROR , USB='(&01)' , SB='(&02)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&01) = Unit Status Byte , (&02) = Sense Bytes.

### Response

Check SCD (&00) and call maintenance if necessary.

## SCD0010

Destination: CONSOLE Routing code: G Weight: 70

Warranty : NO

SCD0010 WARNING; A POSSIBLE INVALID ATTACHMENT OF THE SCD '(&00)' HAS BEEN DETECTED. PORT NUMBER '(&01)' , PORT ADDRESS '(&02)' , USB='(&03)' , SB='(&04)'

### Meaning

An input/output operation by SCDM to the System Connection Director
(&00) failed.
(&03) = Unit Status Byte , (&04) = Sense Bytes.

### Response

Check attachment to port (&02) at SCD (&00) and call maintenance
if necessary.

## SCD0101

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0101 SCD DEVICE '(&00)' DETACHED

### Meaning

The System Connection Director device (&00) is detached from the
system. A program support of the device is only possible if the
device is attached.

### Response

Attach device (&00).

## SCD0102

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0102 ATTACH DEVICE

### Meaning

The device should be attached.

### Response

Attach device.

## SCD0103

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0103 NO I/O RIGHT

### Meaning

The I/O right for the device has been lost.

### Response

Check device status.

## SCD0104

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0104 SCD I/O ERROR

### Meaning

An input/output operation to the System Connection Director failed.

### Response

Check SCDM console messages and call maintenance if necessary.

## SCD0105

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0105 SCD MODIFY I/O FAILED

### Meaning

An input/output operation by SCDM to the System Connection Director
failed.

### Response

Check the SCDM console messages and call maintenance if necessary.

## SCD0106

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0106 INITIALIZATION ERROR

### Meaning

An error occurred in the program initialization.

### Response

Restart program.

## SCD0107

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0107 BOURSE ERROR

### Meaning

Communication problem in the program initialization.

### Response

Restart program.

## SCD0108

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0108 WRONG PARAMETER

### Meaning

The input string contains a syntactical error.

### Response

Correct input and restart order.

## SCD0109

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0109 WRONG SCD ID

### Meaning

The name of the SCD was wrong.

### Response

Correct name and restart order.

## SCD0110

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0110 WRONG PORT ADDRESS

### Meaning

The specification of the SCD port was not correct.

### Response

Correct port address and restart order.

## SCD0111

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0111 REQUEST MEMORY ERROR

### Meaning

The program could not get enough memory for execution.

## SCD0112

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0112 RECONFIGURATION IMPOSSIBLE

### Meaning

The path reconfiguration caused by a SCD port modification failed.

## SCD0113

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0113 PORT ALREADY BLOCKED

### Meaning

A SCD port which should be blocked is already blocked.

## SCD0114

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0114 PORT ALREADY UNBLOCKED

### Meaning

A SCD port which should be unblocked is already unblocked.

## SCD0115

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0115 NO SCD-PORT FOR CHANNEL '(&00)' FOUND. CHECK CONFIGURATION

### Meaning

SCDM didn't found a SCD port for channel (&00) for which a SCD
was generated.

### Response

Check system generation, SCD cables and/or SCD-Port-States.

## SCD0116

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0116 SCD-DEFINITION FOR CHANNEL '(&00)' INCORRECT. CHECK CONFIGURATION

### Meaning

SCDM found a SCD port for channel (&00) for which no SCD was
generated.

### Response

Check system generation, SCD cables and/or SCD-Port-States.

## SCD0117

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0117 NODE DESCRIPTOR INFORMATION FOR CONTROL UNIT '(&00)' AT SCD '(&01)' PORT ADDRESS '(&02)' UNDEFINED. CHECK CONFIGURATION.

### Meaning

SCDM didn't found a link neighbour for the port (&02) at the System
Connection Director (&01). By system generation the control unit
(&00) should be connected to this port.

### Response

Check system generation, SCD cables and/or SCD-Port-states.

## SCD0118

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0118 NODE DESCRIPTOR TYPE FOR CONTROL UNIT '(&00)' AT SCD '(&01)' PORT ADDRESS '(&02)' NOT EQUAL TO DEFINED TYPE. CHECK CONFIGURATION.

### Meaning

SCDM found a mismatch in the generated control unit type and in the
type of the neighbour node of the port (&02) at the System
Connection Director (&01).

### Response

Check system generation, SCD cables and/or SCD-Port-States.

## SCD0119

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0119 NODE DESCRIPTOR INFORMATION FOR CU '(&00)' AT SCD '(&01)' PORT ADDRESS '(&02)' NOT VALID. CHECK CONFIGURATION.

### Meaning

SCDM didn't find a valid link neighbour information for the port
(&02) at System Connection Director (&01) and control unit (&00).

### Response

Check system generation, SCD cables and/or SCD-Port-States.

## SCD0120

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0120 NODE DESCRIPTORS FOR DEVICES ON CONTROL UNIT '(&00)' NOT EQUAL. CHECK CONFIGURATION.

### Meaning

SCDM found different link neighbours for System Connection Director
ports, to which the one and only control unit (&00) schould be
connected.

### Response

Check system generation, SCD cables and/or SCD-Port-States.

## SCD0121

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0121 LINK NEIGHBOUR FOR CHANNEL '(&00)' NOT KNOWN. CHECK CONFIGURATION.

### Meaning

SCDM didn't find a link neighbour for channel (&00).

### Response

Check system generation, SCD cables and/or SCD-Port-States.

## SCD0122

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0122 ADD SCD LINKS AND CHECK SCD CONFIGURATION

### Meaning

Define the links for chained System Connection Directors with
ADD-SCD-LINK and check configuration with CHECK-SCD-CONF.

## SCD0123

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0123 DEDICATED CONNECTION FOR PORT '(&00)' AT SCD '(&01)' MISSING. CHECK CONFIGURATION.

### Meaning

SCDM found a missing dedicated connection for the port (&00) at
the System Connection Director (&01).

### Response

Check SCD configuration.

## SCD0124

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SCD0124 INPUT WRONG; CORRECT AND RETRY.

### Meaning

Wrong SCDM order.

### Response

Correct input and retry.

## SCD0125

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SCD0125 LOADING OF SUBSYSTEM SCDM TERMINATED ABNORMALLY

### Meaning

Subsystem SCDM could not be loaded.

### Response

Contact system administrator.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages