## YDT0000

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT0000 SET-COMM-TRACE successfully completed for (&00)

## YDT0001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT0001 SET-COMM-TRACE has no effect

### Meaning

No changes were required

## YDT0002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT0002 Trace options changed for component (&00)

## YDT0003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT0003 Trace options changed for external user (&00)

## YDT1001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1001 BCAM error: (&00) at T-DIAGDATA-SEND

### Meaning

Call failed because of BCAM version or param error

### Response

See BCAM return code

## YDT1002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1002 Error in parameter (&00)

### Meaning

Command syntactically incorrect

### Response

Correct and retry

## YDT1003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1003 Foreign TSN ((&00)) not possible

### Meaning

No privilege for foreign TSN

### Response

Only own TSN or '*OWN' is allowed

## YDT1004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1004 Foreign UID ((&00)) not possible

### Meaning

No privilege for foreign UID

### Response

Only own UID or '*OWN' is allowed

## YDT1005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1005 Only key word (&00) is allowed

### Meaning

Wrong key word specified

### Response

Correct and retry

## YDT1006

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1006 No event group found for (&00)

### Meaning

Modification of trace options requires an event group

### Response

Retry later

## YDT1007

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1007 No task found for TSN (&00)

## YDT1008

Destination: USER-TASK Routing code: Weight:

Warranty : NO

YDT1008 Userid (&00) does not exist

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages