## HWM0000

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0000 HMW - Messages of the X2000 package SMAWLhwm ( Hardware Monitor )

### Meaning

The X2000 package SMAWLhwm monitors tape devices of the type
9084-110 und 9084-221.
The devices to be monitored must be registered in the file
/etc/host.
The executing cron job
<BASEDIR>/SMAWLhwm/check_dev_status.sh
can be adapted.
The file
/etc/opt/SMAW/X2000/SMAWLhwm.conf
can be supplied e.g. with email addresses.
See the manual
MTC Charger 9084-110 and 9084-221F / Operation under BS2000/OSD
and the documents mentioned there.

## HWM0001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0001 No entry for device type 9084-110/221 in /etc/hosts

### Meaning

There is no entry for a tape device of type 9084-110/221 in /etc/hosts.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Configure the devices to be monitored.
Format of an entry in /etc/hosts:
< IP-Address> <Name> # 9084-110 or 9084-221
If no tape device shall be monitored, deactivate the cron job
<BASEDIR>/SMAWLhwm/check_dev_status.sh.

## HWM0101

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0101 Device (&00): Not reachable

### Meaning

The specified device ist not reachable by the monitor.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Check the status of the device:
-> Failed or switched off or taken out ?
-> Not connected to the LAN / connection interrupted / wrong address ?
If the device shall no longer be monitored, please remove the entry or
the tag 9084 from the /etc/hosts file.

## HWM0111

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0111 Device (&00): Only (&01) cleaning cycles left

### Meaning

With the cleaning tape of the specified device just
a few cleaning cycles can be executed.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Please order a new cleaning tape in due time and
insert it into the device, when RemainingCleanCount = 0.
Reinitialize the value of RemainingCleanCount. This value can
be found in the description of the used cleaning tape.

## HWM0112

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0112 Device (&00): Option AutoClean not activated

### Meaning

The AutoClean option has not been activated for the specified device.
Consequence: No automatic cleaning can be executed.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

To enable automatic cleaning please set the AutoClean option
using the operator panel or the web-interface.

## HWM0113

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0113 Device (&00): Option CleanSlot not activated

### Meaning

The CleanSlot option ( marks the slot as slot for the cleaning tape )
for the specified device has not been activated.
Consequence: No cleaning can be executed.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

To enable cleaning please set the CleanSlot option using the
operator panel or the web-interface.

## HWM0114

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0114 Device (&00): CleanSlot index ( value (&01) ) incorrectly configured

### Meaning

A wrong slot has been chosen to be the slot for the cleaning tape.
Consequence: No cleaning can be executed.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

The correct setting is:
9084-110 --> Slot 10
9084-221 --> Slot 21

## HWM0115

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0115 Device (&00): Clean slot (&01) empty or incorrectly supplied

### Meaning

There is no (valid) cleaning tape in the cleaning slot.
Consequence: No cleaning can be executed.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Please supply the cleaning slot with a correctly labeled cleaning tape.

## HWM0121

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0121 Device (&00): Error state (&01)

### Meaning

The tape library notifies the specified error.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Please check the state of the device.
For this, use also the documentation given in the manual
MTC Charger 9084-110 and 9084-221F / Operation under BS2000/OSD.

## HWM0131

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0131 Device (&00): Erroneous state of power supply #(&01)

### Meaning

The tape library notifies an error concerning the power supply.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Please check the state of the device.
For this, use also the documentation given in the manual
MTC Charger 9084-110 and 9084-221F / Operation under BS2000/OSD.

## HWM0141

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HWM0141 Device (&00): Erroneous state of fan #(&01)

### Meaning

The tape library notifies an error concerning a fan.
( Message displayed by the X2000 package SMAWLhwm ( Hardware Monitor ). )

### Response

Please check the state of the device.
For this, use also the documentation given in the manual
MTC Charger 9084-110 and 9084-221F / Operation under BS2000/OSD.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages