## NDICOPY

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

NDICOPY Copyright (C) (&00) (&01) All Rights Reserved

## NDILOAD

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

NDILOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## NDIREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NDIREVI COMP=NDIMF, VER=012, DATE=170412

### Meaning

NDI0450 - NDI0499: CONFUPD, responsible is OS2
NDI0500 - NDI0549: IOC, responsible is OS2
NDI0580 - NDI0599: IOTRACE, responsible is OS2
NDI0600 - NDI0649: NDIINIT, responsible is OS2
NDI0700 - NDI0899: IOC-CMD, responsible is OS2

## NDI0450

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0450 DEVICE TYPE INVALID OR INCOMPATIBLE WITH TYPE TO BE SUBSTITUTED

### Meaning

The type code does not denote a device type or is, as a device type,
incompatible with the device type to be replaced.

## NDI0451

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0451 DEVICE '(&00)' NOT FOUND

### Meaning

Device mnemonic (&00) does not exist in the device table.

## NDI0452

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0452 SYNTAX ERROR IN OPERAND

## NDI0453

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0453 DEVICE '(&00)' ALREADY EXISTS

### Meaning

The device table already contains another device with mnemonic
(&00).

## NDI0454

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0454 RENAMING OF CONSOLE DEVICE '(&00)' NOT POSSIBLE

### Meaning

The old mnemonic (&00) refers to a console device in the
device table. The mnemonic of a console device cannot be changed.

## NDI0455

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0455 INCORRECT OPERATION

## NDI0456

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0456 SYSTEM ERROR. CONFUPD TERMINATED ABNORMALLY

### Response

Take dump to aid error analysis.

## NDI0458

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0458 VALUE '(&00)' NOT A VALID IOC NUMBER

## NDI0460

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0460 MAXIMUM '(&00)' QUANTITY REACHED

### Meaning

An additional unit of the kind (&00) cannot be defined.
Abbreviations used for (&00):
IOC I/O Controller
CHN Channel
BYC Bytemultiplex Channel
BLC Blockmultiplex Channel
CTL Control Unit
DCU Disk Control Unit
TCU Tape Control Unit
CCU Console Control Unit

## NDI0461

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0461 CONTROL PROGRAM NOT CREATED FOR 'BASIC UPDATE'. 'BASIC UPDATE' NOT AVAILABLE

### Meaning

The control program does not contain the dummy configuration tables
required by the basic update function.

## NDI0462

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0462 DOUBLE DEFINITION OF DEVICE ADDRESS '(&00)'. CONFIGURATION INVALID

### Meaning

It is not possible to define device address (&00) for two devices.

## NDI0463

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0463 DEVICE DEFINITION FOR CONSOLE CONTROL UNIT '(&00)' INCOMPLETE. CONFIGURATION INVALID

### Meaning

For the console control unit (&00), either a display has been defined
without a corresponding hardcopy, or a hardcopy has been defined
without a corresponding display.

## NDI0464

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0464 '(&00)' '(&01)' REFERRED TO BUT NOT DEFINED. CONFIGURATION INVALID

### Meaning

A CHN, CTL or DVC statement refers to a unit (&01) of the kind (&00)
(abbreviation as in NDI0460). However, a statement to define this
unit has not been supplied.

## NDI0465

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0465 MNEMONIC '(&00)' ALREADY USED

### Meaning

The mnemonic (&00) has already been used to define a unit in a previous
statement. The mnemonic cannot be used for a second time.

## NDI0466

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0466 ATTACHMENT NUMBER '(&00)' AT '(&01)' '(&02)' ALREADY DEFINED

### Meaning

An attachment with number (&00) has already been assigned to the
unit (&02) of the kind (&01) (abbreviation as in NDI0460). A second
attachment to this unit with the same number is not possible.

## NDI0467

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0467 IOC NUMBER '(&00)' ALREADY DEFINED

## NDI0468

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0468 DEFINITION OF '(&00)' '(&01)' INCOMPATIBLE WITH ATTACHMENTS. CONFIGURATION INVALID

### Meaning

The unit (&01) of the kind (&00) (abbreviation as in NDI0460) is
incompatible with the attachments assigned to it.

## NDI0469

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0469 INVALID HARDCOPY ASSIGNMENT

## NDI0470

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0470 MAXIMUM '(&00)' QUANTITY FOR '(&01)' '(&02)' REACHED

### Meaning

The assignment of an additional attachment of the kind (&00) to the
unit (&02) of the kind (&01) is not possible (abbreviations as in
NDI0460).

## NDI0471

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0471 REFERENCE TO ADDITIONAL '(&00)' NOT POSSIBLE. MAXIMUM REACHED

### Meaning

The present DVC statement refers to a unit of the kind (&00)
(abbreviation as in NDI0460). However by preceding DVC statements,
the maximum quantity allowed for this kind of unit has already been
introduced into the configuration.

## NDI0472

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0472 NO REFERENCE TO '(&00)' '(&01)'. DEFINITION IGNORED

### Meaning

The unit (&01) of the kind (&00) (abbreviation as in NDI0460) will not
be taken into account, as it is neither a device nor, in another
statement, referred to.

## NDI0473

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0473 NO '(&00)' DEFINITION. CONFIGURATION INCOMPLETE

### Meaning

There must be at least one unit of the kind (&00) (abbreviation as in
NDI0460) in the configuration.

## NDI0474

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0474 NO '(&00)' DEVICE DEFINED. CONFIGURATION INCOMPLETE

### Meaning

There must be at least one device of the kind (&00) in the configuration.

## NDI0475

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0475 MAXIMUM '(&00)' QUANTITY AT CHANNEL '(&01)' EXCEEDED. CONFIGURATION INVALID

### Meaning

At the channel (&01), the maximum number allowed for units of
the kind (&00) (abbreviation as in NDI0460) has been exceeded.

## NDI0476

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0476 INCORRECT DEVICE ADDRESS OF DISPLAY OR HARDCOPY. CONFIGURATION INVALID

### Meaning

The present configuration requires a display with device address '0014'
and a hardcopy with device address '0015' or two units of device-
type '64' with the device addresses '0014' and '0015' to connect
displays. These requirements are not satisfied.

## NDI0477

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0477 INCORRECT HARDCOPY DEFINITION. CONFIGURATION INVALID

### Meaning

The present configuration requires a hardcopy defined with type '0B'.
This requirement is not satisfied.

## NDI0479

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0479 'BASIC UPDATE' ABORTED

### Meaning

The error described in the preceding message caused the basic update to
be terminated abnormally.

## NDI0480

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0480 'BASIC UPDATE' COMPLETED

### Meaning

The configuration tables have been generated.

## NDI0481

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0481 'DEVICE UPDATE' COMPLETED

### Meaning

The device table has been updated.

## NDI0482

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0482 INCORRECT CONSOLE MNEMONIC

### Meaning

The present configuration requires a display with mnemonic 'C2' and
a hardcopy with mnemonic 'C3' or two units of device-type '64' with
mnemonics 'C6' and 'C7' to connect displays. These requirements are
not satisfied.

## NDI0483

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0483 INCORRECT CONSOLE ASSIGNMENT

### Meaning

The present configuration requires a display of device-type '03' or
two units of device-type '64' to connect displays. These requirements
are not satisfied.

## NDI0484

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0484 INCORRECT CHANNEL DEFINITION

### Meaning

A bytemux-channel and a type2-bus-channel are defined in the
present configuration.

## NDI0500

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0500 ERROR IN DJCTRL

## NDI0501

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0501 SAME PATHS TO DIFFERENT PDT ENTRIES

## NDI0502

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0502 BOURSE ERROR

## NDI0503

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0503 IOC NOT AVAILABLE. RESTART NOT POSSIBLE

## NDI0504

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0504 ERROR IN KAI HANDLING

## NDI0505

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0505 ERROR WHILE SCHEDULING CONTINGENCY

## NDI0510

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0510 INVALID CCB ADDRESS

## NDI0511

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0511 INVALID HDV

## NDI0512

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0512 INVALID DEVICE ACCESS IN MAIN

## NDI0513

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0513 INVALID DEVICE ACCESS IN DEREND

## NDI0514

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0514 WAIT CALLER IS NOT EXCP CALLER

## NDI0520

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0520 $RETMEM-ERROR DETECTED BY NDICIODP.

### Meaning

In the module NDICIODP an error was detected for return memory.

## NDI0525

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0525 NDICURP HAS DETECTED AN ERROR BY $GETMEM OR $RETMEM FOR THE CONTROL-PACKET AND WRITE A SERSLOG-ENTRY.

### Meaning

In the module NDICURP an error was detected for allocation or
deallocation of memory for the control-packet.

## NDI0526

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0526 NDICURP HAS DETECTED AN ERROR FOR $DOER- OR $NDPIOL-CALL AND WRITE A SERSLOG-ENTRY.

### Meaning

In the module NDICURP an error was detected for $DOER- or
$NDPIOL-call.

## NDI0530

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0530 $NBCREA-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for bourse-creation.

## NDI0531

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0531 $CREAT-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for task-creation.

## NDI0532

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0532 THE TASK HAS CROSSED THE RESTARTLIMIT.

### Meaning

For the task an restart-routine was declared via #ENER. If this restart-
routine was entered, a restartcounter will be incremented by one.
If the restartcounter has crossed the restartlimit, the task will be
terminated.

## NDI0533

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0533 $ENER-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for the declaration of the
restart-routine via $ENER.

## NDI0534

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0534 $NBRORD-ERROR DETECTED BY NDIAMPR

### Meaning

In the module NDIAMPR an error was detected for receive an order from
an orderbourse.

## NDI0535

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0535 $NBSORD-ERROR DETECTED BY NDIAMPR

### Meaning

In the module NDIAMPR an error was detected for send an order to an
orderbourse.

## NDI0536

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0536 $NBSSIG-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for send an signal to the
bourse.

## NDI0537

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0537 $NBREPLY-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for a request-reply at the
order-bourse.

## NDI0538

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0538 $GETMEM-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for the request of memory.

## NDI0539

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0539 $RETMEM-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for the return of memmory.

## NDI0540

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0540 $DARMGT-ERROR DETECTED BY NDIAMPR.

### Meaning

In the module NDIAMPR an error was detected for establish or release an
device-access-right (DAR).

## NDI0541

Destination: CONSOLE Routing code: G Weight: 99

Warranty : YES

NDI0541 ATTENTION INTERRUPT LIMIT FOR DEVICE '(&00)' EXCEEDED.

### Meaning

Too many attention interrupts received for device (&00).

### Response

Switch off device (&00) and call maintenance.

## NDI0550

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0550 IOCONF PARAMETER SERVICE: (&00) INSTRUCTIONS READ, (&01) INSTRUCTIONS IGNORED DUE TO ERRORS.

### Meaning

(&00) instructions were received and handled by the IOCONF parameter
service, (&01) instructions were ignored because of a syntactical error
or because of invalid params. Up to 10 of these instructions will be
showed by the following NDI0551-messages.

### Response

None. For the next Startup correct your param-file.

## NDI0551

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0551 (&00) ERROR IN THE FOLLOWING INSTRUCTION: (&01)

### Meaning

The IOCONF parameter service detected an error in this instruction.
The instruction is ignored.

### Response

Correct the instruction for the next STARTUP.

## NDI0580

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0580 SYSTEM ERROR IN IOTRACE.

### Response

Take dump for error analysis.

## NDI0581

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0581 ERROR DURING SYSTEM CALL. IOTRACE ABORTED. DIAGNOSTIC INFORMATION: '(&00)'

### Meaning

(&00): Diagnostic information
(Interface name, function id, returncode, call id)

### Response

Contact system administrator.

## NDI0582

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0582 ERROR WHEN ACCESSING IOTRACE MODULE LIBRARY

### Meaning

An error occurred when DSSM attempted to access the IOTRACE module
library.
Possible reasons :
- library does not exist
- library is read-protected
- incorrect version of the subsystem

### Response

Install IOTRACE module library with correct version.
Library must not be read-protected.

## NDI0583

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0583 IOTRACE > (&00)

### Meaning

An IOTRACE information is issued.
(&00) : Self explaining, language-independent text

## NDI0600

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0600 FOUND DEVICE TYPE '(&00)' OF DEVICE '(&01)' INCOMPATIBLE WITH DEVICE TYPE IN SYSTEM TABLES

### Meaning

The physical device, which has the same device address as the device
with mnemonic (&01) in the device table, is found to have device
type (&00). This device type is incompatible with the corresponding
device type in the device table.

### Response

Check, whether the correct BS2000 file was selected for STARTUP.

## NDI0601

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0601 VOLUMES ON '(&00)' (PATH '(&01)') AND '(&02)' (PATH '(&03)') BOTH HAVE THE SAME VSN. POSSIBLY INCORRECT PATH DEFINITION

### Meaning

Due to the BS2000 configuration tables, path (&01) belongs to device
(&00) and path (&03) belongs to device (&02).
This may be not correct, since the volume labels read via both paths
are identical.

### Response

Check, whether the correct BS2000 file was selected for STARTUP.
If the configuration tables are correct, disable the access to one
of the equally labelled volumes.

## NDI0602

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0602 INCONSISTENT SUBCHANNEL NUMBERS. SYSTEM TABLES ASSIGN VALUE '(&00)', IOCF ASSIGNS VALUE '(&01)' TO DEVICE '(&02)'

### Meaning

For the device with mnemonic (&02), the subchannel number (&00) in
the BS2000 configuration tables does not agree with the subchannel
number (&01) in the IOCF.

### Response

Check, whether the correct BS2000 file and the correct IOCF were
selected for STARTUP.

## NDI0603

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0603 CHANNEL PATH WITH ID '(&00)' FOR DEVICE '(&01)' NOT IN SYSTEM TABLES

### Meaning

According to the IOCF, the device with the mnemonic (&01) is attached
to the channel with the number (&00). This attachment has however
not been defined in the BS2000 configuration tables.

### Response

Check, whether the correct BS2000 file and the correct IOCF were
selected for startup.

## NDI0604

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0604 NO AVAILABLE PATH TO DEVICE '(&00)' IN SYSTEM TABLES

### Meaning

There is no path for the device with mnemonic (&00) in the BS2000
configuration tables matching a path for this device in the IOCF.

### Response

Check, whether the correct BS2000 file and the correct IOCF were
selected for startup.

## NDI0605

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0605 CHANNEL TYPE DEFINED FOR DEVICE '(&00)' DIFFERS FROM CHANNEL TYPE INDICATED BY THE DCS

### Meaning

The device with mnemonic &00 is attached to a channel, of which the type
defined in the configuration cards does not agree with the channel type
indicated by the DCS in the subchannel of this device.

## NDI0606

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0606 CHANNEL TYPE DEFINED FOR CHANNEL '(&00)' INCOMPATIBLE WITH TYPE OF CPU OR DIFFERENT FROM CHANNEL TYPE INDICATED BY HARDWARE

### Meaning

The type of the channel with the mnemonic &00 that was defined in the
configuration cards is not allowed for the actual CPU type or does
not agree with the channel type that is indicated by the hardware for this
channel.

## NDI0607

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0607 EXPDT-VERSION (&00) IS INCOMPATIBLE TO BS2-SYSTEM-VERSION (&01).

### Response

Take dump for error analysis.

## NDI0608

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0608 EXPDT IS GENERATED FOR CPU-LINE (&00). ACTUAL CPU-LINE IS (&01).

### Response

Take dump for error analysis.

## NDI0609

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0609 NDIGDAT NOT FOUND IN EOLDTAB.

### Response

Take dump for error analysis.

## NDI0610

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDI0610 DIAGNOSIS COULD NOT BE EXECUTED.

### Response

Take dump for error analysis.

## NDI0700

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

NDI0700 IO INTERRUPT PARAMETERS MODIFIED

### Meaning

IO interrupt parameters have been modified with the command
"MODIFY-IO-PARAMETER".

## NDI0701

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NDI0701 SYNTAX ERROR IN COMMAND '(&00)'. COMMAND REJECTED

## NDI0702

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0702 SYNTAX ERROR IN OPERAND '(&00)'

## NDI0703

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0703 EXECUTION ERROR AT COMMAND '(&00)'

## NDI0704

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDI0704 CHANGE OF IO-CPU DETERMINATIONS FAILED. RC='(&00)'

## NDI0705

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDI0705 IO-CPU INFORMATION FAILED. RC='(&00)'

## NDI0706

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0706 OPERAND '(&00)' NOT SUPPORTED FOR THIS SERVER TYPE

## NDI0707

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0707 MODIFICATION OF IO PARAMETERS NOT POSSIBLE AT THE MOMENT

### Meaning

A change of the IO parameters is not possible, as a previous
modification is not yet completed.

## NDI0708

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0708 COMMAND NOT SUPPORTED

## NDI0720

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NDI0720 SUSPEND-IO REQUEST FOR HA-ID '(&00)' ACCEPTED. TSN OF THE EXECUTING TASK: '(&01)'

### Meaning

The SUSPEND-IO command was accepted and started. The execution is under
control of the specified task. Further messages to the progress of the
request will be sent to console.

## NDI0722

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0722 SUBSYSTEM SHC-OSD NOT AVAILABLE

### Meaning

The function to get the device mnemonics belonging to the HA-ID can not
be performed. The required subsystem SHC-OSD is not active.

### Response

Start subsystem SHC-OSD.

## NDI0723

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0723 SHC-OSD CALL TO GET DEVICES FOR HA-ID '(&00)' RETURNS '(&01)'

### Meaning

The call to the subsystem SHC-OSD to get the devices to the specified
HA-ID failed. (&01) gives a reason or contains the 8 hex-character
error information from SHC-OSD for this call.

## NDI0724

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0724 MEMORY-REQUEST RETURNS ERROR

## NDI0725

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0725 CREATION OF SYSTEM TASK RETURNS ERROR '&00'

## NDI0726

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0726 TOO MANY SUSPEND-IO-REQUESTS AT A TIME

## NDI0727

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0727 SUSPEND-IO REQUEST FOR THIS HA-ID ALREADY EXISTS

## NDI0728

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0728 HA-ID IS UNKNOWN

## NDI0729

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0729 Remote-Copy not active (Source-MN = '(&00)', Target-MN = '(&01)')

## NDI0730

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0730 INTERNAL ERROR

## NDI0731

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0731 Target-Disks not attached (Source-MN = '(&00)', Target-MN = '(&01)')

## NDI0732

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0732 Device Information ($NDIGIN) for disk with mnemonic '(&00)' returns error '(&01)'

## NDI0733

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0733 Mismatch of Remote-Copy types for disks '(&00)' and '(&01)'

## NDI0780

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0780 /SUSPEND-IO for HA-ID '(&00)' successfully completed

## NDI0781

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0781 IO-lock of HA-ID '(&00)' removed. IO resume on '(&01)'-disks

## NDI0790

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0790 /SUSPEND-IO for HA-ID '(&00)' terminated with error

## NDI0791

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0791 Switch of disks for HA-ID '(&00)' to target failed. ('(&01)')

### Meaning

The remount of the disks of the storage-cluster with the specified HA-ID
on the target disks failed. (&01) gives more details of the problem.

## NDI0792

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0792 SUSPEND-IO for HA-ID '(&00)' failed. ('(&01)')

## NDI0794

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0794 Console-Message to SUSPEND-IO request for HA-ID '(&00)' is not possible ('(&01)')

### Meaning

The message NDI0799 to continue a SUSPEND-IO request for the specified
HA-ID could not be sent to console. The request is aborted.

## NDI0795

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0795 Target disk of HA-ID '(&00)' is already in use.('(&01)')

## NDI0797

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0797 IO-REQUESTS FOR HA-ID '(&00)' SUSPENDED. WAITING FOR RESUME... REPLY (R(ESUME))

### Meaning

According to a SUSPEND-IO request for the specified HA-ID IO access
to all related disks is locked. A switch to target disks is possible
now. After reply of the message IO access will be readmitted.

## NDI0798

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0798 INVALID REPLY '(&00)'. REPLY IS IGNORED

## NDI0799

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NDI0799 IO-REQUESTS FOR HA-ID '(&00)' SUSPENDED. WAITING FOR RESUME... REPLY (*TA=ON TARGET, *SO=ON SOURCE)

### Meaning

According to a SUSPEND-IO request for the specified HA-ID IO access
to all related disks is locked. A switch to target disks is possible
now. After reply of the message IO access will be readmitted -
depending on the reply - on the target disks or as before on the
source disks.

## NDI0800

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0800 INTERNAL ERROR ON EXECUTION OF THE COMMAND 'SHOW-FC-INFORMATION'

## NDI0801

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0801 OPERAND ERROR IN COMMAND 'SHOW-FC-INFORMATION'

## NDI0802

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0802 NO MATCHING DATA EXIST

## NDI0803

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0803 MEMORY REQUEST FAILED

## NDI0804

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0804 ERROR ON CONFIGURATION REQUEST

## NDI0805

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0805 ERROR ON PORT-WWPN REQUEST

## NDI0806

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0806 ERROR ON CREATING S VARIABLES

## NDI0807

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NDI0807 ERROR IN OBTAINING THE IO DATA

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages