## ESMT006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESMT006 SYSTEM ERROR: HOLDER TASK TERMINATED ABNORMALLY

### Meaning

Holder task terminated abnormally in module ESMC4 (ENTRY 'ESMREC' or
ENTRY 'ESMCHOL')

### Response

Contact the system administrator

## ESMT007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESMT007 DSSM TASK TERMINATED ABNORMALLY

### Meaning

DSSM task terminated abnormally in module ESMCI (ENTRY 'ESMCIN' or
'ESMRECO')
DSSM: Dynamic Subsystem Management

## ESMT008

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESMT008 TASK CREATED BY CTCS OR HOLDER TASK TERMINATED NORMALLY

### Meaning

Normal termination of a task created in module ESMC4 (ENTRY 'ESMLST') by
CTCS function, or normal termination of a holder task
CTCS: Create Task and Connect to Subsystem

## ESMT009

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESMT009 DSSM TASK TERMINATED NORMALLY

### Meaning

DSSM task terminated normally in module ESMCI (ENTRY 'ESMCIN')
DSSM: Dynamic Subsystem Management

## ESMT010

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ESMT010 CREATOR INTERFACE CALLED WITH INVALID '$DSSMFCT'

### Meaning

Call effected in module ESMC4 (ENTRY 'ESMCRE')

## ESM0200

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

ESM0200 DSSM STARTUP OPERAND VALUE '(&00)' INVALID. ENTER NEW VALUE

### Meaning

A value for a DSSM startup operand is incorrect and a new value,
for example the name of the subsystem catalog, is requested
(&00): value for a DSSM startup operand
DSSM: Dynamic Subsystem Management

### Response

Ask the operator to enter a new value

## ESM0201

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0201 SUBSYSTEM '(&00)' NOT FOUND

### Meaning

Possible reasons:
- spelling error
- missing declaration in the subsystem catalog
(&00): name (and version number) of the subsystem

### Response

Retry with correct name or check if subsystem is declared in the current
subsystem catalog

## ESM0202

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0202 SUBSYSTEM '(&00)' NOT LOADED. COMMAND REJECTED. ENTER /START-SUBSYSTEM

### Meaning

/RESUME-SUBSYSTEM command cannot be processed
(&00): name and version number of the subsystem

### Response

Try /START-SUBSYSTEM command instead of /RESUME-SUBSYSTEM command

## ESM0203

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0203 SUBSYSTEM '(&00)' NOT CREATED

### Meaning

(&00): name and version number of the subsystem

## ESM0204

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0204 FUNCTION '(&01)' FOR SUBSYSTEM '(&00)' ALREADY PROCESSED

### Meaning

Requested function already processed due to the preceding function
(&00): name and version number of the subsystem
(&01): CREATE or DELETE or RESUME or HOLD

## ESM0205

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0205 SUBSYSTEM '(&00)' IS LOCKED

### Meaning

(&00): name and version number of the subsystem

## ESM0206

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0206 SOME ACTIONS IN PROGRESS FOR SUBSYSTEM '(&00)'. NO FURTHER ACTION ON ANOTHER VERSION POSSIBLE

### Meaning

The exchange mechanism is only allowed if one version of the subsystem is
'CREATED' and if all the other versions declared in the catalog have a
status equal to 'NOT-CREATED' or 'LOCKED'.
The exchange is not processed if all the declared versions of the
subsystem have the status 'NOT-CREATED' or 'LOCKED' but the version
specified in the command /START-SUBSYSTEM is simply created.
A version declared with VERSION-COEXISTENCE = *FORBIDDEN cannot coexist
with other versions of the same subsystem.
(&00): name and version number of the subsystem which prevents the
exchange or the coexistence

## ESM0207

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0207 SUBSYSTEM '(&00)' DOES NOT SUPPORT EXCHANGE OF VERSIONS

### Meaning

The specified subsystem version is declared with
VERSION-EXCHANGE=*FORBIDDEN
The requested function is not possible
(&00): name and version number of the subsystem

## ESM0208

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0208 FUNCTION '(&01)' FOR SUBSYSTEM '(&00)' IN PROCESS

### Meaning

If you have requested a function with the operand FORCED=*YES, you have to
wait the completion of the previous function called with FORCED=*NO
If you have requested a function with the operand RESET=*YES, you have to
wait the completion of the previous DELETE/HOLD function
(&00): name and version number of the subsystem
(&01): CREATE or DELETE or RESUME or HOLD

### Response

Verify the status of the subsystem and if it does not suit you, try again.

## ESM0209

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0209 SUBSYSTEM '(&00)' DOES NOT SUPPORT COEXISTENCE OF VERSIONS

### Meaning

The specified subsystem version is declared with
VERSION-COEXISTENCE=*FORBIDDEN.
The required function is not possible.
(&00): name and version number of the subsystem

## ESM0210

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0210 EXCHANGE FOR SUBSYSTEM '(&00)' NOT POSSIBLE BECAUSE THE VERSION TO BE EXCHANGED HAS NEITHER THE STATUS 'CREATED' NOR 'NOT CREATED'

### Meaning

Version to be exchanged is not yet loaded or unloaded
(&00): subsystem name

### Response

Wait for loading or unloading completion before creating the new version

## ESM0211

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0211 OPERAND 'RESET' IN FUNCTION '(&00)' IGNORED FOR SUBSYSTEM '(&01)', BECAUSE NOT IN STATE '(&02)'

### Meaning

(&00): CREATE or RESUME
(&01): subsystem name
(&02): IN-DELETE or IN-HOLD in contradiction to function (&00)

## ESM0212

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0212 SUBSYSTEM '(&00)' ALREADY LOADED, ONLY 'RESUME' PROCESSED

### Meaning

(&00): name and version number of the subsystem

## ESM0213

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0213 OPERAND 'VERSION' MANDATORY IN FUNCTION '(&00)' FOR SUBSYSTEM '(&01)' IF 'RESET=*YES'

### Meaning

(&00): CREATE or RESUME
(&01): subsystem name

## ESM0214

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0214 FUNCTION '(&00)' WITH 'RESET=*YES' PROHIBITED FOR SUBSYSTEM '(&01)'

### Meaning

The subsystem is declared with RESET=*FORBIDDEN in the
//SET-SUBSYSTEM-ATTRIBUTES statement
(&00): CREATE or RESUME
(&01): subsystem name

## ESM0215

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0215 DUE TO VERSION PARALLELISM THE VERSION MUST BE SPECIFIED IN FUNCTION '(&00)' FOR SUBSYSTEM '(&01)'

### Meaning

(&00): requested function
(&01): subsystem name

### Response

Reenter command with VERSION operand

## ESM0216

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0216 FUNCTION '(&01)' STARTED FOR SUBSYSTEM '(&00)'

### Meaning

(&00): name and version number of the subsystem
(&01): function CREATE or DELETE or RESUME or HOLD or RECOVERY

## ESM0217

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0217 FUNCTION '(&00)' OF SYNTAX FILE NOT YET SUPPORTED BY THIS SDF VERSION

### Meaning

(&00): SDF function

## ESM0218

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0218 'CREATE' OR 'RESUME' OR 'DELETE' OR 'HOLD' OR 'REMOVE' OR 'UNLOCK' NOT PROCESSED: SUBSYSTEM '(&00)' FROZEN

### Meaning

The subsystem is frozen until the next /MODIFY-SUBSYSTEM-PARAM command
with a CHANGE-STATE=*YES operand is entered
(&00): subsystem name and subsystem version number

## ESM0219

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

ESM0219 PROBLEM OCCURRED DURING '(&00)' OF SUBSYSTEM '(&01)' VERSION '(&02)'

### Meaning

(&00): INIT-ROUTINE or STOPCOM-ROUTINE or CLOSE-CTRL-ROUTINE or
DEINIT-ROUTINE and a returncode (RC).
RC = X'0000000C' means that the subsystem has rejected the call and is so
reset in the previous state
RC = X'0400000C' means that the subsystem has requested to be locked
(&01): subsystem name
(&02): subsystem version number

## ESM0220

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0220 FUNCTION '(&01)' FOR SUBSYSTEM '(&00)' COMPLETELY PROCESSED

### Meaning

(&00): name and version number of the subsystem
(&01): function CREATE or DELETE or RESUME or HOLD

## ESM0221

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0221 PROBLEM DURING FUNCTION '(&00)' OF SYNTAX FILE '(&01)' FOR SUBSYSTEM '(&02)'

### Meaning

(&00): SDF function
(&01): syntax file name
(&02): name and version number of the subsystem

## ESM0222

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0222 CONCURRENT FORCED REQUEST FOR FUNCTION '(&00)' FOR SUBSYSTEM '(&01)'

### Meaning

The request will soon be fulfilled because a forced service has been
requested by another task
(&00): name and version number of the subsystem
(&01): function DELETE or HOLD

## ESM0223

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0223 'FORCED' REJECTED FOR FUNCTION '(&00)' FOR SUBSYSTEM '(&01)'. TRY OPERAND 'FORCED=*NO' FIRST

### Meaning

(&00): function DELETE or HOLD
(&01): subsystem name

## ESM0224

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0224 REQUESTED FUNCTION '(&01)' FOR SUBSYSTEM '(&00)' REJECTED

### Meaning

The preceding message gives the reason of the error
(&00): name and version number of the subsystem
(&01): function CREATE or DELETE or RESUME or HOLD or UNLOCK

## ESM0225

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0225 OPERAND 'FORCED' FOR FUNCTION '(&00)' PROHIBITED FOR SUBSYSTEM '(&01)'

### Meaning

The subsystem is declared with FORCED-STATE-CHANGE=*FORBIDDEN in the
//SET-SUBSYSTEM-ATTRIBUTES statement
(&00): function DELETE or HOLD
(&01): subsystem name

## ESM0226

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0226 SUBSYSTEM '(&00)' CANNOT BE CREATED BECAUSE SUBSYSTEM '(&01)' NOT LOADED

### Meaning

A link relation exists between both subsystems
Loading of the first subsystem is impossible if the other one is not
loaded
(&00),(&01): subsystem name

## ESM0227

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0227 FUNCTION '(&01)' REJECTED BY SUBSYSTEM '(&00)'

### Meaning

The function is rejected by the subsystem during initialization or
deinitialization
(&00): name and version number of the subsystem
(&01): function CREATE/START-SUBSYSTEM or DELETE/STOP-SUBSYSTEM or
RESUME/RESUME-SUBSYSTEM or HOLD/HOLD-SUBSYSTEM

## ESM0228

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0228 FUNCTION '(&01)' FOR SUBSYSTEM '(&00)' TERMINATED ABNORMALLY

### Meaning

The preceding message gives the reason of the error
When a SYSTEM-ERROR occurs, the subsystem name is set to *UNKNOWN
(&00): name and version number of the subsystem
(&01): function CREATE/START-SUBSYSTEM or DELETE/STOP-SUBSYSTEM or
RESUME/RESUME-SUBSYSTEM or HOLD/HOLD-SUBSYSTEM or UNLOCK/UNLOCK-SUBSYSTEM

## ESM0229

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0229 INVALID HEADER. FUNCTION REJECTED

### Meaning

Possible reasons:
- an invalid interface version is used
- the function is not yet implemented

## ESM0230

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0230 FILE '(&00)' DOES NOT EXIST

### Meaning

(&00): file name

### Response

Create the missing file and try requested function again

## ESM0231

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

ESM0231 SYSTEM ERROR '(&00)' DETECTED BY DSSM

### Meaning

(&00): 1. error in bourse processing; hexadecimal value of
bourse return code follows
2. error in SVC table manipulation
3. error during EXIT routine activation or deactivation
4. error during task communication function
DSSM: Dynamic Subsystem Management

## ESM0232

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0232 WARNING: DEPENDENCE RELATION OR LINK RELATION VIOLATED BY SUBSYSTEM '(&00)'

### Meaning

Execution of the requested function would lead to violation of a
link or dependence relation
(&00): subsystem name

### Response

- if function CREATE or RESUME: create or resume all missing subsystems
- if function DELETE or HOLD: delete or hold all dependent subsystems
- if command /REMOVE-SUBSYSTEM: remove all dependent subsystems

## ESM0233

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0233 MESSAGE FILE '(&00)' NOT DELETED

### Meaning

(&00): name of the subsystem-specific message file

## ESM0234

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0234 DSSM INTERNAL ERROR. CONTACT THE SYSTEM ADMINISTRATOR

### Meaning

Send the following information to the developer:
- console log
- catalog (file) entry
- log of the TSOS task (if any)
- dump of the DSSM task
- DSSMLOG (if any)
DSSM: Dynamic Subsystem Management

## ESM0235

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0235 INVALID STATE FOR SUBSYSTEM '(&00)'

### Meaning

The subsystem state is not suitable for performing the current request
(&00): name and version number of the subsystem

## ESM0236

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0236 TASK FOR SUBSYSTEM '(&00)' NOT AVAILABLE

### Meaning

The subsystem task is not available
Possible reasons :
- the task could not be created due to a system error or a resource
bottleneck
- the task was terminated due to a system error or error of the subsystem
(&00): name and version number of the subsystem

## ESM0237

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0237 'FORCED' FOR FUNCTION 'DELETE' FOR SUBSYSTEM '(&00)' TOO EARLY. TRY AGAIN LATER

### Meaning

The request came before the end of the STOPCOM routine during the current
DELETE function
(&00): name and version number of the subsystem

## ESM0238

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0238 FUNCTION '(&00)' NOT PROCESSED, BECAUSE 'RESET' IN PROCESS

### Meaning

(&00): function DELETE or HOLD

## ESM0239

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0239 FUNCTION '(&00)' PROHIBITED FOR SUBSYSTEM '(&01)'

### Meaning

The subsystem is declared with SUBSYSTEM-HOLD=*FORBIDDEN in the
//SET-SUBSYSTEM-ATTRIBUTES statement
(&00): function DELETE or HOLD
(&01): subsystem name

## ESM0240

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0240 ENTRY '(&01)' FOR SUBSYSTEM '(&00)' NOT FOUND

### Meaning

After the loading of the subsystem one of the following
specified entries was missing:
ENTRY: INIT-ROUTINE, DEINIT-ROUTINE, STOPCOM-ROUTINE, CLOSE-CTRL-ROUTINE,
DYNAMIC-CHECK-ENTRY, INTERFACE-VERSION, SUBSYSTEM-ENTRIES
(&00): name and version number of the subsystem
(&01): name of the entry

## ESM0241

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0241 CHECK PATTERN FOR SUBSYSTEM '(&00)' INVALID

### Meaning

In the specified DYNAMIC-CHECK-ENTRY, the pattern
'name and version number of the subsystem' could not be found or does not
match with the name and version of the subsystem
(&00): name and version number of the subsystem

## ESM0242

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

ESM0242 LOADING OF SUBSYSTEM '(&00)' NOT PERFORMED. BLS RETURN CODE='(&01)'

### Meaning

(&00): name and version number of the subsystem
(&01): return code of the $PBBND1 interface

## ESM0243

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0243 CURRENT DSSM VERSION DOES NOT SUPPORT THE SPECIFIED COMMAND

### Meaning

DSSM: Dynamic Subsystem Management

## ESM0244

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0244 MEMORY POOL HANDLING FOR SUBSYSTEM '(&00)' NOT PROCESSED

### Meaning

A SERSLOG entry with RECTYPE=ESMERR and TITLE ESMEMPB has been written
(&00): name and version number of the subsystem

## ESM0245

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0245 INVALID INTERFACE VERSION IN ENTRY '(&01)' FOR SUBSYSTEM '(&00)'

### Meaning

Calling the INIT, DEINIT, CLOSE-CTRL or STOPCOM routine is unsuccessful,
since
the interface version is not supported by DSSM
(&00): name and version number of the subsystem
(&01): name of the entry where the interface version is declared
DSSM: Dynamic Subsystem Management

### Response

Contact the system administrator or use another subsystem version

## ESM0246

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0246 '(&00)' COMMAND PROHIBITED FOR SUBSYSTEM '(&01)'

### Meaning

The subsystem is declared with STATE-CHANGE-COMMAND=*FORBIDDEN in the
//SET-SUBSYSTEM-ATTRIBUTES statement
(&00): CREATE or RESUME or HOLD or DELETE or UNLOCK
(&01): subsystem name

## ESM0247

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0247 SYNTAX FILE IS NOT COMPATIBLE WITH THIS VERSION OF DSSM

### Response

Use the syntax file corresponding to the current DSSM Version

## ESM0248

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0248 SUBSYSTEM '(&00)' CANNOT BE INSTALLED

### Meaning

(&00): subsystem name

## ESM0249

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0249 SUBSYSTEM '(&00)' CANNOT BE DEINSTALLED

### Meaning

(&00): subsystem name

## ESM0250

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0250 SYSTEM ERROR: DSSM BOURSE NOT AVAILABLE; BOURSE RETURN CODE: '(&00)'

### Meaning

Possible reasons:
Error in bourse processing ,DSSM abnormally terminated or not yet
available
(&00): hexadecimal value of bourse function return code
DSSM: Dynamic Subsystem Management

## ESM0251

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0251 CONNECTION ERROR

## ESM0252

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0252 EXCHANGE FOR SUBSYSTEM '(&00)' NOT POSSIBLE BECAUSE THE VERSION TO BE EXCHANGED IS FROZEN

### Meaning

Version to be exchanged has been frozen by
/MODIFY-SUBSYSTEM-PARAMETER CHANGE-STATE=*NO command
Requested function not possible while subsystem is frozen
(&00): name and version number of the subsystem

## ESM0253

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0253 EXCHANGE FOR SUBSYSTEM '(&00)' NOT POSSIBLE BECAUSE FUNCTION 'DELETE' FOR THE VERSION TO BE EXCHANGED IS PROHIBITED

### Meaning

Version to be exchanged is declared with SUBSYSTEM-HOLD=*FORBIDDEN
The requested function is not possible
(&00): name and version number of the subsystem

## ESM0254

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0254 COMMAND '(&00)' COMPLETELY PROCESSED

### Meaning

(&00): command name

## ESM0255

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0255 '(&00)' COMMAND NOT PROCESSED

### Meaning

The reason of the error is given either in the preceding
messages or in the SYSLST
(&00): command name

## ESM0256

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0256 WHEN 'VERSION-PARALLELISM' REQUESTED, OPERAND 'VERSION' MANDATORY IN 'CREATE' FUNCTION FOR SUBSYSTEM '(&00)'

### Meaning

(&00): subsystem name

### Response

Reenter command specifying the VERSION operand

## ESM0257

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0257 OPERANDS 'RESET' AND 'VERSION-PARALLELISM=*EXCHANGE-MODE' MAY NOT BE SPECIFIED TOGETHER IN 'CREATE' FUNCTION FOR SUBSYSTEM '(&00)'

### Meaning

(&00): name and version number of the subsystem

### Response

Reenter the command without specifying VERSION-PARALLELISM=*EXCHANGE-MODE

## ESM0258

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0258 SUBSYSTEM '(&00)' NOT PRELOADED

### Meaning

The specified subsystem is declared with CREATION-TIME=*BEFORE-DSSM-LOAD,
but is not preloaded
(&00): name and version number of the subsystem

## ESM0259

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0259 SUBSYSTEM '(&00)' CANNOT BE RUN ON THE CURRENT BS2000 SYSTEM

### Meaning

A dependence relation has been declared between (&00) and 'CP', and
the current CP version is not in the range
(&00): name and version number of the subsystem

## ESM0260

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0260 ERROR OCCURRED DURING READING OF CATALOG '(&00)'. DMS RETURN CODE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

SPLDMS interface returned a DMS error
For more detailed information about the DMS error code enter /HELP-MSG
in system mode or see the BS2000 manual 'System Messages'
(&00): specified catalog name
(&01): DMS return code of the SPLDMS interface

### Response

Contact the system administrator

## ESM0261

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0261 NUMBER OF SUBSYSTEMS OR CALL ENTRIES IN CATALOG '(&00)' EXCEEDS LIMIT

### Meaning

(&00): specified catalog name

## ESM0262

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0262 SPECIFIED FILE '(&00)' NOT A VALID SUBSYSTEM CATALOG RC '(&01)'

### Meaning

We have found some inconsistencies during reading of the catalog
(&00): specified input string
(&01): return code
RC=1 file is not a catalog or is a catalog of a too old version
RC=2 catalog entry of the file has been modified since catalog generation
by SSCM
or the catalog has been modified without using SSCM
RC=3.x catalog has been modified without using SSCM. Catalog size is
invalid
RC=4.x catalog has been modified without using SSCM. number of subsystem
and/or number of relation invalid
RC=5.x catalog has been modified without using SSCM. Catalog contents is
corrupted

### Response

The subsystem catalog must be generated again

## ESM0263

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0263 ADDITION OF NEW CATALOG '(&00)' SUCCESSFUL

### Meaning

(&00): specified catalog name

## ESM0264

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0264 WARNING: CREATION-TIME OF SUBSYSTEM '(&00)' IS '*BEFORE-DSSM-LOAD', '*AT-DSSM-LOAD', '*MANDATORY-AT-STARTUP', '*BEFORE-SYSTEM-READY' OR '*AFTER-SYSTEM-READY'

### Meaning

The specified subsystem could not be created due to operand
CREATION-TIME of //SET-SUBSYSTEM-ATTRIBUTES statement in the catalog
(&00): name and version number of the subsystem

## ESM0265

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0265 ALTERATION OF ADDRESS SPACE STRIP BY NEW CATALOG '(&00)'. COMMAND NOT PROCESSED

### Meaning

The length of the address space to be reserved is greater in the new
catalog than in the current one. That may happen if subsystems
declared with MEMORY-CLASS=*LOCAL-PRIVILEGED are added to the new catalog
(&00): specified file name

## ESM0266

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0266 NEW CATALOG '(&00)' CHANGES THE PLACE OF SUBSYSTEM '(&01)' IN ADDRESS SPACE STRIP. COMMAND NOT PROCESSED

### Meaning

(&00): specified file name
(&01): name and version number of the subsystem

## ESM0267

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0267 SPECIFIED COMMAND PROCESSED ONLY WHEN SUBSYSTEM '(&00)' DELETED

### Meaning

The CREATION-TIME operand of the /MODIFY-SUBSYSTEM-PARAMETER command is
only
changed for a deleted subsystem
(&00): name and version number of the subsystem

### Response

Delete the specified subsystem. The CREATION-TIME operand of the
/MODIFY-SUBSYSTEM-PARAMETER command will be changed implicitly

## ESM0268

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0268 SUBSYSTEM '(&00)' HAS BECOME 'CREATION-TIME=*AT-SUBSYSTEM-CALL'

### Meaning

Possible reasons:
- the previously issued /MODIFY-SUBSYSTEM-PARAMETER command has been
processed
- the subsystem had been added with the /ADD-SUBSYSTEM command
(&00): name and version number of the subsystem

## ESM0269

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0269 SUBSYSTEM '(&00)' MUST HAVE AT LEAST ONE ENTRY WITH 'MODE=(&01)' TO BECOME '*AT-SUBSYSTEM-CALL(ON-ACTION=(&02))'

### Meaning

(&00): name and version number of the subsystem
(&01): entry mode that is necessary
(&02): action that induces the creation

## ESM0270

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0270 SEND SUBSYSTEM CATALOG FILE WITH CONSOLE OR TERMINAL LOG (/MOD-JOB-OPT OPER-INTER=*YES,LOG=PAR(LIST=*YES)) TO DIAGNOSTIC STAFF

## ESM0271

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0271 SEND DSSMLOG FILE TO DIAGNOSTIC STAFF

## ESM0272

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0272 HOLDER TASK '(&00)' TERMINATED ABNORMALLY

### Meaning

(&00): Task Sequence Number (TSN)

## ESM0273

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0273 TASK '(&00)' TERMINATED ABNORMALLY. DUMP OF DSSM TASK EFFECTED; SEND DUMP TO DIAGNOSTIC STAFF

### Meaning

(&00): Task Sequence Number (TSN)

## ESM0274

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0274 NEW CATALOG SMALLER THAN OLD CATALOG

### Meaning

The entire old catalog is not contained in the new catalog to
be used for the /ADD-SUBSYSTEM command

## ESM0275

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0275 SUBSYSTEM '(&00)' MISSING IN NEW CATALOG OR NOT IN SAME POSITION OR REMOVED IN OLD CATALOG

### Meaning

(&00): name and version number of the subsystem

## ESM0276

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0276 NEW CATALOG HAS ADDED OR REMOVED LINK OR DEPENDENCE RELATIONS FOR SUBSYSTEM '(&00)' FROM THE OLD CATALOG

### Meaning

(&00): name and version number of the subsystem

## ESM0277

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0277 NEW AND OLD SUBSYSTEMS SPECIFIED IN SAME //ASSIGN-HOLDER-TASK STATEMENT

## ESM0278

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0278 CATALOG '(&00)' INCOMPATIBLE WITH SYSTEM (XS OR NXS)

### Meaning

(&00): catalog name

## ESM0279

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0279 SHUTDOWN FOR SUBSYSTEM '(&00)' NOT POSSIBLE

### Meaning

(&00): name and version number of the subsystem

## ESM0280

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0280 '/MODIFY-SUBSYSTEM-PARAMETER' COMMAND NOT PROCESSED FOR SUBSYSTEM '(&00)' TO AVOID INCONSISTENCY IN CATALOG

### Meaning

(&00): name and version number of the subsystem

## ESM0281

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0281 MESSAGE FILE '(&00)' NOT ADDED TO SYSTEM MESSAGE FILE

### Meaning

(&00): name of the message file

## ESM0282

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0282 SYSTEM ERROR: DSSM BOURSE NOT CREATED; BOURSE RETURN CODE: '(&00)'

### Meaning

(&00): hexadecimal value of bourse function return code

## ESM0284

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0284 SUBSYSTEM CATALOG NOT LOADED FROM FILE '(&00)'. DMS RETURN CODE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The SPL interface returned an error
Possible reasons:
- subsystem catalog file not correct
- startup parameter service not provided with the correct file name
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'
(&00): file name
(&01): DMS error code

### Response

- generate the subsystem catalog
- provide the startup parameter service with the file name
- try the startup again

## ESM0285

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0285 ERROR '(&00)' ON '(&01)' OF DSSM. PLEASE ENTER A NEW VALUE ('(&02)')

## ESM0286

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0286 ERROR '(&00)' FOR SUBSYSTEM '(&01)'. PLEASE ENTER A NEW VALUE ('(&02)')

## ESM0287

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0287 DSSM ROUTINE FOR ENTRY '(&01)' OF SUBSYSTEM '(&00)' NOT GENERATED

### Meaning

(&00): name and version number of the subsystem
(&01): entry name

## ESM0288

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

ESM0288 SYSTEM-ERROR: DSSM BOURSE NOT AVAILABLE; BOURSE RETURN CODE: '(&00)'

### Meaning

Possible reasons:
- error in bourse processing
- DSSM terminated abnormally
- DSSM not yet initialized
(&00): hexadecimal value of bourse function return code

## ESM0290

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0290 //SEPARATE-ADDRESS-SPACE STATEMENT NOT PROCESSED

### Meaning

Not enough memory available to install the subsystems which are
specified in the //SEPARATE-ADDRESS-SPACE statement

### Response

Delete some of the subsystems in the same holder task

## ESM0291

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0291 SUBSYSTEM NOT CREATED AUTOMATICALLY

## ESM0292

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0292 NOT ENOUGH MEMORY AVAILABLE TO INSTALL SUBSYSTEM '(&00)'

### Meaning

(&00): name and version number of the subsystem

## ESM0293

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0293 ISL ENTRY '(&00)' NOT DECLARED IN ISL TABLE FOR SUBSYSTEM '(&01)'

### Meaning

Entry (&00) not usable
(&00): entry name
(&01): subsystem name

### Response

Have this entry inserted in the ISL table

## ESM0294

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0294 SYSTEM ERROR: STARTUP/SHUTDOWN TASK NOT NOTIFIED. BOURSE RETURN CODE: '(&00)'

### Meaning

In order to synchronously initialize itself, DSSM has locked the
startup/shutdown
task but cannot release it any more
(&00): hexadecimal value of bourse function return code

## ESM0295

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0295 DSSM DATA NOT INITIALIZED

### Meaning

DSSM: Dynamic Subsystem Management

## ESM0296

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0296 SYSTEM ERROR: REQM NOT PERFORMED

## ESM0297

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0297 DSSM ISL ENTRY '(&00)' NOT FOUND

### Meaning

(&00): entry name
DSSM: Dynamic Subsystem Management

## ESM0298

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0298 /SHOW-SUBSYSTEM-INFO SUBSYSTEM-NAME=*ALL COMMAND NOT PERFORMED. TRY AGAIN LATER

### Meaning

This error is due to a lake of memory in class 4 or 5

## ESM0299

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0299 ERROR OCCURRED DURING HOLDER TASK RECOVERY PROCESSING

## ESM0300

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0300 DATA CONTAINED IN DSSM CATALOG ARE INCONSISTENT. CONTACT THE SYSTEM ADMINISTRATOR

### Meaning

DSSM: Dynamic Subsystem Management

### Response

Contact the system administrator

## ESM0301

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0301 LOOP IN 'FUNCTIONAL DEPENDENCE' OR 'REFERENCE' RELATIONS

### Meaning

Loop exists after combining the two catalogs during /ADD-SUBSYSTEM
with TYPE=*NEW-SUBSYSTEMS

## ESM0302

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0302 IN THE CURRENT CATALOG, THERE IS ALREADY ANOTHER VERSION OF SUBSYSTEM '(&00)' DECLARED WITH 'CREATION-TIME=*AT-SUBSYSTEM-CALL'

### Meaning

Several versions of a subsystem with 'CREATION-TIME=*AT-SUBSYSTEM-CALL'
are permitted only if:
- they are declared with 'VERSION-COEXISTENCE=*ALLOWED'
- their entries declared with 'MODE=*SVC' have a 'FUNCTION-NUMBER' and a
'FUNCTION-VERSION' specified
- their entries declared with 'MODE=*ISL' and 'CONNECTION-ACCESS=*SYSTEM'
have a 'FUNCTION-NUMBER' and a 'FUNCTION-VERSION' specified
(&00): subsystem name

## ESM0303

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0303 DIFFERENT VERSIONS OF SUBSYSTEM '(&00)' MAY NOT BE CREATED AUTOMATICALLY

### Meaning

There are several versions declared (in old and new catalogs) with
CREATION-TIME during STARTUP, and /ADD-SUBSYSTEM was called with
TYPE=*NEW-SUBSYSTEMS
(&00): name and version number of the subsystem

## ESM0304

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0304 SUBSYSTEM '(&00)' WITH 'CREATIO-TIME=*BEFORE-SYSTEM-READY'HAS LINK RELATION TO '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE/AT-DSSM-LOAD', '*MANDATORY-AT-STARTUP' OR '*BEFORE-SYSTEM-READY'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0305

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0305 OPERAND ERROR: '(&00)' WITH 'CREATION-TIME=*AFTER-SYSTEM-READY' HAS LINK RELATION TO '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE/AT-DSSM-LOAD', '*BEFORE/AFTER-SYSTEM-READY' OR '*MANDARORY-AT-STARTUP'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0306

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0306 OPERAND ERROR: '(&00)' WITH 'CREATION-TIME=*BEFORE-DSSM-LOAD' HAS RELATION TO '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE-DSSM-LOAD'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0307

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0307 OPERAND ERROR: '(&00)' WITH 'CREATION-TIME=*AT-DSSM-LOAD' HAS RELATION TO '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE-DSSM-LOAD' OR '*AT-DSSM-LOAD'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0308

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0308 OPERAND ERROR: '(&00)' WITH 'STOP-AT-SHUTDOWN=*NO' HAS RELATION TO '(&01)' WITH 'STOP-AT-SHUTDOWN=*YES'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0309

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0309 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-ACCESS=*SYSTEM' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'SUBSYSTEM-ACCESS=*HIGH OR *LOW'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0310

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0310 OPERAND ERROR: SUBSYSTEM '(&00)' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-PRIVILEGED'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0311

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0311 OPERAND ERROR: SUBSYSTEM '(&00)' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0312

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0312 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*MANDATORY-AT-STARTUP' HAS RELATION TO SUBSYSTEM '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE- OR *AT-DSSM-LOAD' OR '*MANDATORY-AT-STARTUP'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0313

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0313 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*SYSTEM-GLOBAL' DEPENDS ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-PRIVILEGED'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0314

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0314 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*SYSTEM-GLOBAL' DEPENDS ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0315

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0315 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-ACCESS=*SYSTEM' DEPENDS ON SUBSYSTEM '(&01)' WITH 'SUBSYSTEM-ACCESS=*HIGH OR *LOW'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0316

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0316 SAME SVC- OR SYSTEM-EXIT-NUMBER IN DIFFERENT SUBSYSTEMS: '(&00)' - '(&01)' NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0317

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0317 SAME COMBINATION 'SVC-NUMBER, FUNCTION-NUMBER ANDFUNCTION-VERSION' IN DIFFERENT SUBSYSTEMS: '(&00)' - '(&01)' NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0318

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0318 SAME COMBINATION 'SVC-NUMBER, FUNCTION-NUMBER AND FUNCTION-VERSION' IN SUBSYSTEMS: '(&00)' - '(&01)' WITH 'VERSION-COEXISTENCE=*ALLOWED' OR 'VERSION-EXCHANGE=*ALLOWED' NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0319

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0319 FOR ISL ENTRY, SAME COMBINATION 'FUNCTION-NUMBER AND AND FUNCTION-VERSION' IN SUBSYSTEMS: '(&00)' - '(&01)' NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0320

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0320 FOR ISL ENTRY, SAME COMBINATION 'FUNCTION-NUMBER AND FUNCTION-VERSION' IN SUBSYSTEMS: '(&00)' - '(&01)' WITH 'VERSION-COEXISTENCE=*ALLOWED' OR 'VERSION-EXCHANGE=*ALLOWED' NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0321

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0321 OPERAND ERROR: OPERANDS 'SIZE' AND 'START-ADDRESS' OF SUBSYSTEMS: '(&00)' AND '(&01)' ARE NOT PROCESSABLE

### Meaning

The subsystems (&00) and (&01) overlap each other because of the
specified operands SIZE and START-ADDRESS
One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0322

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0322 NUMBER OF DEFINED RELATIONS IN CATALOG '(&00)' EXCEEDS LIMIT

### Meaning

Maximum is 4096 relations (dependence or link) including present
relations
(&00): specified catalog name

## ESM0323

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0323 STANDARD VERSION OF SUBSYSTEM '(&00)' CANNOT BE CHANGED BY /ADD-SUBSYSTEM COMMAND

### Meaning

(&00): name and version number of the subsystem

## ESM0324

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0324 SOME WARNINGS WERE WRITTEN TO SYSLST

### Meaning

At least one of the subsystems cannot be automatically created because
of the specified CREATION-TIME

## ESM0325

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0325 ERROR DURING '(&00)' COMMAND. MORE PRECISE MESSAGE ON SYSLST

### Meaning

(&00): command name

## ESM0326

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0326 COMMAND '(&00)' ABNORMALLY TERMINATED

### Meaning

(&00): name of command

## ESM0327

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0327 SYSTEM ERROR: ERROR DURING TRANSFER TO DSSM BOURSE. BOURSE RETURN CODE: '(&00)'

### Meaning

A SERSLOG entry with RECTYPE=ESMERR and TITLE ESMBSTC has been written
(&00): hexadecimal value of bourse function return code
DSSM: Dynamic Subsystem Management

## ESM0328

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0328 IMPOSSIBLE TO CREATE DSSM COMMISSION LIST DURING STARTUP

### Meaning

DSSM cannot run. STARTUP will be informed
DSSM: Dynamic Subsystem Management

## ESM0329

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0329 SAME SVC NUMBER ONCE WITH AND ONCE WITHOUT 'F-NUM F-VERS' NOT ALLOWED IN SUBSYSTEM ENTRIES '(&00)' AND '(&01)'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0330

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0330 NEW CATALOG CONTAINS OLD SUBSYSTEM '(&00)' WHICH IS NOT ACCEPTED BY /ADD-SUBSYSTEM WITH 'TYPE=*NEW-SUBSYSTEMS'

### Meaning

(&00): name and version number of the subsystem

## ESM0331

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0331 SUBSYSTEM '(&00)' IN THE NEW CATALOG WAS DECLARED '*LOCAL-PRIVILEGED' WHICH IS NOT ACCEPTED BY /ADD-SUBSYSTEM WITH 'TYPE=*NEW-SUBSYSTEMS'

### Meaning

(&00): name and version number of the subsystem

## ESM0332

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0332 VERSION OF CATALOG '(&00)' IS INCOMPATIBLE WITH CURRENT DSSM VERSION

### Meaning

This catalog version is not supported by the current DSSM version
(&00): specified catalog name
DSSM: Dynamic Subsystem Management

## ESM0333

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0333 OPERAND ERROR: 'TSN' AND 'VERSION-COEXISTENCE=*ALLOWED' OR 'VERSION-EXCHANGE=*ALLOWED' IS NOT ALLOWED FOR 'WORK-TASK' SUBSYSTEM '(&00)'

### Meaning

The TSN operand was given in the new/old catalog and the subsystem was
declared in the old/new catalog and /ADD-SUBSYSTEM was called with
TYPE=*NEW-SUBSYSTEMS
(&00): name and version number of the subsystem

## ESM0334

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0334 /ADD-SUBSYSTEM COMMAND SUCCESSFULLY PROCESSED BUT THERE WAS A REQUEST MEMORY FAILURE DURING THE BUILDING OF THE HISTORIC ARRAY OF ADDED CATALOGS

### Meaning

The subsystem configuration is correct but the historic array of added
catalogs returned by the /SHOW-SUBSYSTEM-INFO command will be meaningless
due to a request memory problem

## ESM0335

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0335 SAME ISL ENTRY ONCE WITH AND ONCE WITHOUT 'F-NUM F-VERS' NOT ALLOWED IN SUBSYSTEM ENTRIES '(&00)' AND '(&01)'

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): subsystem name, subsystem version number and entry name

## ESM0336

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0336 SAME ISL ENTRY WITHOUT 'F-NUM F-VERS' IN SUBSYSTEMS '(&00)' AND '(&01)' IS NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog and
/ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem

## ESM0337

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0337 SUBSYSTEM '(&00)' HAS LINK RELATION TO SUBSYSTEM '(&01)'. TWO VERSIONS '(&02)' WITH 'VERSION-COEXISTENCE=*ALLOWED' OR 'VERSION-EXCHANGE=*ALLOWED' ARE NOT ALLOWED

### Meaning

One subsystem is declared in the old, one in the new catalog
and /ADD-SUBSYSTEM was called with TYPE=*NEW-SUBSYSTEMS
(&00),(&01): name and version number of the subsystem
(&02): subsystem version numbers

## ESM0338

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0338 SUBSYSTEM '(&00)' HAS REJECTED THE DELETE ORDER

### Meaning

The CLOSE-CTRL routine of the subsystem has returned a negative returncode
(&00): name and version number of the subsystem

## ESM0339

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0339 NO SYNCHRONOUS SERVICE ALLOWED FOR SUBSYSTEM '(&00)' BECAUSE TASK IS CONNECTED TO IT

### Meaning

(&00): name and version number of the subsystem

## ESM0340

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0340 RESERVATED ADDRESS-SPACE EXHAUSTED FOR SUBSYSTEMS WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

There is not enough free space in the address space strip for
the private slices of subsystems

## ESM0341

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0341 NO LOCAL SUBSYSTEM CATALOG LOADED

### Meaning

Either a local catalog has been loaded but already unloaded or no local
catalog has been loaded

## ESM0342

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0342 LOCAL SUBSYSTEM CATALOG '(&00)' CONTAINS PRIVILEGED SUBSYSTEM '(&01)'

### Meaning

(&00): name of local catalog
(&01): name and version number of the subsystem

## ESM0343

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0343 CATALOG '(&00)' CONTAINS SUBSYSTEMS WITH 'MEMORY-CLASS=*BY-SLICE' WHICH IS NOT ACCEPTED BY /ADD-SUBSYSTEM WITH 'TYPE=*EXTENDED-ACTIVE-CONFIGURATION'

### Meaning

(&00): specified file name

### Response

Retry with /ADD-SUBSYSTEM TYPE=*NEW-SUBSYSTEMS

## ESM0344

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0344 A LOCAL SUBSYSTEM CATALOG IS ALREADY LOADED

### Meaning

First unload previously loaded local subsystem catalog and retry loading
of the new one

## ESM0345

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0345 SIZE ADJUSTMENT FOR SUBSYSTEM WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

An odd value of parameter size for a subsystem with
'MEMORY-CLASS=*BY-SLICE' has been made even
by increase therefore address space has been recomputed.
The SPARC processor has a physical page size of 8KB,
so the size parameter for subsystems with
'MEMORY-CLASS=*BY-SLICE' on SX servers must be an even
number of 4KB pages. However, as an odd number of pages
was defined, DSSM has increased the defined value by 1.

## ESM0346

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0346 DELETE OF SUBSYSTEM '(&00)' INTERRUPTED BECAUSE CREATION OF THE NEW VERSION '(&01)' IS NOT POSSIBLE

### Meaning

(&00): name and version number of the subsystem
(&01): subsystem version number
No connection interruption is permitted during an exchange of this
subsystem

## ESM0347

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0347 ENTRY '(&00)' OF SUBSYSTEM '(&01)' LOADED AT ADDRESS '(&02)'. USER COMMENT: '(&03)'

### Meaning

the display of subsystem addresses has been requested via a break point
(&00): name and type of entry
(&01): subsystem name and version
(&02): loading address of the entry
(&03): user defined comment

## ESM0348

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0348 THE HOLDER TASK OF SUBSYSTEM '(&00)' IS STOPPED. CONTINUE? REPLY (C=CONTINUE, R=REPEAT, EOT=C)

### Meaning

the display of subsystem addresses has been requested via a break point
the previous message(s) gives the asked addresses
(&00): subsystem name and version

### Response

CONTINUE: continue and call the subsystem routines
REPEAT: repeat the message(s) with addresses

## ESM0349

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0349 COMMAND '(&00)' FORBIDDEN WHILE A PROGRAM IS LOADED

### Meaning

(&00): Command name

## ESM0350

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0350 INTERNAL DSSM PROBLEM DURING COMMAND PROCESSING

### Meaning

During processing of the requested function, internal problem causes
abnormal termination of the DSSM task

### Response

Recovery of the DSSM task is started. Try the command again

## ESM0351

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0351 TSN '(&00)' FOR SUBSYSTEM '(&01)' ALREADY USED

### Meaning

Possible reason :
- TSN has been used by another user
- Task is locked in its termination processing
e.g. task wait acknowledge at console
(&00): TSN of task to be created for subsystem
(&01): name and version number of the subsystem

## ESM0352

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0352 TASK '(&00)' MAY NOT BE CREATED FOR SUBSYSTEM '(&01)'

### Meaning

The task could not be created due to system error
or resource bottleneck
(&00): TSN of the task
(&01): name and version number of the subsystem

## ESM0353

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0353 NO DSSM RECOVERY POSSIBLE : CATALOG NO MORE AVAILABLE

## ESM0354

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0354 TOO MUCH DSSM RECOVERIES

### Meaning

Only two successive DSSM recoveries are tried

## ESM0355

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0355 STARTUP CONTINUES WITHOUT CREATION OF THE SUBSYSTEMS DECLARED WITH CREATION-TIME='(&00)'

### Meaning

(&00): *BEFORE-SYSTEM-READY/*AFTER-SYSTEM-READY
due to DSSM task crash, STARTUP continues even if one class of
automatically created subsystems is not present

## ESM0356

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0356 PROBLEM WHEN STARTING DSSM RECOVERY

### Meaning

Impossible to initialize DSSM recovery processing

## ESM0357

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0357 COEXISTENCE NOT ALLOWED FOR LOCAL SUBSYSTEM

### Meaning

Another version of the local subsystem is already started.
To start the requested version, stop first the local version already
started

## ESM0358

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0358 LOCAL '(&00)' OF MESSAGE FILE '(&01)' NOT POSSIBLE

### Meaning

(&00) : function that fails activation or deactivation
(&01) : message file name

## ESM0359

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0359 SYSTEM ERROR DURING LOCAL CATALOG MANAGEMENT

### Meaning

A system error has been detected by local catalog management.
Possible reasons are : access to ETCBDSSM or EXVTDSSM failed or it is
impossible to create a DSMUSE for the task.

## ESM0360

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0360 SYSTEM ERROR DURING ACCESS TO XVT OR TCB TABLES

### Meaning

Possible reasons are : access to ETCBDSSM or EXVTDSSM failed or it is
impossible to create a DSMUSE for the task.

## ESM0361

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0361 SYSTEM ERROR DURING ACCESS OF '(&00)' TABLE FOR SUBSYSTEM '(&01)'

### Meaning

(&00): name of the table
(&01): name and version number of the subsystem

## ESM0362

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0362 /SHOW-SUBSYSTEM-ATTRIBUTES COMMAND NOT PERFORMED. TRY AGAIN LATER

### Meaning

This error is due to a lake of memory in class 4 or 5

## ESM0363

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0363 COMMAND REJECTED DUE TO MONJV PROCESSING ERROR

### Meaning

An error has occurred during MONJV processing, see conslog for more detail

## ESM0364

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0364 WARNING: MONJV MACRO ERROR '(&00)' ON JV '(&02)'. IN SYSTEM MODE: /HELP-MSG JVS(&01)

### Meaning

An access to the MONJV '(&02)' was not successful
&00: MONJV macro return code
01: MONJV not accessible
02: MONJV in use
03: the JV specified is no MONJV
04: MONJV can not be created
06: MONJV name is invalid
07: MONJV has been opened already by "Job Acceptance"
but is not yet linked to a task
09: the link name *SMONJVP cannot be assigned to the MONJV
Consult message JVS(&01)

## ESM0400

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0400 'CREATE' OR 'RESUME' SUBSYSTEM '(&00)' WITH 'SYNCHRONOUS=(&01)' AND 'RESET=(&02)'

### Meaning

(&00): name and version number of the subsystem
(&01),(&02): *YES or *NO

## ESM0401

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0401 INITIALIZATION OF DSSM ABORTED. NO SUBSYSTEM AVAILABLE IN THIS SESSION

### Meaning

The preceding message gives the reason of the error
DSSM: Dynamic Subsystem Management

### Response

Contact the system administrator

## ESM0402

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0402 'CREATE' OR 'RESUME' SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-PARAMETER=(&01)'

### Meaning

(&00): name and version number of the subsystem
(&01): string specified in the command (first part)

## ESM0403

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0403 DMS ERROR '(&01)': SUBSYSTEM CATALOG '(&00)' DOES NOT EXIST. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The SPL interface returned an error
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'
(&00): name of file containing the subsystem catalog
(&01): DMS error code

## ESM0404

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0404 NO CL4 MEMORY AVAILABLE

### Response

A SERSLOG entry is written

## ESM0405

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

ESM0405 ERROR WHEN LOADING REMAINING DSSM CODING

### Meaning

DSSM: Dynamic Subsystem Management

## ESM0406

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0406 NO BOURSE FOR REPLY TO DSSM COMMISSIONS AVAILABLE; BOURSE RETURN CODE: '(&00)'

### Meaning

The commissions to the DSSM task are processed via the DSSM bourse and a
reply bourse
A SERSLOG entry is written
(&00): hexadecimal value of bourse function return code
DSSM: Dynamic Subsystem Management

## ESM0407

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0407 THE DSSM TASK CANNOT BE CREATED OR STARTED

### Meaning

DSSM: Dynamic Subsystem Management

## ESM0408

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0408 DSSM VERSION '(&00)' INITIATED SUCCESSFULLY; CATALOG '(&01)' USED

### Meaning

(&00): version number with format nn.n
(&01): catalog name
DSSM: Dynamic Subsystem Management

## ESM0409

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0409 DSSM NOT INITIATED

### Meaning

DSSM: Dynamic Subsystem Management

## ESM0410

Destination: CONSOLE Routing code: @ (conslog) Weight: 70

Warranty : NO

ESM0410 SUBSYSTEM '(&00)' IS UNLOCKED

### Meaning

(&00): name and version number of the subsystem

## ESM0412

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0412 DSSM INTERNAL ERROR DURING SHUTDOWN. DSSM SHUTDOWN NOT PROCESSED

### Meaning

DSSM: Dynamic Subsystem Management

## ESM0413

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0413 ERROR WHEN CALLING A BOURSE FUNCTION. BOURSE RETURN CODE '(&00)'

### Meaning

A SERSLOG entry is written
(&00): Value of the bourse function return code

## ESM0414

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0414 SYNTAX ERROR IN VERSION FORMAT

## ESM0415

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0415 SYNTAX ERROR IN INSTALLATION-UNIT FORMAT

## ESM0416

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0416 WRONG DSSM STARTUP OPERAND '(&00)'. OPERAND REJECTED

### Meaning

Operand (&00) will not be processed

## ESM0417

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0417 TASK CANNOT BE CONNECTED TO SUBSYSTEMS WITH 'MEMORY-CLASS=(&00)'

### Meaning

Either the reservation of address space strip failed
at task creation, or the task has been created before
the creation of the address space strip for *BY-SLICE
, or the command RELEASE-SUBSYSTEM-SPACE MEMORY-TYPE=*ALL
or MEMORY-TYPE=*BY-SLICE has been given
(&00): *LOCAL-PRIVILEGED or *BY-SLICE

### Response

Start a new task to access to *BY-SLICE subsystems

## ESM0418

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0418 ADDRESS SPACE STRIP TOO LARGE FOR THIS SESSION

### Meaning

In this session DSSM tries to load the subsystems into CL4 memory

### Response

Correct the faulty catalog

## ESM0419

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ESM0419 DSSM NOT AVAILABLE. DSSM TASK DESTROYED

### Meaning

The DSSM task has been destroyed during the startup phase of DSSM
DSSM: Dynamic Subsystem Management

## ESM0420

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0420 ACCESS TO CENTRAL TABLES FAILED

### Meaning

Decoupling access to XVT or TCB not processed

## ESM0421

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0421 ACCESS ERROR TO CATALOG FILE '(&00)'. DMS RETURN CODE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The SPL interface returned an error
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'
(&00): specified catalog file
(&01): DMS error code

## ESM0422

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0422 FORMAT ERROR IN CATALOG FILE '(&00)'

### Meaning

Either an invalid catalog version or an incompatible type of installation
was specified
(&00): specified catalog file

## ESM0423

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0423 MEMORY MANAGEMENT ERROR DURING COMMAND PROCESSING

### Meaning

Memory management cannot process unreserved request

## ESM0424

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0424 DSSM INTERNAL ERROR DURING COMMAND PROCESSING

### Meaning

DSSM cannot access system anchor or task anchor

### Response

Contact the system administrator

## ESM0425

Destination: CONSOLE Routing code: @ (conslog) Weight: 70

Warranty : NO

ESM0425 'DELETE' OR 'HOLD' SUBSYSTEM '(&00)' WITH 'FORCED=*YES'

### Meaning

(&00): name and version number of the subsystem

## ESM0426

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0426 ADDRESS OF RESERVED CL5 MEMORY AREA FOR PRIVILEGED SUBSYSTEMS IS '(&00)'

### Meaning

(&00): address of the specified memory area

## ESM0427

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0427 ADDRESS OF RESERVED CL5 MEMORY AREA FOR NON-PRIVILEGED SUBSYSTEMS IS '(&00)'

### Meaning

(&00): address of the specified memory area

## ESM0428

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0428 'CREATE' OR 'RESUME' OF SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-PARAMETER=(&01)' (CONTINUED)

### Meaning

(&00): name and version number of the subsystem
(&01): string specified in the command (second part if any)

## ESM0429

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0429 SUBSYSTEMS WITH 'MEMORY-CLASS=*BY-SLICE' NOT AVAILABLE ON THIS BS2000 VERSION

### Meaning

In the catalog, there are subsystems declared with the
attribute 'MEMORY-CLASS=*BY-SLICE', that can only
be loaded on and after BS2000/OSD-BC V3

### Response

To use these subsystems, modify their 'MEMORY-CLASS' with the
command /MODIFY-SUBSYSTEM-PARAMETER

## ESM0430

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0430 SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*BY-SLICE' NOT AVAILABLE ON THIS BS2000 VERSION

### Meaning

The subsystem is declared with the attribute
'MEMORY-CLASS=*BY-SLICE' and can only
be loaded on and after BS2000/OSD-BC V3
(&00): name and version number of the subsystem

### Response

To use this subsystem, you must modify its 'MEMORY-CLASS'
with the command /MODIFY-SUBSYSTEM-PARAMETER

## ESM0431

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0431 PRIVILEGE ERROR: COMMAND NOT ALLOWED FOR CALLER

## ESM0432

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0432 ERROR DURING LOGGING FILE ACTIVATION BY CLTF

### Meaning

Possible CLTF message in console logging

## ESM0433

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0433 SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*BY-SLICE' NOT AVAILABLE

### Meaning

The subsystem can not be loaded due to a previous
reservation error during the DSSM startup phase
(&00): name and version number of the subsystem

## ESM0434

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0434 ECMF ERROR FOR SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

The subsystem is not available due to an error
of the ECMF function
A SERSLOG entry is written
ECMF: Extended Cross Memory Facility
(&00): name and version number of the subsystem

## ESM0435

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0435 ADDRESS OF RESERVED CL5 MEMORY AREA FOR SUBSYSTEMS WITH 'MEMORY-CLASS=*BY-SLICE' IS '(&00)'

### Meaning

(&00): address of the specified memory area

## ESM0436

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0436 SUBSYSTEMS WITH "BY-PROGRAM" DEFINED ENTRIES ARE ONLY POSSIBLE FROM BLSSERV V2.1A

### Meaning

Bad version of subsystem BLSSERV has been started or subsystem BLSSERV is
not present.

## ESM0440

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0440 SUBSYSTEM WITH MEMORY-CLASS=*BY-SLICE CANNOT BE REMOVED

### Meaning

subsystem with memory-class=*by-slice cannot be removed

## ESM0500

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0500 '(&00)' COPYRIGHT (C)'(&01)' FUJITSU TECHNOLOGY SOLUTIONS GMBH. ALL RIGHTS RESERVED

### Meaning

(&00): name and version number of the subsystem
(&01): copyright year

## ESM0501

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0501 '(&00)' COPYRIGHT (C) '(&02)',(&01). ALL RIGHTS RESERVED

### Meaning

(&00): name and version number of the subsystem
(&01): copyright text given by subsystem administrator
(&02): copyright year

## ESM0504

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0504 CONNECTION TO SUBSYSTEM '(&00)' NOT POSSIBLE BECAUSE TASK IS ALREADY CONNECTED TO SUBSYSTEM '(&01)'

### Meaning

The two subsystems must have separate address spaces at catalog
generation time
(&00): subsystem name and version number to which the task is trying
to connect
(&01): subsystem name and version number to which the task is
already connected

## ESM0600

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0600 SINGLE VERSION '(&00)' NOT ALLOWED WITH SUBSYSTEM NAME VALUE EQUAL TO '*ALL'

### Meaning

(&00): subsystem version

## ESM0601

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0601 SUBSYSTEM NOT FOUND. FUNCTION TERMINATED

### Meaning

Either the subsystem does not exist in the configuration
Or the caller has not enough privilege to obtain the information

## ESM0602

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0602 SYSTEM (REQM) ERROR. FUNCTION TERMINATED ABNORMALLY

## ESM0603

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0603 VERSION '(&00)' NOT ALLOWED WITH SUBSYSTEM NAME SPECIFIED WITH WILDCARD

### Meaning

(&00): subsystem version

## ESM0604

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0604 VERSION '(&00)' NOT ALLOWED WITH SUBSYSTEM NAME EQUAL TO '*NON-PRIVILEGED-CLASS-5'

### Meaning

(&00): subsystem version

## ESM0605

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0605 SUBSYSTEM '(&00)' LOCKED DUE TO ERROR

### Meaning

Subsystem (&00) is locked due to a previous error during function CREATE
or
DELETE or RESUME or HOLD
(&00): name and version number of the subsystem

## ESM0606

Destination: CONSOLE Routing code: * (main console) Weight: 90

Warranty : NO

ESM0606 SYSTEM ERROR WHEN SETTING TSOS PRIVILEGE

## ESM0607

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0607 VERSION '(&00)' NOT ALLOWED WITH SUBSYSTEM NAME EQUAL TO '*ALL-CLASS-5'

### Meaning

(&00): subsystem version

## ESM0608

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0608 SUBSYSTEM VERSION NOT FOUND. FUNCTION ABORTED

## ESM0609

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

ESM0609 WARNING: TASK DISCONNECTED FROM ENTRY '(&00)' IN SUBSYSTEM '(&01)' BY ADMINISTRATOR

### Meaning

(&00): call entry name
(&01): subsystem name

## ESM0610

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

ESM0610 NO SUBSYSTEM FOR OPERAND VALUE '(&00)'

### Meaning

(&00): *NON-PRIVILEGED-CLASS-5 / *ALL-CLASS-5

## ESM0611

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0611 NO CONNECTION TABLE FOR THIS TASK

### Meaning

The pointer to the table of connections for this task has not been
initialized

## ESM0612

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0612 LOADING OF SUBSYSTEM '(&00)' NOT PERFORMED: MANDATORY REP FILE '(&01)' IS MISSING OR INVALID

### Meaning

(&00): name and version number of the subsystem
(&01): REP file name

## ESM0613

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0613 CHANGE OF MEMORY-CLASS OR SYNTAX FILE OR INSTALLATION-USERID THAT INVOLVES A SYNTAX FILE MODIFICATION IS NOT PERMITTED FOR SUBSYSTEM '(&00)'.

### Meaning

(&00): name and version number of the subsystem
This subsystem must be deleted by /STOP-SUBSYSTEM command

## ESM0614

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0614 NON-PRIVILEGED SUBSYSTEM '(&00)' CANNOT DECLARE A SYNTAX FILE: 'CONNECTION-SCOPE=*PROGRAM' MISSING IN ENTRY '(&01)'

### Meaning

(&00): name and version number of the subsystem
(&01): entry name

## ESM0615

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

ESM0615 SUBSYSTEM '(&00)' WITH 'LIBRARY=*CPLINK' CANNOT DECLARE A REP FILE

### Meaning

(&00): name and version number of the subsystem

## ESM0616

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0616 WARNING: 'CLOSE-CTRL-ROUTINE', 'STOPCOM-ROUTINE' AND 'DEINIT-ROUTINE' NOT DEFINED, VALUE '*NO' IS ASSUMED FOR 'STOP-AT-SHUTDOWN' OPERAND

## ESM0617

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0617 SUBSYSTEM '(&00)' HAS CHANGED 'MEMORY-CLASS'. ALL MEMORY PARAMETERS MUST BE SPECIFIED

## ESM0618

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0618 SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*BEFORE-DSSM-LOAD' AND 'LIBRARY=*CPLINK' MUST MODIFY 'LIBRARY' WHEN 'CREATION-TIME' IS MODIFIED

## ESM0619

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0619 SUBSYSTEM '(&00)' CANNOT BECOME A WORK TASK SUBSYSTEM

### Meaning

subsystem is not WORK TASK and has defined an init-routine, and a
close-ctrl-, stopcom- or deinit-routine *DYNAMIC
(&00): name and version number of the subsystem

## ESM0620

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0620 SUBSYSTEM '(&00)' MUST KEEP THE CHARACTERISTICS OF A WORK TASK SUBSYSTEM

### Meaning

subsystem is WORK TASK, it must define an init-routine entry, and a
dynamic close-ctrl-, stopcom- or deinit-routine
(&00): name and version number of the subsystem

## ESM0621

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0621 NONPRIVILEGED SUBSYSTEM '(&00)' MAY NOT DEFINE 'INIT-ROUTINE' NOR 'CLOSE-CTRL-ROUTINE' NOR 'STOPCOM-ROUTINE' NOR 'DEINIT-ROUTINE'

## ESM0622

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0622 'CLOSE-CTRL-ROUTINE' AND/OR 'STOPCOM-ROUTINE' AND/OR 'DEINIT-ROUTINE' SPECIFIED AS '*DYNAMIC' AND NO 'INIT-ROUTINE' DEFINED IN SUBSYSTEM '(&00)'

## ESM0623

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0623 'INTERFACE-VERSION' MUST BE GIVEN IN SUBSYSTEM '(&00)': 'INIT-ROUTINE' AND/OR 'CLOSE-CTRL-ROUTINE' AND/OR 'STOPCOM-ROUTINE' AND/OR 'DEINIT-ROUTINE' DECLARED

## ESM0624

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0624 SUBSYSTEM '(&00)' WITH 'STOP-AT-SHUTDOWN=*NO' HAS REFERENCE TO SUBSYSTEM '(&01)' WITH 'STOP-AT-SHUTDOWN=*YES'

### Meaning

(&00), (&01): name and version number of the subsystem

## ESM0625

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0625 INCONSISTENCY BETWEEN OPERANDS 'FORCED-STATE-CHANGE' AND 'SUBSYSTEM-HOLD' IN SUBSYSTEM '(&00)'

### Meaning

FORCED-STATE-CHANGE=*ALLOWED cannot be used with SUBSYSTEM-HOLD=*FORBIDDEN
(&00): name and version number of the subsystem

## ESM0626

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0626 INCONSISTENCY BETWEEN 'RESET' AND 'SUBSYSTEM-HOLD' OPERANDS IN SUBSYSTEM '(&00)'

### Meaning

RESET=*ALLOWED cannot be used with SUBSYSTEM-HOLD=*FORBIDDEN
(&00): name and version number of the subsystem

## ESM0627

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0627 INCONSISTENCY BETWEEN OPERANDS 'RESTART-REQUIRED' AND 'INIT-ROUTINE' IN SUBSYSTEM '(&00)'

### Meaning

An INIT-ROUTINE must be declared if RESTART-REQUIRED=*YES
(&00): name and version number of the subsystem

## ESM0628

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0628 SUBSYSTEM '(&00)' HAS ENTRY MODE SYSTEM-EXIT, CANNOT DECLARE 'VERSION-COEXISTENCE=*ALLOWED'

### Meaning

(&00): name and version number of the subsystem

## ESM0630

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0630 SAME ISL ENTRY OR SAME SVC NUMBER WITH SAME 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN SUBSYSTEMS: '(&00)' - '(&01)' WITH 'VERSION-COEXISTENCE' IS NOT ALLOWED

### Meaning

(&00): ,(&01)name and version number of the subsystem

## ESM0631

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0631 SAME 'TSN' AND 'VERSION-COEXISTENCE/-EXCHANGE=*ALLOWED' NOT ALLOWED FOR WORK TASK SUBSYSTEMS '(&00)' AND '(&01)'

### Meaning

(&00): ,(&01)name and version number of the subsystem

## ESM0632

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0632 OPERAND ERROR: ONLY ONE VERSION OF SUBSYSTEM '(&01)' CAN BE RELATED BY SUBSYSTEM '(&00)' IF ONE OF THE VERSIONS BECOME 'VERSION-EXCHANGE/-COEXISTENCE=*ALLOWED'

### Meaning

(&00): ,(&01)name and version number of the subsystem

## ESM0633

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0633 PRIVILEGED SUBSYSTEM '(&00)' CANNOT BECOME NON-PRIVILEGED

### Meaning

(&00): name and version number of the subsystem

## ESM0634

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0634 SUBSYSTEM '(&00)' CANNOT HAVE LINK RELATION TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

(&00),(&01): name and version number of the subsystem

## ESM0635

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0635 SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*SYSTEM-GLOBAL' CANNOT DEPEND ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-PRIVILEGED' OR 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

(&00),(&01): name and version number of the subsystem

## ESM0636

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0636 'START-ADDRESS' MUST BE A MULTIPLE OF X'100000' IN SUBSYSTEM '(&00)'

### Meaning

(&00): name and version number of the subsystem

## ESM0637

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0637 FOR 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED' OPERAND 'SIZE' AND 'START-ADDRESS' OF SUBSYSTEM '(&00)' AND SUBSYSTEM '(&01)' NOT PROCESSABLE

### Meaning

The subsystems (&00) and (&01) overlap each other in the same holdertask
because of the specified operands SIZE and START-ADDRESS
(&00),(&01): name and version number of the subsystem

## ESM0638

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0638 ENTRY '(&00)' 'CONNECTION-ACCESS=*SYSTEM' MAY NOT BE USED IN SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

(&00): name of the entry
(&01): name and version number of the subsystem

## ESM0639

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0639 ENTRY '(&00)': ONLY 'CONNECTION-SCOPE=*PROGRAM' MAY BE USED WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED' IN SUBSYSTEM '(&01)'

### Meaning

(&00): name of the entry
(&01): name and version number of the subsystem

## ESM0640

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0640 SUBSYSTEM '(&00)' DECLARED WITH 'CREATION-TIME=*BEFORE-DSSM-LOAD' MAY NOT HAVE A MESSAGE FILE

### Meaning

(&00): name and version number of the subsystem

## ESM0641

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0641 SUBSYSTEM '(&00)' DECLARED WITH 'CREATION-TIME=*BEFORE-DSSM-LOAD' OR 'CREATION-TIME=*AT-DSSM-LOAD' MAY NOT HAVE A SYNTAX FILE

### Meaning

(&00): name and version number of the subsystem

## ESM0642

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

ESM0642 FUNCTION REMOVE TERMINATED ABNORMALLY

### Meaning

The preceding message gives the reason of the error

## ESM0643

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0643 INTERNAL ERROR OCCURRED DURING 'SAVE' PROCESSING

### Meaning

An internal error occurs during the backup processing; It may be an
abnormal termination, a bad pointer initialization or an empty catalog

### Response

Collect relevant information (sled and serslog) and send it to Software
Maintenance

## ESM0644

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0644 CATALOG CONTAINS CHECK INCONSISTENCIES

### Meaning

During the CHECK-CATALOG processing, DSSM has met some inconsistencies.
It can be relations inconsistencies or cycle for example

## ESM0645

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0645 FILE '(&00)' ALREADY CATALOGED

### Meaning

(&00): Name of the catalog to save

### Response

Change the name of the result catalog or erase the file and enter the same
/SAVE-SUBSYSTEM-CATALOG command

## ESM0646

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0646 ERROR OCCURRED DURING '(&00)' FUNCTION PROCESSING

### Meaning

An error occurs during the removal processing; It may be a problem during
access to preroutines or call entries tables or during standard version
recomputing
An error occurs during the modification processing; It may be a problem
during standard version recomputing
(&00): REMOVE or UPDATE function

### Response

Collect relevant information (sled and serslog) and send it to Software
Maintenance

## ESM0647

Destination: CONSOLE Routing code: @ (conslog) Weight: 50

Warranty : NO

ESM0647 '(&00)' FOR SUBSYSTEM '(&01)' MODIFIED. NEW VALUE : '(&02)'

### Meaning

(&00): Subsystem attribute
(&01): Subsystem name and version number
(&02): Subsystem attribute value

## ESM0648

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0648 ERROR OCCURRED DURING SAVE PROCESSING

### Meaning

At least an error occurs during save processing

### Response

The preceding messages will help you to find the reason and to solve the
problem. Correct and retry

## ESM0649

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0649 SUBSYSTEM '(&00)' DECLARED WITH CREATION-TIME=*BEFORE-DSSM-LOAD MUST HAVE A DYNAMIC-CHECK-ENTRY

### Meaning

(&00): Subsystem name and version number

### Response

Declare a DYNAMIC-CHECK-ENTRY

## ESM0650

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0650 SUBSYSTEM '(&00)' WITH 'STOP-AT-SHUTDOWN=*YES' CANNOT BE REFERENCED BY SUBSYSTEM '(&01)' WITH 'STOP-AT-SHUTDOWN=*NO'

### Meaning

(&00): ,(&01)name and version number of the subsystem

## ESM0651

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0651 SUBSYSTEM '(&00)' WITH AN INIT-ROUTINE AND A CLOSE-CTRL-ROUTINE MUST HAVE A DEINIT-ROUTINE OF SAME TYPE AS THE CLOSE-CTRL-ROUTINE

### Meaning

(&00): name and version number of the subsystem

## ESM0653

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0653 INVALID ENTRY NAME '(&00)' IN SUBSYSTEM '(&01)'

### Meaning

(&00): ENTRY name
(&01): Subsystem name and version number

## ESM0654

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0654 DIFFERENT VERSIONS OF SUBSYSTEMS '(&00)' - '(&01)' WITH 'CREATION-TIME=*AT-SUBSYSTEM-CALL' AND 'VERSION-COEXISTENCE=*FORBIDDEN' NOT ALLOWED

### Meaning

(&00),(&01): Subsystem name and version number

## ESM0655

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0655 SUBSYSTEM '(&00)' HAS THE AUTOMATIC CREATION-TIME '(&01)' THAT IS DIFFERENT FROM THE SPECIFIED CREATION-TIME '(&02)'

### Meaning

(&00): Subsystem name and version number.
(&01),(&02): Subsystem Creation-time.

### Response

You can only specify the same creation-time as the other version.
Or you can give the creation-time '*AT-CREATION-REQUEST' to the other
version and retry your previous /MOD-SUBSYS-PAR command.

## ESM0656

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0656 VALUE '*AT-CREATION-REQUEST' IS ASSUMED AS 'CREATION-TIME' FOR SUBSYSTEM '(&00)'

### Meaning

(&00): Subsystem name and version number.

## ESM0657

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0657 INCONSISTENCY IN LOGICAL-ID FOR SUBSYSTEM '(&00)'

### Meaning

if a LOGICAL-ID is given for one subsystem file, a logical-id must exist
for each subsystem file.
(&00): Subsystem name and version number.

### Response

Correct the command and retry.

## ESM0658

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0658 NO FILE CORRESPONDING TO LOGICAL-ID '(&01)' FOR SUBSYSTEM '(&00)'

### Meaning

For the specified logical-id, no file can be found.
(&00): Subsystem name and version number.
(&01): LOGICAL-ID of the file.

## ESM0659

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0659 MESSAGE FILE '(&01)' CAN NOT BE DEACTIVATED FOR SUBSYSTEM '(&00)'

### Meaning

The message file can not be deactivated but, in case of message file
exchange, the new one has been successfully activated.
(&00): Subsystem name and version number.
(&01): Message file.

## ESM0660

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0660 NEW MESSAGE FILE '(&01)' CAN NOT BE ACTIVATED FOR SUBSYSTEM '(&00)'

### Meaning

The message file can not be activated but, in case of message file
exchange, the old one remains activated.
(&00): Subsystem name and version number.
(&01): New message file.

## ESM0661

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM0661 THE DSSM-ROSI INTERFACE ON SUBSYSTEM '(&00)' GIVES X'(&01)' AS RETURN CODE AND '(&02)' AS USED REPFILE

### Meaning

Diagnose message for $ESMURF processing
(&00): Subsystem name and version number
(&01): Return code
(&02): Used repfile

## ESM0662

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0662 NO VALUE PREVIOUSLY GIVEN FOR THE LOGICAL-ID OF '(&00)' FOR SUBSYSTEM '(&01)'

### Meaning

'*UNCHANGED' or '*REFRESH' can not be used if no value has been previously
given for the LOGICAL-ID.
(&00): Concerned subsystem file.
(&01): Subsystem name and version number

## ESM0663

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0663 NO VALUE PREVIOUSLY GIVEN FOR THE DEFAULT-NAME OF '(&00)' FOR SUBSYSTEM '(&01)'

### Meaning

'*UNCHANGED' can not be used if no value has been previously given for the
DEFAULT-NAME.
(&00): Concerned subsystem file.
(&01): Subsystem name and version number

## ESM0664

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0664 SUBSYSTEM '(&00)' INSTALLED WITH IMON MUST SPECIFY AN INSTALLATION-UNIT

### Meaning

(&00): name and version of the subsystem

## ESM0665

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0665 'DEFAULT-NAME' USED FOR FILES OF SUBSYSTEM '(&00)'

### Meaning

(&00): name and version of the subsystem

## ESM0666

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0666 SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*BY-SLICE' MUST BE DEFINED WITH 'SUBSYSTEM-LOAD-MODE=*ADVANCED'

### Meaning

(&00): name and version of the subsystem

## ESM0667

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0667 'MEMORY-CLASS=*BY-SLICE' MAY NOT BE USED FOR SUBSYSTEM '(&01)' WITH ENTRY '(&00)' WITH 'CONNECTION-ACCESS=*SYSTEM'

### Meaning

(&00): name of the entry
(&01): name and version number of the subsystem

## ESM0668

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0668 SUBSYSTEM '(&00)' CANNOT HAVE REFERENCE TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

(&00),(&01): name and version number of the subsystem

## ESM0669

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

ESM0669 SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-ACCESS=*SYSTEM' CANNOT DEPEND ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

(&00),(&01): name and version number of the subsystem

## ESM0670

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0670 PROBLEM OCCURRED DURING WRITING TO SYSLST. SYSFILE RETURN CODE = X'(&00)'

### Meaning

(&00): Hexadecimal value of the SYSFILE interface error byte

## ESM0671

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0671 PROBLEM OCCURRED DURING WRITING TO SYSOUT

## ESM0672

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

ESM0672 PROBLEM OCCURRED DURING OPS BUFFER FILLING

### Meaning

OPS: Output Presentation Service

## ESM0673

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0673 SPECIFIED '(&00)' MISSING FOR SUBSYSTEM '(&01)'. ENTER NEW VALUE OR TYPE TERMINATE (FN=FILENAME; TERMINATE; EOT=TERMINATE)

### Meaning

A subsystem file can not be found. Enter a new file name or type terminate
(&00): type of missing file
(&01): Subsystem name and version number

### Response

Enter response

## ESM0674

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0674 SPECIFIED '(&00)' MISSING FOR SUBSYSTEM '(&01)'. ENTER NEW VALUE, TYPE TERMINATE OR TYPE IGNORE(FN=FILENAME; TERMINATE; EOT=TERMINATE; IGNORE)

### Meaning

Subsystem information file can not be found. Enter new filename, type
ignore to continue startup or type terminate
(&00): type of missing file
(&01): Subsystem name and version number

### Response

Enter response

## ESM0675

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

ESM0675 A MANDATORY SUBSYSTEM COULD NOT BE STARTED. CONTINUE STARTUP PROCESSING? YES, NO ?(YES; NO; EOT=YES).

### Meaning

Mandatory subsystem (with creation-time *AT-DSSM-LOAD or
*MANDATORY-AT-STARTUP) can not be started.

## ESM0676

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0676 OPERAND ERROR: ENTRY '(&00)': ONLY 'MODE=*LINK' MAY BE USED WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

(&00): ENTRY name.

## ESM0677

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM0677 OPERAND ERROR: ENTRY '(&00)': ONLY 'CONNECTION-SCOPE=*TASK' OR 'CONNECTION-SCOPE=*PROGRAM' MAY BE USED WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

(&00): ENTRY name.

## ESM1000

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

ESM1000 WAIT TIME DEFINED FOR SHUTDOWN BOURSE ELAPSED

### Meaning

The shutdown processing of DSSM can not be terminated during wait on
shutdown bourse.
Wait time defined for machine C30-C50 is 900 seconds for other machine it
is 600 seconds

## ESM1012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1012 STATEMENT ABORTED ON USER REQUEST

## ESM1013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1013 CATALOG '(&00)' IS EMPTY

### Meaning

(&00): current catalog name.

## ESM1200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1200 CATALOG '(&00)' GENERATED

### Meaning

(&00): catalog name.

## ESM1206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1206 CATALOG INCONSISTENT

## ESM1209

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1209 CATALOG CONTAINS INCONSISTENT RELATIONS

## ESM1210

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1210 CATALOG '(&00)' GENERATED WITH FORCED='(&01)'

### Meaning

(&00): catalog name
(&01): operand value.

## ESM1617

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1617 OPERAND ERROR: SUBSYSTEM '(&00)' WITH SEVERAL REFERENCE RELATIONS TO SUBSYSTEM '(&01)' AND 'VERSION-EXCHANGE/-COEXISTENCE=*ALLOWED' NOT ALLOWED

### Meaning

(&00): name and version number of the subsystem
(&01): name of the subsystem.

## ESM1618

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1618 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*MANDATORY-AT-STARTUP' HAS RELATION TO SUBSYSTEM '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE-DSSM-LOAD/*AT-DSSM-LOAD/*MANDATORY-AT-STARTUP'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1620

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1620 DIFFERENT VERSIONS OF SUBSYSTEM '(&00)' - '(&01)' WITH 'CREATION-TIME=*AT-SUBSYSTEM-CALL' AND 'VERSION-COEXISTENCE=FORBIDDEN' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1621

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1621 OPERAND ERROR: SAME 'TSN' AND 'VERSION-COEXISTENCE/-EXCHANGE=*ALLOWED' NOT ALLOWED FOR WORK TASK SUBSYSTEMS '(&00)' AND '(&01)'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1626

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1626 SAME ISL ENTRY WITH SAME 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN SUBSYSTEMS: '(&00)' - '(&01)' WITH 'VERSION-COEXISTENCE=*ALLOWED' IS NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1627

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1627 SAME ISL ENTRY WITH SAME 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN DIFFERENT SUBSYSTEMS '(&00)' - '(&01)' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1628

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1628 SAME SVC-NUMBER WITH SAME 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN SUBSYSTEMS '(&00)' - '(&01)' WITH 'VERSION-COEXISTENCE=*ALLOWED' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1629

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1629 SAME SVC-NUMBER WITH SAME 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN DIFFERENT SUBSYSTEMS '(&00)' - '(&01)' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1631

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1631 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*AT-DSSM-LOAD' HAS RELATION TO SUBSYSTEM '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE-DSSM-LOAD/*AT-DSSM-LOAD'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1632

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1632 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*BEFORE-DSSM-LOAD' HAS RELATION TO SUBSYSTEM '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE-DSSM-LOAD

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1633

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1633 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'STOP-AT-SHUTDOWN=*NO' HAS REFERENCE TO SUBSYSTEM '(&01)' WITH 'STOP-AT-SHUTDOWN=*YES'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1634

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1634 SAME SVC NUMBER WITH AND WITHOUT 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN '(&00)' - '(&01)' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1635

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1635 SAME ISL ENTRY IN DIFFERENT SUBSYSTEMS '(&00)' - '(&01)' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1636

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1636 SAME ISL ENTRY WITH AND WITHOUT 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' IN '(&00)' - '(&01)' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1644

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1644 FILE '(&00)' WITH LOGICAL-ID '(&01)' DOES NOT EXIST.

### Meaning

(&00): file name.
(&01): LOGICAL-ID of the file.

## ESM1645

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1645 LOGICAL-ID '(&00)' HAS NO ASSOCIATED PATH-NAME.

### Meaning

(&00): LOGICAL-ID of the file.

## ESM1650

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1650 SUBSYSTEM '(&00)' NOT YET DECLARED

### Meaning

(&00): name and version number of the subsystem.

## ESM1656

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1656 DIFFERENT VERSIONS OF SUBSYSTEMS '(&00)' - '(&01)' DECLARED WITH 'CREATION-TIME=*AT-SUBSYSTEM-CALL' AND 'FUNCTION-NUMBER' AND 'FUNCTION-VERSION' NOT SPECIFIED NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1657

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1657 DIFFERENT VERSIONS OF SUBSYSTEMS '(&00)' - '(&01)' DECLARED WITH 'CREATION-TIME=*BEFORE-DSSM-LOAD/*AT-DSSM-LOAD/MANDATORY-AT-STARTUP/*BEFORE -SYSTEM-READY/*AFTER-SYSTEM-READY' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1658

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1658 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*BEFORE-SYSTEM-READY' HAS RELATION TO SUBSYSTEM '(&01)' WITH 'CREATION-TIME' NOT EQUAL TO '*BEFORE-DSSM-LOAD/*AT-DSSM-LOAD/*MANDATORY-AT-STARTUP/*BEFORE-SYSTEM-READY '

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1659

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1659 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-ACCESS=*SYSTEM' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'SUBSYSTEM-ACCESS=*LOW/*HIGH'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1660

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1660 OPERAND ERROR: SUBSYSTEM '(&00)' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-PRIVILEGED'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1661

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1661 OPERAND ERROR: SUBSYSTEM '(&00)' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1663

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1663 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*SYSTEM-GLOBAL' DEPENDS ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-PRIVILEGED'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1664

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1664 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*SYSTEM-GLOBAL' DEPENDS ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1665

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1665 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'SUBSYSTEM-ACCESS=*SYSTEM' DEPENDS ON SUBSYSTEM '(&01)' WITH 'SUBSYSTEM-ACCESS=*LOW/*HIGH'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1668

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1668 OPERAND ERROR: SUBSYSTEM '(&00)' HAS LINK RELATION TO SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1669

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1669 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'MEMORY-CLASS=*SYSTEM-GLOBAL' DEPENDS ON SUBSYSTEM '(&01)' WITH 'MEMORY-CLASS=*BY-SLICE'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1670

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1670 SAME SVC NUMBER OR SAME SYSTEM-EXIT NUMBER IN DIFFERENT SUBSYSTEMS: '(&00)' - '(&01)' NOT ALLOWED

### Meaning

(&00), (&01): name and version number of the subsystem/
call ENTRY name.

## ESM1671

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1671 RANGE ERROR REPORT FOR SUBSYSTEM '(&00)' VERSION '(&01)'

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1672

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1672 VERSION RANGE '(&00)'-'(&01)' NOT SATISFIED BY SUBSYSTEM '(&02)'

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1673

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1673 CYCLE IN RELATION BETWEEN SUBSYSTEM '(&00)' VERSION '(&01)' AND SUBSYSTEM '(&02)' VERSION '(&03)'

### Meaning

(&00), (&01): name of the subsystem
(&01), (&03): version number of the subsystem.

## ESM1683

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1683 OPERAND ERROR: SUBSYSTEM '(&00)' WITH 'CREATION-TIME=*AFTER-SYSTEM-READY' HAS RELATION TO SUBSYSTEM '(&01)' WITH INCOMPATIBLE 'CREATION-TIME'

### Meaning

(&00), (&01): name and version number of the subsystem.

## ESM1684

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1684 OPERAND ERROR: FOR 'MEMORY-CLASS=*LOCAL-UNPRIVILEGED' OPERAND 'SIZE' AND 'START-ADDRESS' OF SUBSYSTEM '(&00)' AND SUBSYSTEM '(&01)' NOT PROCESSABLE

### Meaning

The subsystems (&00) and (&01) overlap each other because of
the specified operands SIZE and START-ADDRESS.
(&00), (&01): name and version number of the subsystem.

## ESM1806

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1806 DMS ERROR '(&00)' ON FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

During processing, a DMS error was detected by the program.
For more detailed information about the DMS error code enter /HELP-MSG
in system mode or see the BS2000 manual 'System Messages'.
(&00): DMS error code
(&01): file name.

### Response

Check the error cause and issue the statement again.

## ESM1820

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1820 FILE '(&00)' IS NOT A DSSM CATALOG OR HAS AN INVALID VERSION

### Meaning

(&00): catalog name.

## ESM1821

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1821 CHECK REPORT:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1822

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1822 **** NO ERROR ****

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1823

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1823 CHECK OF LINK REFERENCES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1824

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1824 VERSION RANGE CHECK:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1825

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1825 LINK RELATION CHECK:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1826

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1826 CHECK OF FUNCTIONAL DEPENDENCE:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1827

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1827 DEPENDENCE RELATION CHECK:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1828

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1828 CHECK OF RELATED FILES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM1830

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM1830 CYCLE CHECK:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM4009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM4009 ********************************************************************

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM4010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM4010 * (&00) * SUBSYSTEM NAME: (&01) VERSION: (&02) *

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management.

## ESM5000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5000 NO SUBSYSTEM CORRESPONDING TO SELECTION

### Meaning

Catalog does not contain the subsystem given in the statement.

## ESM5001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5001 SHOW REPORT:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5002 SUBSYSTEM CATALOG: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5003 FORCED GENERATION: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5004 HSI : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5005 CONTAINED SUBSYSTEMS:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5006 NAME VERSION NAME VERSION

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5007 ---- ------- ---- -------

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5008 (&00) (&01) (&02) (&03)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5009 ********************************************************************

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5010 * (&00) * SUBSYSTEM NAME: (&01) VERSION: (&02) *

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5011 REP-FILE-MANDATORY : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5012 GENERAL ATTRIBUTES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5013 CREATION-TIME : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5014 STOP-AT-SHUTDOWN : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5015 SUBSYSTEM-HOLD : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5016 STATE-CHANGE-CMDS : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5017 FORCED-STATE-CHANGE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5018 RESET : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5019

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5019 RESTART-REQUIRED : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5020 VERSION-COEXISTENCE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5021 VERSION-EXCHANGE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5022

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5022 INTERNAL ENTRIES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5023 INIT-ROUTINE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5024 STOPCOM-ROUTINE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5025 DEINIT-ROUTINE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5026 DYNAMIC-CHECK-ENTRY : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5027 INTERFACE-VERSION : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5028

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5028 MEMORY ATTRIBUTES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5029 MEMORY-CLASS: (&00) SUBSYSTEM-ACCESS: (&01)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5030 SIZE : (&00) START-ADDRESS : (&01)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5031 RELATIVE LOCATION IN ADDRESS SPACE STRIPE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5032 RELATED FILES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5033

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5033 INSTALLATION-USERID : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5034

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5034 LIBRARY : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5035 MESSAGE-FILE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5036 SUBSYSTEM-INFO-FILE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5037

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5037 REP-FILE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5038

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5038 LINK ATTRIBUTES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5039

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5039 LINK-ENTRY: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5040

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5040 AUTOLINK : (&00) UNRESOLVED: (&01) CHECK-REFERENCE: (&02)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5041 REFERENCED SUBSYSTEMS:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5042

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5042 NAME LOWEST VERSION HIGHEST VERSION

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5043

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5043 ---- -------------- ---------------

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5044

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5044 **** NONE ****

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5045

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5045 (&00) (&01) (&02)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5046

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5046 FUNCTIONAL DEPENDENCE WITH SUBSYSTEMS:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5047 SEPARATE-ADDRESS-SPACE FROM SUBSYSTEMS:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5048

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5048 NAME NAME NAME NAME

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5049

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5049 ---- ---- ---- ----

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5050 (&00) (&01) (&02) (&03)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5051 SHARED-HOLDER-TASK: (&00) WITH SUBSYSTEMS:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5052 NAME VERSION NAME VERSION

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5053 ---- ------- ---- -------

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5054 **** WORK TASK ****

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5055 (&00) (&01) (&02) (&03)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5056

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5056 SUBSYSTEM-ENTRIES:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5057

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5057 NAME: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5058 MODE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5059 NUMBER : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5060

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5060 CALL-BY-SYSTEM-EXIT: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5061 FUNCTION-NUMBER : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5062

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5062 FUNCTION-VERSION : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5063

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5063 CONNECTION-ACCESS : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5064

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5064 CONNECTION-SCOPE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5065

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5065 SUMMARY:

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5070

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5070 CE-BY-PROGRAM : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5071

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5071 DUMMY-ENTRY : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5076

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5076 (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5077

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5077 SYNTAX-FILE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5078

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5078 COPYRIGHT : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5079

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5079 YEAR : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5080

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5080 CLOSE-CTRL-ROUTINE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5081

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5081 SUBSYSTEM-LOAD-MODE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5082

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5082 | GENERAL ATTRIBUTES | INTERNAL ENTRIES | SUBSYST | MEMORY| RELATED FILES |

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5083

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5083 | C S | C D | ENTRIES | | I | H

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5084

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5084 | R H C C C X R | L S Y | | | M R S N | O

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5085

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5085 | E U O F H O C E | O T D N | | A | S E Y F | L

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5086

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5086 NR SS-NAME VERSION STD | A T M O R K E H S | S O E C | S | C C | G P N O | D

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5087

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5087 | T D H M R E L X A T | I E P I H | Y | L C | F F F F | E

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5088

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5088 | I O O A C S I I N A | N C C N E | S S | A E | I I I I | R

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5089

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5089 | M W L N E E N S G R | I T O I C | V E | S S | L L L L | I

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5090

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5090 | E N D D D T K T E T | T L M T K | C X | S S | E E E E | D

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5091

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5091 --------------------------------------------------------------------------- --------------------------------------------------------

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5092

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5092 FIRST-CONNECTION : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5093

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5093 LOGICAL-ID : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5094

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5094 DEFAULT-NAME : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5095

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5095 INSTALLATION-UNIT : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5096

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5096 ON-ACTION : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5101 INVALID '*CURRENT' VALUE: NO SSD-OBJ IN PROCESS

## ESM5102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5102 FORMAT OF FILE '(&00)' INVALID

### Meaning

The file must be a SSD-OBJ file created by DSSM

## ESM5103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5103 FILE '(&00)' IS EMPTY

## ESM5104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5104 SSD-OBJ FILE: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5105 SSD-NAME : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5106

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5106 SSD-VERSION : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5107 DOMAIN : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5108 CORRECTION : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5109 (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5110 **************************************************************

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5111 * SUBSYSTEM NAME: (&00) VERSION: (&01) *

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5120 DSSM VERSION: (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5121 CATALOG VERSION: (&00) (&01)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5122 STATUS OF THE SUBSYSTEM : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5123

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5123 MONITORING JOB VARIABLE : (&00)

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5124 * (&00) * LOCAL SUBSYSTEM NAME: (&01) VERSION: (&02) *

### Meaning

This message is used internally by DSSM for its information reporting.
DSSM: Dynamic SubSystem Management

## ESM5151

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5151 SSD-OBJ FILE '(&00)' ALREADY EXISTS

### Meaning

(&00): SSD-OBJ file name.

## ESM5152

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5152 SSD-OBJ FILE '(&00)' CREATED

### Meaning

(&00): SSD-OBJ file name.

## ESM5153

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5153 INCOMPATIBLE SSD-OBJ FILE '(&00)' CANNOT BE PROCESSED

## ESM5154

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ESM5154 SSD-OBJ FILE IS CORRUPTED

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages