# IOD

## IOD0001

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0001 IOD_Vxx RELEASE SL=mmm *** IOD IPL READY ***

### Meaning

The IOD (I/O handler for bus devices whose I/Os are performed via X2000) issues this
message on every IPL of a VM.

## IOD0859

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0859 IOT11 NO PCIB ADDITIONAL SPACE AVAILABLE

### Meaning

A new device has been configured in X2000. The device could not be activated because
the IOD was not assigned sufficient memory.

### Response

Check the X2000/system memory configuration. Configure the device again. A reboot of
the system can probably solve the problem.

## IOD0869

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0869 IOT01 DEVICE MN=xxxx DEACTIVATED

### Meaning

The configuration data of the device with the mnemonic name xxxx has been modified. The
device has therefore been deactivated. The device can no longer be operated by BS2000
(condition code 3).

## IOD0869

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0869 RKF05 DEVICE MN=xxxx ACTIVATED

### Meaning

A new or existing device with the mnemonic name xxxx has been activated. The device can
now be operated from BS2000.

## IOD0879

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0879 IOD_Vxx SL=mmm. * Device configuration request from X2000 *
IOD0879 RKF00 PCIB INVALID CHN=yy UA=zz - REQUEST REJECTED

### Meaning

A new device has been configured in X2000. The data passed from X2000 is incorrect. (CHN=host connector number=CHPID)

### Response

Repeat configuration in X2000. If this repetition is unsuccessful, an IOHDUMP should be
generated and then analyzed or sent to a Support Center.

## IOD0879

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0879 IOD_Vxx SL=mmm. * Device configuration request from X2000 *
IOD0879 RKF04 DEVICE CHN=xx UA=yy OF TYPE vv CANNOT BE ADDED - REQUEST REJECTED

### Meaning

A device has been configured or modified in X2000. IOD does not support the entered
device type.

### Response

Repeat the configuration in X2000 with a valid device type. If a device of type vv is
absolutely necessary, contact the X2000 development team.

## IOD0880

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0879 IOD_Vxx SL=mmm. * Device configuration request from X2000 *
IOD0880 DEVICE MN=xxxx WAS ALREADY DEFINED ON HC=ch Unit= ua - REQUEST REJECTED

### Meaning

A device has been configured or modified in X2000. IOD does not support the entered
device type.

### Response

Repeat the configuration in X2000 with a valid device type. If a device of type vv is
absolutely necessary, contact the X2000 development team.

## IOD0888

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0888 IOD_Vxx SL=mmm *** IOD NON FATAL ERROR! ***
IOD0888 *** ERROR CODE=modyyy *** CHECK IOHDUMP!

### Meaning

IOD has detected an error but the system continues to run. An IOHDUMP has been generated which is stored under /var/opt/SMAW/X2000/dump/ .

### Response

Analyze the IOHDUMP with mdebug or send it to the Support Center.

## IOD0999

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0999 IOD_Vxx SL=mmm *** IOD ABNORMAL END ***
IOD0999 *** ERROR CODE=modyyy *** START IMPL!

### Meaning

IOD has detected an internal error. The system run should be terminated. An IOHDUMP
was generated and saved in the directory /var/opt/SMAW/X2000/dump/.

### Response

Analyze the IOHDUMP with mdebug or send it to the Support Center.

## IOD0999

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

IOD0999 *** ERROR CODE = FWI011 *** START INIT!

### Meaning

Initialization of the subchannels of a VM failed.

### Response

Diagnose the cause of the error and repeat IPL of the VM.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages