## NLK1001

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK1001 ISL: PARAMETER LIST NOT ALLOCATED. TASK TERMINATED ABNORMALLY. TAKE DUMP

### Meaning

A system function was called via ISL without a parameter list.

### Response

Take a system dump and send it to the diagnose.

## NLK1002

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK1002 ISL: PARAMETER LIST NOT ALIGNED ON WORD BOUNDARY. TASK TERMINATED ABNORMALLY.

### Meaning

A system function was called via ISL with a parameter list which
was not fullword aligned.

### Response

Take a system dump and send it to the diagnose.

## NLK2001

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK2001 DSL: CALLER OF ETMSWPS WITHOUT PROGRAM MANAGER ENVIRONMENT. TASK TERMINATED ABNORMALLY. TAKE DUMP

### Meaning

The caller of the function 'switch program stack' is not an
SPL-environment-procedure.

### Response

Take a system dump to determine the caller.

## NLK2002

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK2002 DSL: DSL-EXTENT-PATTERN 'DSLE' OVERWRITTEN. TASK TERMINATED ABNORMALLY.

### Meaning

At DSL-Overflow the check-pattern 'DSLE' wasn't found. ment-procedure.

### Response

Take a system dump to determine the procedure which had overwritten.

## NLK2003

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK2003 MEMORY-REQUEST REJECTED. TASK ABNORMALY TERMINATED.

### Meaning

There is no memory available for a longjmp-trace

### Response

Take a systemdump to determine the reason

## NLK3001

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK3001 SVC: CALL FROM TPR WITH A PARAMETER LIST NOT ALIGNED ON WORD BOUNDARY. TASK TERMINATED ABNORMALLY. TAKE DUMP

### Response

Take systemdump and send it to the diagnose.

## NLK3002

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NLK3002 SVC: CALL FROM TU WITH A PARAMETER LIST NOT ALIGNED ON WORD BOUNDARY. TASK TERMINATED ABNORMALLY. TAKE DUMP

### Response

Take systemdump and send it to the diagnose.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages