## SGUCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGUCOPY Copyright (C) '(&00)' '(&01)' All Rights reserved

## SGULOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGULOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## SGU0001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0001 Error at SINF call

### Response

Contact Your System Administrator or Customer Support.

## SGU0002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0002 System version not supported

### Meaning

SMPGEN-U can not yet be called in this version of BS2000.

## SGU0003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0003 Error at SDF call. Returncode '(&00)'

### Meaning

Returncode (&00) at RDATA call.

### Response

Analyse the returncode.

## SGU0004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0004 Unknown SMPGEN statement, statement version or operand value

### Response

Check the SMPGEN-U syntaxfile

## SGU0005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0005 Semantic error '(&00)' in SMPGEN statement

### Meaning

'(&00)' : detailled error specification :
1 = pubset id and volumeset ids must be different from each other
2 = The pubset specified as ATTRIBUTE-ORIGIN
must be one of the pubsets to be converted
3 = The id of the control volumeset must be
one of the pubset ids
4 = all the volumeset ids must be different from each other
5 = TEXT-OUTPUT=*NONE and STRUCTURE-OUTPUT=*NONE
must not be specified together

### Response

Enter a correct SMPGEN statement.

## SGU0006

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0006 The subsystem SMPGEN-S is not declared

### Response

Add the SMPGEN-S declaration to the subsystem catalog.

## SGU0007

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0007 Incompatible subsystem version of subsystem SMPGEN-S

### Meaning

The version of the subsystem SMPGEN-S is not compatible
with the version of the subsystem SMPGEN-U.

### Response

Correct Your subsystem catalog.

## SGU0008

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SGU0008 The subsystem SMPGEN-S cannot be loaded

### Response

Contact Your system operator or system administrator.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages