## CRYCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CRYCOPY Copyright (C) '(&01)' '(&00)' All Rights Reserved

## CRYLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CRYLOAD Subsystem '(&00)', Version '(&01)' of '(&02)' loaded

## CRYSTRT

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CRYSTRT Subsystem '(&00)', Version '(&01)' of '(&02)' started

## CRY0001

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

CRY0001 CRYPT '(&00)' ACTIVE

### Meaning

The CRYPT task was successfully initialized.
CRYPT version (&00) is active.

## CRY0002

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

CRY0002 CRYPT TERMINATED

### Meaning

CRYPT has been terminated.

## CRY0003

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

CRY0003 ABNORMAL TASK TERMINATION OF CRYPT TASK

### Meaning

Abnormal task termination of the CRYPT task.

### Response

Take dump.

## CRY0004

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

CRY0004 CRYPT NOT STARTED. REASON: (&00)

### Meaning

CRYPT has not been started.

## CRY0010

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

CRY0010 TRACE '(&00)' NOT INITIALIZED

### Meaning

The initialization for the trace (&00)
has not been successful.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages