## NLX0001

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX0001 Unrecoverable error in subsystem NSM

### Meaning

A serslog with this ID was written.

### Response

Save the Serslogfile and inform the diagnosegroup.

## NLX0003

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX0003 Lock hold at stop of NSM

### Meaning

A serslog with this ID was written with more details.

### Response

Save the Serslogfile and inform the diagnosegroup.

## NLX0004

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX0004 Recoverable error in subsystem NSM

### Meaning

A serslog with this ID was written.

### Response

Save the Serslogfile and inform the diagnosegroup.

## NLX0100

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX0100 Bourse error in subsystem NSM

### Meaning

The bourse of Subsystem NSM is destroyed.
NSM was terminated abnormally.

### Response

Inform the diagnosegroup.
To join the XCS again a BS2000-restart is necessary.

## NLX1000

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1000 Internal version '(&00)' and date '(&01)' of NSM

### Meaning

The internal version and date are given.

## NLX1001

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1001 Internal error in subsystem NSM, host leaves XCS

### Meaning

There is an internal error in Subsystem NSM.

### Response

Save the Serslogfile and inform the diagnosegroup.

## NLX1002

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1002 Locks held during delete of subsystem NSM

### Meaning

A system component held a global lock during delete of subsystem NSM.
See serslogentry NLX0003 for more details.

### Response

Inform the diagnosegroup, supply serslog.
To join the XCS again a BS2000-restart is necessary.

## NLX1005

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1005 The version of the host to join the xcs is incompatible with version of one host in the xcs

### Meaning

The version of the host to join the xcs is incompatible with
version of one host in the xcs. The host aborts the join.

### Response

Use compatible versions of NSM on all hosts of XCS.

## NLX1006

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1006 Internal error in subsystem NSM

### Meaning

There is an internal error in Subsystem NSM.
Processing continues.

### Response

Save the Serslogfile and inform the diagnosegroup.

## NLX1007

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1007 Error '(&00)' during creation of GS-partition of NSM

### Meaning

Problems during creation of GS-Partition 'NSM'.
Type /HELP-MSG (&00) for more information.

## NLX1008

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1008 Not enough GS available for Partition 'NSM', '(&00)' MB required

## NLX1009

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1009 Command SET-NSM-ENVIRONMENT is only allowed in NSM configuration file

## NLX1010

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1010 DMS-Error '(&00)' during processing of file '(&01)'

### Meaning

DMS-Error during processing of SYSSII-File.

## NLX1011

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1011 Syntax-Error in line '(&00)' of file '(&01)'

### Meaning

Error during processing of SYSSII-File. Processing aborted.

## NLX1012

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1012 No use of GS by NSM: GSUSAGE is LOCAL or no GS AVAILABLE

## NLX1013

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1013 GS partition 'NSM' with '(&00)' MB created

## NLX1014

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1014 GS partition 'NSM' in use by XCS-function 'NSG'

## NLX1015

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1015 Global Store access failed

### Meaning

Error during global store access.
NSM is using MSCF communication temporarily.

## NLX1016

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1016 Global Store access permanently failed.

### Meaning

Global store access permanently failed.
NSM uses MSCF for communication.

## NLX1017

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1017 Invalid GS configuration. XCS-join aborted.

### Meaning

The global store access is of type 'GLOBAL'
but no shared GS during XCS-JOIN.

### Response

Modify parameter GSUSAGE of subsystem GSMAN or
make the Global Store shared.

## NLX1018

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1018 Resource bottleneck, host leaves XCS

### Meaning

A resource bottleneck is the reason that NSM is not
able to keep XCS-global data consistent. Host leaves XCS.

## NLX1019

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1019 Error during processing of command '(&00)'. Processing of command aborted

### Meaning

(&00): command MODIFY-NSM-ENVIRONMENT
or SHOW-NSM-CONFIGURATION.

### Response

Contact the system administrator.

## NLX1020

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1020 No information found for specified selection

### Meaning

No information is available matching the selection criteria specified in
command /SHOW-NSM-CONFIGURATION.

### Response

Reenter the command specifying a different selection criterium.

## NLX1021

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1021 Subsystem info file not valid. Defaults used.

### Meaning

Subsystem info file does not exist or
contains no valid command.

### Response

Correct the file.

## NLX1030

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1030 Command with Communication-Switch from MSCF to GS accepted

### Meaning

The request to switch the communication from *BY-MSCF to
*BY-GS specified in Command MODIFY-NSM-ENVIRONMENT is started.

### Response

## NLX1031

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1031 Command with Communication-Switch from MSCF to GS executed

### Meaning

The request to switch the communication from *BY-MSCF to
*BY-GS specified in Command MODIFY-NSM-ENVIRONMENT is
executed with success.

### Response

## NLX1032

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1032 Command with Communication-Switch from MSCF to GS on all Hosts executed

### Meaning

The request to switch the communication from *BY-MSCF to
*BY-GS specified in Command MODIFY-NSM-ENVIRONMENT is
executed with success on all hosts of the xcs.

### Response

## NLX1033

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1033 Command with Communication-Switch from MSCF to GS not accepted, Error Code '(&00)'.

### Meaning

The request to switch the communication from *BY-MSCF to
*BY-GS specified in command MODIFY-NSM-ENVIRONMENT is rejected.
The error code '(&00)' classifies the possible reasons.
(&00): Meaning of the error codes:
01: The requested state *BY-GS is already active.
02: The request to switch the communication is still active.
03: The communication state is not MSCF-ACTIVE.
04: A xcs reconfiguration is active.
05: A switch of communication is initiated already on another
host.
06: Not all hosts in the xcs supported the requested function.

### Response

## NLX1034

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1034 Command with Communication-Switch from MSCF to GS failed

### Meaning

The request to switch the communication from *BY-MSCF to
*BY-GS specified in Command MODIFY-NSM-ENVIRONMENT failed.

### Response

## NLX1040

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1040 Command with Communication-Switch from GS to MSCF accepted

### Meaning

The request to switch the communication from *BY-GS to
*BY-MSCF specified in Command MODIFY-NSM-ENVIRONMENT is started.

### Response

## NLX1041

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1041 Command with Communication-Switch from GS to MSCF executed

### Meaning

The request to switch the communication from *BY-GS to
*BY-MSCF specified in Command MODIFY-NSM-ENVIRONMENT is
executed with success.

### Response

## NLX1042

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1042 Command with Communication-Switch from GS to MSCF on all Hosts executed

### Meaning

The request to switch the communication from *BY-GS to
*BY-MSCF specified in Command MODIFY-NSM-ENVIRONMENT is
executed with success on all hosts of the xcs.

### Response

## NLX1043

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1043 Command with Communication-Switch from GS to MSCF is rejected, Error Code '(&00)'.

### Meaning

The request to switch the communication from *BY-GS to
*BY-MSCF specified in command MODIFY-NSM-ENVIRONMENT is rejected.
The error code '(&00)' classifies the possible reasons.
(&00): Meaning of the error codes:
01: The requested state *BY-MSCF is already active.
02: The request to switch the communication is still active.
03: The communication state is not GS-ACTIVE.
04: A xcs reconfiguration is active.
05: A switch of communication is initiated already on another
host.
06: Not all hosts in the xcs supported the requested function.

### Response

## NLX1044

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1044 MINIMUM-DELAY-TIME must be smaller than MAXIMUM-DELAY-TIME. Values unchanged.

## NLX1045

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NLX1045 MINIMUM-DELAY-TIME must be smaller than MAXIMUM-DELAY-TIME. Defaultvalues used.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages