## UTMCRSH

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

UTMCRSH UTM TERMINATES BS2000 SYSTEM RUN FOR DIAGNOSTIC REASON

### Meaning

UTM terminates the BS2000 system run to obtain full diagnostics.
This diagnostic method can only be switched on by a REP.

### Response

Look why this REP is active and examine SLED.

## UTMKDCM

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

UTMKDCM KDCMON TERMINATED BY '/STOP-SUBSYSTEM KDCMON,FORCED=YES'

### Meaning

The system administrator has deleted the KDCMON subsystem, thereby
automatically terminating all tasks still connected to KDCMON.

### Response

This is an informational message.

## UTMREVI

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

UTMREVI COMP=UTMMF,VER=V07.0A00,DATE=190802,COMPNR=51318026

### Meaning

This is the message concerning the version of the message file.

### Response

This is an informational message.

## UTMTRMA

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

UTMTRMA TASK TERMINATION, BECAUSE OF AN UTM INTERNAL ERROR

### Meaning

UTM terminates a task of the UTM application with $TERM UNIT=STEP, because
an UTM error occurred (term application).
This is the normal error processing of an UTM internal error.
The processing continues with the next /SET-JOB-STEP command.

### Response

The reaction to this message is given in the UTM manual
"Messages, Debugging and Diagnostics in BS2000/OSD".

## UTMTTRM

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

UTMTTRM TASK TERMINATION, BECAUSE OF INCORRECT UTM START PROCEDURE

### Meaning

UTM terminates a task of the UTM application with $TERM UNIT=TASK because
an incorrect start procedure has reloaded the UTM application program
after a start error or after a normal or abnormal application shutdown.

### Response

Correct the start procedure in accordance with description in the
UTM manual "Using openUTM Applications under BS2000/OSD".

## UTM0100

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

UTM0100 (&00)

### Meaning

The reason for this UTM message is explained in the UTM manual
"Messages, Debugging and Diagnostics in BS2000/OSD".

### Response

The reaction to this message is given in the UTM manual
"Messages, Debugging and Diagnostics in BS2000/OSD".

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages