## DER0002

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0002 Invalid $DOER call parameters

### Meaning

The $DOER parameter area, the attached CCB, or the CCW-chain
contains at least one invalid parameter.
The TERMINATION code and the REASON code give more detailed
information on the reason.
----- Text 1 -----------------------------------------------------
BYTE 0-1 : DIAGNOSTIC ERROR-ID (FOR D.E.R.-DEVELOPMENT USAGE).
BYTE 2-3 : TERMINATION CODE (TC) OF D.E.R.
BYTE 4-7 : ADDRESS OF $DOER CALL.
BYTE 8-95: DDCB (IF TC>2) OR $NJATIP-PARAMS (IF TC=1).
BYTE 96->: CCB (IF TC>3).
----- Dump 1 ----------------------------------------------------
H 0 REASON Code
H 2 TERMINATION CODE
A 4 CALLER ADDRESS
XL(NJAHEADL) 8 DDCB (88 bytes, with TC=3 or 4)
XL(IDZCCBLN) 96 CCB (256 bytes, with TC=4)
----- TERMINATION Codes (TC) ------------------------------------
1 invalid parameters on $NJATIP-call
2 invalid DDCB address
3 invalid parameters in DDCB
4 invalid parameters in DDCB or CCB
----- REASON Codes ----------------------------------------------
1 DDCB not allocated
2 invalid user id
3 CCB address is zero
4 D.E.R. called by ADAM with NOACT
5 D.E.R. called by ADAM with A(DDP)=0
6 no HW-LRC in CCB
7 invalid address of CCW chain in CCB
8 no DDP module defined in NKATSOSM for dev.tp.
9 invalid FHDR values
10 invalid device type
11 invalid TIP-FHDR values
12 error during task independent processing
13 invalid channel type in CCB
14 no hardware error in channel registers of CCB
15 $ALESRV-error
16 NJAXINI-error

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0003

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0003 Error during device detach ($NJADEV)

### Meaning

An error occurred during a device detach ($NJADEV).
The parameter area of the unsuccessful function call is dumped.
There are the following possible reasons:
a) $GETMEM error (get memory)
----- Text 1 -----
$GETMEM ERROR IN MODULE NJACCPAG - NJAPDEV
----- Dump 1 -----
XL(NVAG#) 0 $GETMEM parameter area
b) $RECONF error (detach device)
----- Text 1 -----
$RECONF ERROR IN MODULE NJACCPAG - NJAPDEV
----- Dump 1 -----
XL30 0 $RECONF parameter area
XL(NVAR#) 30 $RETMEM parameter area

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0004

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0004 Error during path remove ($NJAPTH)

### Meaning

An error occurred during removing a device path ($NJAPTH).
The parameter area of the unsuccessful function call is dumped.
There are the following possible reasons:
a) $GETMEM error (get memory)
----- Text 1 -----
$GETMEM ERROR IN MODULE NJACCPAG - NJAPPTH
----- Dump 1 -----
XL(NVAG#) 0 $GETMEM parameter area
b) $RECONF error (remove path)
----- Text 1 -----
$RECONF ERROR IN MODULE NJACCPAG - NJAPPTH
----- Dump 1 -----
XL35 0 $RECONF parameter area
XL(NVAR#) 35 $RETMEM parameter area

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0005

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0005 Error during call to a HISTORY function in the TAPE-D.E.R

### Meaning

An error occurred during a call to a D.E.R.-HISTORY-function in the
TAPE-D.E.R.
The parameter area of the unsuccessful function call is dumped.
There are the following possible reasons:
a) $NJHINI error (initialize history table)
b) $NJHADD error (add HISTORY record)
c) $NJHEVA error (evaluate history table)
----- Text 1 -----
ERROR DURING CALL OF A HISTORY-FUNCTION IN MODULE NJTACT
----- Dump 1 -----
XL1 0 error code
XL7 1 *reserved
XL(NJHI#) 8 $NJHINI parameter area
XL(NJHA#) 8+NJHI# $NJHADD parameter area
XL(NJHE#) 8+NJHI#+NJHE# $NJHEVA parameter area
----- ERROR Codes -----
1 $NJHINI-error
2 $NJHADD error at recovery action 1 or 2
3 $NJHADD error at recovery action 3
4 $NJHEVA error at recovery action 1 or 2
5 $NJHEVA error at recovery action 3

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0006

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0006 Error during call to Hardware Error Logging processing

### Meaning

An error occurred during a call to the hardware error logging function
($HELTPR).
The parameter area of the unsuccessful function call is dumped.
----- Text 1 -----
ERROR DURING CALL OF $HELTPR IN MODULE NJACCRES, PROCEDURE NJARHEL
----- Dump 1 -----
XL(HEL2#) 0 $HELTPR parameter area

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0007

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0007 Error in D.E.R server task

### Meaning

An error occurred during processing in the D.E.R.-server-task DER1.
The parameter area of the unsuccessful function call is dumped.
There are the following possible reasons:
a) $ENER error (enable task error recovery)
----- Text 1 -----
$ENER ERROR IN MODULE NJACCPAG - NJAPTSK
----- Dump 1 -----
XL(ENER#) 0 $ENER parameter area
b) $NBRSIG error (receive signal)
----- Text 1 -----
$NBRSIG ERROR IN MODULE NJACCPAG - NJAPTSK
----- Dump 1 -----
XL(NTBR#) 0 $NBRSIG parameter area
c) Parameter error in Server-Task-Order (NJMSRVO parameter area)
----- Text 1 -----
SLOT-DATA ERROR IN MODULE NJACCPAG - NJAPTSK
----- Dump 1 -----
XL(NJAB#) 0 NJMSRVO parameter area

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0008

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0008 Error during processing an asynchronous D.E.R call

### Meaning

An error occurred during an asynchronous D.E.R.-processing
(task independent processing: TIP).
The parameter area of the unsuccessful function call is dumped.
There are the following possible reasons:
a) $RETSL error (return slot)
----- Text 1 -----
$RETSL ERROR IN MODULE NJAMAIN - NJAMTIP
----- Dump 1 -----
XL(NVSR#) 0 $RETSL parameter area
b) Invalid function header data of NJMSRVO (server task order).
----- Text 1 -----
FHDR ERROR IN MODULE NJAMAIN - NJAMTIP
----- Dump 1 -----
XL(NJAB#) 0 NJMSRVO parameter area

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

## DER0009

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

DER0009 Error when calling the D.E.R asynchronously

### Meaning

An error occurred when calling the D.E.R asynchronously
(task independent processing: TIP).
There are the following possible reasons:
a) $GETS error (get slot)
The $GETS-returncode and the slotpool-id are dumped.
----- Text 1 -----
$GETS ERROR IN MODULE NJACCPAG - NJAPTIP
----- Dump 1 -----
XL4 0 Slotpool id
XL4 4 $GETS returncode from R15
b) $NBSSIG error (send signal)
The parameter area of the unsuccessful function call is dumped.
----- Text 1 -----
$NBSSIG ERROR IN MODULE NJACCPAG - NJAPTIP
----- Dump 1 -----
XL(NTBS#) 0 $NTBS parameter area

### Response

Call the software service.
Diagnostic material: This SERSLOG record.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages