## NVLCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NVLCOPY COPYRIGHT (C) (&00) (&01) ALL RIGHTS RESERVED

## NVLLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NVLLOAD PROGRAM '(&00)', VERSION '(&01)' OF '(&02)' LOADED FROM FILE '(&03)'

## NVL0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0000 VOLIN VERSION (&00) READY

## NVL0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0001 VOLIN RESTRICTED TO SYSTEM ADMINISTRATOR. VOLIN TERMINATED

## NVL0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0002 ENTER VSN AND DEVICE TYPE AND / OR UNIT, OR TERMINATE VOLIN WITH 'END'

### Meaning

The message announces the first RDATA for a parameter set.

## NVL0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0003 ENTER ADDITIONAL INITIALIZATION PARAMETERS OR TERMINATE INPUT WITH 'EOT=YES'

## NVL0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0004 SYNTAX ERROR IN PARAMETER '(&00)'

### Meaning

Certain errors don't allow to determine the erroneous parameter.
In this case an empty string is indicated.
If 'END' is indicated as erroneous parameter, a typing error in any other
parameter may be possible. The erroneous parameter itself therefore can
not be identified.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0005 KEY WORD '(&00)' INCORRECT OR INVALID

### Meaning

Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0006 VSN AND / OR DEVICE TYPE AND / OR UNIT NOT SPECIFIED. ALL GIVEN PARAMETERS WILL BE IGNORED

### Meaning

VOLIN expects as obligate input the VSN and at least one of the two items
device type or unit (device mn).
For a Repair job with input unit, the input VSN is not necessary.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0007 THE VALUE SPECIFIED AS SIZE OF THE F1-LABEL IS TOO HIGH

### Meaning

The parameter F1-Label-Size (SDF syntax) resp. F1SIZE/VTOC (ISP syntax)
exceeds the limit 32766 or the number of blocks available on the disk.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0008 DEVICE TYPE AND / OR UNIT UNKNOWN OR NOT IN SYSTEM

### Meaning

The disk type specified by the parameter DEVICE (ISP syntax only) or
determined by the parameter UNIT could not be found in the VOLIN disk
characteristic tables.
If no typing error was made when specifying this parameters, it is
not possible to format and initialize the disk with the current VOLIN
version.
The device type STDDISK is not allowed for VOLIN.

## NVL0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0009 TRACK NUMBER OF DEFECTIVE TRACK INVALID

### Meaning

The number of a track specified as defective is not within the limits
imposed by the hardware.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0010

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0010 DISK '(&00)': STANDARD VOLUME LABEL INVALID

### Meaning

The disk pack assigned for the initialization of disk (&00) does not carry
a valid BS2000 standard volume label (SVL).
The initialization is terminated if the disk was requested by means of
parameter OVERWRITE-DISK (SDF syntax) resp. parameter CHECK (ISP syntax).
The disk pack remains unchanged. If a scratch disk pack was requested, the
further processing depends on the reply to the subsequent message(s).
Label creation only and not a emulated volume:
messages NVL0039 and NVL0040 follow.
Else:
message NVL0032 follows.

## NVL0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0011 VALUE OF PARAMETER 'F1SIZE' NOT POSITIVE

### Meaning

Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0012 EXISTING ALTERNATE TRACK AREA ON DISK '(&00)' DOES NOT HAVE STANDARD SIZE

### Meaning

Without formatting, the old alternate track area remains unchanged.
Note: By using disks with different alternate track areas it may cause
FDDRL problems.

## NVL0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0013 ERROR WHEN ACQUIRING DEVICE OR DISK. ERROR CODE: '(&00)'

### Meaning

(&00) = 3003: device temporarily not available (allocated to another task)
3103: device permanently not available (not attached)
3203: device allocation not allowed
3303: device not defined
4004: volume temporarily not available
4104: volume permanently not available (rejected by operator)
4204: volume allocation not allowed
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

### Response

Check the device or disk status and enable allocation for special use.

## NVL0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0014 DEVICE REQUESTED IN PARAMETER 'UNIT' DOES NOT MATCH DEVICE TYPE IN PARAMETER 'DEVICE'

### Meaning

Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0015 VOLIN: SYSTEM ERROR WHILE PAGE FIXING. INITIALIZATION TERMINATED WITH DUMP

### Meaning

It is not possible to fix a page required for I/O.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0016

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0016 VOLIN: ERROR AT MEMORY RELEASE.

### Meaning

If class 3 memory, initialization is terminated with dump.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0017

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0017 INITIALIZATION OF VOLUME '(&00)' ON UNIT '(&01)' COMPLETED. VOLUME FORMAT: '(&02)'

### Meaning

The volume (&00) may now be used in BS2000.

## NVL0018

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0018 VOLUME '(&00)' CANNOT BE USED DUE TO ERROR(S). INITIALIZATION TERMINATED ABNORMALLY

### Meaning

More detailed error messages precede this message.

## NVL0019

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0019 SYSTEM ERROR. INITIALIZATION ABORTED. VOLIN TERMINATED. DUMP WRITTEN TO 'SYSLST'

### Meaning

The program detects an illogical condition causing the program to
terminate
abnormally.
Possible reasons:
- a system error
- a VOLIN program error
- a hardware error on the disk used or its controller.
Under IPL-Exec, the dump is issued directly on printer. If no printer is
connected, the dump is lost.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0020

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0020 DEFECTIVE TRACK '(&01)' ON DISK '(&00)' COULD NOT BE FLAGGED AS DEFECTIVE. INITIALIZATION ABORTED. CONTACT MAINTENANCE

### Response

Ask the maintenance staff to check the disk.

## NVL0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0021 TOO MANY DEFECTIVE TRACKS ON DISK '(&00)'. INITIALIZATION ABORTED. CONTACT MAINTENANCE

### Meaning

The alternate track area is already exhausted, but another defective
track has been discovered on volume (&00).

## NVL0022

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0022 FORMATTING COMPLETED. TEST PATTERN '(&00)' WRITTEN ON ALL BLOCKS OF DISK '(&01)'

## NVL0023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0023 ALTERNATE TRACK '(&00)' ON DISK '(&01)' DEFECTIVE

## NVL0024

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0024 OVERWRITE DISK '(&00)' IN NEW FORMAT '(&01)'? REPLY (Y=YES; N=NO)

### Meaning

This is the last opportunity to prevent the BS2000 disk (&00) from
being overwritten in case the wrong disk is mounted or assigned.

### Response

Y: the disk pack will be overwritten in format (&01)
N: the disk pack remains unchanged; a new mount message is displayed;
another disk pack can be assigned.

## NVL0025

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0025 VTOC OF DISK '(&00)' CANNOT BE WRITTEN. INITIALIZATION ABORTED. CONTACT MAINTENACE

### Meaning

Possible reasons:
- the IPL,- SVL-, and format 5 labels could not be written to the volume
table of contents (VTOC) of disk (&00)
- the corresponding tracks were known to be defective.

### Response

Contact the maintenance staff to check the disk pack.

## NVL0026

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0026 DEVICE ERROR ON DISK '(&00)' DURING INITIALIZATION. REPLY (R=RETRY; T=TERMINATE INITIALIZATION)

### Meaning

A device error on disk (&00) could not be corrected by the error recovery
routine.

### Response

R: retry error recovery again
T: terminate the initialization of this volume.
If this message recurs, contact the maintenance staff to check the disk
and
its control unit.

## NVL0027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0027 SYSTEM ERROR (REQM). VOLIN ABORTED DUE TO INSUFFICIENT MEMORY

### Meaning

It is not possible to obtain sufficient memory for the I/O and the
work pages.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0029 TRACK '(&01)' ON DISK '(&00)' DEFECTIVE. TRACK '(&02)' ASSIGNED IN ALTERNATE TRACK AREA

## NVL0030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0030 REPLY TO PRECEDING MESSAGE INVALID. CORRECT REPLY

## NVL0031

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0031 INITIALIZATION STARTED FOR VOLUME '(&00)' ON UNIT '(&01)' IN FORMAT '(&02)'

## NVL0032

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0032 OVERWRITE NON-STANDARD DISK '(&00)' ON DEVICE '(&01)' IN NEW FORMAT '(&02)'? REPLY (Y=YES; N=NO)

### Meaning

The disk pack assigned by the operator is no BS2000 disk because
it has no valid standard volume label (SVL).

### Response

Y: the correct disk has been assigned
N: the wrong disk is mounted.
A new mount message follows for mounting the correct disk specified.

## NVL0033

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0033 RELEASE STARTED FOR VOLUME '(&00)' ON UNIT '(&01)'

### Meaning

Release of disk by SPACEPRO.

## NVL0034

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0034 VOLIN: SYSTEM ERROR DURING '(&00)'. INITIALIZATION TERMINATED WITH DUMP

### Response

Send the error documentation to diagnosis department.

## NVL0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0035 VERSIONS OF VOLIN AND BS2000 NOT COMPATIBLE. VOLIN TERMINATED ABNORMALLY

### Meaning

The VOLIN version started has not been released for the BS2000 version of
the current system.

## NVL0036

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0036 READ ERROR ON SYSDATA

### Meaning

An access error or
a record with more than 251 characters was encountered on SYSDTA.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0037

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0037 DISK '(&00)'. ASSIGNED DISK PACK IS VSN '(&01)', FORMAT '(&02)'. DEVICE TYPE '(&03)' ENCODED IN VOLUME LABEL DOES NOT AGREE WITH CURRENT DEVICE TYPE '(&04)'

### Meaning

The device type encoded in the volume label is (&03). However, according
to the system tables the disk device on which the disk pack is mounted
has the device type (&04).
The initialization is terminated, if the disk pack was requested by means
of parameter OVERWRITE-DISK (SDF syntax) resp. CHECK (ISP syntax). The
disk pack remains unchanged.
If a scratch disk pack was requested, the further processing depends on
the reply to the subsequent message(s):
Label creation only and not an emulated volume:
messages NVL0039 and NVL0040 follow.
Else:
message NVL0032 follows.

### Response

Check whether a wrong device type was assigned to the disk pack at
the system generation (UGEN) or the system initialization (CONFUPD).
If so, do not use the disk device for initialization.
If not, the disk pack is defective and must be formatted.

## NVL0038

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0038 DISK '(&00)'. ASSIGNED DISK PACK NOT EMPTY. OLD VSN '(&01)', EXISTING FORMAT '(&02)'

### Meaning

The disk pack assigned for initialization of disk (&00) is a BS2000
disk with VSN (&01) and format (&02).
The subsequent message NVL0024 permits the disk to be rejected.

## NVL0039

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0039 DISK '(&00)'. FORMATTING OF ASSIGNED DISK PACK REQUIRED BUT LABEL CREATION ONLY IS SPECIFIED

### Meaning

The disk pack assigned for the initialization of disk (&00) has to be
formatted but the parameter FUNCTION=*CREATE-LABELS-ONLY (SDF syntax)
resp. FMT=NO or FMT=0 (ISP syntax) is specified.
The subsequent message NVL0040 permits to withdraw this parameter or to
reject the disk pack.

## NVL0040

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0040 OVERWRITE NON-STANDARD DISK '(&00)' ON DEVICE '(&01)', USING THE STANDARD PARAMETER FOR FORMATTING? REPLY (Y=YES; N=NO)

### Meaning

The disk pack assigned is not a standard BS2000 disk.
For the initialization of a BS2000 disk, the disk pack has to be
formatted. The creation of lables only is not sufficient.
If desired, the specification to create labels only is ignored, and the
disk pack is formatted, using the standard values of the formatting
parameters.

### Response

Y: the disk pack is overwritten and formatted in accordance with the
message.
N: the disk pack remains unchanged.
A new mount message follows for mounting another disk pack.

## NVL0041

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0041 DISK DEVICE '(&00)' AND/OR DISK PACK MOUNTED ON IT REJECTED. NEW MOUNT REQUEST FOR INITIALIZATION OF DISK '(&01)' FOLLOWS

### Meaning

The system administrator rejected disk device (&00) and/or the disk pack
mounted on it.

## NVL0042

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0042 VOLIN ACQUIRES DISK DEVICE AND DISK PACK FOR INITIALIZATION OR REPAIR OF DISK '(&00)'

### Meaning

If the operating system cannot assign the device automatically, a mount
message is issued by the device management.

## NVL0043

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0043 DISK '(&00)'. PARAMETERS 'OVERWRITE-DISK' (SDF) RESP. 'CHECK' (ISP) AND/OR 'UNIT' PERMIT NO OTHER DEVICE ASSIGNMENT. INITIALIZATION TERMINATED ABNORMALLY

### Meaning

The initialization of disk (&00) cannot be retried with another disk pack,
because parameters OVERWRITE-DISK (SDF syntax) resp. CHECK (ISP syntax)
and/or UNIT require a particular disk pack.
particular disk pack.

### Response

Change the parameter(s) OVERWRITE-DISK resp. CHECK and/or UNIT and retry
the initialization.

## NVL0044

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0044 ALTERNATE CYLINDER '(&00)' OF DISK '(&01)' DEFECTIVE. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact a technician to check the disk pack.

## NVL0045

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0045 BLOCK NUMBER INVALID FOR DEFECTIVE BLOCK

### Meaning

The block number of a block flagged as defective is not contained within
the limits imposed by the hardware.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0046

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0046 DEFECTIVE SECTOR '(&01)' ON DISK '(&00)' CANNOT BE FLAGGED. INITIALIZATION TERMINATED ABNORMALLY

### Meaning

(&00) = VSN
(&01) = Physical block offset on volume (phys. RBN, not PHP!)

### Response

Contact the maintenance staff to check the disk pack.

## NVL0047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0047 WARNING: ALTERNATE BLOCK '(&00)' ON DISK '(&01)' DEFECTIVE

## NVL0048

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0048 WARNING: SECTOR '(&01)' ON DISK '(&00)' DEFECTIVE. ALTERNATE SECTOR ASSIGNED

### Meaning

(&00) = VSN
(&01) = Phys. block offset on volume (phys. RBN, not PHP!)

## NVL0049

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0049 DEVICE CHARACTERISTICS ON DISK '(&00)' CANNOT BE READ. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0050 DEFECTS LIST ON DISK '(&00)' CANNOT BE READ. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk pack.

## NVL0051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0051 ALTERNATE BLOCK AREA EXHAUSTED. FOR FORMATTING DISK PACK '(&00)' AGAIN, CONTACT MAINETANCE

### Meaning

There are no more alternate blocks on the cylinder.

## NVL0052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0052 TOO MANY DEFECTIVE BLOCKS ON DISK '(&00)'. INITIALIZATION TERMINATED ABNOMALLY. CONTACT MAINTENANCE

### Meaning

A defective block was found on disk (&00), but the alternate cylinder
has become exhausted.

## NVL0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0053 TRACK ASSIGNMENT NOT PERMITTED FOR DEVICE TYPE '(&00)'

### Meaning

The track assignment is not permitted for FBA disks.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0054

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0054 INVALID BLOCK SIZE ON DISK '(&00)'. INITIALIZATION TERMINATED ABNORMALLY

### Meaning

The disk has been formatted with a block size unknown to VOLIN.

### Response

Contact the maintenance staff to format the disk again.

## NVL0055

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0055 UNRECOVERABLE ERROR WHEN TESTING DISK. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0056

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0056 UNRECOVERABLE ERROR WHEN READING IDENTIFIER. INITIALIZATION TERMINATED ABNOMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0057

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0057 UNRECOVERABLE ERROR WHEN FORMATTING A CYLINDER. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0058

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0058 UNRECOVERABLE ERROR WHEN FORMATTING A USER BLOCK IDENTIFIER. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0059

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0059 UNRECOVERABLE ERROR WHEN FORMATTING AN ALTERNATE BLOCK IDENTIFIER. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0060

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0060 UNRECOVERABLE ERROR WHEN FORMATTING A DEFECTIVE BLOCK. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0061

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0061 INVALID DEVICE CHARACTERISTICS ON DISK '(&00)'. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0062

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0062 Volume '(&00)' with '(&01)' HP exceeds maximum volume capacity of 32 GB

### Meaning

BS2000 supports a maximum of 16777215 halfpages (each 2048 bytes) per
volume, i.e. approximately 32 GB.

## NVL0063

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0063 Unit '(&00)' is still cached, formatting in this state is not allowed

### Meaning

Before formatting, the disk has to be removed from cache. Please use PCA.

## NVL0065

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0065 DEVICE REQUESTED IN PARAMETER VALUE 'UNIT=(&00)' IS UNKNOWN

### Meaning

(&00): mnemonic device name (mn).
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0066

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0066 DISK '(&00)', FORMAT '(&01)': ASSIGNED VSN '(&02)' AND FORMAT '(&03)'. FORMATTING OF ASSIGNED DISK PACK REQUIRED BUT LABEL CREATION ONLY IS SPECIFIED

### Meaning

The subsequent message NVL0067 permits to withdraw the specification to
create labels only or to reject the disk pack.

## NVL0067

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0067 OVERWRITE STANDARD DISK '(&00)', USING THE STANDARD PARAMETER FOR FORMATTING? REPLY (Y=YES; N=NO)

### Meaning

The disk pack assigned is a standard BS2000 disk.
For the initialization of a BS2000 disk with given format, the disk pack
has to be formatted.
If desired, the specification to create labels only is ignored, and the
disk pack is formatted using the standard values of the formatting
parameters.

### Response

Y: the disk pack is overwritten and formatted in accordance with the
message
N: the state of the disk pack remains unchanged.
A new mount message follows for mounting another disk pack.

## NVL0068

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0068 VOLIN: '(&00)' SYSTEM ERROR. PROGRAM RUN ABORTED

### Response

If this message recurs again, send the error documentation to
diagnosis department.

## NVL0070

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0070 WARNING: EXCESSIVE DATA CHECKS OCCURRING FOR TRACK '(&00)' ON DISK '(&01)'. CONTACT MAINTENANCE

### Meaning

During the skip displacement processing for the specified track the
number of the data checks exceeded the device type specified threshold.
The surface checking and the formatting continues.

### Response

Although this is intended as a warning, the maintenance staff
should be called, especially if this message is issued for multiple
tracks.

## NVL0071

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0071 UNRECOVERABLE I/O ERROR DURING ANALYSIS OF TRACK '(&00)' ON DISK '(&01)'. VOLIN RUN ABORTED

## NVL0072

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0072 WARNING: DEFECTIVE DIAGNOSTIC TRACK '(&00)' ON DISK '(&01)'

### Meaning

This information is for the maintenance staff only.
Because of a surface error the specified track of the diagnostic area has
been flagged as defective.
The correct format of the user tracks established before is not affected.

## NVL0073

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0073 FUNCTION 'SKIP DISPLACEMENT' APPLIED TO '(&00)' TRACKS

### Meaning

The given number of tracks have been checked and corrected by the aid of
the function 'skip displacement' or an attempt has been made to correct
them before the need of an 'alternate track assignment' turned out.

## NVL0074

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0074 HOME ADDRESS OR R0 COUNT FIELD OF TRACK '(&00)' DEFECTIVE, DISK '(&01)' USELESS

### Meaning

The track analysis detected an unrecoverable error in the home address or
in the count field of record 0 (R0) of the specified track. The formatting
of the disk is not possible.

## NVL0075

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0075 ATTACHED DEVICE TYPE DOES NOT MATCH REQUESTED DEVICE TYPE

### Meaning

The disk type specified in parameter 'DEVICE' (ISP syntax only) or
determined by UNIT input (that is the generated type) does not match the
type of the attached device. Capacity of the attached device is lower
than that of the expected one.
Initialization will be terminated abnormally.

### Response

Restart VOLIN after correction of UGEN parameter.

## NVL0076

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0076 CAPACITY OF ATTACHED DEVICE GREATER THAN THAT OF THE REQUESTED DEVICE. REPLY (C=CONTINUE; T=TERMINATE)

### Meaning

The disk type specified in parameter 'DEVICE' (ISP syntax only) or
determined by UNIT input (that is the generated type) does not match the
type of the attached device. Capacity of the attached device is greater
than that of the expected one.

### Response

C: Continue, format and initialize disk
T: Terminate initialization abnormally.

## NVL0077

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0077 FORMATTING COMMAND FOR DISK (&00) (&01) IN PROCESS, PLEASE WAIT

### Meaning

For FBA disks, before writing the check pattern, a single formatting
command will be executed. This process may take some time, the duration
depends on disk type and number of parallel VOLIN processes. The end of
this process is shown by the message NVL0078.
&00 = VSN
&01 = Drive A or B when formatting a Dual Pair (RAID1 on 3421), or '_'

## NVL0078

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0078 FORMATTING COMMAND FOR DISK (&00) (&01) COMPLETED, CHECK OF VOLUME STARTS.

### Meaning

For FBA disks, before writing the check pattern, a single formatting
command will be executed. The formatting command is now completed. The
writing of the check pattern has been started. The progress will be shown
by message NVL0079.
&00 = VSN
&01 = Drive A or B when formatting a Dual Pair (RAID1 on 3421), or '-'

## NVL0079

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0079 (&00) PER CENT OF DISK (&01) (&02) ARE PROCESSED

### Meaning

The message shows the progress of a formatting process of VOLIN.
&00 = value of per cent in steps of ten
&01 = VSN
&02 = drive A or B when formatting a Dual Pair (RAID1 on 3421), or '-'

## NVL0080

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0080 DALTA ASSIGNED ALTERNATE TRACK '(&00)' TO PRIMARY TRACK '(&01)' ON DISK PACK '(&02)'

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).

## NVL0081

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0081 WARNING: ALTERNATE TRACK AREA ON DISK PACK '(&00)' EXHAUSTED

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).

## NVL0082

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0082 WARNING: MORE THAN 2/3 OF ALTERNATE TRACKS ON DISK PACK '(&00)' ASSIGNED

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).

## NVL0083

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0083 WARNING: DALTA FLAGGED ALTERNATE TRACK '(&00)' ON DISK PACK '(&01)' AS DEFECTIVE

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).

## NVL0084

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0084 WARNING: DALTA CANNOT READ PHYSICAL BLOCK '(&00)' ON DISK PACK '(&01)'. DEFECTIVE TRACK '(&02)' NOT FLAGGED

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).

## NVL0085

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0085 WARNING: DALTA IS PROCESSING TRACK '(&00)' ON DISK PACK '(&01)'. DISK DEVICE '(&02)' NOT OPERABLE AT THIS MOMENT

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).

### Response

Ensure that the disk device is operable.

## NVL0086

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0086 DALTA LOST DEVICE RESERVATION DURING ALTERNATE TRACK ASSIGNMENT. CHECK PHYSICAL BLOCKS '(&00) TO (&01)' ON DISK PACK '(&02)'

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
Updates performed by another system parallel to DALTA in this block range
may be lost.

## NVL0087

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0087 DALTA CANNOT COMPLETE ALTERNATE TRACK ASSIGNMENT. CHECK PHYSICAL BLOCKS '(&00) TO (&01)' ON DISK PACK '(&02)'

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
The access to the specified blocks in this range may have become
impossible.

## NVL0088

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0088 DALTA CANNOT COMPLETE SVL UPDATE ON DISK PACK '(&00)'

### Meaning

A message of the Dynamic Alternate Track Allocater (DALTA).
The contents of the standard volume label (SVL) may have been written back
incompletely.

## NVL0089

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0089 DALTA IS PROCESSING PHYSICAL BLOCK '(&00)' ON DISK PACK '(&01)', DISK DEVICE '(&02)' INOPERABLE

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
For disk devices D3434-30, D34211-3, D34211-4 and D34211-5 this message
indicates the logical block number. The actual physical block number is
shown in the sensebytes (SB3-6).

### Response

Ensure that the disk device is operable.

## NVL0090

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0090 DALTA LOST DEVICE RESERVATION DURING ALTERNATE BLOCK ASSIGNMENT. CHECK PHYSICAL BLOCK '(&00)' ON DISK PACK '(&01)'

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
Updates performed by another system parallel to DALTA on this block
may be lost.
For disk devices D3434-30, D34211-3, D34211-4 and D34211-5 this message
indicates the logical block number. The actual physical block number is
shown in the sensebytes (SB3-6).

## NVL0091

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0091 DALTA REALLOCATED PHYSICAL BLOCK '(&00)' ON DISK PACK '(&01)'

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
For disk devices D3434-30, D34211-3, D34211-4 and D34211-5 this message
indicates the logical block number. The actual physical block number is
shown in the sensebytes (SB3-6).

## NVL0092

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0092 DALTA CANNOT READ PHYSICAL BLOCK '(&00)' ON DISK PACK '(&01)'. PHYSICAL BLOCK NOT REALLOCATED

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
For disk devices D3434-30, D34211-3, D34211-4 and D34211-5 this message
indicates the logical block number. The actual physical block number is
shown in the sensebytes (SB3-6).

## NVL0093

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0093 DALTA CANNOT REALLOCATE PHYSICAL BLOCK '(&00)' ON DISK PACK '(&01)'

### Meaning

A message of the Dynamic Alternate Track Allocator (DALTA).
The access to the specified block may have become impossible.
For disk devices D3434-30, D34211-3, D34211-4 and D34211-5 this message
indicates the logical block number. The actual physical block number is
shown in the sensebytes (SB3-6).

## NVL0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0100 INITIALIZATION OR LOADING OF SUBSYSTEM VOLIN NOT POSSIBLE: ERROR CODE '(&00)'

### Meaning

Return code description:
X'0041FFFF': error during the subsystem connection.
Reasons: - see detailed console messages.
- simultaneous loading of VOLIN subsystem (SS).
In this case wait and retry.

### Response

Check the DSSM context (DSSM: Dynamical SubSystem Management).

## NVL0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0101 LOADING OF SUBSYSTEM VOLIN VIA COMMAND NOT POSSIBLE

### Meaning

The subsystem will be loaded in program VOLIN.

## NVL0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0102 VERSIONS OF TU PROGRAM PART AND SUBSYSTEM VOLIN INCONSISTENT. VOLIN RUN ABORTED

### Meaning

The version of the interface parameter list does not agree with this one
required by the subsystem.

### Response

Check DSSM context (DSSM: Dynamical SubSystem Management).

## NVL0103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0103 ADDRESS OF INTERFACE PARAMETER LIST CHANGED. VOLIN RUN ABORTED

### Meaning

The address of the interface parameter list has been changed after the
initialization of the subsystem.
This is not allowed.

### Response

Send the error documentation to diagnosis department.

## NVL0104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0104 SPECIFIED VALUE OF PARAMETER 'FORMAT' DOES NOT AGREE WITH PHYSICAL DISK STRUCTURE OF '(&00)'. INITIALIZATION TERMINATED ABNORMALLY

## NVL0108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0108 SPECIFICATION OF DEFECT AREAS ARE IGNORED DUE TO FORMAT CHANGE

### Meaning

The physical disk format should be changed.
In this case specification of DEFECT areas cannot be checked.
It is ignored.

## NVL0109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0109 PRIVATE DISKS ARE ONLY PERMITTED FOR AN ALLOCATION UNIT OF 6 K

### Meaning

If no allocation unit was given explicitely, the allocation unit given
implicitely by a format statement is not permitted.

## NVL0110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0110 DISK CAPACITY TOO SMALL FOR DISK ADMINISTRATION DATA. DISK HAS TO BE FORMATTED

### Meaning

The capacity is too small for disk administration data
(IPL, SVL and format 5 labels).

### Response

The disk has to be formatted.

## NVL0111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0111 UTILITY ROUTINE '(&00)' VERSION (&01) READY FOR INPUT

## NVL0119

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0119 TRACK REPAIR FOR DUALCOPY DISK '(&00)' IN STATE 'IN-HOLD' IS REQUIRED

## NVL0120

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0120 START REPAIR FOR VSN '(&00)', UNIT '(&01)', DEVICE TYPE '(&02)' ? REPLY (Y=YES; N=NO)

### Meaning

One/several track(s) or sector(s) should be repaired. Check the assignment
before action will be started.

### Response

Y: The repair will be started.
N: The action will be skipped.

## NVL0121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0121 REPAIR FOR VSN '(&00)' IS REQUIRED BUT PARAMETER 'DEFECTS' IS NOT DEFINED.

### Meaning

One/several track(s) or sector(s) should be repaired, but track or sector
address is not defined.

## NVL0122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0122 REPAIR IS NOT SUPPORTED FOR DEVICE TYPE '(&00)'.

### Meaning

The device type assigned is not in the list of device types supported
by the VOLIN repair function.

## NVL0123

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0123 DUALCOPY DISK '(&00)' IS 'IN-HOLD', BUT PARAMETER 'DUALCOPY=NO', START TRACK REPAIR ? REPLY (Y=YES; N=NO)

### Meaning

One/more track(s) should be repaired. The SECONDARY disk of the DualCopy
pair is in state 'IN-HOLD', but the parameter 'DUALCOPY' is 'NO' or not
specified. Repair of the SECONDARY starts, if the request is not rejected.

### Response

Y: The track repair will be started.
N: The action will be terminated.

## NVL0124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0124 WARNING: TRACK REPAIR FOR VSN '(&00)', TRACK '(&01)', BLOCK '(&02)', BLOCK CONTENT IS LOST !

### Meaning

The track repair function cannot read the physical record (PAM block)
with the given PHP (physical halfpage) number. The content of the record
is lost, it will be filled up with binary zeros. The file containing
the lost record should be restored from the last back-up.

## NVL0125

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0125 REPAIR CAN BE USED IN BS2000 ONLY

### Meaning

The repair function can only be used under BS2000 (also from SIR), but not
under IPL-EXEC (first installation).

## NVL0126

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0126 TRACK REPAIR FOR VSN '(&00)', TRACK '(&01)' IS TERMINATED

### Meaning

The given track is repaired successfully if no error message (NVL0124
or NVL0131) occurred previously for this track.

## NVL0127

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0127 TRACK REPAIR FOR DUALCOPY DISK '(&00)' IS REQUIRED, BUT STATE IS NOT 'IN-HOLD'

### Meaning

One/more tracks(s) should be repaired, but the disk is not in DualCopy
state 'IN-HOLD', but either in state 'IN-COPY' or in state 'ACTIVE'.

## NVL0128

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0128 REPAIR FOR OTHER THAN PRIMARY TRACK '(&00)' IMPOSSIBLE

### Meaning

Only primary tracks - not alternates or CE tracks - can be repaired.

## NVL0129

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0129 FORMATTING OF DUALCOPY DISK '(&00)' IN STATE 'IN-HOLD', 'ACTIVE' OR 'IN-COPY' IS NOT POSSIBLE

### Meaning

A DualCopy disk can be formatted in 'DEACTIVATED' state only.

## NVL0130

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0130 INITIALIZATION OR FORMATTING OF DUALCOPY DISK '(&00)' IN STATE 'IN-HOLD' OR 'IN-COPY' IS NOT POSSIBLE

### Meaning

A DualCopy disk can be formatted in 'DEACTIVATED' state only and
initialized in 'DEACTIVATED' or 'ACTIVE' state only.

## NVL0131

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0131 WARNING: TRACK REPAIR FOR VSN '(&00)', TRACK '(&01)', BLOCK '(&02)' TO BLOCK '(&03)', TRACK CONTENT IS LOST !

### Meaning

During the track repair function the content of the track was lost.
The track data are undefined. The PHP (physical halfpage) numbers of
the records on the track are notified.

## NVL0132

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0132 REPAIR FOR FBA DISK OF A RAID1 PAIR IMPOSSIBLE

### Meaning

VOLIN isn't able to repair a single sector on an FBA disk which is part of
a RAID1 pair, since the device can't be determined definitely.

## NVL0133

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0133 WARNING: SECTOR '(&00)' OF VOLUME '(&01)' CAN'T BE READ. CONTENTS OF BLOCK '(&02)' LOST

### Meaning

When preserving a record before reassigning a sector of an FBA disk
an error occurred.
&00 = phys. RBN, decimal
&01 = VSN
&02 = PHP#, decimal

### Response

The file concerned (see PHP#) has to be restored from last backup after
reassignment has been completed correctly.

## NVL0134

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0134 SECTOR '(&00)' ON VOLUME '(&01)' CAN'T BE REASSIGNED, BLOCK '(&02)' REMAINS DEFECTIVE

### Meaning

During reassigning a sector of an FBA disk an error occurred.
&00 = phys. RBN, decimal
&01 = VSN
&02 = PHP#, decimal

### Response

The file concerned must be erased by /DELETE-FILE ...,OPTION=DESTROY
and has to be restored from last backup (implicitly to another place).

## NVL0135

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0135 SECTOR '(&00)' OF VOLUME '(&01)' CAN'T BE WRITTEN AFTER REASSIGNMENT, BLOCK '(&02)' REMAINS DEFECTIVE

### Meaning

During restoring data into a sector of an FBA disk previously reassigned
an error occurred.
&00 = phys. RBN, decimal
&01 = VSN
&02 = PHP#, decimal

### Response

The file concerned must be erased by /DELETE-FILE ...,OPTION=DESTROY
and has to be restored from last backup (implicitly to another place).

## NVL0136

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0136 SECTOR '(&00)', BLOCK '(&01)' OF VOLUME '(&02)' REPAIRED

### Meaning

In order to skip a defective sector of an FBA disk an alternate sector has
been assigned and written without errors.
&00 = phys. RBN, decimal
&01 = PHP#, decimal
&02 = VSN

### Response

If the contents of the original sector couldn't be saved before the
reassignment (NVL0133) the file concerned (see PHP#) has to be restored
from last backup.

## NVL0138

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0138 Track '(&01)' on disk '(&00)' defective. No alternate track assigned, because option is set to suppress alternate track / block assignement

## NVL0139

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0139 Sector '(&01)' on disk '(&00)' defective. No alternate block assigned, because option is set to suppress alternate track / block assignement

### Meaning

(&00) = VSN
(&01) = Phys. block offset on volume (phys. RBN, not PHP!)

## NVL0140

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0140 INITIALIZATION FOR A GS-VOLUME '(&00)' REJECTED, BECAUSE OF SUBSYSTEM GSVOL BEING NOT AVAILABLE (RC='(&01)' AT CALL OF INTERFACE '(&02)')

### Meaning

To initialize a GS-VOLUME, VOLIN needs the subsystem GSVOL.
&00 = VSN
Meaning of RC (Subcode1):
41 = Subsystem not loaded
42 = Subsystem not connected

### Response

Examine the state of subsystem GSVOL, if necessary load subsystem by
START-SUBSYSTEM GSVOL (RC=41).

## NVL0141

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0141 FORMATTING NOT APPLICABLE TO GS-VOLUMES. VOLIN CONTINUES WITH GENERATION OF LABELS FOR GS-VOLUME '(&00)'

### Meaning

The format of a GS-Volume is fixed by the command CREATE-GS-VOLUME, the
physical formatting is not possible. The physical deleting is also done
by CREATE-GS-VOLUME automatically. VOLIN only generates BS2000-Labels for
the GS-VOLUME.
&00 = VSN

## NVL0144

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0144 FORMAT '(&00)' FOR GS-VOLUME '(&01)' DOES NOT AGREE WITH THE FORMAT '(&02)' FIXED BY CREATE-GS-VOLUME. FORMAT CHANGE NOT POSSIBLE. VOLIN IS TERMINATED

### Meaning

The format of a GS-Volume is fixed by the command CREATE-GS-VOLUME. It
can't be changed by the VOLIN instruction FORMAT. The VOLIN instruction
FORMAT is only used to set the Allocation Unit.
&01 = VSN
This message is issued if VOLIN is called by SIR. VOLIN is terminated.

## NVL0145

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0145 FORMAT '(&00)' FOR GS-VOLUME '(&01)' DOES NOT AGREE WITH THE FORMAT '(&02)' FIXED BY CREATE-GS-VOLUME. FORMAT CHANGE NOT POSSIBLE. REPLY (C=CONTINUE; T=TERMINATE)

### Meaning

The format of a GS-Volume is fixed by the command CREATE-GS-VOLUME. It
can't be changed by the VOLIN instruction FORMAT. The VOLIN instruction
FORMAT is only used to set the Allocation Unit.
&01 = VSN
This message is issued, if VOLIN operates as independent program (not
under SIR).

### Response

C: Continue initialization with format fixed by CREATE-GS-VOLUME and with
default value for allocation unit.
T: Terminate initialization.

## NVL0146

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0146 DISK CAPACITY GREATER EQUAL 32GB IS NOT PERMITTED FOR PRIVATE DISKS

## NVL0147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0147 A REQUEST THAT EXCEEDS THE REAL CAPACITY OF THE ATTACHED DEVICE WILL BE IGNORED.

### Meaning

A DEVICE CAN BE FORMATED ONLY WITH ITS REAL MAXIMUM CAPACITY.

## NVL0148

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0148 (&00) SESSION FOR DEVICE (&01) TERMINATED

### Meaning

SNAP/CLONE session for device (&01) terminated by VOLIN.

## NVL0149

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0149 TERMINATION OF (&00) SESSION FOR DEVICE (&01) FAILED

### Meaning

Termination of SNAP/CLONE session for device (&01) by VOLIN failed.

## NVL0150

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0150 INITIALIZATION OF (&00) DEVICE (&01) NOT ALLOWED

### Meaning

SNAP/CLONE device (&01) may not be overwritten by VOLIN.

## NVL0151

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0151 TERMINATE (&00) SESSION FOR DEVICE (&01) ? REPLY (Y=YES; N=NO; C=CANCEL)

### Meaning

SNAP/CLONE session for device (&01) active.

### Response

Y: Terminate SNAP/CLONE session and
continue volume initialization.
N: Continue volume initialization without
termination of SNAP/CLONE session.
C: Cancel volume initialization.

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages