## SEZREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SEZREVI COMP=SEZMF,VERS=91A,DATE=200212

## SEZ0006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0006 INTERNAL SYSTEM ERROR

### Meaning

Internal program error.

### Response

If the program does not terminate with a dump, initiate a dump and send
an error report for system diagnosis.

## SEZ0007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0007 BLOCK NUMBER DOES NOT EXIST

### Meaning

Internal program error.

### Response

If the program does not terminate with a dump, initiate a dump and send
an error report for system diagnosis.

## SEZ0008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0008 INVALID BLOCK HEADER

### Meaning

Internal program error.

### Response

If the program does not terminate with a dump, initiate a dump and send
an error report for system diagnosis.

## SEZ0010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0010 MAXIMUM NUMBER OF DATABASES ALREADY REACHED

### Meaning

No open is performed for this database.

### Response

Release all free databases using RELEASE-USER-RESOURCES and reopen
rejected data base.

## SEZ0020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0020 DMS ERROR '(&01)' DURING PROCESSING OF THE FILE '(&00)'. ISSUE /HELP-MSG DMS(&01) IN SYSTEM MODE

### Meaning

The file (&00) can no longer be processed. Enter /HELP-MSG in system mode
or refer to the BS2000 'System Messages' manual for further information
on the DMS error code.

### Response

Submit the error documentation and an error report for system diagnosis.

## SEZ0024

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0024 FILE: (&00) BLOCK NUMBER: (&01)

### Meaning

Output of file and block number, if block head error was detected.

## SEZ0025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0025 FILE '(&00)' CATALOGUED UNDER MORE THAN ONE BS2000 CATALOG ID OR THE CATALOG ID IS NOT IN THE SESAM CATID LIST

### Meaning

The file may only be catalogued under one catalog ID. SESAM files may not
differ in just the catalog ID. If a catid list is assigned, a file can
only be created with a catalog ID of this list.

### Response

Change the file name or delete at least one of the files. Change the
catalog ID list.

## SEZ0030

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0030 FILE '(&00)' OPENED

### Meaning

The fact that the file was opened is logged.

## SEZ0031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0031 FILE '(&00)' CLOSED

### Meaning

The fact that the file was closed is logged.

## SEZ0032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0032 FILE '(&00)' EMPTY

### Meaning

(&00) is empty, so it cannot be read-accessed.

### Response

This message does not require a response. Any measures necessary are
taken in response to subsequent messages.

## SEZ0033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0033 FILE '(&00)' CANNOT BE CREATED ON MEDIA SPECIFIED IN MEDIA TABLE

### Meaning

Because of an error or lack of space, the file (&00) cannot be created
on any of the media defined in the media table for this file type.
DEVICE REQUEST is defined in the media table for this file type. You are
therefore requested by the console to enter a medium.

### Response

Respond to the input request that follows.

## SEZ0034

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0034 PLEASE ENTER NEW MEDIUM FOR FILE (&00). RESPONSE (PUBLIC [<CATID>]; PRIVATE [<CATID>],<DEVICE-TYPE>,<VSN>[,<VSN>,.. ]; IGNORE)

### Meaning

A device must be entered on which the file (&00) is to be created.
PUBLIC [catid]: The file is to be created on pubset [with specified
catid].
PRIVATE [catid],device-type,<vsn>[,<vsn>,... ]: The file is to be created
on private disks [with the specified catid] with the specified VSNs
and device-type. At most six vsns could be specified.
IGNORE: The file will not be created (file type CATREC, PBI and DDLTA)
or an attempt is made to create the file with the next sequence number
on the same medium (file type DALOG and CATLOG).

### Response

Respond to the request. The DBH is halted until a response is entered.
If IGNORE is entered for the file type CATREC, PBI or DDLTA, the statement
which caused the request is rejected. If IGNORE is entered for the file
type DALOG or CATLOG, an attempt is made to create the file with the next
sequence number on the existing medium. This can be successful if space
has been created on the medium. After three unsuccessful attempts, the
database is locked for further changes.

## SEZ0035

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0035 INVALID ENTRY. REPLY (PUBLIC [<CATID>]; PRIVATE [<CATID>],<DEVICE-TYPE>, <VSN>[,<VSN>,.. ]; IGNORE)

### Meaning

The reply was invalid.
Possible causes:
- Syntax error
- The specified PVS is inaccessible either generally or for this user ID.
- The specified volume type is not known in the system.

### Response

Enter correct reply.

## SEZ0036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0036 FASTPAM ERROR '(&01)' WHILE PROCESSING THE FILE (&00). ENTER: /HELP-MSG DFP(&01) IN SYSTEM MODE

### Meaning

An error (&01) occurred while processing the file (&00). Enter /HELP-MSG
in system mode or refer to the BS2000 'System Messages' manual for
further information on the FASTPAM error code.

### Response

If the current function has been aborted with a dump, submit the error
documentation and an error report for diagnosis.

## SEZ0037

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0037 FASTPAM RETURNS '(&00)' WITH SUBCODE '(&01)'. IN SYSTEM MODE: /HELP-MSG DFP(&00)

### Meaning

FASTPAM returns (&00) for ENABLE or DISABLE. Enter /HELP-MSG in system
mode or refer to the BS2000 manual 'System Messages' for further
information on the FASTPAM error code. If the error occurs on ENABLE,
SESAM switches to UPAM.

### Response

Correct the cause of the error. If a system error appears to the cause,
submit the error documentation and error message to the system diagnosis
department.

## SEZ0038

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEZ0038 SESAM CONTINUES WITH UPAM

### Meaning

FASTPAM has returned an error. SESAM continues with UPAM.

### Response

Correct the error shown in the previous message.

## SEZ0039

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEZ0039 SESAM CONTINUES WITH FASTPAM IN TEST MODE

### Meaning

A FASTPAM authorization is missing; see previous message.
SESAM operates with FASTPAM in test mode.

### Response

Correct the error shown in the previous message.

## SEZ0040

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEZ0040 THE OPTIONS REQUIRED (&00) FPAMACCS. TOO MUCH FOR FASTPAM WITHOUT RESIDENT AREAS

### Meaning

The FASTPAM authorization is missing.
Not even the use of FASTPAM without resident areas is possible because
the number of FPAMACCs required for the options is higher than 500.

### Response

Change the options and apply for FASTPAM authorization or use UPAM.

## SEZ0041

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEZ0041 THE OPTIONS REQUIRED (&00) FPAMACCS. TOO MUCH FOR FASTPAM

### Meaning

The number of FPAMACCs required for the options is higher than 5000.

### Response

Change the options or use UPAM.

## SEZ0042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEZ0042 SESAM USES THE FASTPAM ACCESS METHOD WITH RESIDENT AREAS

### Meaning

SESAM/SQL uses the FASTPAM access mode for all files except for the
database files that are stored on shared or protected private disks
(SPD or PPD).
The minimum requirement for the number of resident pages (specified in
the START command for the DBH start via parameter RESIDENT-PAGES) could
be satisfied.

## SEZ0101

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0101 ERROR DURING INITIALIZATION OF THE MODULE TABLE

### Meaning

Internal program error.

### Response

Submit error message with dump to system diagnosis department.

## SEZ0102

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0102 ERROR WHILE ENTERING MODULE '(&00)' IN THE MODULE TABLE

### Meaning

Internal program error.

### Response

Submit error message with dump to system diagnosis department.

## SEZ0103

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0103 ERROR WHILE RELOADING MODULE '(&00)', BIND RETURNCODE: '(&01)'

### Meaning

Possible causes of error:
a) Unable to find module (&00) in the SESAM module library.
b) Module (&00) has the wrong correction or version status.

## SEZ0104

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0104 SYMBOL '(&00)' NOT FOUND, BIND RETURNCODE: '(&01)'

### Meaning

Internal program error.

### Response

Submit error message with dump to system diagnosis department.

## SEZ0105

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0105 WRONG ILCS VERSION

### Meaning

Possible causes of error:
Wrong CRTE library assigned.

### Response

Check the CRTE library assignment. If this error message persists,
submit it with dump to the system diagnosis department.

## SEZ0106

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0106 OUT OF MEMORY FOR INITIALIZATION OF THE ILCS

### Meaning

Possible causes of error:
The public space limit of the user ID is too small.

### Response

Check the user attributes or public space limit and increase if necessary.

## SEZ0107

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0107 INTERNAL ERROR DURING INITIALIZATION OF THE ILCS

### Meaning

Internal program error.

### Response

Submit error message with dump to system diagnosis department.

## SEZ0108

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0108 UNEXPECTED RETURN VALUE DURING INTIALIZATION OF THE ILCS

### Meaning

Internal program error.

### Response

Submit error message with dump to system diagnosis department.

## SEZ0109

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0109 THE USED SESAM MODULE LIBRARY DOES NOT SUPPORT THIS HARDWARE.

### Meaning

The release item SYSLNK.SESAM-SQL.xxx does not support SX hardware.

### Response

Assign SESAM module library SPULNK.SESAM-SQL.xxx and start the
program again.

## SEZ0110

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ0110 PROGRAM LIBRARY CANNOT BE IDENTIFIED.

### Meaning

The program library the program is started from cannot be identified.

## SEZ1001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1001 READ/WRITE ERROR OCCURRED FOR FILE '(&00)'. DMS ERROR: '(&01)'. ISSUE /HELP-MSG DMS(&01) IN SYSTEM MODE

### Meaning

Read or write error (possibly hardware error). Enter /HELP-MSG in system
mode or refer to the BS2000 'System Messages' manual for further
information on the DMS error code.

### Response

Correct the DMS error and repeat the statement.

## SEZ1002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1002 DMS ERROR '(&01)' ON OPENING THE FILE '(&00)'. ISSUE /HELP-MSG DMS(&01) IN SYSTEM MODE

### Meaning

Error on opening the file. Enter /HELP-MSG in system mode or refer to the
BS2000 'System Messages' manual for further information on the DMS error
code.

### Response

Correct the DMS error and repeat the statement.

## SEZ1003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1003 DMS ERROR '(&01)' WHEN CLOSING FILE '(&00)' OR DURING TAPE SWAPPING. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or refer to the BS2000 'System Messages' manual.

### Response

The program is terminated, restart session.

## SEZ1004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1004 FILE ACCESS WITHOUT PREVIOUS OPEN

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1005 INTERNAL PROGRAM ERROR. MAXIMUM NUMBER OF FILES EXCEEDED

### Response

In the case of program termination without TERMD, create a dump, send
error message.

## SEZ1006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1006 READ OPERATION ON OUTPUT FILE '(&00)'

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1007 WRITE OPERATION ON INPUT FILE '(&00)'

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1008 SECOND OPEN ON FILE '(&00)' WITHOUT PREVIOUS CLOSE

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1009 WAIT OPERATION ON FILE '(&00)' WITHOUT A PREVIOUS READ OPERATION

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1010 WAIT OPERATION ON FILE '(&00)' WITHOUT A PREVIOUS WRITE OPERATION

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1011 INPUT ERROR: INVALID OP-CODE

### Meaning

An invalid operation code was specified in the parameter.

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ1012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1012 DB NAME IN THE ASSIGNED FILE DOES NOT MATCH THE ONE IN THE REQUESTED FILE

## SEZ1013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1013 FILE '(&00)' CATALOGUED ON SEVERAL PVS'S

### Response

Ensure that the file name is unique across all public volume sets.

## SEZ1014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1014 FILE '(&00)' NOT AVAILABLE. DMS ERROR '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or refer to the BS2000 'System Messages' manual.

### Response

Catalog file, repeat session.

## SEZ1015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1015 GENERAL INPUT ERROR: ADDRESS OF I/O AREA INVALID

### Response

In the case of a program termination without TERMD, create and send dump.

## SEZ1016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1016 INPUT ERROR: BLOCK LENGTH/NUMBER OF BLOCKS INVALID

### Response

In the case of a program termination without TERMD, create and send dump.

## SEZ1017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1017 FILE '(&00)' HAS NOT BEEN CREATED IN THE CURRENT VERSION OR ILLEGAL

### Meaning

The program is aborted.

### Response

Allocate correct file from current version, repeat session.

## SEZ1018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1018 GENERAL INPUT ERROR

### Meaning

Invalid input parameter.

### Response

Program is terminated, repeat session.

## SEZ1019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1019 SESAM FILE NAME '(&00)', LINK NAME '(&01)'

### Meaning

An open was executed on the SESAM file.

## SEZ1020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1020 USER FILE NAME '(&00)'

### Meaning

An open was executed on the user file name.

## SEZ1021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1021 A READ/WRITE ERROR OCCURRED IN FILE '(&00)'

## SEZ1022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1022 DMS ERROR CODE '(&01)' FOR FILE '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

A DMS error occurred in system macros. For more detailed information about
the DMS error code enter /HELP-MSG in system mode or refer to the BS2000
manual 'System Messages'.

### Response

Program is terminated. Repeat session.

## SEZ1023

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1023 INVALID FILE ALLOCATION. LINK NAME: (&00)

### Meaning

Program is terminated.

### Response

Allocate correct file. Repeat session.

## SEZ1024

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1024 REQUESTED: SESAM FILE NAME: (&00)

## SEZ1025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1025 ............USER FILE NAME: (&00)

## SEZ1026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1026 ALLOCATED: SESAM FILE NAME: (&00)

## SEZ1027

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1027 .............USER FILE NAME: (&00)

## SEZ1028

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1028 INVALID DEVICE TYPE ASSIGNED FOR DA-LOG FILE

### Meaning

'Magnetic tape cartridge' was assigned as device type for the DA-LOG file.

### Response

Assign disk or tape for DA-LOG file.

## SEZ1029

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1029 DMS ERROR '(&01)' OCCURRED BY 'RELEASE'. LINKNAME: '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

RELEASE invalid executed For more detailed information about the DMS
error code enter /HELP-MSG in system mode or refer to the BS2000
'System Messages' manual.

## SEZ1030

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1030 DMS ERROR '0927' WHEN WRITING FILE '(&00)' (PAM-EVENTING-ERROR). IN SYSTEM MODE /HELP-MSG DMS0927

### Meaning

An error occurred in PAM eventing when writing the DA-LOG file. The reason
for the error has been entered in the event control block. For more
detailed information about the DMS error code enter /HELP-MSG in system
mode or refer to the BS2000 'System Messages' manual.

## SEZ1031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1031 CONTINUATIONFILE '(&00)' WILL BE OPENED

### Meaning

In a configurationfile the continuationfile (&00) was defined.
Therefore the continuationfile will be opened.

## SEZ1032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1032 FILE '(&00)' NOT FOUND

### Meaning

The continuationfile (&00) should be opened. The file could not be found.

### Response

Create the file by BS2000 file command.

## SEZ1033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1033 DUPLICATE OF CATID '(&00)' IS IGNORED.

### Meaning

A catid is defined repeatedly in the catid file. Duplicates are
ignored.

### Response

Correct the catid file before you start the program again.
If the current program is a SESAM DBH, you can reassign another or the
corrected catid file already in the current DBH session using the
administration statement MODIFY-CATID-LIST.

## SEZ1034

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1034 DEFAULT CATID '(&00)' OF THE CURRENT USER ID IS MISSING IN CATID FILE.

### Meaning

The default catid of the current user ID must be contained in the catid
list. Since it was not defined in the catid file, it was implicitly
transferred to the internal catid list.

### Response

Correct the catid file before you start the program again.

## SEZ1035

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1035 CATID '(&00)' WAS NOT TRANSFERRED TO CATID LIST.

### Meaning

A catid must consist of uppercase letters or digits only. Wildcard
symbols are not permitted.

### Response

Correct the catid file before you start the program again.
If the current program is a SESAM DBH, you can reassign another or the
corrected catid file already in the current DBH session using the
administration statement MODIFY-CATID-LIST.

## SEZ1036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1036 FILE (&00) ASSIGNED WITH LINK NAME SESAMCID WAS NOT FOUND.

### Meaning

The specified file was not found, and hence no catid list is operative.

### Response

Check the file name.
If the current program is a SESAM DBH, you can reassign another catid
file already in the current DBH session using the administration
statement MODIFY-CATID-LIST.

## SEZ1037

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1037 FILE (&00) ASSIGNED WITH LINK NAME SESAMCID IS EMPTY.

### Meaning

The specified file is empty, and hence no catid list is operative.

### Response

Check the file and the file name respectively.
If the current program is a SESAM DBH, you can reassign another or the
corrected catid file already in the current DBH session using the
administration statement MODIFY-CATID-LIST.

## SEZ1038

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ1038 FILE (&00) NOT CATALOGUED UNDER ANY CATID. AT LEAST ONE OF THE PUBSETS ADDRESSED IN THE CATID LIST IS NOT ACCESSIBLE. INVOLVED CATID: (&01)

### Meaning

The file is not catalogued under any catid of the catid list. In addition,
at least one of the DMS errors DMS0501, DMS0512 or DMS051B has occurred.
So the reason may be the fact that at least one of the pubsets addressed
in the catid list is temporarily not accessible or that the catid is
simply misspelt.
This is only a matter of warning, since the nonexistence of a file
does not essentially indicate an error.

### Response

- If the existence of the file is required and it belongs to a pubset
that is not accessible at present, ask the system administrator to
make the pubset available.
- If the existence of the file is required and the appropriate catid
is missing in the catid file or is misspelt, correct the catid file
before you start the program again.
If the current program is a SESAM DBH, you can reassign another or the
corrected catid file already in the current DBH session using the
administration statement MODIFY-CATID-LIST.

## SEZ2002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2002 SYNTACTICAL ERROR IN FILE NAME '(&00)'

### Meaning

The specified file name is invalid (CATALOG ID or USER ID too long).

### Response

Correct the file name.

## SEZ2003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2003 SPACE ALLOCATION FOR WORK FILE TOO SMALL; MIN. SPACE = ((&00),(&01))

### Meaning

The work file allocated by means of LINKNAME is too small.

### Response

Reenter /CREATE-FILE command with the necessary SPACE option.

## SEZ2101

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2101 ERROR DURING OPEN OF THE MAIL PARAMETER FILE

### Meaning

An error occured during the open of the mail parameter file.

### Response

Check the file

## SEZ2102

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2102 ERROR DURING READING OF THE MAIL PARAMETER FILE

### Meaning

An error occurred while reading the mail parameter file.

### Response

Check the file

## SEZ2103

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2103 ERROR DURING OPEN OF THE TEMPORARY MAIL FILE

### Meaning

An error occurred during the open of the temporary file used for the
function COLLECT
of the mail functions of SESAM.

### Response

Check the file.
Handle a possible shortage of disc space.

## SEZ2104

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2104 ERROR DURING CLOSE OF THE TEMPORARY MAIL FILE

### Meaning

An error occurred during the close of the temporary file used for the
function COLLECT
of the mail functions of SESAM.
Therefore the file cannot be sent by mail.

### Response

Check the file.

## SEZ2105

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2105 ERROR DURING WRITING THE TEMPORARY MAIL FILE

### Meaning

An error ocurred during writing the temporary mail file used for the
function COLLECT.

### Response

Handle a possible shortage of disc space.

## SEZ2110

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2110 MAIL SERVICE NOT AVAILABLE

### Meaning

nail service is not running

### Response

Check whether the mail service is installed und active.

## SEZ2111

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2111 ERROR DURING SENDING A MAIL.

### Meaning

An error was signalled during sending a mail.

### Response

The mail services stated an error.
It could be an error in the receipient address.

## SEZ2120

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2120 NO MAIL RECIPIENT PROVIDED.

### Meaning

No mail recipient found in the mail parameter file.

### Response

Check the file.

## SEZ2121

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ2121 ONLY THE FIRST 100 MESSAGE NUMBERS USED

### Meaning

More than 100 mail numbers found in the mail parameter file.
Only the first 100 will be used.

### Response

Check the file.

## SEZ3001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3001 FILE ACCESS WITHOUT PREVIOUS OPEN

### Response

In the case of program termination without TERMD, create dump. Send error
message.

## SEZ3002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3002 INPUT ERROR: INVALID OP CODE

### Meaning

An invalid operation code was specified in the operand.

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ3003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3003 SECOND OPEN ISSUED FOR FILE '(&00)' WITHOUT PRIOR CLOSE

### Response

In case of a program termination without TERMD, take dump.

## SEZ3004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3004 INTERNAL PROGRAM ERROR. MAXIMUM NUMBER OF FILES EXCEEDED

### Response

In the case of program termination without TERMD, create a dump, send
error message.

## SEZ3006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3006 RECORD- OR BLOCKSIZE INVALID IN PARAMETER AREA

### Response

Take dump.

## SEZ3007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3007 GENERAL INPUT ERROR

### Response

In the case of a program termination without TERMD, create a dump. Send
error message.

## SEZ3008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3008 OPEN PROCESSED FOR SESAM FILE '(&00)' WITH LINKNAME '(&01)'

## SEZ3009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3009 OPEN PROCESSED FOR USER FILE '(&00)'

## SEZ3010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3010 DMS ERROR '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or refer to the BS2000 'System Messages' manual.

## SEZ3011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3011 FILE NAME '(&00)', LINK NAME '(&01)'

### Meaning

DMS error occurred regarding file.

### Response

Program is terminated, repeat program run.

## SEZ3012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3012 FILE ATTRIBUTES OF FILE '(&00)' DEFINED INCOMPLETELY

### Meaning

The file has not been defined completely in the /FILE command.

### Response

Correct the /FILE command.

## SEZ3013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ3013 FILE '(&00)' CATALOGUED ON SEVERAL PVS'S

### Response

Ensure that the file name is unique across all public volume sets.

## SEZ4000

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4000 'PCB' ALREADY MODIFIED WITH 'CONTXT'

### Meaning

With CONTXT the register and/or the program counter have already been
modified in the actual interrupt state.

## SEZ4001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4001 PROGRAM RUNTIME EXCEEDED AT INSTRUCTION COUNTER '(&00)'

### Meaning

(&00): instruction counter.

### Response

Increase the CPU time available for the program run (Increase CPU-LIMIT
parameter in the ENTER-JOB or START-PROGRAM command or use a job class
with a higher time limit).

## SEZ4002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4002 ERROR. INTERRUPT WEIGHT '(&00)' AT INSTRUCTION COUNTER '(&01)'

### Response

Forward dump for SESAM diagnosis.

## SEZ4003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4003 PROGRAM ERROR. INTERRUPT WEIGHT '(&00)' AT INSTRUCTION COUNTER '(&01)'

### Response

Forward dump for SESAM diagnosis.

## SEZ4004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4004 ADMINISTRATION STATEMENT '(&00)' AT INSTRUCTION COUNTER '(&01)'

## SEZ4005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4005 ADMINISTRATION STATEMENT REJECTED

### Meaning

The administration statement cannot be processed at the moment.

### Response

Try later.

## SEZ4010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4010 ADMINISTRATION STATEMENT: (&00)

## SEZ4600

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEZ4600 PROGRAM '(&00)', VERSION (&01) STARTED; TSN: (&02)

## SEZ4601

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : YES

SEZ4601 PROGRAM '(&00)' TERMINATED NORMALLY

## SEZ4602

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : YES

SEZ4602 PROGRAM '(&00)' TERMINATED WITH ERRORS

### Response

Analyze further error messages and reload program if necessary.

## SEZ4603

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : YES

SEZ4603 PROGRAM '(&00)' TERMINATED WITH WARNING

### Meaning

Program (&00) executed without error. Inconsistencies were, however,
detected during processing.

### Response

Consult the SYSLST log.

## SEZ4611

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4611 THE INPUT RECORD WAS TRUNCATED. READ IN AGAIN? RESPONSE (Y=YES; N=NO)

### Meaning

A previous input was longer than the input buffer provided. The part of
the input which exceeded the end of the input buffer was therefore
truncated.

### Response

- Respond to the message with "Y" and then repeat input in shortened form
or
- Respond to the message with "N". This causes the truncated part of the
record to be ignored. The part of the record which was read in will be
processed by the program.

## SEZ4651

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4651 DIFFERENT SESAM VERSIONS; VERSION OF DYNAMICALLY LOADING LLM: (&00); DYNAMICALLY LOADED LLM (NAME/VERSION): (&01) / (&02)

### Meaning

The dynamically loaded LLM has a different version from the dynamically
loading LLM. The program run is aborted.

### Response

Assign the correct SESAM module library and restart the program.

## SEZ4652

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4652 MODULE (&00) OF VERSION (&01) COULD NOT BE LOADED.

### Meaning

The module (&00) of version (&01) is not in the
SESAM module library.
The program run is aborted.

### Response

Assign the correct SESAM module library and restart the program.

## SEZ4656

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4656 MODULE CONTAINING SESAM MODULE TABLE NOT FOUND IN ANY SEARCHED LIBRARY. LOADING ABORTED

### Response

Inform diagnostics department.

## SEZ4659

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4659 VERSION VALIDITY CHECK: THE DYNAMICALLY LOADED MODULE (&00) IS NOT A SESAM MODULE

## SEZ4700

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4700 SEBSORT CONTROL STATEMENTS MISSING

### Response

Repeat SEBSORT run using complete set of control characters.

## SEZ4701

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4701 INVALID SEBSORT CONTROL STATEMENT

### Response

Correct statement and reload SEBSORT.

## SEZ4702

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4702 FILE NO ZD-UNS FILE OR DATABASE NAME >17 CHARACTERS

### Response

Repeat SEBSORT run with ZD-UNS file or correct the database name.

## SEZ4703

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4703 RECORD OR PRIMARY KEY VALUE LENGTH IS MISSING OR NOT A THREE DIGIT NUMBER

### Meaning

The length entry is mandatory or the length is > 3 digits.

### Response

Repeat session with length entry.

## SEZ4704

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4704 SORT-ERROR. REPEAT SESSION

## SEZ4705

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4705 SEBSORT: INPUT AND OUTPUT

### Meaning

Header line.

## SEZ4706

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ4706 THE FILE TO BE SORTED IS NOT A ZD-UNS FILE

### Response

Repeat SEBSORT run by using correct file.

## SEZ5000

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5000 MEDIA RECORD USED '(&00)'

### Meaning

The specified media catalog will be used during the current SESAM DBH
session.

## SEZ5001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5001 FILE '(&00)' CREATED ON MEDIA RECORD NO. '(&01)'

### Meaning

The file has been created in accordance with the specifications made in
the media record.

## SEZ5005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5005 LAST MEDIA RECORD OF MEDIA CATALOG '(&00)' FOR FILE TYPE '(&01)' REACHED

### Meaning

When creating the current file of file type (&01), the last media record
of the media catalog is used. If a DMS error occurs and no backup device
has been requested as part of termination processing, the SESAM run will
be terminated with 'consistency check AA 80/06'.

### Response

Delete files.

## SEZ5014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5014 DEVICE TYPE UNKOWN

### Meaning

Defined device type not specified in the device table.

### Response

Repeat input with correct device type.

## SEZ5020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5020 DUE TO DMS ERROR '(&01)' FILE '(&00)' IS CREATED ON THE PVS WITH STANDARD CATALOG ID. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

No files can be set up on the PVS refereed to in the last record of the
media catalog ('PVS cat-id'). The catalog ID cannot be accessed under the
current user ID due to DMS error (&01). The file (&00) has therefore been
created on the PVS with the standard catalog ID.

### Response

Access file via standard PVS. Modify media catalog record, or inform the
system administrator if required.

## SEZ5021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5021 CREATED JV '(&00)' CONTAINS: '(&01)'

## SEZ5100

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5100 ERROR '(&00)' DURING JV MACRO CALL FOR JV '(&01)'. IN SYSTEM MODE: /HELP-MSG JVS(&00)

### Meaning

While processing the Job-Variable (&01) JVS returned the unexpected
error code (&00).

### Response

For more detailed information about the JVS error code enter /HELP-MSG
in system mode or refer to the BS2000 'System Messages' manual.

## SEZ5101

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5101 ERROR DURING LINKING THE TEXT-MODULE FOR PROCESSING THE JOB-VARIABLES

### Meaning

The text-module SEZTXT for processing the JVs could not be linked or
the extern references to it were not resolved.

### Response

Make sure that the text-module SEZTXT is in the SESAM-library or
check the /START-PROGRAM command.

## SEZ5102

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5102 JOB-VARIABLE NOT IN THE TEXT-MODULE

### Meaning

The JV to be processed is not in the text-module SEZTXT for processing
the JVs.

### Response

Correct the text-module SEZTXT.

## SEZ5103

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5103 ERROR IN TEXT-MODULE FOR PROCESSING THE JOB-VARIABLES

### Meaning

The text-module SEZTXT for processing the JVs has the wrong format.

### Response

Correct the text-module SEZTXT.

## SEZ5104

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5104 ERROR ON PROCESSING THE INSERTS IN THE JOB-VARIABLE

### Meaning

The inserts in the contents of the Job-Variable are supplied by the
program different as they are described in the text-module SEZTXT.

### Response

Correct the text-module SEZTXT.

## SEZ5105

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ5105 ERROR ON PROCESSING THE SUFFIX OF THE JV-NAME

### Meaning

The suffix of the JV-Name supplied by the program
is different from the one described in the text module SEZTXT.

### Response

Correct the text module SEZTXT.

## SEZ8001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEZ8001 DUMP WAS CREATED

### Meaning

A dump of this task was created

### Response

-

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages