## NBR0001

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0001 /CANCEL-RUN-PROCESS: SPECIFIED RUN ID NOT FOUND

## NBR0002

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0002 USER NOT ALLOWED TO CANCEL THE SPECIFIED /RUN SEQUENCE. /CANCEL-RUN-PROCESS REJECTED

### Meaning

If the system parameter NBCONOPI is set to 'Y', a /RUN command sequence
may only be cancelled, if the issuer of the /CANCEL-RUN-PROCESS has the
privilege TSOS or the same operator Id. as the issuer of the /RUN comma
nd

## NBR0007

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 00

Warranty : NO

NBR0007 SYSTEM ERROR IN MODULE NBRSMSG

### Meaning

Task anchor function failed. Command cannot be processed

## NBR0008

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR0008 MACRO CALL FAILED IN MODULE NBATOP

## NBR0031

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0031 NO MESSAGE OUTSTANDING ON THE CONSOLE

### Meaning

Reply to a /SHOW-PENDING-MSG command.

## NBR0032

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0032 NO MESSAGE OUTSTANDING ON ANY CONSOLE

### Meaning

Reply to a /SHOW-PENDING-MSG command.

## NBR0033

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0033 NO MESSAGE MATCHES THE SPECIFIED SELECTION CRITERIA

### Meaning

Response to a /SHOW-PENDING-MSG command.

## NBR0034

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0034 ERROR IN PROCESSING OF COMMAND '/(&00)'; REASON: '(&01)'

### Meaning

(&01): 1 = bourse error
2 = error in $MSG7X
3 = error in $NBSRV
4 = error in $TYPIO
5 = error in $TSNGET
6 = error in $GETMEM

## NBR0086

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0086 THE MESSAGES FROM FOLLOWING USER-ID'S ARE SUBSCRIBED BY THIS CONSOLE:

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION. The list of the subscribed
messages will be output by the message NBR0090.

## NBR0087

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0087 THE MESSAGES FROM FOLLOWING TASKS ARE SUBSCRIBED BY THIS CONSOLE:

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION. The list of the subscribed
messages will be output by the message NBR0090.

## NBR0088

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0088 THE MESSAGES FROM FOLLOWING JOB NAMES ARE SUBSCRIBED BY THIS CONSOLE:

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION. The list of the subscribed
messages will be output by the message NBR0090.

## NBR0089

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0089 THE MESSAGES FROM FOLLOWING CONSOLES ARE SUBSCRIBED BY THIS CONSOLE:

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION. The list of the subscribed
messages will be output by the message NBR0090.

## NBR0090

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0090 (&00) (&01) (&02) (&03) (&04)

### Meaning

This message contains a list of subscribed messages or message groups.

## NBR0091

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0091 SOME MESSAGES SUBSCRIPTIONS IGNORED

### Meaning

Output of the command MODIFY-MSG-SUBSCRIPTION. Some of the specified
messages were already subscribed or unsubscribed.

## NBR0092

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0092 TELESERVICE MESSAGES ALREADY SUBSCRIBED BY CONSOLE '(&00)'

## NBR0093

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0093 THE FOLLOWING MESSAGE KEYS ARE SUBSCRIBED BY THIS CONSOLE:

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION. The list of the subscribed
messages will be output by the message NBR0090.

## NBR0094

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0094 THERE ARE NO SUBSCRIBED MESSAGES FOR THIS CONSOLE

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION.

## NBR0095

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0095 UNSUBSCRIBED MESSAGES WILL NOT BE DELIVERED TO THIS CONSOLE

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION.

## NBR0096

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0096 UNSUBSCRIBED MESSAGES WILL ALSO BE DELIVERED TO THIS CONSOLE

### Meaning

Output of the command SHOW-MSG-SUBSCRIPTION.

## NBR0200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0200 COMMAND NOT YET AVAILABLE

### Meaning

Server of the operator command still unknown or not available.

### Response

Load command server (eventually subsystem) and retry command input.

## NBR0600

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0600 THE LAST MESSAGE RECEIVED BY CONSOLE '(&00)' WAS PRODUCED (&01) MINUTES AGO

### Meaning

(&00): console mnemonic or authorization name.

## NBR0601

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR0601 SOME MESSAGES DISCARDED SINCE THE DESTINATION APPLICATION DID NOT RECEIVE THEM JUST IN TIME

## NBR0602

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0602 MESSAGE JAM ON CONSOLE ((&00))

### Meaning

For 1 minute or more none of the waiting messages could be output on this
physical console.

## NBR0666

Destination: CONSOLE Routing code: * (main console) Weight: 45

Warranty : NO

NBR0666 PLEASE ANSWER CMD REQUESTS (MARKED WITH '&') WITH COLON AND QUESTIONS (MARKED WITH '?') WITH FULL STOP !

## NBR0667

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0667 PLEASE ANSWER EMERGENCY QUESTIONS WITH DUMMY TSN

### Meaning

The dummy TSN is P during startup and else E

## NBR0668

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR0668 EMERGENCY QUESTION DEQUEUED

## NBR0669

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0669 EMERGENCY QUESTIONS MUST BE ANSWERED FROM PHYSICAL CONSOLES

## NBR0701

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0701 ROUTING BOURSE PROBLEM IN 'NBRMAIN'. A SNAP-DUMP WILL BE TAKEN

## NBR0704

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0704 LOGGING BOURSE PROBLEM - SYSTEM CRASH

## NBR0705

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0705 '(&00)' SUBSTITUTE CONSOLE FOR '(&01)'

### Meaning

In reply to /CONSOLE HELP the current substitute console is displayed.

## NBR0706

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0706 TEST OUTPUT FOR CONSOLE '(&00)'

### Meaning

Test output in order to check console (&00). If this message appears on
another console, console (&00) is defective.
(&00): console mnemonic.

## NBR0707

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0707 PROCESSING OF COMMAND '(&00)' FROM RUN SEQUENCE INITIATED

### Meaning

If a command from a RUN sequence is routed for processing to the
relevant operator task by the UCON task, the RUN input originator is
notified accordingly.

## NBR0708

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0708 NOT ALL QUESTIONS DISPLAYED

### Meaning

There exist more open questions than displayed due to limit. Further
questions can be processed after answering some of these questions.

### Response

Enter /STA MSG to display further questions when appropriate.

## NBR0709

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0709 COMMAND CANCEL-RUN-PROCESS SIMULATED BY UCON FOR '(&00)'

## NBR0710

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0710 'SWITCH OFF' OF MAIN CONSOLE NOT PERMITTED

## NBR0711

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0711 CONSOLE '(&00)' SWITCHED OFF

## NBR0712

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0712 CONSOLE '(&00)' SWITCHED ON

## NBR0713

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0713 ALL CONSOLES INOPERABLE

### Meaning

All physical consoles became inoperable. As long as no console is
available, the substitute console routine will produce no messages.

## NBR0714

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0714 CONSOLE '(&00)' GETS ALL ITS FUNCTIONS BACK

## NBR0715

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0715 CONSOLE '(&00)' SWITCHED ON BY SYSTEM

## NBR0717

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0717 APPLICATION '(&00)' REJECTED. REASON: '(&01)'

### Meaning

(&01): 1, syntactical error
2, invalid name
3, authorization name already assigned
4, invalid or missing password
5, permanent BCAM error
6, unauthorized station name, see class 2 option 'NBBAPRIV'
7, processor name not equal to home processor
see class 2 option 'NBBAPRIV'
8, task for password/chipcard check could not be created
9, no free entry in the application table; no connection possible
10, the application has authentified itself with an invalid chipcard
11, internal error during authentification; authentification aborted
12, the application should authentify itself with a chipcard, but
the DCAM version is < V10; an authentification is impossible
13, the application should authentify itself with a chipcard, but
the inputing terminal has no chipcard reader; an
authentification is impossible
14, the application sent a letter that is not part of the
authentification protocol; authentification aborted
15, subsystem for chip card authentification does not exist
16, KVP-protocol error
17, during the application connection a letter could not be sent
or received
18, equivocal Connection Id; repeat connection request
19, unknown operator identification (no JOIN-Entry for this
Op. Id.)
20, User Id. expired
?, other errors

## NBR0718

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0718 INVALID 'NBRCONS' ORDER OR INVALID CONSOLE MNEMONIC IN NBRCONS ORDER. IGNORED ORDER:

### Meaning

Possible reasons:
- the job sent to NBRCONS is incorrect.
- the entered console mnemonic does not exist.
The job cannot be executed.
An error logging entry is written.

## NBR0719

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0719 'NBRCONS' ORDER REJECTED BY KTT BOURSE ROUTINE. REJECTED ORDER:

### Meaning

Possible reasons:
- console mnemonic unknown to console driver task (KTT).
- invalid text length of the output.
The job cannot be executed.
An error logging entry is written.

## NBR0720

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0720 $BTIMEL PARAMETER ERROR

## NBR0721

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR0721 APPLICATION '(&00)' NO LONGER CONNECTED WITH '$CONSOLE'

## NBR0722

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0722 COMMAND '/ASR' REJECTED; 'SUPPRESS' RESTRICTED TO PHYSICAL CONSOLES

## NBR0723

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0723 '(&00)' '(&01)' MESSAGES HAVE BEEN SUPPRESSED

### Meaning

The generation and output of '(&00)' '(&01)' messages has been suppressed
because of possible system overburdening. This became necessary because
the frequency of events leading to such a message exceeded the system
output speed.

## NBR0724

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : YES

NBR0724 '/ASR' FUNCTION 'SUPPRESS' IS NO LONGER SUPPORTED. PLEASE USE COMMAND '/RESET-MSG-BUFFER'

## NBR0725

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0725 THE /BROADCAST COMMAND HAS BEEN INCOMPLETELY PROCESSED; (&00) = (&01) + (&02) + (&03) + (&04) TASKS HAVE NOT RECEIVED THE BROADCAST TEXT

### Meaning

(&01) - Number of tasks which have temporarily suppressed the broadcast
function
(&02) - Number of tasks which are in "hold" (pended indefinitely) or in
"destroy" and cannot receive the broadcast text
(&03) - Number of tasks for whom the activation of the contingency which
sends the broadcast text ran erroneously
(&04) - Number of tasks for whom the broadcast text could not be built,
due to a memory shortage

## NBR0726

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0726 TASK IDENTIFIED BY STATION '(&00)' AND PROCESSOR '(&01)' NOT FOUND. /MESSAGE COMMAND CANNOT BE EXECUTED.

## NBR0727

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0727 PARAMETER ERROR IN $POSTMS MACRO CALL.

### Meaning

The macro $POSTMS was called with a false UNIT, FUNCTION or VERSION
number.

## NBR0739

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0739 COMMAND /(&00) STILL WAITING FOR COMPLETION; INPUT COUNTER = (&01)

### Meaning

After input of the command /SHUTDOWN the command /(&00) is not yet
completed and/or not removed from the administration in UCON. The number
of inputs of the same command is displayed in (&01). This message is
only output in system mode intolerant for diagnostic purpose
- (&00) : full command name
- (&01) : number of inputs

### Response

Check the correct usage of GC $NBSRV in the command server of the
mentioned command

## NBR0740

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0740 COMMAND COMPLETED '(&00)'; (RESULT: SC2=(&01), SC1=(&02), MC=(&03)); DATE: (&04)

### Meaning

The command (&00) is terminated if it executes in an administrable mode.
The result (&01) and (&02) and also the message (&03) is corresponding to
the ISL rules.
ISL: Indirect Standard Procedure Linkage.
(&01)/(&02): subcode2/subcode1, return code
(&03) : main code, message number 7 characters.

## NBR0741

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0741 COMMAND SUCCESS UNCERTAIN '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0742

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0742 COMMAND NOT ALLOWED '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0743

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0743 COMMAND NOT AVAILABLE '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0744

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0744 COMMAND '(&00)' NOT FOUND OR AMBIGUOUS ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0745

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0745 COMMAND ID INVALID : '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0746

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0746 COMMAND CANCELLED '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

### Meaning

The command was cancelled either because of the input of
/CANCEL-RUN-PROCESS, or the disconnection of the input console.

## NBR0747

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR0747 COMMAND ID AMBIGUOUS : '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

### Meaning

This command identifier is already given to another command.

### Response

Type your command with another command identifier or wait until
the identifier is not in use anymore.

## NBR0748

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0748 SYSTEM SHUTDOWN IN PROGRESS. COMMAND IGNORED '(&00)'; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

### Meaning

No further command input from console is possible after /SHUTDOWN END
with exception of /SHOW-PENDING-MSG

## NBR0749

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0749 COMMAND FROM /RUN FILE CANCELLED: '(&00)' ; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0750

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0750 D A T E : '(&00)'

## NBR0751

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0751 REJ1 TEXT NOT RECOGNIZED..... : (&00)

## NBR0752

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR0752 ERROR DURING PROCESSING OF OPS-VARIABLE '(&00)'; (RESULT: SC2=(&01), SC1=(&02), MC=(&03))

## NBR0753

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0753 REJ12 NBMHE/NBMAP ERROR IN PROTOCOL

## NBR0755

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0755 REJ5 DESTINATION NOT FOUND... : (&00)

## NBR0756

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0756 REJ6 NO MATCH FOR REPLY...... : (&00)

## NBR0757

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0757 REJ7 USER NOT ALLOWED TO REPLY: (&00)

## NBR0758

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0758 REJ8 CONSOLE SWITCHED OFF. INPUT IGNORED

## NBR0759

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0759 REJ9 CONSOLE MN INOPERABLE. INPUT IGNORED

## NBR0760

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0760 REJ10 QUESTION IDENTIFICATION ALREADY EXISTING

## NBR0761

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0761 REJ11 MESSAGE CANNOT BE MATCHED TO AN ORDER

## NBR0768

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0768 COMMAND PROCESSING INDUCED. PROCESS TERMINATION WILL NOT BE DISPLAYED

## NBR0779

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR0779 RUN ID '(&00)'. READING OF /RUN COMMAND SEQUENCE COMPLETED

## NBR0780

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR0780 COMMAND '(&00)' FORWARDED

## NBR0781

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR0781 OPERANDS REPLACED WITH: '(&00)'

## NBR0790

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0790 CONSOLE '(&00)' CONNECTED TO SYSTEM APPLICATION '$CONSOLE '

## NBR0791

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

NBR0791 CONSOLE '(&00)' DISCONNECTED FROM SYSTEM APPLICATION '$CONSOLE'

## NBR0792

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0792 QUESTION '(&00)' FROM '(&01)' ANSWERED BY '(&02)'. REPLY: '(&03)'. MSG-ID: '(&04)'

### Meaning

The question asked by (&01) having the serial number (&00) was answered
by (&02). The reply is sent to all authorized applications having
received this question. (&04) was the MSG-ID of the question.

## NBR0793

Destination: CONSOLE Routing code: E Weight: 50

Warranty : NO

NBR0793 ANOTHER /RUN COMMAND ALREADY IN PROCESS. COMMAND SUSPENDED

## NBR0796

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0796 RUN ID '(&00)'. MISSING OR INVALID PASSWORD IN /RUN COMMAND. COMMAND REJECTED

## NBR0797

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR0797 APPLICATION '(&00)' CONNECTED WITH '$CONSOLE', PROCESSOR NAME '(&01)', STATION NAME '(&02)'

## NBR080X

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR080X ERROR DURING OPR PARAMETER SERVICE PROCESSING OF DEFINE-CONSOLE. RESMODE VALUE NOT ALLOWED FOR THIS CONSOLE

## NBR0802

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0802 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'DEFINE-CONSOLE'. CONSOLE (&00) HARDCOPY MODE HCC=Y FOR UNDEFINED HARDCOPY

### Meaning

In OPR-Parameter DEFINE-CONSOLE the operand HCC=Y is made without the
corresponding operand HC=mn

### Response

Add HC=mn in OPR-Parameter DEFINE-CONSOLE

## NBR0804

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0804 INCORRECT SQE FROM ECTYP - SYSTEM TERMINATION

## NBR0805

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0805 MESSAGE COUNTER UNDERFLOW - SYSTEM TERMINATION

## NBR0806

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0806 SQE ACKNOWLEDGEMENT COUNTER UNDERFLOW - SYSTEM TERMINATION

## NBR0807

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0807 $IBCAM PARAMETER ERROR IN UCON - SYSTEM TERMINATION

## NBR0808

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0808 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF '(&00)'. NUMBER OF '(&01)' EXCEEDED

### Meaning

An attempt was made to define more console mnemonics than entered in the
console table.
The number of entries is limited to 24.
The number of MSG IDs is limited to 50.

## NBR0809

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0809 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF '(&00)'. (&01) CONSOLE MNEMONICS NOT DEFINED

### Meaning

(&00): possible commands:
/DEFINE-CONSOLE
/SET-FILTER
(&01): number of console mnemonics

### Response

Change the console mnemonics in the parameter file in accordance with the
console table

## NBR0810

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0810 CLASS 2 OPTION 'MSGDEST' NOT PLAUSIBLE. INPUT IGNORED

### Meaning

The console mnemonic or the application name does not exist. If there are
no meaningful values given for MSGDEST, the default value '<*' will be
assumed. Then console messages without destination will be sent to the
main console (and some other consoles having the authorization code '*')

## NBR0812

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0812 THE COMMAND '(&00)' IS NO LONGER SUPPORTED

## NBR0814

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0814 SNAP DUMP TAKEN DUE TO A SERIOUS $NBSRV ERROR

## NBR0815

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0815 (&00)

### Meaning

This message is used for output of lists by several commands.

## NBR0816

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0816 $NBSRV WITH 'TYPE=BEGIN,BRIDGE=(&00)' INVALID

### Meaning

The function $NBSRV was called with TYPE=BEGIN and an invalid
BRIDGE operand which does not point to a Store Queue Entry (SQE).

## NBR0817

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0817 NBSRV COUNTER PROBLEM IN COMMAND SQE - CRASH

## NBR0818

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0818 ERROR DURING PROCESSING OF COMMAND '/(&00)'. RESTART OF OPERATOR TASK

## NBR0819

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0819 NBSRV REPORTS INVALID COMMAND ENVIRONMENT

## NBR0820

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NBR0820 MAY '(&00)' BECOME MAIN CONSOLE? REPLY (Y=YES; N=NO)

### Response

Y: console (&00) becomes main console
N: console (&00) does not become main console

## NBR0821

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0821 COMMAND '/ASR MAIN' REJECTED BY THE MAIN CONSOLE

## NBR0822

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0822 COMMAND '/ASR' REJECTED; 'MAIN' RESTRICTED TO PHYSICAL CONSOLES

### Meaning

The operator command '/ASR MAIN' must neither be entered from
authorized applications nor from teleservice consoles

## NBR0823

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0823 CONSOLE ALREADY MAIN CONSOLE. COMMAND '/ASR MAIN' IGNORED

## NBR0824

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0824 '/ASR DEST': MESSAGES WITHOUT DESTINATION VALUE OUTPUT TO DEFAULT DESTINATION '(&00)'

## NBR0825

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0825 '/ASR HELP': THIS CONSOLE IS '(&00)'

## NBR0826

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0826 RUN ID '(&00)'. RECORD IN /RUN COMMAND FILE OR LIBRARY-ELEMENT TOO LONG. READING ABORTED

## NBR0827

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0827 RUN ID '(&00)'. RECORD IN /RUN COMMAND FILE NOT RECOGNIZED. READING ABORTED

## NBR0828

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0828 RUN ID '(&00)'. READING OF /RUN COMMAND FILE OR LIBRARY-ELEMENT ABORTED WITH COMMAND '/CANCEL-RUN-PROCESS'. SOME RECORDS IGNORED

## NBR0829

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0829 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'DEFINE-CONSOLE'. CONSOLE '(&00)' NOT OF TYPE SKP

## NBR0830

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0830 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'DEFINE-CONSOLE'. DEVICE WITH MN '(&00)' NOT OF TYPE CONSOLE

## NBR0831

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0831 ERROR DURING OPR PARAMETER SERVICE PROCESSING. NUMBER OF 'APPLICATION NAMES' EXCEEDED - '(&00)' NOT ADDED

## NBR0832

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0832 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'ADD-CMD-ENTRY'. CMD '(&00)' ALREADY EXISTS

### Meaning

To add further SAME-NAME all other declarations must be identically with
original definition

## NBR0833

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0833 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'ADD-CMD-ENTRY'. SAME-NAME '(&00)' ALREADY EXISTS OR TOO LONG

## NBR0834

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0834 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'ADD-CMD-ENTRY'. CMD '(&00)' NOT ADDED

## NBR0835

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0835 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF 'SET-CMD-CODE' CONCERNING CMD '(&00)'

## NBR0836

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0836 MAXIMUM NUMBER OF OPERATOR COMMANDS EXCEEDED. CMD '(&00)' NOT ADDED

### Meaning

The Operator Command Table contains already the maximum number of entries.
It is not possible to insert further commands

### Response

Please check OPR Parameter Service

## NBR0837

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0837 ERROR DURING OPR PARAMETER SERVICE PROCESSING OF '(&00)'. (&01) CONSOLE MNEMONICS NOT DEFINED FOR (&02)

## NBR0838

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR0838 COMMAND (&00) WITHOUT COMMAND SERVER ENTRY ANNOUNCED

## NBR0840

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

NBR0840 THE CURRENT LOGGING FILE NAME IS '(&00)'

## NBR0841

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0841 ERROR AT UCON BOURSE WITH IDENTIFIER: (&00). $NBSSIG/$NBRSIG/$NBCAN PARAMETER LIST: '(&01)'. SERSLOG RECORD WRITTEN

## NBR0842

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0842 DUE TO CONTINGENCY ERROR RECORD '(&00)' NOT LOGGED ON SYSLST. $NCTING PARAMETER LIST: '(&01)'. SERSLOG RECORD WRITTEN

## NBR0843

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0843 DUE TO TIAM ERROR RECORD '(&00)' NOT LOGGED ON SYSOUT. YTIPW PARAMETER LIST: '(&01)'. SERSLOG RECORD WRITTEN

## NBR0844

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0844 ERROR WHEN RELEASING MEMORY OF SQE AT '(&00)'. $RETMEM-/(NBLOCK-) MAIN RETURN CODE: '(&01)'. SERSLOG RECORD WRITTEN

## NBR0845

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0845 SYSTEM FUNCTION DURING PROCESSING IN OPR SUBSYSTEM PROCESSED UNSUCCESSFULLY. ABNORMAL TASK TERMINATION

## NBR0846

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR0846 SERIOUS PARAMETER ERROR IN TYPIO CALL. ABNORMAL TASK TERMINATION

## NBR0847

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0847 ************ CLOG TASK TERMINATION AND RESTART - ONE RECORD MISSING IN THE LOGGING FILE ***********

### Meaning

An abnormal task termination occurred during logging of an SQE. This SQE
has been written into the SERSLOG file.

## NBR0848

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0848 THE TEXT '(&00)' COULDN'T REACH THE QUESTION SENDER BECAUSE OF CONTINGENCY ERROR. $NCTING PARAMETER LIST: '(&01)'

## NBR0851

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0851 ERROR DURING COORDINATION OF MESSAGE AND REPLY - SNAP-DUMP AND ABNORMAL TASK TERMINATION

## NBR0852

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0852 A TASK TRIED TO OUTPUT A COMMAND BOUND TEXT, BUT HAS NO COMMAND ENVIRONMENT

## NBR0857

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0857 AFTER OUTPUT OF EMERGENCY MESSAGE SWITCH BACK TO PAGEABLE STORAGE NOT POSSIBLE

## NBR0858

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0858 Output of emergency question without console table

## NBR0862

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0862 MSG-ID : .. MSG-ID : .. MSG-ID : .. MSG-ID : ..

### Meaning

The message whose message ID (message code) is marked with
* is suppressed for the console where the command has been issued.
+ is suppressed for other consoles or authorized applications.
*+ is suppressed for the console where the command has been issued
and for other consoles or authorized applications.

## NBR0863

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0863 MSG-ID : .. SUPPRESSED ON:

## NBR0864

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0864 SYNTAX ERROR

## NBR0865

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0865 APPLICATION '(&00)' NOT FOUND

## NBR0866

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0866 CONSOLE '(&00)' NOT FOUND

## NBR0868

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0868 (&00) SUPPRESSED MESSAGES

## NBR0869

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0869 (&00) SUPPRESSED MESSAGES IN SYSTEM

## NBR0870

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0870 MESSAGE '(&00)' NOT SUPPRESSED

## NBR0871

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0871 '/SHOW-MESS-SUPPR' NOT PROCESSED

## NBR0872

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR0872 MESSAGE '(&00)' SUPPRESSED

## NBR0873

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0873 NO SUPPRESSED MESSAGES

## NBR0874

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0874 MESSAGE (&00) WAS SUPPRESSED AT NONE OF THE SPECIFIED CONSOLES OR APPLICATIONS

### Meaning

- The message (&00) is suppressed at some of the consoles or
applications which are not mentioned within the command.
- The suppression of message (&00) remains unchanged.
- For more information please use the command
SHOW-MESSAGE-SUPPRESSION

## NBR0875

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR0875 DUE TO MEMORY SHORTAGE CURRENTLY NO FURTHER MESSAGES CAN BE MADE SUPPRESSABLE BY /SET-MESSAGE-SUPPRESSION

### Meaning

Due to memory shortage the table of suppressable messages cannot be
extended. The command /SET-MESSAGE-SUPPRESSION could be executed
partially only or not at all.

### Response

- Please enter the command /SHOW-MESSAGE-SUPPRESSION in order to
check whether and which modifications are done by the command
/SET-MESSAGE-SUPPRESSION .
- Please retry the command /SET-MESSAGE-SUPPRESSION later.

## NBR0876

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR0876 DUE TO MEMORY SHORTAGE IT IS CURRENTLY NOT POSSIBLE TO DISPLAY THE LIST OF MESSAGES WHICH ARE TO BE SUPPRESSED

### Response

Please retry the command /SHOW-MESSAGE-SUPPRESSION later.

## NBR0877

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR0877 TABLE LOCK NOT GRANTED. THE COMMAND COULD NOT BE EXECUTED

### Response

- Please retry the command later.
- If this message occurs permanently when entering some commands,
then please take a SLED.

## NBR0881

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0881 MAXIMUM NUMBER OF SUPPRESSABLE MESSAGES REACHED

### Meaning

The command /SET-MESSAGE-SUPPRESSION could be executed partially
only or not at all.

### Response

- Please list all suppressd messages by means of
/SHOW-MESSAGE-SUPPRESSION .
- So you can check whether or which modifications are done by
/SET-MESSAGE-SUPPRESSION .
- Please cancel the suppression of some message, whose suppression
is less urgent, with the command /RESET-MESSAGE-SUPPRESSION ,
before you retry the command /SET-MESSAGE-SUPPRESSION .

## NBR0882

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR0882 '/SET-MESS-SUPPR' NOT PROCESSED

## NBR0883

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0883 OPERAND 'CONSOLE' OR 'APPLICATION' MAY ONLY BE ISSUED FROM MAIN CONSOLE IF OPERATOR MODE 'WITHOUT LOGON'

## NBR0884

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0884 COMMAND PARTIALLY EXECUTED

## NBR0890

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0890 THE LAST FEW RECORDS OF THE CONSLOG FILE CAN'T BE READ

### Response

If this information is desired, repeat /TURN.

## NBR0891

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0891 BOURSE PROBLEM DURING PROCESSING OF /CHANGE-CONSLOG COMMAND, PLEASE CANCEL TASK '(&00)'

### Response

Enter /CANCEL-JOB to cancel task

## NBR0897

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0897 '/RESET-MESS-SUPPR' NOT PROCESSED

## NBR0898

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR0898 CMD RESERVED FOR CONSOLES

## NBR0901

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0901 ROUTING BOURSE PROBLEM IN 'ECCLP' - RUN-READ-TASK TERMINATED

## NBR0902

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0902 COMMAND BOURSE PROBLEM IN 'ECCLP' - RUN-READ-TASK TERMINATED

## NBR0903

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0903 RUN BOURSE PROBLEM IN 'ECCLP' - RUN-READ-TASK TERMINATED

## NBR0904

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0904 LAST POSSIBLE SERIAL NUMBER OF SYS.CONSLOG FILE REACHED. '/CHANGE-CONSLOG' NOT PROCESSED

### Meaning

A new logging file (SYS.CONSLOG) cannot be opened. The command is not
processed, because console logging is mandatory.

## NBR0905

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0905 CONSLOG INACTIVE

## NBR0906

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0906 CONSLOG WILL BE TERMINATED

## NBR0907

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR0907 COMMAND '(&00)' EXECUTED FOR CONSLOG FILE (&01)

## NBR0920

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0920 INVALID OPERAND VALUE IN '/MODIFY-CONS-OPTIONS'. (&00) VALUE '(&01)' USED

### Meaning

Invalid operand value for:
- 'UPDATE-INTERVAL='
- 'MESSAGE-REPLACE-RATE='
- 'QUEUE-WARNING='
- 'PROTECTED-LINES='
(&00): MAXIMUM or MINIMUM
(&01): value.

## NBR0921

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0921 MEMORY SHORTAGE. RETRY COMMAND LATER.

### Meaning

A $GETMEM could not be processed.

## NBR0922

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0922 '/MODIFY-CONS-OPTIONS' AS SPECIFIED ONLY PERMITTED FROM MAIN CONSOLE OR FROM AUTHORIZED USER PROCESS AND ONLY IF SYSTEM PARAMETER 'NBCONOPI = N'

### Meaning

If the system parameter 'NBCONOPI' is set to 'Y', the command /MODIFY-CON
SOLE-OPTIONS can only be entered at the concerned physical console. Then
the parameter 'C-U' within the command is superflouos

## NBR0923

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0923 THE COMMAND CONTAINS AN INVALID CONSOLE MNEMONIC. COMMAND NOT PROCESSED

### Meaning

Possible error reasons:
- The operating works with "logical" consoles. A "logical" console
consists of one (device types CONSFK, CON3027 or CON3027C) or two
devices. The two devices that build a logical console are: a display
(device type CON38) and a hardcopy (device type CON3803 or CON3888).
The name of a "logical" console consisting of two devices is the name
of the display. If the mnemonic mentioned in the command is the name of
a hardcopy, the command will be rejected.
- The command was entered by an application and contains no console
mnemonic (C-U=*OWN is the implicit value); an application, not being a
console, cannot change it's parameters. The command will be rejected.

## NBR0924

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0924 /M-C-O ENTERED FOR A CONSOLE WHOSE TYPE IS NOT CON38, BUT SOME OF IT'S PARAMETERS MAKE SENSE ONLY FOR THIS CONSOLE TYPE. COMMAND NOT OR INCOMPLETELY EXECUTED

### Meaning

The console type is not CON38; only the parameters U-I and Q-W are
meaningful for non CON38 consoles. If existent, these parameters will be
executed; all other parameters will be ignored.

## NBR0925

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0925 OPERAND VALUE 'F-H=NO' NOT ALLOWED

### Meaning

The class 2 option NBKOPPEL does not allow the use of the operand 'F-H=NO'
in /MODIFY-CONS-OPTIONS

## NBR0926

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0926 ERROR IN COMMAND SERVER. COMMAND NOT OR INCOMPLETELY PROCESSED

### Meaning

Possible reasons:
- An invalid function or version number or an invalid action code in macro
$NBMCMN
- The order could not be sent to the Console Driver Task KTT (error in the
$NBCCALL macro execution)
- The KTT return information about the execution of the command could not
be received (error in macro $NBRSIG)
- Invalid KTT return code
- KTT return code <> "Command completed" or "False HSI". Possible reasons:
a) The command server sent KTT an invalid order
b) The KTT order contained an invalid console mnemonic
In most of the above cases, the operands U-I and / or Q-W, if present,
could have been executed

## NBR0927

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0927 /MODIFY-CONS-OPTIONS COMMAND EXECUTION COMPLETED WITH ERRORS

### Meaning

The command has been executed, but operand M-R-R or P-L had an invalid
value, which has been replaced with a standard, correct value.

## NBR0928

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0928 THE /S-C-O COMMAND CANNOT SUPPLY ALL PARAMETER VALUES

### Meaning

The command was entered for a console of device type CON3027 or
CON3027C, for which only the parameters U-I and Q-W are relevant; this is
why no values are given for the other parameters

## NBR0940

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR0940 NO POINTER ON TCB OPERATOR AREA. COMMAND CANNOT BE EXECUTED.

## NBR0941

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR0941 I OP-BROADCAST I OP-MSG I SYSTEM-MSG I INFO-OUTPUT

## NBR0942

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR0942 (&00)(&01)(&02)(&03)

## NBR0950

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0950 SYNTAX ERROR: PARAMETER "TO=OPERATOR" NOT ALLOWED WHEN THE COMMAND COMES FROM A CONSOLE

## NBR0951

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0951 ERROR DURING RELEASE OF MEMORY IN 'ECCOSOUT'

### Meaning

Error occurred during the release of class 4 or class 5 memory (/TURN).

## NBR0952

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0952 CONSOLE LOGGING NOT POSSIBLE WITH CLASS 2 OPTION 'NBLOGENF' BEING SET: SYSTEM CRASH

### Meaning

The CLOG task cannot complete console logging. Class 2 option 'NBLOGENF'
forced a system crash. If the class 2 option had not been set, the system
would continue to work without console logging.

## NBR0953

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NBR0953 ERROR DURING CONSOLE LOGGING PROCESSING. SHOULD ANOTHER WRITE BE STARTED AFTER CORRECTING THE ERROR ? REPLY (R=RETRY; H=HALT=SYSTEM TERMINATION)

### Meaning

The operator can remove the error reason which prevented the CLOG task
from continuing the logging file (SYS.CONSLOG).
This is only possible if the class 2 option 'NBLOGENF' has been set.

### Response

R: the CLOG task retries console logging.
H: the CLOG task causes a system crash.

## NBR0954

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0954 MESSAGE FOR BATCH TASK WITH TSN '(&00)' NOT POSSIBLE

## NBR0960

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

NBR0960 MESSAGE (&00) ORDERED FOR TELESERVICE

## NBR0961

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NBR0961 NO MESSAGE ORDERED FOR TELESERVICE

## NBR0962

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NBR0962 MESSAGE (&00) WAS NOT ORDERED

## NBR0963

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0963 MSG ORDER FOR (&00) MUSTN'T BE REMOVED

## NBR0970

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0970 OPERATOR TASK WITH TSN '(&00)' CREATED FOR CONSOLE '(&01)'

## NBR0971

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR0971 SHUTDOWN IN PROCESS. NO OPERATOR TASK CREATION

### Meaning

After input of /SHUTDOWN GRADUALLY no further operator task is created.

## NBR0972

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0972 OPERATOR TASK WITH TSN '(&00)' CREATED FOR PROCESSING OF /RUN COMMAND SEQUENCES

## NBR0973

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0973 SYSTEM TASK CREATION FAILURE: SYSTEM TERMINATION

## NBR0974

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0974 OPERATOR TASK WITH TSN '(&00)': 'COMMUNICATION-INTERVAL-LIMIT' EXCEEDED FOR COMMAND '/(&01)' FROM CONSOLE '(&02)'

### Meaning

The Communication Interval Limit (CIL) for command processing in the
operator task has been exceeded. Processing continues in this task. For
further commands from this console a new operator task will be created.

## NBR0975

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0975 MEMORY REQUEST FAILURE. SYSTEM TERMINATION

## NBR0976

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0976 BOURSE CALL FAILURE: SYSTEM TERMINATION

## NBR0977

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0977 LOCK MANAGER CALL FAILURE: SYSTEM TERMINATION

## NBR0980

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0980 OPERATOR ROLE '(&01)' ASSIGNED TO OPERATOR ID '(&00)'

### Meaning

The operator ID has all authorizations defined in the operator ROLE.
(&00): operator ID.
(&01): operator ROLE.

## NBR0981

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0981 INPUT OF COMMAND '/(&00)' NOT PERMITTED FROM CONSOLE

### Meaning

In the current compatible mode for the system operating (system
parameter NBCONOPI=N), the authorization of the operator with
Operator-Roles is not supported for consoles.

## NBR0982

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0982 NO OPERATOR ID FOR APPLICATION '(&00)'

### Meaning

The command was entered by an authorized application with no operator ID.
(&00): application name.

## NBR0983

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0983 INTERNAL ERROR IN COMMAND SERVER OF '/(&00)'

### Meaning

(&00): command name

## NBR0984

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0984 OPERATOR ROLE '(&01)' REJECTED FOR OPERATOR ID '(&00)'. REASON: '(&02)'

### Meaning

(&02): 0, no authorization for this operator ROLE
1, invalid operator ID
2, invalid operator ROLE
?, other errors.

## NBR0985

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0985 OPERATOR ROLE '(&01)' ALREADY ASSIGNED TO OPERATOR ID '(&00)'

### Meaning

The operator ROLE was already successfully requested by the operator ID.
(&00): operator ID.
(&01): operator ROLE.

## NBR0986

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0986 OPERATOR ROLE '(&01)' NOT ASSIGNED TO OPERATOR ID '(&00)'

### Meaning

The operator ID doesn't have the authorizations of the specified
operator ROLE.
(&00): operator ID.
(&01): operator ROLE.

## NBR0987

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0987 NO OPERATOR-ROLE ASSIGNED TO OPERATOR ID '(&00)'

### Meaning

The operator ID doesn't have any authorization for an operator ROLE.
(&00): operator ID.

## NBR0988

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0988 OPERATOR ID '(&00)': ALL OPERATOR ROLES RELEASED

### Meaning

The operator ID has released all formerly assigned operator ROLES.
(&00): operator ID.

## NBR0989

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0989 OPERATOR ID '(&00)': NOT ALL REQUESTED OPERATOR ROLES ASSIGNED

### Meaning

Not all operator ROLEs mentioned in the list could be assigned to the
own operator ID.
(&00) operator ID.

## NBR0990

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0990 OPERATOR ID '(&00)': NOT ALL MENTIONED OPERATOR ROLES FOUND

### Meaning

Not all operator ROLEs mentioned in the list are assigned to the own
operator ID.
(&00) operator ID.

## NBR0991

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0991 INPUT OF COMMAND '/(&00)' NOT PERMITTED IN CMDFILE

## NBR0999

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR0999 MESSAGE SATURATION. INTERVAL MODE (M-R-R=7) IN USE FOR CONSOLE '(&00)'

### Meaning

The number of Store Queue Entries (SQE) waiting to be output on the
console (&00) is greater than half its permissible maximum. Therefore the
output speed is set to the maximum speed.
Message replace rate=7,
interval between two outputs=255 ms.

## NBR1000

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1000 COMMAND '/RUN' RECEIVED. RUN ID '(&00)' ASSIGNED

## NBR1001

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1001 RUN ID '(&01)'. READING OF /RUN COMMAND FILE '(&00)' STARTED

## NBR1002

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1002 RUN ID '(&01)'. FILE '(&00)' SPECIFIED IN COMMAND '/RUN' INVALID OR DOES NOT EXIST. COMMAND REJECTED

## NBR1003

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1003 RUN ID '(&00)'. READ ERROR DURING PROCESSING OF /RUN COMMAND SEQUENCE. READING ABORTED

### Meaning

Records which have been successfully read before the read error
occured will still be processed.

## NBR1004

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1004 RUN ID '(&00)'. READING OF /RUN COMMAND SEQUENCE INTERRUPTED BY COMMAND '/ASTOP'

## NBR1005

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1005 RUN ID '(&00)'. COMMAND '/AGOGO' MISSING. WAITING TIME ELAPSED. READING OF /RUN COMMAND SEQUENCE CONTINUES

## NBR1006

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1006 NO /RUN COMMAND SEQUENCE IN /ASTOP CONDITION. COMMAND '/AGOGO' IGNORED

## NBR1007

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1007 RUN ID '(&00)'. COMMAND '/AGOGO' ACKNOWLEDGED. PROCESSING OF /RUN COMMAND SEQUENCE CONTINUES

## NBR1008

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1008 RUN ID '(&00)'. COMMAND '/AGOGO' ACKNOWLEDGED. ANOTHER /AGOGO COMMAND EXPECTED

## NBR1009

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1009 THE FOLLOWING ROUTINGCODES ARE NOT ASSIGNED TO '*IPL': (&00)

### Meaning

Console display of messages sent via routing codes (&00) cannot be
guaranteed due to (possibly missing) DEFINE-CONSOLE- and SET-CODE-
Instructions in OPR parameter service. These messages might be written
to the logging file (SYS.CONSLOG.) only

### Response

1.) Non-displayed messages can be shown with /TURN
2.) Please check instructions in OPR parameter service before starting
the next session

## NBR1010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1010 THE FOLLOWING ROUTINGCODES ARE NOT ASSIGNED TO ANY PHYSICAL CONSOLES: (&00)

### Meaning

Console display of messages sent via routing codes (&00) cannot be
guaranteed due to (possibly missing) DEFINE-CONSOLE- and SET-CODE-
Instructions in OPR parameter service. These messages might be written
to the logging file (SYS.CONSLOG.) only

### Response

1.) The mentioned routing codes can be assigned to some consoles with
/ASR ADD,...
2.) Non-displayed messages can be shown with /TURN
3.) Please check instructions in OPR parameter service before starting
the next session

## NBR1011

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1011 RUN ID '(&01)'. RECORD '(&00)' READ

### Meaning

Record '(&00)' read from /RUN command sequence. RUN ID '(&01)'

## NBR1012

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1012 RUN ID '(&00)'. NUMBER OF /AGOGO-COMMANDS AWAITED IN /ASTOP-COMMAND CORRECTED TO (&01)

## NBR1013

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1013 USER NOT ALLOWED TO ACKNOWLEDGE THE CURRENT /RUN SEQUENCE. /AGOGO REJECTED

### Meaning

If the system parameter NBCONOPI is set to 'Y', a /RUN command sequence
may only be acknowledged, if the issuer of the /AGOGO has either the pri
vilege TSOS or the same operator id. as the issuer of the /RUN command

## NBR1014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1014 A /RUN CMD WAS ENTERRED FROM A CONSOLE WHICH HAS BECOME INACTIVE OR INOPERABLE. /RUN CMD NOT PROCESSED

### Meaning

If the system parameter NBCONOPI ist set to 'Y', /RUN sequences enterred
from consoles which became inactive or inoperable will not be started

## NBR1015

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1015 RUN-ID '(&00)': SPECIFIED /RUN COMMAND FILE IS NOT SHARABLE OR PROTECTED BY GUARDS. /RUN CMD NOT PROCESSED

### Meaning

The specified /RUN command file belongs to a foreign user and is
not sharable or protected by GUARDS even against reading access.

## NBR1016

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1016 RUN ID '(&00)': SPECIFIED /RUN COMMAND FILE IS LOCKED. TRY LATER

## NBR1017

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1017 RUN ID '(&00)': CATALOG NOT AVAILABLE. /RUN NOT PROCESSED

## NBR1018

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1018 RUN ID '(&00)': /RUN COMMAND FILE IS EMPTY. /RUN COMMAND IGNORED

## NBR1019

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1019 INCONSISTENT SQE CONCATENATION - SYSTEM TERMINATION

## NBR1020

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1020 $NBCCALL LINKAGE OR BOURSE PROBLEM DETECTED BY NBRCONS

## NBR1021

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1021 ERROR IN SQE RELEASE MECHANISM NBLOCK - SYSTEM TERMINATION

## NBR1022

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1022 THE SEARCHED MESSAGE IS JUST TO BE SENT ONTO CONSOLE - DIAGNOSTIC SYSTEM TERMINATION

### Meaning

The message number looked for by a diagnostic Rep in module ECTYP is
just to be sent onto console. The system will be terminated in order
to find the issuer of the message in the SLED

## NBR1030

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1030 THE SET OF AUTHORIZATION-CODES MUST NOT BE MODIFIED FOR OR BY AUTHORIZED APPLICATIONS WITH DYNAMIC AUTHORIZATION NAMES. /ASR CMD REJECTED

## NBR1031

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1031 '/ASR' COMMAND ONLY PARTIALLY EXECUTED, SINCE IT CONTAINS SOME ILLEGAL ACTIONS CONCERNING AUTHORIZED APPLICATIONS WITH DYNAMIC AUTHORIZATION NAMES

## NBR1032

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1032 FILTER FOR AUTHORIZED APPLICATIONS WITH DYNAMIC AUTHORIZATION NAMES MAY ONLY BE MODIFIED BY THEMSELVES. /ASR COMMAND REJECTED

## NBR1033

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1033 '/ASR' FUNCTION 'MAIN' IS NO LONGER SUPPORTED. PLEASE USE COMMAND '/REQUEST-MAIN-CONSOLE-FUNCTIONS'

## NBR1034

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1034 '/ASR' FUNCTION 'DESTINATION' IS NO LONGER SUPPORTED. PLEASE USE COMMAND '/SHOW-SYSTEM-PARAMETERS' AND LOOK FOR SYSTEM PARAMETER 'MSGDEST'

## NBR1035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1035 THIS OPERAND COMBINATION IN '/ASR' COMMAND IS ILLEGAL WHEN SYSTEM PARAMETER 'NBCONOPI' IS SET TO 'Y'

## NBR1036

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1036 THIS OPERAND COMBINATION IN '/ASR' COMMAND CAN ONLY BE PARTIALLY EXECUTED DUE TO SYSTEM PARAMETER 'NBCONOPI = Y'

## NBR1042

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1042 CLASS 5 MEMORY SHORTAGE. COMMAND (&00) NOT PROCESSED. NO FILTERS CAN BE USED

## NBR1043

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1043 /MODIFY-CONSOLE-OPTIONS NOT ALLOWED FOR APPLICATIONS SINCE SYSTEM PARAMETER 'NBCONOPI' IS SET TO 'Y'

## NBR1050

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1050 APPLICATION '(&00)' HAS NO CODES

## NBR1051

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1051 APPLICATION '(&00)' CODES: (&01)

## NBR1052

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1052 CONSOLE '(&00)' ASSIGNED CODES: (&01)

## NBR1053

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1053 CONSOLE '(&00)' TEMPORARY CODES: (&01)

## NBR1054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1054 CONSOLE '(&00)' IMPLICIT CODES: (&01)

## NBR1055

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1055 CONSOLE '(&00)' HAS NO ASSIGNED CODES

## NBR1056

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1056 TASK '(&00)' HAS NO CODES

## NBR1057

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1057 TASK '(&00)' CODES: (&01)

## NBR1058

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1058 /SHOW-CONSOLE-STATUS: (&00) FURTHER APPLICATIONS WITH DYNAMICAL AUTHORIZATION NAMES ARE NOT CONNECTED

## NBR1060

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1060 ROUTING-CODE '(&00)' NOT ASSIGNED

## NBR1061

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1061 ROUTING-CODE '(&00)' FILTER NONE

## NBR1062

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1062 ROUTING-CODE '(&00)' FILTER: (&01)

## NBR1063

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1063 FILTER (&00) ROUTING-CODES: (&01)

## NBR1064

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1064 FILTER (&00) ROUTING-CODES NONE

## NBR1065

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1065 ALL FILTERS ROUTING-CODES: (&00)

## NBR1066

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1066 ALL FILTERS ROUTING-CODES NONE

## NBR1070

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : YES

NBR1070 'CONSOLE=*OWN' RESTRICTED TO CONSOLES

## NBR1071

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1071 MAIN CONSOLE IS '(&00)'

## NBR1072

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1072 CONSOLE '(&00)' DOES NOT EXIST

## NBR1073

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : YES

NBR1073 NONE OF THE CONSOLE NAMES IN '/SHOW-CONSOLE-STATUS' FOUND. CMD REJECTED

## NBR1074

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : YES

NBR1074 SOME CONSOLE NAMES IN '/SHOW-CONSOLE-STATUS' NOT FOUND. CMD ONLY EXECUTED PARTIALLY

## NBR1075

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1075 APPLICATION '(&00)' PROCESSOR '(&01)' STATION '(&02)'

## NBR1076

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1076 APPLICATION '(&00)' STATES: (&01)

## NBR1077

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1077 CONSOLE '(&00)' STATES: (&01)

## NBR1078

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1078 CONSOLE '(&00)' OPERATOR-ID '(&01)'

## NBR1079

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1079 APPLICATION '(&00)' OPERATOR-ID '(&01)'

## NBR1080

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1080 CMD RESTRICTED TO PHYSICAL CONSOLES

## NBR1081

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1081 THIS CONSOLE IS THE MAIN CONSOLE. '/REQUEST-MAIN-CONSOLE-FUNCTIONS' IGNORED

## NBR1082

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1082 '/REQUEST-MAIN-CONSOLE-FUNCTIONS' REJECTED BY THE MAIN CONSOLE

## NBR1083

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1083 '/REQUEST-MAIN-CONSOLE-FUNCTIONS' BUSY. TRY LATER

## NBR1084

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1084 '/REQUEST-MAIN-CONSOLE-FUNCTIONS' FAILED DUE TO MEMORY OR TASK SATURATION

## NBR1085

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1085 ALLOW '(&00)' TO BECOME MAIN CONSOLE? REPLY (Y=YES, N=NO)

## NBR1099

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1099 THE PARAMETER 'SYSLST' CANNOT BE USED BY CONSOLES

## NBR1111

Destination: CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1111 NO OUTPUT OF COMMAND/SERVER-CONNECTION(S), SET OF CONNECTIONS EMPTY

## NBR1112

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1112 NO COMMAND/SERVER CONNECTION, SPECIFIED ENTRY NAME NOT KNOWN AS SYMBOL FOR AN ENTRY ADDRESS

## NBR1113

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1113 NO COMMAND/SERVER CONNECTION, COMMAND HAS ALREADY MAXIMUM NUMBER OF CONNECTIONS

## NBR1114

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1114 NO COMMAND/SERVER DISCONNECTION, COMMAND/SERVER CONNECTION DOES NOT EXIST OR SERVER HAS STATIC DEFINITION

## NBR1115

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1115 SEMANTICAL OPERAND ERROR

## NBR1116

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1116 INTERNAL ERROR. INFORMATION FOR DIAGNOSTIC WRITTEN

## NBR1117

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1117 COMMAND NAME '(&00)' NOT USABLE AS SAME-NAME

### Meaning

Command name (&00) cannot be used as SAME-NAME because it is already
otherwise in use or it is not shorter than the related command name.

## NBR1118

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1118 COMMAND /CONNECT-CMD-SERVER PROCESSED SUCCESSFULLY, BUT AT LEAST ONE SAME-NAME WAS REJECTED

### Meaning

/CONNECT-CMD-SERVER was processed successfully. But at least one
command name specified as SAME-NAME was rejected because it is already
otherwise in use.

## NBR1119

Destination: CONSOLE Routing code: K Weight: 99

Warranty : NO

NBR1119 COMMAND /CONNECT- OR /DISCONNECT-CMD-SERVER DOES NOT COME FROM A $CONSOLE APPLICATION

### Meaning

The commands /CONNECT-CMD-SERVER or /DISCONNECT-CMD-SERVER cannot be
entered from a physical console, but only from $CONSOLE applications.

## NBR1121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBR1121 OPERATOR-TASK COULD NOT BE CONNECTED TO SUBSYSTEM SDF

### Meaning

During the first processing of a command in an operator task, the
subsystem SDF could not be connected. The command was aborted.

### Response

Please inform your system administrator.

## NBR1122

Destination: CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1122 USE /HELP-MSG-INFORMATION MSG-IDENTIFICATION=NBR1123 FOR EXPLANATION OF OUTPUT

## NBR1123

Destination: CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1123 STRUCTURE OF OUTPUT OF /SHOW-CMD-ATTRIBUTES:

### Meaning

! Command !C!P!T!M! Server !CIL!A!P!
+-------------+ ! ! ! ! ! ! ! !
! Auth.-Code ! ! ! ! ! ! ! !
+---------------+ ! ! ! ! ! ! !
! Password P=yes ! ! ! ! ! ! !
! possible N=no ! ! ! ! ! ! !
+-----------------+ ! ! ! ! ! !
! Type I=int E=ext ! ! ! ! ! !
+-------------------+ +-----------+ ! ! !
! Method of call ! ! ! !
! D=direct S=SDF $=$CONSOLE ! ! ! !
! - =not available ! ! ! !
+---------------------------------+ ! ! !
! Comm.-Interval Unit = 5 seconds ! ! !
+-------------------------------------+ ! !
! Administrability A=yes N=no ! !
+---------------------------------------+ !
! Priority of server 1=max 4=min !
+-----------------------------------------+

## NBR1124

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1124 COMMAND /CONNECT-CMD-SERVER WITH OPERAND COMPLETION-CONTROL=YES DOES NOT COME FROM APPLICATION WITH $CONSOLE-INTERFACEVERSION 2

## NBR1125

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1125 COMMAND COMPLETED BUT AUTHORIZATION-CODE AND / OR SAME-NAME IGNORED

### Meaning

Authorization code and / or command synonyms can be used only at first
definition

## NBR1199

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1199 INTERNAL SYSTEM ERROR IN UCON-TASK

### Meaning

During the processing of an operator command input from an user-task
a serious system error occured in the UCON-task.

### Response

Please take a SLED and contact your customer support.

## NBR1200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1200 TASK '(&01)' FOR OPERATOR '(&00)' CONNECTED TO SUBSYSTEM OPERATING

### Meaning

The connection to the subsystem operating was successfully completed for
the task (&01) of operator (&00). The SCI is available for this task.

## NBR1201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1201 TASK '(&01)' OF OPERATOR '(&00)' DISCONNECTED FROM SUBSYSTEM OPERATING

### Meaning

The connection to the subsystem Operating of the task (&01) of operator
(&00) is lost. The SCI is no longer available for this task.

## NBR1202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1202 '(&00)' PARAM SETS FOR CONSOLES ONLY ALLOWED FOR *IPL

## NBR1203

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1203 OPERAND 'REPLACEMENT' IN 'DEFINE-CONSOLE' PARAMETER SET IGNORED

## NBR1206

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 66

Warranty : NO

NBR1206 COMMAND CODE '@' FOR COMMAND (&00) MANDATORY

## NBR1207

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 66

Warranty : NO

NBR1207 SET-CODE PARAMETER ONLY FOR IPL CONSOLE ALLOWED

## NBR1210

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1210 ERROR IN THE COMMUNICATION PROTOCOL BETWEEN USER-TASK AND UCON-TASK

### Meaning

An error occured in the communication protocol between user-task (SCI)
and UCON-Task.

### Response

Please repeat your command input.

## NBR1211

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1211 THE USER-TASK COULD NOT BE CONNECTED WITH UCON

### Meaning

The user-task could not be connected to UCON task. The connection is
necessary for the processing of the entered command.

### Response

Please save your SERSLOG-file and contact your customer support.

## NBR1212

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1212 INTERNAL ERROR DURING COMMAND PROCESSING

### Meaning

An internal error occured during the common processing of an operator-
command in the user-task.

### Response

Please save your SERSLOG-File and contact your customer support.

## NBR1213

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1213 BOURSE EVENT FROM UCON-TASK FOR USER-TASK LOST

### Meaning

A bourse event for the user-task was lost during the communication
between UCON-task and user-task. The processing of the command was
aborted.

### Response

Please repeat your command input.

## NBR1214

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1214 REPLY COULD NOT BE SENT TO THE SENDER OF THE PENDING MESSAGE

### Meaning

The reply entered for the pending message as a part of the command
dialog could not be sent to the origin of the pending message. The
command processing was aborted.

### Response

Please repeat your command input.

## NBR1215

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR1215 INPUT COMMAND STRING EXCEEDS ALLOWED LENGTH

### Meaning

The input command string exceeds the length of 2044 characters,
which is the maximal length for commands processed by the program
interface CMD.

### Response

Please repeat your command input using abbreviations.

## NBR1216

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1216 THE BCAM APPLICATION '$CONSOLE' COULD NOT BE ENABLED. 'ENABAP' RETURNCODE '(&00)'

## NBR1217

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR1217 ENABLING THE BCAM-APPLICATION '$CONSOLE' WILL BE RETRIED

## NBR1300

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR1300 PLAM VERSION (&00) USED FOR READING A /RUN PROCEDURE FROM LIBRARY

## NBR1301

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1301 PROCESSING OF /RUN COMMAND ABORTED. DURING PROCESSING OF PLAM MACRO '(&00)' THE RETURNCODE (&01) OCCURED. RUN-ID '(&02)'

### Meaning

A bad returncode (&01) occurred during execution of the
PLAM macro '(&00)'. The processing of the /RUN command was
aborted. Concerned RUN-ID '(&02)'.

### Response

An explanation of the received PLAM returncode can be displayed
with '/HELP PLA(&01)' .
Please ask the system administrator to check the contents
and status of the library.

## NBR1302

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

NBR1302 READING ELEMENT '(&00)' OF LIBRARY '(&01)' STARTED. RUN-ID '(&02)'

## NBR1303

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1303 RUN ID '(&00)': THE LIBRARY-ELEMENT SPECIFIED IN /RUN COMMAND IS EMPTY OR DOES NOT CONTAIN ANY RECORDS OF THE EXPECTED RECORD TYPE

### Meaning

The library-element specified in the /RUN command is empty or does
only contain records which do not belong to the expected record type.
Only records with format A and record type 1 will be read and
processed.

## NBR1304

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1304 RUN ID '(&00)'. THE LIBRARY ELEMENT SPECIFIED IN /RUN COMMAND IS LOCKED. PLEASE TRY COMMAND LATER

## NBR1305

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1305 RUN-ID (&00): THE LIBRARY SPECIFIED IN /RUN COMMAND DOES NOT EXIST

### Meaning

The library specified in /RUN command does not exist.

### Response

Please check also the cat-ID, user-ID and the availability
of the catalogue.

## NBR1306

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1306 THE LIBRARY SPECIFIED IN /RUN COMMAND EXISTS AS FILE, BUT IS NOT A LIBRARY

### Meaning

The file specified as library in the /RUN command exists, but is
not a library.

### Response

Please check the file attributes.

## NBR1307

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1307 RUN ID '(&00)': LIBRARY-ELEMENT IN /RUN COMMAND NOT FOUND

### Meaning

The library specified in /RUN command exists, but the specified
element cannot be found in the library.
Possible reasons:
- The element does not exist.
- The element-type is different from 'J'.
- The library is empty.

### Response

- Please ask the system administrator to check the contents of
the library.

## NBR1308

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1308 RUN-ID '(&00)': PASSWORD FOR LIBRARY IN /RUN COMMAND MISSING OR WRONG OR OTHER MISSING AUTHORIZATION

## NBR1309

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR1309 RUN-ID '(&00)': PLAM NOT AVAILABLE. /RUN COMMAND WITH LIBRARY CURRENTLY NOT POSSIBLE

### Meaning

The access method PLAM is currently not available. So /RUN commands
can only be processed if they do not use any libraries.

### Response

Please contact the system administrator.
When PLAM is available again, the /RUN command can be repeated.

## NBR1310

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1310 RUN-ID '(&00)': THE FOREIGN LIBRARY SPECIFIED WITHIN /RUN COMMAND IS NOT SHARABLE OR PROTECTED BY GUARDS. COMMAND REJECTED

### Meaning

The library or file specified in /RUN command belongs to a foreign
user and is either not sharable or protected by GUARDS against
reading access. The command cannot be processed.
Furthermore, it was to not possible to check whether the file
specified as library is really a library.

### Response

Please contact the owner of the library or file.

## NBR1311

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1311 PLAM VERSION (&00) TOO OLD. /RUN COMMAND REJECTED

### Meaning

The used PLAM version (&00) is too old and not supported by the
/RUN command. The minimum PLAM Version is V3.4A. So /RUN commands
can only be processed if they do not use any library.

### Response

Please contact the system administrator.

## NBR1312

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR1312 THE LIBRARY SPECIFIED IN /RUN COMMAND IS MIGRATED.

### Meaning

In order to avoid waiting times in the operating the /RUN command
was not processed.

### Response

Please ask the owner or the system administrator for making the
library available again.

## NBR2000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR2000 MEMORY SATURATION. CMD NOT PROCESSED

## NBR3000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3000 SYSTEM EVENT STREAM FILE '(&00)' OPENED

### Meaning

The System Event Stream File '(&00)' was opened during the
successful initialization of the System Event Stream Task (SEST).

## NBR3001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3001 SYSTEM EVENT STREAM FILE '(&00)' REOPENED AFTER SUCCESSFUL RECOVERY OF SEST

### Meaning

The System Event Stream File '(&00)' was reopened after the
successful recovery of the System Event Stream Task (SEST).

## NBR3002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3002 EVENT STREAM SERVICE TERMINATED NORMALLY

### Meaning

The Event Stream Service was terminated normally during system
shutdown.

## NBR3010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3010 INITIALIZATION ERROR IN SEST. SYSTEM ESS NOT AVAILABLE.

### Meaning

A serious error occured during the initialization of the System
Event Stream Task (SEST). ESS is not available during this session.

### Response

Please contact your customer support.

## NBR3011

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3011 RECOVERY ERROR IN SEST. SYSTEM ESS NOT AVAILABLE ANY MORE

### Meaning

A serious error occured during the task recovery of the System
Event Stream Task (SEST). ESS for System Event Streams is no more
available during this session.

### Response

Please contact your customer support.

## NBR3012

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3012 INITIALIZATION ERROR IN UEST '(&00)' OF USER ID '(&01)'

### Meaning

A serious error occured during the initialization of the User
Event Stream Task '(&00)' for user-id '(&01)'.

### Response

Please contact your system administrator.

## NBR3013

Destination: CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

NBR3013 ERROR IN ESS. ES-TASK TERMINATED ABNORMALLY

### Meaning

A serious error occured during the ESS-processing. The ES-task
was terminated abnormally.

### Response

Please contact your customer support.

## NBR3014

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3014 TERMINATION ERROR IN UEST '(&00)' OF USER ID '(&01)'

### Meaning

A serious error occured during the task termination of the User
Event Stream Task '(&00)' of user id '(&01)'.

### Response

Please contact your system administrator.

## NBR3015

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

NBR3015 SPACE REORGANIZATION FOR SYSTEM EVENT STREAM FILE '(&00)' PROCESSED

### Meaning

The space reorganization of the System Event Stream File is processed
because the size of file has already reached the size set by the value of
the class-2-system-parameter NBESSIZE.
The reorganization consists in elimination of the oldest records of the
file.

### Response

The size of the System Event Stream File during a session depends
directly on the amount of produced system events and the setting of
synchronous events to be logged for all assigned event streams of type
system (command /ASSIGN-SYSEVENT ..., ADD-SYNCH-EVENTS=...).

## NBR3016

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3016 PERMANENT DMS ERROR '(&00)' DURING PROCESSING OF THE SYSTEM EVENT STREAM FILE (R=RETRY / T=TERMINATE) ?

### Meaning

A permanent DMS error occured during the processing of the SYSTEM EVENT
STREAM file. Accepted replies:
R=RETRY: Retry the DMS function after error processing i.e. task
recovery (default value).
T=TERMINATE: Terminate the processing of the SYSTEM EVENT STREAM file.
The System Event Stream Service is no longer available
in the current session.

### Response

Take appropriate action to eliminate the reason for the DMS error.
Answer with T=TERMINATE, if the DMS error can't be eliminated.
Ignoring this situation may lead to serious shortages of system memory.

## NBR3017

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3017 DMS ERROR '(&00)' DURING PROCESSING OF THE PUT-MACRO FOR EVENT STREAM FILE: (&01)

### Meaning

During the processing of the PUT macro for the EVENT STREAM file the
specified DMS errors occured.
The internal error recovery was started.

### Response

Take appropriate action to eliminate the error situation if possible.

## NBR3018

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR3018 DMS ERROR '(&00)' DURING ACCESSING EVENT STREAM FILE: (&01)

### Meaning

During an access to the EVENT STREAM file the specified DMS error
occured.
The internal error recovery was started.

### Response

Please take an appropriate action to eliminate the error situation
if possible.

## NBR3020

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3020 *** TASK RECOVERY FOR TASK 'SEST' SUCCESSFULLY PROCESSED ***

### Meaning

The task recovery of the System Event Stream Task 'SEST' was
successfully processed, after abnormal task termination due to an
internal error.

### Response

Please contact your customer support.

## NBR3021

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3021 *** TIME SWITCH TO/FROM DAYLIGHT SAVING TIME TOOK PLACE ***

### Meaning

In the meantime between logging of the previous and the actual record
the seasonal time switch to daylight saving time (or viceversa) took
place.

## NBR3022

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3022 INITIALIZATION ERROR IN UEST

### Meaning

A serious error occured during the initialization of the User
Event Stream Task.

### Response

Please contact your system administrator.

## NBR3100

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3100 EVENT STREAM '(&00)' WITH TSN '(&01)' ASSIGNED TO USER TASK '(&02)'

### Meaning

Due to the command /ASSIGN-SYSEVENT the event stream '(&00)'
was assigned to user-task '(&02)'.

### Response

With /ASSIGN-SYSEVENT TO=*DUMMY the assignment can be lifted.

## NBR3102

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3102 AMBIGUOUS LOG-ID '(&00)' FOR EVENT STREAM

### Meaning

The selected LOG-ID for the event stream is ambiguous.

### Response

Select other LOG-ID when entering the command /ASSIGN-SYSEVENT.

## NBR3103

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3103 NO EVENT STREAM ASSIGNED

### Meaning

No event stream is currently assigned to the own user task.

### Response

For assignment of an event stream enter the command /ASSIGN-SYSEVENT.

## NBR3104

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3104 NO EVENT STREAM MATCHES THE SELECTION CRITERIA

## NBR3105

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3105 NO EVENT STREAM EXISTENT

## NBR3106

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3106 EVENT STREAM '(&00)' ALREADY ASSIGNED, OPERAND OPEN-MODE=*CREATE REJECTED

### Meaning

An already existing event stream can't be assigned with OPEN-MODE=*CREATE.

### Response

Try the assignment with OPEN-MODE=*OUTPUT or OPEN-MODE=*EXTEND.

## NBR3107

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3107 USER EVENT STREAM FILE '(&00)' LOCKED, COMMAND REJECTED

### Meaning

The user event stream file '(&00)' is currently locked and can't
be reopened.

### Response

Check if any presentation function of ESS has opened the file

## NBR3108

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3108 EVENT STREAM '(&00)' DOES NOT EXIST

## NBR3110

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3110 EVENT STREAM '(&00)' CLOSED FOR TASK '(&02)' WITH USER ID '(&01)'

## NBR3111

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3111 ERROR IN CREATION OF UEST

## NBR3112

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3112 SYSTEM EVENT STREAM TASK 'SEST' NOT EXISTENT

### Meaning

The ESS is not available for system event streams during this
session, because the task 'SEST' does not exist any more.

## NBR3113

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3113 NO EVENT STREAM ASSIGNED, BECAUSE OF /SHUTDOWN QUIET IN PROCESS

### Meaning

No new event stream will be assigned after the input of command
/SHUTDOWN QUIET.

## NBR3114

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3114 REQUESTED ES-FILE '(&00)' NOT CATALOGUED

### Meaning

The ES-File of the mentioned event stream is not catalogued, i.e.
the presentation of the event stream is not possible. The reason
is the recent termination of the event stream.

## NBR3115

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3115 SUBSYSTEM FHS-TPR NOT AVAILABLE

### Meaning

The subsystem FHS-TPR is not available. The presentation service was
terminated, because a preparation of output masks is not possible in
the moment.

## NBR3116

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3116 LIBRARY CONTAINING NECESSARY FHS-MASKS NOT FOUND

### Meaning

The Filename of the FHS-mask-library of the subsystems BS2CP and/or
FHS-TPR is invalid. The installation path couldn't be found neither with
IMON nor on the standard installation path (user-id TSOS).

### Response

Please contact your system administrator.

## NBR3199

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NBR3199 INTERNAL ERROR IN COMMAND SERVER

## NBR4711

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBR4711 '(&00)' ERROR IN MODULE '(&01)'. RETURN CODE '(&02)'

## NBR4712

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR4712 '(&00)' ERROR IN MODULE NBOFILT - SERSLOG ENTRY WRITTEN

## NBR4713

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR4713 '(&00)' ERROR IN MODULE NBOCSTA - SERSLOG ENTRY WRITTEN

## NBR4714

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR4714 '(&00)' ERROR IN MODULE NBOMFRA - SERSLOG ENTRY WRITTEN

## NBR4715

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

NBR4715 '(&00)' ERROR IN MODULE NBORUNP - SERSLOG RECORD WRITTEN

©2020 Fujitsu Technology Solutions GmbH | BS2000 OSD/BC System Messages